diff --git a/arch/arm/dts/Makefile b/arch/arm/dts/Makefile
index f8f52943..a56b820a 100644
--- a/arch/arm/dts/Makefile
+++ b/arch/arm/dts/Makefile
@@ -119,6 +119,7 @@ dtb-$(CONFIG_ROCKCHIP_RK3368) += \
 	rk3368-px5-evb.dtb \
 
 dtb-$(CONFIG_ROCKCHIP_RK3399) += \
+	rk3399-clockworkpi-a06.dtb \
 	rk3399-evb.dtb \
 	rk3399-ficus.dtb \
 	rk3399-firefly.dtb \
diff --git a/arch/arm/dts/rk3399-clockworkpi-a06.dts b/arch/arm/dts/rk3399-clockworkpi-a06.dts
new file mode 100644
index 00000000..9717c1c7
--- /dev/null
+++ b/arch/arm/dts/rk3399-clockworkpi-a06.dts
@@ -0,0 +1,165 @@
+/*
+ * (C) Copyright 2016 Rockchip Electronics Co., Ltd
+ *
+ * SPDX-License-Identifier:     GPL-2.0+
+ */
+
+/dts-v1/;
+#include <dt-bindings/pwm/pwm.h>
+#include <dt-bindings/pinctrl/rockchip.h>
+#include "rk3399.dtsi"
+#include "rk3399-opp.dtsi"
+
+/ {
+	model = "Clockworkpi A06";
+	compatible = "clockwork,devterm-a06", "rockchip,rk3399";
+
+	chosen {
+		stdout-path = "serial2:1500000n8";
+	};
+
+	vdd_center: vdd-center {
+		compatible = "pwm-regulator";
+		pwms = <&pwm3 0 25000 1>;
+		regulator-name = "vdd_center";
+		regulator-min-microvolt = <800000>;
+		regulator-max-microvolt = <1400000>;
+		regulator-init-microvolt = <950000>;
+		regulator-always-on;
+		regulator-boot-on;
+		status = "okay";
+	};
+
+	vccsys: vccsys {
+		compatible = "regulator-fixed";
+		regulator-name = "vccsys";
+		regulator-boot-on;
+		regulator-always-on;
+	};
+
+	vcc3v3_sys: vcc3v3-sys {
+		compatible = "regulator-fixed";
+		regulator-name = "vcc3v3_sys";
+		regulator-always-on;
+		regulator-boot-on;
+		regulator-min-microvolt = <3300000>;
+		regulator-max-microvolt = <3300000>;
+	};
+
+	vcc_phy: vcc-phy-regulator {
+		compatible = "regulator-fixed";
+		regulator-name = "vcc_phy";
+		regulator-always-on;
+		regulator-boot-on;
+	};
+
+	vcc5v0_host: vcc5v0-host-en {
+		compatible = "regulator-fixed";
+		regulator-name = "vcc5v0_host";
+		gpio = <&gpio4 25 GPIO_ACTIVE_HIGH>;
+	};
+
+	vcc5v0_typec0: vcc5v0-typec0-en {
+		compatible = "regulator-fixed";
+		regulator-name = "vcc5v0_typec0";
+		gpio = <&gpio1 3 GPIO_ACTIVE_HIGH>;
+	};
+
+	vcc5v0_typec1: vcc5v0-typec1-en {
+		compatible = "regulator-fixed";
+		regulator-name = "vcc5v0_typec1";
+		gpio = <&gpio1 4 GPIO_ACTIVE_HIGH>;
+	};
+
+	clkin_gmac: external-gmac-clock {
+		compatible = "fixed-clock";
+		clock-frequency = <125000000>;
+		clock-output-names = "clkin_gmac";
+		#clock-cells = <0>;
+	};
+
+};
+
+&saradc {
+	status = "okay";
+};
+
+&sdmmc {
+	bus-width = <4>;
+	status = "okay";
+};
+
+&sdhci {
+	bus-width = <8>;
+	mmc-hs400-1_8v;
+	mmc-hs400-enhanced-strobe;
+	non-removable;
+	status = "okay";
+};
+
+&uart2 {
+	status = "okay";
+};
+
+&usb_host0_ehci {
+	status = "okay";
+};
+
+&usb_host0_ohci {
+	status = "okay";
+};
+
+&usb_host1_ehci {
+	status = "okay";
+};
+
+&usb_host1_ohci {
+	status = "okay";
+};
+
+&i2c0 {
+	status = "okay";
+	clock-frequency = <400000>;
+	i2c-scl-falling-time-ns = <50>;
+	i2c-scl-rising-time-ns = <100>;
+	u-boot,dm-pre-reloc;
+
+	rk808: pmic@1b {
+		compatible = "rockchip,rk808";
+		clock-output-names = "xin32k", "wifibt_32kin";
+		interrupt-parent = <&gpio0>;
+		interrupts = <4 IRQ_TYPE_LEVEL_LOW>;
+		pinctrl-names = "default";
+		pinctrl-0 = <&pmic_int_l>;
+		reg = <0x1b>;
+		rockchip,system-power-controller;
+		#clock-cells = <1>;
+		u-boot,dm-pre-reloc;
+		status = "okay";
+
+		vcc12-supply = <&vcc3v3_sys>;
+
+		regulators {
+			vcc33_lcd: SWITCH_REG2 {
+				regulator-always-on;
+				regulator-boot-on;
+				regulator-name = "vcc33_lcd";
+			};
+		};
+	};
+};
+
+&pinctrl {
+	pmic {
+		pmic_int_l: pmic-int-l {
+			rockchip,pins =
+				<1 21 RK_FUNC_GPIO &pcfg_pull_up>;
+		};
+
+		pmic_dvs2: pmic-dvs2 {
+			rockchip,pins =
+				<1 18 RK_FUNC_GPIO &pcfg_pull_down>;
+		};
+	};
+};
+
diff --git a/configs/clockworkpi-a06-rk3399_defconfig b/configs/clockworkpi-a06-rk3399_defconfig
new file mode 100644
index 00000000..d2003073
--- /dev/null
+++ b/configs/clockworkpi-a06-rk3399_defconfig
@@ -0,0 +1,53 @@
+CONFIG_ARM=y
+CONFIG_ARCH_ROCKCHIP=y
+CONFIG_SYS_TEXT_BASE=0x00200000
+CONFIG_NR_DRAM_BANKS=1
+CONFIG_ENV_OFFSET=0x3F8000
+CONFIG_ROCKCHIP_RK3399=y
+CONFIG_TARGET_EVB_RK3399=y
+CONFIG_DEBUG_UART_BASE=0xFF1A0000
+CONFIG_DEBUG_UART_CLOCK=24000000
+CONFIG_DEFAULT_DEVICE_TREE="rk3399-clockworkpi-a06"
+CONFIG_DEBUG_UART=y
+CONFIG_DEFAULT_FDT_FILE="rockchip/rk3399-clockworkpi-a06.dtb"
+CONFIG_MISC_INIT_R=y
+# CONFIG_DISPLAY_CPUINFO is not set
+CONFIG_DISPLAY_BOARDINFO_LATE=y
+# CONFIG_SPL_RAW_IMAGE_SUPPORT is not set
+CONFIG_SPL_STACK_R=y
+CONFIG_SPL_STACK_R_MALLOC_SIMPLE_LEN=0x10000
+CONFIG_TPL=y
+CONFIG_CMD_BOOTZ=y
+CONFIG_CMD_GPT=y
+CONFIG_CMD_MMC=y
+CONFIG_CMD_USB=y
+# CONFIG_CMD_SETEXPR is not set
+CONFIG_CMD_TIME=y
+CONFIG_SPL_OF_CONTROL=y
+CONFIG_OF_SPL_REMOVE_PROPS="pinctrl-0 pinctrl-names clock-names interrupt-parent assigned-clocks assigned-clock-rates assigned-clock-parents"
+CONFIG_ENV_IS_IN_MMC=y
+CONFIG_SYS_RELOC_GD_ENV_ADDR=y
+CONFIG_ROCKCHIP_GPIO=y
+CONFIG_SYS_I2C_ROCKCHIP=y
+CONFIG_MMC_DW=y
+CONFIG_MMC_DW_ROCKCHIP=y
+CONFIG_MMC_SDHCI=y
+CONFIG_MMC_SDHCI_ROCKCHIP=y
+CONFIG_PMIC_RK8XX=y
+CONFIG_REGULATOR_RK8XX=y
+CONFIG_RAM_RK3399_LPDDR4=y
+CONFIG_BAUDRATE=1500000
+CONFIG_DEBUG_UART_SHIFT=2
+CONFIG_SYSRESET=y
+CONFIG_USB=y
+CONFIG_USB_XHCI_HCD=y
+CONFIG_USB_XHCI_DWC3=y
+CONFIG_USB_EHCI_HCD=y
+CONFIG_USB_EHCI_GENERIC=y
+CONFIG_USB_KEYBOARD=y
+CONFIG_DM_VIDEO=y
+CONFIG_DISPLAY=y
+CONFIG_VIDEO_ROCKCHIP=y
+CONFIG_DISPLAY_ROCKCHIP_HDMI=y
+CONFIG_SPL_TINY_MEMSET=y
+CONFIG_ERRNO_STR=y
