(module QFN48 (layer F.Cu) (tedit 5FC2AEB8)
  (descr "<b>Quad Flat No-Lead Package (QFN), 48 Pins, Exposed Pad, 6 x 6 Body</b>")
  (fp_text reference U5 (at 0 0 -270) (layer F.SilkS)
    (effects (font (size 0.57912 0.57912) (thickness 0.115824)) (justify left bottom))
  )
  (fp_text value AXP209 (at -3.81 5.08 -180) (layer F.Fab)
    (effects (font (size 0.77216 0.77216) (thickness 0.061772)) (justify left bottom))
  )
  (fp_line (start -3 -3) (end 3 -3) (layer F.Fab) (width 0.127))
  (fp_line (start 3 -3) (end 3 3) (layer F.Fab) (width 0.127))
  (fp_line (start 3 3) (end -3 3) (layer F.Fab) (width 0.127))
  (fp_line (start -3 3) (end -3 -3) (layer F.Fab) (width 0.127))
  (fp_line (start -3.81 -3.81) (end 3.81 -3.81) (layer F.SilkS) (width 0.127))
  (fp_line (start 3.81 -3.81) (end 3.81 3.81) (layer F.SilkS) (width 0.127))
  (fp_line (start 3.81 3.81) (end -3.81 3.81) (layer F.SilkS) (width 0.127))
  (fp_line (start -3.81 3.81) (end -3.81 -3.81) (layer F.SilkS) (width 0.127))
  (fp_poly (pts (xy -3.81 -3.81) (xy -3.81 -2.54) (xy -2.54 -3.81)) (layer F.SilkS) (width 0))
  (fp_poly (pts (xy -3 -3) (xy -3 -2.5) (xy -2.5 -3)) (layer F.Fab) (width 0))
  (fp_line (start -3.81 -3.81) (end 3.81 -3.81) (layer F.CrtYd) (width 0.0508))
  (fp_line (start 3.81 -3.81) (end 3.81 3.81) (layer F.CrtYd) (width 0.0508))
  (fp_line (start 3.81 3.81) (end -3.81 3.81) (layer F.CrtYd) (width 0.0508))
  (fp_line (start -3.81 3.81) (end -3.81 -3.81) (layer F.CrtYd) (width 0.0508))
  (fp_poly (pts (xy -2.1 2.1) (xy 2.1 2.1) (xy 2.1 -2.1) (xy -2.1 -2.1)) (layer F.Mask) (width 0))
  (fp_poly (pts (xy -2.1 2.1) (xy 2.1 2.1) (xy 2.1 -2.1) (xy -2.1 -2.1)) (layer B.Mask) (width 0))
  (fp_poly (pts (xy -1.7 1.7) (xy 1.7 1.7) (xy 1.7 -1.7) (xy -1.7 -1.7)) (layer F.Paste) (width 0))
  (pad 1 smd rect (at -3 -2.2) (size 1 0.2) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.0508))
  (pad 2 smd rect (at -3 -1.8) (size 1 0.2) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.0508))
  (pad 3 smd rect (at -3 -1.4) (size 1 0.2) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.0508))
  (pad 4 smd rect (at -3 -1) (size 1 0.2) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.0508))
  (pad 5 smd rect (at -3 -0.6) (size 1 0.2) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.0508))
  (pad 6 smd rect (at -3 -0.2) (size 1 0.2) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.0508))
  (pad 7 smd rect (at -3 0.2) (size 1 0.2) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.0508))
  (pad 8 smd rect (at -3 0.6) (size 1 0.2) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.0508))
  (pad 9 smd rect (at -3 1) (size 1 0.2) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.0508))
  (pad 10 smd rect (at -3 1.4) (size 1 0.2) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.0508))
  (pad 11 smd rect (at -3 1.8) (size 1 0.2) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.0508))
  (pad 12 smd rect (at -3 2.2) (size 1 0.2) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.0508))
  (pad 13 smd rect (at -2.2 3 90) (size 1 0.2) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.0508))
  (pad 14 smd rect (at -1.8 3 90) (size 1 0.2) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.0508))
  (pad 15 smd rect (at -1.4 3 90) (size 1 0.2) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.0508))
  (pad 16 smd rect (at -1 3 90) (size 1 0.2) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.0508))
  (pad 17 smd rect (at -0.6 3 90) (size 1 0.2) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.0508))
  (pad 18 smd rect (at -0.2 3 90) (size 1 0.2) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.0508))
  (pad 19 smd rect (at 0.2 3 90) (size 1 0.2) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.0508))
  (pad 20 smd rect (at 0.6 3 90) (size 1 0.2) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.0508))
  (pad 21 smd rect (at 1 3 90) (size 1 0.2) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.0508))
  (pad 22 smd rect (at 1.4 3 90) (size 1 0.2) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.0508))
  (pad 23 smd rect (at 1.8 3 90) (size 1 0.2) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.0508))
  (pad 24 smd rect (at 2.2 3 90) (size 1 0.2) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.0508))
  (pad 25 smd rect (at 3 2.2 180) (size 1 0.2) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.0508))
  (pad 26 smd rect (at 3 1.8 180) (size 1 0.2) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.0508))
  (pad 27 smd rect (at 3 1.4 180) (size 1 0.2) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.0508))
  (pad 28 smd rect (at 3 1 180) (size 1 0.2) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.0508))
  (pad 29 smd rect (at 3 0.6 180) (size 1 0.2) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.0508))
  (pad 30 smd rect (at 3 0.2 180) (size 1 0.2) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.0508))
  (pad 31 smd rect (at 3 -0.2 180) (size 1 0.2) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.0508))
  (pad 32 smd rect (at 3 -0.6 180) (size 1 0.2) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.0508))
  (pad 33 smd rect (at 3 -1 180) (size 1 0.2) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.0508))
  (pad 34 smd rect (at 3 -1.4 180) (size 1 0.2) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.0508))
  (pad 35 smd rect (at 3 -1.8 180) (size 1 0.2) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.0508))
  (pad 36 smd rect (at 3 -2.2 180) (size 1 0.2) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.0508))
  (pad 37 smd rect (at 2.2 -3 270) (size 1 0.2) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.0508))
  (pad 38 smd rect (at 1.8 -3 270) (size 1 0.2) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.0508))
  (pad 39 smd rect (at 1.4 -3 270) (size 1 0.2) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.0508))
  (pad 40 smd rect (at 1 -3 270) (size 1 0.2) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.0508))
  (pad 41 smd rect (at 0.6 -3 270) (size 1 0.2) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.0508))
  (pad 42 smd rect (at 0.2 -3 270) (size 1 0.2) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.0508))
  (pad 43 smd rect (at -0.2 -3 270) (size 1 0.2) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.0508))
  (pad 44 smd rect (at -0.6 -3 270) (size 1 0.2) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.0508))
  (pad 45 smd rect (at -1 -3 270) (size 1 0.2) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.0508))
  (pad 46 smd rect (at -1.4 -3 270) (size 1 0.2) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.0508))
  (pad 47 smd rect (at -1.8 -3 270) (size 1 0.2) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.0508))
  (pad 48 smd rect (at -2.2 -3 270) (size 1 0.2) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.0508))
  (pad GND$1 thru_hole circle (at -1.2 -1.2) (size 0.6096 0.6096) (drill 0.3048) (layers *.Cu *.Mask)
    (solder_mask_margin 0.0508) (zone_connect 2))
  (pad GND$2 thru_hole circle (at 0 -1.2) (size 0.6096 0.6096) (drill 0.3048) (layers *.Cu *.Mask)
    (solder_mask_margin 0.0508) (zone_connect 2))
  (pad GND$3 thru_hole circle (at 1.2 -1.2) (size 0.6096 0.6096) (drill 0.3048) (layers *.Cu *.Mask)
    (solder_mask_margin 0.0508) (zone_connect 2))
  (pad GND$4 thru_hole circle (at -1.2 0) (size 0.6096 0.6096) (drill 0.3048) (layers *.Cu *.Mask)
    (solder_mask_margin 0.0508) (zone_connect 2))
  (pad GND$5 thru_hole circle (at 0 0) (size 0.6096 0.6096) (drill 0.3048) (layers *.Cu *.Mask)
    (solder_mask_margin 0.0508) (zone_connect 2))
  (pad GND$6 thru_hole circle (at 1.2 0) (size 0.6096 0.6096) (drill 0.3048) (layers *.Cu *.Mask)
    (solder_mask_margin 0.0508) (zone_connect 2))
  (pad GND$7 thru_hole circle (at -1.2 1.2) (size 0.6096 0.6096) (drill 0.3048) (layers *.Cu *.Mask)
    (solder_mask_margin 0.0508) (zone_connect 2))
  (pad GND$8 thru_hole circle (at 0 1.2) (size 0.6096 0.6096) (drill 0.3048) (layers *.Cu *.Mask)
    (solder_mask_margin 0.0508) (zone_connect 2))
  (pad GND$9 thru_hole circle (at 1.2 1.2) (size 0.6096 0.6096) (drill 0.3048) (layers *.Cu *.Mask)
    (solder_mask_margin 0.0508) (zone_connect 2))
  (model ${KISYS3DMOD}/Package_DFN_QFN.3dshapes/QFN-48-1EP_7x7mm_P0.5mm_EP5.15x5.15mm.step
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
