##############################################################
#
# Xilinx Core Generator version 13.2
# Date: Sun Oct 16 18:54:12 2011
#
##############################################################
#
#  This file contains the customisation parameters for a
#  Xilinx CORE Generator IP GUI. It is strongly recommended
#  that you do not manually alter this file as it may cause
#  unexpected and unsupported behavior.
#
##############################################################
#
#  Generated from component: xilinx.com:ip:blk_mem_gen:6.2
#
##############################################################
#
# BEGIN Project Options
SET addpads = false
SET asysymbol = true
SET busformat = BusFormatAngleBracketNotRipped
SET createndf = false
SET designentry = Verilog
SET device = xc3s400
SET devicefamily = spartan3
SET flowvendor = Other
SET formalverification = false
SET foundationsym = false
SET implementationfiletype = Ngc
SET package = pq208
SET removerpms = false
SET simulationfiles = Behavioral
SET speedgrade = -4
SET verilogsim = true
SET vhdlsim = false
# END Project Options
# BEGIN Select
SELECT Block_Memory_Generator xilinx.com:ip:blk_mem_gen:6.2
# END Select
# BEGIN Parameters
CSET additional_inputs_for_power_estimation=false
CSET algorithm=Minimum_Area
CSET assume_synchronous_clk=true
CSET axi_id_width=4
CSET axi_slave_type=Memory_Slave
CSET axi_type=AXI4_Full
CSET byte_size=9
CSET coe_file=no_coe_file_loaded
CSET collision_warnings=ALL
CSET component_name=cx4_datram
CSET disable_collision_warnings=false
CSET disable_out_of_range_warnings=false
CSET ecc=false
CSET ecctype=No_ECC
CSET enable_a=Always_Enabled
CSET enable_b=Always_Enabled
CSET error_injection_type=Single_Bit_Error_Injection
CSET fill_remaining_memory_locations=true
CSET interface_type=Native
CSET load_init_file=false
CSET memory_type=True_Dual_Port_RAM
CSET operating_mode_a=WRITE_FIRST
CSET operating_mode_b=WRITE_FIRST
CSET output_reset_value_a=0
CSET output_reset_value_b=0
CSET pipeline_stages=0
CSET port_a_clock=100
CSET port_a_enable_rate=100
CSET port_a_write_rate=50
CSET port_b_clock=100
CSET port_b_enable_rate=100
CSET port_b_write_rate=50
CSET primitive=8kx2
CSET read_width_a=8
CSET read_width_b=8
CSET register_porta_input_of_softecc=false
CSET register_porta_output_of_memory_core=false
CSET register_porta_output_of_memory_primitives=false
CSET register_portb_output_of_memory_core=false
CSET register_portb_output_of_memory_primitives=false
CSET register_portb_output_of_softecc=false
CSET remaining_memory_locations=77
CSET reset_memory_latch_a=false
CSET reset_memory_latch_b=false
CSET reset_priority_a=CE
CSET reset_priority_b=CE
CSET reset_type=SYNC
CSET softecc=false
CSET use_axi_id=false
CSET use_byte_write_enable=false
CSET use_error_injection_pins=false
CSET use_regcea_pin=false
CSET use_regceb_pin=false
CSET use_rsta_pin=false
CSET use_rstb_pin=false
CSET write_depth_a=3072
CSET write_width_a=8
CSET write_width_b=8
# END Parameters
# BEGIN Extra information
MISC pkg_timestamp=2011-03-11T08:24:14.000Z
# END Extra information
GENERATE
# CRC: a7d60fbd
