[Settings]
Archive=0
Flash OS=0
Fargo=0
Use Data Variable=0
Data Variable=
Copy Data Variable=1
Copy Data Variable if Archived=1
Pack=0
Packed Variable=
Project Name=pstarter
GCC Switches=-Os -Wall -W -Wwrite-strings -ffunction-sections -fdata-sections
GNU Assembler Switches=--defsym ttunpack=1 -l
Assembler Switches=-g -t
Debug Info=0
Standard Library=1
Initialize BSS=1
Optimize NOPs=1
Optimize Returns=1
Optimize Branches=1
Optimize Moves=1
Optimize Tests=1
Optimize Calculations=1
Remove Unused Sections=1
Cut Unused Ranges=1
Reorder Sections=0
Merge Constants=1
Binary Output=0
Command Line=
Post-Build Process=

[Library Options]
Use TI-89=1
Use TI-92 Plus=1
Use V200=1
Optimize Calc Consts=0
Use Kernel=0
Use PreOS=0
Minimum AMS Version Defined=1
Minimum AMS Version=1.00
Unofficial OS Support=0
Reloc Format=AMS
ROM Call Format=Direct
BSS Ref Format=Kernel
Data Ref Format=Kernel
Use F-Line Jumps=0
Use 4-Byte F-Line Jumps=0
Optimize ROM Calls=0
Use Internal F-Line Emulator=0
Use Return Value=0
Enable Error Return=0
Save Screen=1

[File Editing]
Open File=E:\TI-89\pstarter\pstarter.s

[Included Files]
GNU Assembler File 1=pstarter.s
Text File 1=pstarter.txt
Header File 1=pst-ttup.h
Header File 2=pst-ttuf.h
Header File 3=pst-lzma.h
Header File 4=pst-shrn.h

