#
#  Copyright (c) 2012-2015, ARM Limited. All rights reserved.
#  Copyright (c) 2015, Intel Corporation. All rights reserved.<BR>
#
#  SPDX-License-Identifier: BSD-2-Clause-Patent
#

################################################################################
#
# FD Section
# The [FD] Section is made up of the definition statements and a
# description of what goes into  the Flash Device Image.  Each FD section
# defines one flash "device" image.  A flash device image may be one of
# the following: Removable media bootable image (like a boot floppy
# image,) an Option ROM image (that would be "flashed" into an add-in
# card,) a System "Flash"  image (that would be burned into a system's
# flash) or an Update ("Capsule") image that will be used to update and
# existing system flash.
#
################################################################################

[FD.ARM_VEXPRESS_CTA15A7_EFI]
BaseAddress   = 0xB0000000|gArmTokenSpaceGuid.PcdFdBaseAddress  # The base address of the Firmware in remapped DRAM.
Size          = 0x000E0000|gArmTokenSpaceGuid.PcdFdSize         # The size in bytes of the FLASH Device
ErasePolarity = 1
BlockSize     = 0x00001000
NumBlocks     = 0xE0

0x00000000|0x000E0000
gArmTokenSpaceGuid.PcdFvBaseAddress|gArmTokenSpaceGuid.PcdFvSize
FV = FVMAIN_COMPACT

################################################################################
#
# FV Section
#
# [FV] section is used to define what components or modules are placed within a flash
# device file.  This section also defines order the components and modules are positioned
# within the image.  The [FV] section consists of define statements, set statements and
# module statements.
#
################################################################################
[FV.FvMain]
BlockSize          = 0x40
NumBlocks          = 0         # This FV gets compressed so make it just big enough
FvAlignment        = 8         # FV alignment and FV attributes setting.
ERASE_POLARITY     = 1
MEMORY_MAPPED      = TRUE
STICKY_WRITE       = TRUE
LOCK_CAP           = TRUE
LOCK_STATUS        = TRUE
WRITE_DISABLED_CAP = TRUE
WRITE_ENABLED_CAP  = TRUE
WRITE_STATUS       = TRUE
WRITE_LOCK_CAP     = TRUE
WRITE_LOCK_STATUS  = TRUE
READ_DISABLED_CAP  = TRUE
READ_ENABLED_CAP   = TRUE
READ_STATUS        = TRUE
READ_LOCK_CAP      = TRUE
READ_LOCK_STATUS   = TRUE
FvNameGuid         = 73dcb643-3862-4904-9076-a94af1890243

  INF MdeModulePkg/Core/Dxe/DxeMain.inf

  #
  # PI DXE Drivers producing Architectural Protocols (EFI Services)
  #
  INF ArmPkg/Drivers/CpuDxe/CpuDxe.inf
  INF MdeModulePkg/Core/RuntimeDxe/RuntimeDxe.inf
  INF MdeModulePkg/Universal/SecurityStubDxe/SecurityStubDxe.inf
  INF MdeModulePkg/Universal/CapsuleRuntimeDxe/CapsuleRuntimeDxe.inf
  INF MdeModulePkg/Universal/Variable/RuntimeDxe/VariableRuntimeDxe.inf
  INF MdeModulePkg/Universal/FaultTolerantWriteDxe/FaultTolerantWriteDxe.inf
  INF MdeModulePkg/Universal/MonotonicCounterRuntimeDxe/MonotonicCounterRuntimeDxe.inf
  INF MdeModulePkg/Universal/ResetSystemRuntimeDxe/ResetSystemRuntimeDxe.inf
  INF EmbeddedPkg/RealTimeClockRuntimeDxe/RealTimeClockRuntimeDxe.inf
  INF EmbeddedPkg/MetronomeDxe/MetronomeDxe.inf

  INF MdeModulePkg/Universal/HiiDatabaseDxe/HiiDatabaseDxe.inf

  #
  # Multiple Console IO support
  #
  INF MdeModulePkg/Universal/Console/ConPlatformDxe/ConPlatformDxe.inf
  INF MdeModulePkg/Universal/Console/ConSplitterDxe/ConSplitterDxe.inf
  INF MdeModulePkg/Universal/Console/GraphicsConsoleDxe/GraphicsConsoleDxe.inf
  INF MdeModulePkg/Universal/Console/TerminalDxe/TerminalDxe.inf
  INF MdeModulePkg/Universal/SerialDxe/SerialDxe.inf

  INF ArmPkg/Drivers/ArmGic/ArmGicDxe.inf
  INF ArmPkg/Drivers/TimerDxe/TimerDxe.inf
  INF Platform/ARM/Drivers/NorFlashDxe/NorFlashDxe.inf
  INF ArmPlatformPkg/Drivers/LcdGraphicsOutputDxe/LcdGraphicsOutputDxe.inf
  INF ArmPlatformPkg/Drivers/SP805WatchdogDxe/SP805WatchdogDxe.inf

  #
  # Platform
  #
  INF Platform/ARM/VExpressPkg/Drivers/ArmVExpressDxe/ArmHwDxe.inf

  #
  # Multimedia Card Interface
  #
  INF EmbeddedPkg/Universal/MmcDxe/MmcDxe.inf
  INF Platform/ARM/VExpressPkg/Drivers/PL180MciDxe/PL180MciDxe.inf

  #
  # Filesystems
  #
!ifndef $(ARM_BIGLITTLE_TC2)
  INF ArmPkg/Filesystem/SemihostFs/SemihostFs.inf
!endif

  #
  # FAT filesystem + GPT/MBR partitioning
  #
  INF MdeModulePkg/Universal/Disk/DiskIoDxe/DiskIoDxe.inf
  INF MdeModulePkg/Universal/Disk/PartitionDxe/PartitionDxe.inf
  INF FatPkg/EnhancedFatDxe/Fat.inf
  INF MdeModulePkg/Universal/Disk/UnicodeCollation/EnglishDxe/EnglishDxe.inf

  # Versatile Express FileSystem
  INF Platform/ARM/Drivers/BootMonFs/BootMonFs.inf

  #
  # USB support
  #
  INF Platform/ARM/VExpressPkg/Drivers/Isp1761UsbDxe/Isp1761UsbDxe.inf

  #
  # Android Fastboot
  #
  INF EmbeddedPkg/Application/AndroidFastboot/AndroidFastbootApp.inf
  INF EmbeddedPkg/Drivers/AndroidFastbootTransportUsbDxe/FastbootTransportUsbDxe.inf
  INF Platform/ARM/VExpressPkg/Drivers/ArmVExpressFastBootDxe/ArmVExpressFastBootDxe.inf

  # ACPI Support
  INF MdeModulePkg/Universal/Acpi/AcpiTableDxe/AcpiTableDxe.inf

  #
  # Networking stack
  #
!include Platform/ARM/VExpressPkg/ArmVExpress-networking.fdf.inc

  INF Platform/ARM/VExpressPkg/Drivers/Lan9118Dxe/Lan9118Dxe.inf

  #
  # UEFI application
  #
  INF ShellPkg/Application/Shell/Shell.inf

  #
  # Bds
  #
  INF MdeModulePkg/Universal/BootManagerPolicyDxe/BootManagerPolicyDxe.inf
  INF MdeModulePkg/Universal/DevicePathDxe/DevicePathDxe.inf
  INF MdeModulePkg/Universal/DisplayEngineDxe/DisplayEngineDxe.inf
  INF MdeModulePkg/Universal/SetupBrowserDxe/SetupBrowserDxe.inf
  INF MdeModulePkg/Universal/BdsDxe/BdsDxe.inf
  INF MdeModulePkg/Application/UiApp/UiApp.inf

  # FV Filesystem
  INF MdeModulePkg/Universal/FvSimpleFileSystemDxe/FvSimpleFileSystemDxe.inf

  #
  # FDT installation
  #
  # The UEFI driver is at the end of the list of the driver to be dispatched
  # after the device drivers (eg: Ethernet) to ensure we have support for them.
  INF Platform/ARM/Drivers/FdtPlatformDxe/FdtPlatformDxe.inf

  # Example to add a Device Tree to the Firmware Volume
  #FILE FREEFORM = PCD(gArmVExpressTokenSpaceGuid.PcdFdtVExpressHwA15x2A7x3) {
  #  SECTION RAW = Platform/ARM/VExpressPkg/Fdts/vexpress-v2p-ca15_a7.dtb
  #}

[FV.FVMAIN_COMPACT]
FvBaseAddress      = 0xB0000000
FvForceRebase      = TRUE
FvAlignment        = 8
ERASE_POLARITY     = 1
MEMORY_MAPPED      = TRUE
STICKY_WRITE       = TRUE
LOCK_CAP           = TRUE
LOCK_STATUS        = TRUE
WRITE_DISABLED_CAP = TRUE
WRITE_ENABLED_CAP  = TRUE
WRITE_STATUS       = TRUE
WRITE_LOCK_CAP     = TRUE
WRITE_LOCK_STATUS  = TRUE
READ_DISABLED_CAP  = TRUE
READ_ENABLED_CAP   = TRUE
READ_STATUS        = TRUE
READ_LOCK_CAP      = TRUE
READ_LOCK_STATUS   = TRUE

  INF ArmPlatformPkg/PrePi/PeiMPCore.inf

  FILE FV_IMAGE = 9E21FD93-9C72-4c15-8C4B-E77F1DB2D792 {
    SECTION GUIDED EE4E5898-3914-4259-9D6E-DC7BD79403CF PROCESSING_REQUIRED = TRUE {
      SECTION FV_IMAGE = FVMAIN
    }
  }


################################################################################
#
# Rules are use with the [FV] section's module INF type to define
# how an FFS file is created for a given INF file. The following Rule are the default
# rules for the different module type. User can add the customized rules to define the
# content of the FFS file.
#
################################################################################


############################################################################
# Example of a DXE_DRIVER FFS file with a Checksum encapsulation section   #
############################################################################
#
#[Rule.Common.DXE_DRIVER]
#  FILE DRIVER = $(NAMED_GUID) {
#    DXE_DEPEX    DXE_DEPEX               Optional $(INF_OUTPUT)/$(MODULE_NAME).depex
#    COMPRESS PI_STD {
#      GUIDED {
#        PE32     PE32                    $(INF_OUTPUT)/$(MODULE_NAME).efi
#        UI       STRING="$(MODULE_NAME)" Optional
#        VERSION  STRING="$(INF_VERSION)" Optional BUILD_NUM=$(BUILD_NUMBER)
#      }
#    }
#  }
#
############################################################################

[Rule.Common.SEC]
  FILE SEC = $(NAMED_GUID) RELOCS_STRIPPED {
    TE  TE    Align = 32                $(INF_OUTPUT)/$(MODULE_NAME).efi
  }

[Rule.Common.PEI_CORE]
  FILE PEI_CORE = $(NAMED_GUID) {
    TE     TE                           $(INF_OUTPUT)/$(MODULE_NAME).efi
    UI     STRING ="$(MODULE_NAME)" Optional
  }

[Rule.Common.PEIM]
  FILE PEIM = $(NAMED_GUID) {
     PEI_DEPEX PEI_DEPEX Optional       $(INF_OUTPUT)/$(MODULE_NAME).depex
     TE       TE                        $(INF_OUTPUT)/$(MODULE_NAME).efi
     UI       STRING="$(MODULE_NAME)" Optional
  }

[Rule.Common.DXE_CORE]
  FILE DXE_CORE = $(NAMED_GUID) {
    PE32     PE32                       $(INF_OUTPUT)/$(MODULE_NAME).efi
    UI       STRING="$(MODULE_NAME)" Optional
  }

[Rule.Common.UEFI_DRIVER]
  FILE DRIVER = $(NAMED_GUID) {
    DXE_DEPEX    DXE_DEPEX              Optional $(INF_OUTPUT)/$(MODULE_NAME).depex
    PE32         PE32                   $(INF_OUTPUT)/$(MODULE_NAME).efi
    UI           STRING="$(MODULE_NAME)" Optional
  }

[Rule.Common.DXE_DRIVER]
  FILE DRIVER = $(NAMED_GUID) {
    DXE_DEPEX    DXE_DEPEX              Optional $(INF_OUTPUT)/$(MODULE_NAME).depex
    PE32         PE32                   $(INF_OUTPUT)/$(MODULE_NAME).efi
    UI           STRING="$(MODULE_NAME)" Optional
  }

[Rule.Common.DXE_RUNTIME_DRIVER]
  FILE DRIVER = $(NAMED_GUID) {
    DXE_DEPEX    DXE_DEPEX              Optional $(INF_OUTPUT)/$(MODULE_NAME).depex
    PE32         PE32                   $(INF_OUTPUT)/$(MODULE_NAME).efi
    UI           STRING="$(MODULE_NAME)" Optional
  }

[Rule.Common.UEFI_APPLICATION]
  FILE APPLICATION = $(NAMED_GUID) {
    UI     STRING ="$(MODULE_NAME)" Optional
    PE32   PE32                         $(INF_OUTPUT)/$(MODULE_NAME).efi
  }

[Rule.Common.UEFI_DRIVER.BINARY]
  FILE DRIVER = $(NAMED_GUID) {
    DXE_DEPEX DXE_DEPEX Optional      |.depex
    PE32      PE32                    |.efi
    UI        STRING="$(MODULE_NAME)" Optional
    VERSION   STRING="$(INF_VERSION)" Optional BUILD_NUM=$(BUILD_NUMBER)
  }

[Rule.Common.UEFI_APPLICATION.BINARY]
  FILE APPLICATION = $(NAMED_GUID) {
    PE32      PE32                    |.efi
    UI        STRING="$(MODULE_NAME)" Optional
    VERSION   STRING="$(INF_VERSION)" Optional BUILD_NUM=$(BUILD_NUMBER)
  }
