#/** @file
#  Component description file for ArmMaliDpLib module
#
#  Copyright (c) 2017-2018, Arm Limited. All rights reserved.
#
#  SPDX-License-Identifier: BSD-2-Clause-Patent
#**/

[Defines]
  INF_VERSION                    = 0x00010019
  BASE_NAME                      = ArmMaliDpLib
  FILE_GUID                      = 36C47FED-2F3F-49C7-89CE-31B13F0431D8
  MODULE_TYPE                    = BASE
  VERSION_STRING                 = 1.0
  LIBRARY_CLASS                  = LcdPlatformLib

[Sources.common]
  ArmMaliDpLib.c

[Packages]
  ArmPlatformPkg/ArmPlatformPkg.dec
  MdePkg/MdePkg.dec
  Platform/ARM/VExpressPkg/ArmVExpressPkg.dec

[LibraryClasses]
  BaseLib

[FixedPcd.common]
  gArmPlatformTokenSpaceGuid.PcdArmLcdDdrFrameBufferBase
  gArmPlatformTokenSpaceGuid.PcdArmLcdDdrFrameBufferSize
  gArmPlatformTokenSpaceGuid.PcdGopPixelFormat

  # MaxMode must be one number higher than the actual max mode,
  # i.e. for actual maximum mode 2, set the value to 3.
  # See Section 12.9 of the UEFI Specification 2.7
  gArmVExpressTokenSpaceGuid.PcdArmMaliDpMaxMode

