#
#  Copyright (c) 2011, 2012, ARM Limited. All rights reserved.
#  Copyright (c) 2017 - 2018, Hisilicon Limited. All rights reserved.
#  Copyright (c) 2017 - 2018, Linaro Limited. All rights reserved.
#
#  SPDX-License-Identifier: BSD-2-Clause-Patent
#

[DEFINES]

################################################################################
#
# FD Section
# The [FD] Section is made up of the definition statements and a
# description of what goes into  the Flash Device Image.  Each FD section
# defines one flash "device" image.  A flash device image may be one of
# the following: Removable media bootable image (like a boot floppy
# image,) an Option ROM image (that would be "flashed" into an add-in
# card,) a System "Flash"  image (that would be burned into a system's
# flash) or an Update ("Capsule") image that will be used to update and
# existing system flash.
#
################################################################################
[FD.D06]

BaseAddress   = 0x204800000|gArmTokenSpaceGuid.PcdFdBaseAddress  # The base address of the Firmware in NOR Flash.

Size          = 0x00400000|gArmTokenSpaceGuid.PcdFdSize         # The size in bytes of the FLASH Device
ErasePolarity = 1

# This one is tricky, it must be: BlockSize * NumBlocks = Size
BlockSize     = 0x00010000
NumBlocks     = 0x40

################################################################################
#
# Following are lists of FD Region layout which correspond to the locations of different
# images within the flash device.
#
# Regions must be defined in ascending order and may not overlap.
#
# A Layout Region start with a eight digit hex offset (leading "0x" required) followed by
# the pipe "|" character, followed by the size of the region, also in hex with the leading
# "0x" characters. Like:
# Offset|Size
# PcdOffsetCName|PcdSizeCName
# RegionType <FV, DATA, or FILE>
#
################################################################################

0x00000000|0x00100000
gArmTokenSpaceGuid.PcdSecureFvBaseAddress|gArmTokenSpaceGuid.PcdSecureFvSize
FILE = Platform/Hisilicon/D06/Sec/FVMAIN_SEC.Fv

0x00100000|0x00280000
gArmTokenSpaceGuid.PcdFvBaseAddress|gArmTokenSpaceGuid.PcdFvSize
FV = FVMAIN_COMPACT

0x00380000|0x00020000
gHisiTokenSpaceGuid.PcdTrustedFirmwareBL1Base
FILE = Platform/Hisilicon/D06/bl1.bin
0x003A0000|0x00020000
FILE = Platform/Hisilicon/D06/fip.bin

0x003C0000|0x0000e000
gEfiMdeModulePkgTokenSpaceGuid.PcdFlashNvStorageVariableBase64|gEfiMdeModulePkgTokenSpaceGuid.PcdFlashNvStorageVariableSize
DATA = {
  ## This is the EFI_FIRMWARE_VOLUME_HEADER
  0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00,
  0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00,
  # FileSystemGuid: gEfiSystemNvDataFvGuid         =
  0x8D, 0x2B, 0xF1, 0xFF, 0x96, 0x76, 0x8B, 0x4C,
  0xA9, 0x85, 0x27, 0x47, 0x07, 0x5B, 0x4F, 0x50,
  # FvLength: 0x20000
  0x00, 0x00, 0x02, 0x00, 0x00, 0x00, 0x00, 0x00,
  #Signature "_FVH"       #Attributes
  0x5f, 0x46, 0x56, 0x48, 0xff, 0xfe, 0x04, 0x00,
  #HeaderLength #CheckSum #ExtHeaderOffset #Reserved #Revision
  0x48, 0x00, 0x36, 0x09, 0x00, 0x00, 0x00, 0x02,
  #Blockmap[0]: 2 Blocks * 0x10000 Bytes / Block
  0x02, 0x00, 0x00, 0x00, 0x00, 0x00, 0x01, 0x00,
  #Blockmap[1]: End
  0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00,
  ## This is the VARIABLE_STORE_HEADER
  #Signature: gEfiVariableGuid =
  #  { 0xddcf3616, 0x3275, 0x4164, { 0x98, 0xb6, 0xfe, 0x85, 0x70, 0x7f, 0xfe, 0x7d }}
  0x16, 0x36, 0xcf, 0xdd, 0x75, 0x32, 0x64, 0x41,
  0x98, 0xb6, 0xfe, 0x85, 0x70, 0x7f, 0xfe, 0x7d,
  #Size: 0xe000 (gEfiMdeModulePkgTokenSpaceGuid.PcdFlashNvStorageVariableSize) - 0x48 (size of EFI_FIRMWARE_VOLUME_HEADER) = 0xdFB8
  0xB8, 0xdF, 0x00, 0x00,
  #FORMATTED: 0x5A #HEALTHY: 0xFE #Reserved: UINT16 #Reserved1: UINT32
  0x5A, 0xFE, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00
}

0x003CE000|0x00002000
gEfiMdeModulePkgTokenSpaceGuid.PcdFlashNvStorageFtwWorkingBase64|gEfiMdeModulePkgTokenSpaceGuid.PcdFlashNvStorageFtwWorkingSize
#NV_FTW_WORKING
DATA = {
  # EFI_FAULT_TOLERANT_WORKING_BLOCK_HEADER->Signature = gEdkiiWorkingBlockSignatureGuid          =
  0x2B, 0x29, 0x58, 0x9E, 0x68, 0x7C, 0x7D, 0x49,
  0xA0, 0xCE, 0x65, 0x0 , 0xFD, 0x9F, 0x1B, 0x95,
  # Crc:UINT32            #WorkingBlockValid:1, WorkingBlockInvalid:1, Reserved
  0xE2, 0x33, 0xF2, 0x03, 0xFE, 0xFF, 0xFF, 0xFF,
  # WriteQueueSize: UINT64 #Size: 0x2000 - 0x20 (FTW_WORKING_HEADER) = 0x1FE0
  0xE0, 0x1F, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00
}

0x003D0000|0x00010000
gEfiMdeModulePkgTokenSpaceGuid.PcdFlashNvStorageFtwSpareBase64|gEfiMdeModulePkgTokenSpaceGuid.PcdFlashNvStorageFtwSpareSize

0x003E0000|0x00010000

0x003F0000|0x00010000
FILE = Platform/Hisilicon/D06/CustomData.Fv

################################################################################
#
# FV Section
#
# [FV] section is used to define what components or modules are placed within a flash
# device file.  This section also defines order the components and modules are positioned
# within the image.  The [FV] section consists of define statements, set statements and
# module statements.
#
################################################################################

[FV.FvMain]
BlockSize          = 0x40
NumBlocks          = 0         # This FV gets compressed so make it just big enough
FvAlignment        = 16        # FV alignment and FV attributes setting.
ERASE_POLARITY     = 1
MEMORY_MAPPED      = TRUE
STICKY_WRITE       = TRUE
LOCK_CAP           = TRUE
LOCK_STATUS        = TRUE
WRITE_DISABLED_CAP = TRUE
WRITE_ENABLED_CAP  = TRUE
WRITE_STATUS       = TRUE
WRITE_LOCK_CAP     = TRUE
WRITE_LOCK_STATUS  = TRUE
READ_DISABLED_CAP  = TRUE
READ_ENABLED_CAP   = TRUE
READ_STATUS        = TRUE
READ_LOCK_CAP      = TRUE
READ_LOCK_STATUS   = TRUE

  APRIORI DXE {
    INF MdeModulePkg/Universal/PCD/Dxe/Pcd.inf
  }

  INF MdeModulePkg/Core/Dxe/DxeMain.inf
  INF MdeModulePkg/Universal/PCD/Dxe/Pcd.inf

  INF Platform/Hisilicon/D06/Drivers/IoInitDxe/IoInitDxe.inf
  INF Platform/Hisilicon/D06/Drivers/Sas/SasDxeDriver.inf
  #
  # PI DXE Drivers producing Architectural Protocols (EFI Services)
  #
  INF ArmPkg/Drivers/CpuDxe/CpuDxe.inf
  INF MdeModulePkg/Core/RuntimeDxe/RuntimeDxe.inf

  INF MdeModulePkg/Universal/SecurityStubDxe/SecurityStubDxe.inf
  INF Platform/Hisilicon/D06/Drivers/SFC/SfcDxeDriver.inf

  INF Platform/Hisilicon/D06/Drivers/OemNicConfig2PHi1620/OemNicConfig2P.inf
  INF Silicon/Hisilicon/Drivers/FlashFvbDxe/FlashFvbDxe.inf
  INF MdeModulePkg/Universal/FaultTolerantWriteDxe/FaultTolerantWriteDxe.inf
  INF MdeModulePkg/Universal/Variable/RuntimeDxe/VariableRuntimeDxe.inf

  INF MdeModulePkg/Universal/CapsuleRuntimeDxe/CapsuleRuntimeDxe.inf
  INF MdeModulePkg/Universal/MonotonicCounterRuntimeDxe/MonotonicCounterRuntimeDxe.inf

  INF MdeModulePkg/Universal/ResetSystemRuntimeDxe/ResetSystemRuntimeDxe.inf
  INF EmbeddedPkg/RealTimeClockRuntimeDxe/RealTimeClockRuntimeDxe.inf
  INF EmbeddedPkg/MetronomeDxe/MetronomeDxe.inf

  INF MdeModulePkg/Universal/HiiDatabaseDxe/HiiDatabaseDxe.inf

  #
  # Multiple Console IO support
  #
  INF MdeModulePkg/Universal/Console/ConPlatformDxe/ConPlatformDxe.inf
  INF MdeModulePkg/Universal/Console/ConSplitterDxe/ConSplitterDxe.inf
  INF MdeModulePkg/Universal/Console/GraphicsConsoleDxe/GraphicsConsoleDxe.inf
  INF MdeModulePkg/Universal/Console/TerminalDxe/TerminalDxe.inf
  INF MdeModulePkg/Universal/SerialDxe/SerialDxe.inf
  INF EmbeddedPkg/Drivers/ConsolePrefDxe/ConsolePrefDxe.inf

  INF ArmPkg/Drivers/ArmGic/ArmGicDxe.inf
  INF ArmPkg/Drivers/TimerDxe/TimerDxe.inf

  INF MdeModulePkg/Universal/WatchdogTimerDxe/WatchdogTimer.inf

  #
  # FAT filesystem + GPT/MBR partitioning
  #
  INF MdeModulePkg/Universal/Disk/DiskIoDxe/DiskIoDxe.inf
  INF MdeModulePkg/Universal/Disk/PartitionDxe/PartitionDxe.inf
  INF FatPkg/EnhancedFatDxe/Fat.inf
  INF MdeModulePkg/Universal/Disk/UnicodeCollation/EnglishDxe/EnglishDxe.inf
  INF MdeModulePkg/Universal/ReportStatusCodeRouter/RuntimeDxe/ReportStatusCodeRouterRuntimeDxe.inf
  INF MdeModulePkg/Universal/StatusCodeHandler/RuntimeDxe/StatusCodeHandlerRuntimeDxe.inf

  #
  # Usb Support
  #


  INF MdeModulePkg/Bus/Pci/EhciDxe/EhciDxe.inf

  INF MdeModulePkg/Bus/Pci/XhciDxe/XhciDxe.inf
  INF MdeModulePkg/Bus/Usb/UsbBusDxe/UsbBusDxe.inf
  INF MdeModulePkg/Bus/Usb/UsbKbDxe/UsbKbDxe.inf
  INF MdeModulePkg/Bus/Usb/UsbMouseDxe/UsbMouseDxe.inf
  INF MdeModulePkg/Bus/Usb/UsbMassStorageDxe/UsbMassStorageDxe.inf

  INF Platform/Hisilicon/D06/Drivers/Ipmi/IpmiInterfaceDxe/IpmiInterfaceDxe.inf
  INF Platform/Hisilicon/D06/Drivers/GetInfoFromBmc/GetInfoFromBmc.inf
  INF MdeModulePkg/Universal/SmbiosDxe/SmbiosDxe.inf
  INF Silicon/Hisilicon/Drivers/Smbios/SmbiosMiscDxe/SmbiosMiscDxe.inf
  INF Silicon/Hisilicon/Drivers/Smbios/AddSmbiosType9/AddSmbiosType9.inf
  INF Silicon/Hisilicon/Drivers/Smbios/MemorySubClassDxe/MemorySubClassDxe.inf
  INF Silicon/Hisilicon/Drivers/Smbios/ProcessorSubClassDxe/ProcessorSubClassDxe.inf
  INF Platform/Hisilicon/D06/Drivers/TransferSmbiosInfo/TransSmbiosInfo.inf
  INF Platform/Hisilicon/D06/Drivers/IpmiMiscOpDxe/IpmiMiscOpDxe.inf
  INF Platform/Hisilicon/D06/Drivers/IpmiWatchdogDxe/IpmiWatchdogDxe.inf

  #
  #ACPI
  #
  INF MdeModulePkg/Universal/Acpi/AcpiTableDxe/AcpiTableDxe.inf
  INF Silicon/Hisilicon/Drivers/HisiAcpiPlatformDxe/AcpiPlatformDxe.inf

  INF RuleOverride=ACPITABLE Silicon/Hisilicon/Hi1620/Hi1620AcpiTables/AcpiTablesHi1620.inf
  INF Silicon/Hisilicon/Drivers/AcpiPlatformDxe/AcpiPlatformDxe.inf
  INF Silicon/Hisilicon/Hi1620/Drivers/Apei/Apei.inf

  INF Silicon/Hisilicon/Hi1620/Pptt/Pptt.inf

  #
  #Network
  #
!include NetworkPkg/Network.fdf.inc

  #
  # PCI Support
  #
  INF Silicon/Hisilicon/Drivers/PciPlatform/PciPlatform.inf
  INF ArmPkg/Drivers/ArmPciCpuIo2Dxe/ArmPciCpuIo2Dxe.inf
  INF MdeModulePkg/Bus/Pci/PciHostBridgeDxe/PciHostBridgeDxe.inf
  INF MdeModulePkg/Bus/Pci/PciBusDxe/PciBusDxe.inf
  INF Platform/Hisilicon/D06/Drivers/PcieRasInitDxe/PcieRasInitDxe.inf
  INF Platform/Hisilicon/D06/Drivers/RasInitDxe/RasInitDxe.inf

  # VGA Driver
  #
  INF Platform/Hisilicon/D06/Drivers/Sm750Dxe/UefiSmi.inf
  INF MdeModulePkg/Bus/Pci/NvmExpressDxe/NvmExpressDxe.inf
  INF MdeModulePkg/Bus/Pci/SataControllerDxe/SataControllerDxe.inf
  INF MdeModulePkg/Bus/Ata/AtaAtapiPassThru/AtaAtapiPassThru.inf
  INF MdeModulePkg/Bus/Ata/AtaBusDxe/AtaBusDxe.inf

  INF Silicon/Hisilicon/Hi1620/Drivers/Pl011DebugSerialPortInitDxe/Pl011DebugSerialPortInitDxe.inf
  INF SignedCapsulePkg/Universal/SystemFirmwareUpdate/SystemFirmwareReportDxe.inf
  INF MdeModulePkg/Universal/EsrtDxe/EsrtDxe.inf

  #
  # Build Shell from latest source code instead of prebuilt binary
  #
  INF ShellPkg/Application/Shell/Shell.inf

  INF MdeModulePkg/Application/UiApp/UiApp.inf
  #
  # Bds
  #
  INF MdeModulePkg/Universal/DevicePathDxe/DevicePathDxe.inf

  INF MdeModulePkg/Universal/MemoryTest/NullMemoryTestDxe/NullMemoryTestDxe.inf
  INF MdeModulePkg/Universal/DisplayEngineDxe/DisplayEngineDxe.inf
  INF MdeModulePkg/Universal/SetupBrowserDxe/SetupBrowserDxe.inf
  INF MdeModulePkg/Universal/DriverHealthManagerDxe/DriverHealthManagerDxe.inf
  INF MdeModulePkg/Universal/BdsDxe/BdsDxe.inf

[FV.FVMAIN_COMPACT]
FvAlignment        = 16
ERASE_POLARITY     = 1
MEMORY_MAPPED      = TRUE
STICKY_WRITE       = TRUE
LOCK_CAP           = TRUE
LOCK_STATUS        = TRUE
WRITE_DISABLED_CAP = TRUE
WRITE_ENABLED_CAP  = TRUE
WRITE_STATUS       = TRUE
WRITE_LOCK_CAP     = TRUE
WRITE_LOCK_STATUS  = TRUE
READ_DISABLED_CAP  = TRUE
READ_ENABLED_CAP   = TRUE
READ_STATUS        = TRUE
READ_LOCK_CAP      = TRUE
READ_LOCK_STATUS   = TRUE

  APRIORI PEI {
    INF  MdeModulePkg/Universal/PCD/Pei/Pcd.inf
  }
  INF ArmPlatformPkg/PrePeiCore/PrePeiCoreMPCore.inf
  INF MdeModulePkg/Core/Pei/PeiMain.inf
  INF ArmPlatformPkg/PlatformPei/PlatformPeim.inf

  INF MdeModulePkg/Universal/FaultTolerantWritePei/FaultTolerantWritePei.inf
  INF MdeModulePkg/Universal/Variable/Pei/VariablePei.inf

  INF Silicon/Hisilicon/Drivers/VersionInfoPeim/VersionInfoPeim.inf

  INF Platform/Hisilicon/D06/Drivers/Ipmi/IpmiInterfacePei/IpmiInterfacePei.inf
  INF Platform/Hisilicon/D06/MemoryInitPei/MemoryInitPeim.inf
  INF ArmPkg/Drivers/CpuPei/CpuPei.inf
  INF MdeModulePkg/Universal/PCD/Pei/Pcd.inf
  INF MdeModulePkg/Universal/ReportStatusCodeRouter/Pei/ReportStatusCodeRouterPei.inf
  INF MdeModulePkg/Universal/StatusCodeHandler/Pei/StatusCodeHandlerPei.inf
  INF Platform/Hisilicon/D06/EarlyConfigPeim/EarlyConfigPeimD06.inf

  INF MdeModulePkg/Core/DxeIplPeim/DxeIpl.inf

  INF RuleOverride = FMP_IMAGE_DESC Platform/Hisilicon/D06/Drivers/SystemFirmwareDescriptor/SystemFirmwareDescriptor.inf
  FILE FV_IMAGE = 9E21FD93-9C72-4c15-8C4B-E77F1DB2D792 {
    SECTION GUIDED EE4E5898-3914-4259-9D6E-DC7BD79403CF PROCESSING_REQUIRED = TRUE {
      SECTION FV_IMAGE = FVMAIN
    }
  }
[FV.CapsuleDispatchFv]
FvAlignment        = 16
ERASE_POLARITY     = 1
MEMORY_MAPPED      = TRUE
STICKY_WRITE       = TRUE
LOCK_CAP           = TRUE
LOCK_STATUS        = TRUE
WRITE_DISABLED_CAP = TRUE
WRITE_ENABLED_CAP  = TRUE
WRITE_STATUS       = TRUE
WRITE_LOCK_CAP     = TRUE
WRITE_LOCK_STATUS  = TRUE
READ_DISABLED_CAP  = TRUE
READ_ENABLED_CAP   = TRUE
READ_STATUS        = TRUE
READ_LOCK_CAP      = TRUE
READ_LOCK_STATUS   = TRUE

  INF SignedCapsulePkg/Universal/SystemFirmwareUpdate/SystemFirmwareUpdateDxe.inf

[FV.SystemFirmwareUpdateCargo]
FvAlignment        = 16
ERASE_POLARITY     = 1
MEMORY_MAPPED      = TRUE
STICKY_WRITE       = TRUE
LOCK_CAP           = TRUE
LOCK_STATUS        = TRUE
WRITE_DISABLED_CAP = TRUE
WRITE_ENABLED_CAP  = TRUE
WRITE_STATUS       = TRUE
WRITE_LOCK_CAP     = TRUE
WRITE_LOCK_STATUS  = TRUE
READ_DISABLED_CAP  = TRUE
READ_ENABLED_CAP   = TRUE
READ_STATUS        = TRUE
READ_LOCK_CAP      = TRUE
READ_LOCK_STATUS   = TRUE

  FILE RAW = 642e4fcf-2df7-4415-8b70-a03909c57b55 { # PcdEdkiiSystemFirmwareFileGuid
    FD = D06
  }

  FILE RAW = ce57b167-b0e4-41e8-a897-5f4feb781d40 { # gEdkiiSystemFmpCapsuleDriverFvFileGuid
    FV = CapsuleDispatchFv
  }

  FILE RAW = 812136D3-4D3A-433A-9418-29BB9BF78F6E { # gEdkiiSystemFmpCapsuleConfigFileGuid
    Platform/Hisilicon/D06/Capsule/SystemFirmwareUpdateConfig/SystemFirmwareUpdateConfig.ini
  }

[FmpPayload.FmpPayloadSystemFirmwarePkcs7]
IMAGE_HEADER_INIT_VERSION = 0x02
IMAGE_TYPE_ID             = df8fe8d1-e937-45b8-9691-c4b5e183874e # PcdSystemFmpCapsuleImageTypeIdGuid
IMAGE_INDEX               = 0x1
HARDWARE_INSTANCE         = 0x0
MONOTONIC_COUNT           = 0x1
CERTIFICATE_GUID          = 4AAFD29D-68DF-49EE-8AA9-347D375665A7 # PKCS7

  FV = SystemFirmwareUpdateCargo

[Capsule.D06FirmwareUpdateCapsuleFmpPkcs7]
CAPSULE_GUID                = 6dcbd5ed-e82d-4c44-bda1-7194199ad92a # gEfiFmpCapsuleGuid
CAPSULE_HEADER_SIZE         = 0x20
CAPSULE_HEADER_INIT_VERSION = 0x1

  FMP_PAYLOAD = FmpPayloadSystemFirmwarePkcs7


!include Silicon/Hisilicon/Hisilicon.fdf.inc

