#
#  Copyright (c) 2011-2015, ARM Limited. All rights reserved.
#  Copyright (c) 2014 - 2018, Linaro Limited. All rights reserved.
#  Copyright (c) 2015 - 2016, Intel Corporation. All rights reserved.
#
#  SPDX-License-Identifier: BSD-2-Clause-Patent
#
#

################################################################################
#
# Defines Section - statements that will be processed to create a Makefile.
#
################################################################################
[Defines]
  PLATFORM_NAME                  = RdkQemu
  PLATFORM_GUID                  = 2D89EF13-B604-4550-B080-5E2E5E382854
  PLATFORM_VERSION               = 0.1
  DSC_SPECIFICATION              = 0x00010005
  OUTPUT_DIRECTORY               = Build/RDK-$(ARCH)
  SUPPORTED_ARCHITECTURES        = AARCH64|ARM
  BUILD_TARGETS                  = DEBUG|RELEASE
  SKUID_IDENTIFIER               = DEFAULT
  FLASH_DEFINITION               = Platform/Comcast/RDKQemu/RDKQemu.fdf

  #
  # Defines for default states.  These can be changed on the command line.
  # -D FLAG=VALUE
  #
  DEFINE SECURE_BOOT_ENABLE      = TRUE

  #
  # Network definition
  #
  DEFINE NETWORK_SNP_ENABLE             = FALSE
  DEFINE NETWORK_TLS_ENABLE             = FALSE
  DEFINE NETWORK_IP6_ENABLE             = FALSE
  DEFINE NETWORK_HTTP_BOOT_ENABLE       = TRUE
  DEFINE NETWORK_ALLOW_HTTP_CONNECTIONS = TRUE

!include ArmVirtPkg/ArmVirt.dsc.inc

[LibraryClasses.common]
  ArmLib|ArmPkg/Library/ArmLib/ArmBaseLib.inf
  ArmMmuLib|ArmPkg/Library/ArmMmuLib/ArmMmuBaseLib.inf

  # Virtio Support
  VirtioLib|OvmfPkg/Library/VirtioLib/VirtioLib.inf
  VirtioMmioDeviceLib|OvmfPkg/Library/VirtioMmioDeviceLib/VirtioMmioDeviceLib.inf
  QemuFwCfgLib|ArmVirtPkg/Library/QemuFwCfgLib/QemuFwCfgLib.inf
  QemuFwCfgS3Lib|OvmfPkg/Library/QemuFwCfgS3Lib/BaseQemuFwCfgS3LibNull.inf

  ArmPlatformLib|ArmPlatformPkg/Library/ArmPlatformLibNull/ArmPlatformLibNull.inf

  TimerLib|ArmPkg/Library/ArmArchTimerLib/ArmArchTimerLib.inf
  NorFlashPlatformLib|ArmVirtPkg/Library/NorFlashQemuLib/NorFlashQemuLib.inf

  CapsuleLib|MdeModulePkg/Library/DxeCapsuleLibNull/DxeCapsuleLibNull.inf
  BootLogoLib|MdeModulePkg/Library/BootLogoLib/BootLogoLib.inf
  PlatformBootManagerLib|ArmVirtPkg/Library/PlatformBootManagerLib/PlatformBootManagerLib.inf
  PlatformBmPrintScLib|OvmfPkg/Library/PlatformBmPrintScLib/PlatformBmPrintScLib.inf
  CustomizedDisplayLib|MdeModulePkg/Library/CustomizedDisplayLib/CustomizedDisplayLib.inf
  FrameBufferBltLib|MdeModulePkg/Library/FrameBufferBltLib/FrameBufferBltLib.inf
  QemuBootOrderLib|OvmfPkg/Library/QemuBootOrderLib/QemuBootOrderLib.inf
  FileExplorerLib|MdeModulePkg/Library/FileExplorerLib/FileExplorerLib.inf
  PciPcdProducerLib|ArmVirtPkg/Library/FdtPciPcdProducerLib/FdtPciPcdProducerLib.inf
  PciSegmentLib|MdePkg/Library/BasePciSegmentLibPci/BasePciSegmentLibPci.inf
  PciHostBridgeLib|ArmVirtPkg/Library/FdtPciHostBridgeLib/FdtPciHostBridgeLib.inf
  RdkBootManagerLib|Platform/Comcast/Library/RdkBootManagerLib/RdkBootManagerLib.inf

[LibraryClasses.common.PEIM]
  ArmVirtMemInfoLib|ArmVirtPkg/Library/QemuVirtMemInfoLib/QemuVirtMemInfoPeiLib.inf

[LibraryClasses.common.DXE_DRIVER]
  ReportStatusCodeLib|MdeModulePkg/Library/DxeReportStatusCodeLib/DxeReportStatusCodeLib.inf

[LibraryClasses.common.UEFI_DRIVER]
  UefiScsiLib|MdePkg/Library/UefiScsiLib/UefiScsiLib.inf

################################################################################
#
# Pcd Section - list of all EDK II PCD Entries defined by this Platform
#
################################################################################

[PcdsFeatureFlag.common]
  gUefiOvmfPkgTokenSpaceGuid.PcdQemuBootOrderPciTranslation|TRUE
  gUefiOvmfPkgTokenSpaceGuid.PcdQemuBootOrderMmioTranslation|TRUE

  ## If TRUE, Graphics Output Protocol will be installed on virtual handle created by ConsplitterDxe.
  #  It could be set FALSE to save size.
  gEfiMdeModulePkgTokenSpaceGuid.PcdConOutGopSupport|TRUE
  gEfiMdeModulePkgTokenSpaceGuid.PcdConOutUgaSupport|FALSE

[PcdsFixedAtBuild.common]
  gArmPlatformTokenSpaceGuid.PcdCoreCount|1
!if $(ARCH) == AARCH64
  gArmTokenSpaceGuid.PcdVFPEnabled|1
!endif

  gArmPlatformTokenSpaceGuid.PcdCPUCoresStackBase|0x4007c000
  gArmPlatformTokenSpaceGuid.PcdCPUCorePrimaryStackSize|0x4000
  gEfiMdeModulePkgTokenSpaceGuid.PcdMaxVariableSize|0x2000
  gEfiMdeModulePkgTokenSpaceGuid.PcdMaxAuthVariableSize|0x2800

  # Size of the region used by UEFI in permanent memory (Reserved 64MB)
  gArmPlatformTokenSpaceGuid.PcdSystemMemoryUefiRegionSize|0x04000000

  ## Trustzone enable (to make the transition from EL3 to EL2 in ArmPlatformPkg/Sec)
  gArmTokenSpaceGuid.PcdTrustzoneSupport|FALSE

  #
  # ARM PrimeCell
  #

  ## PL011 - Serial Terminal
  gEfiMdePkgTokenSpaceGuid.PcdUartDefaultBaudRate|38400

  ## Default Terminal Type
  ## 0-PCANSI, 1-VT100, 2-VT00+, 3-UTF8, 4-TTYTERM
!if $(TTY_TERMINAL) == TRUE
  gEfiMdePkgTokenSpaceGuid.PcdDefaultTerminalType|4
!else
  gEfiMdePkgTokenSpaceGuid.PcdDefaultTerminalType|1
!endif

  #
  # ARM Virtual Architectural Timer -- fetch frequency from QEMU (TCG) or KVM
  #
  gArmTokenSpaceGuid.PcdArmArchTimerFreqInHz|0

  # System Memory Base -- fixed at 0x4000_0000
  gArmTokenSpaceGuid.PcdSystemMemoryBase|0x40000000

  # initial location of the device tree blob passed by QEMU -- base of DRAM
  gArmVirtTokenSpaceGuid.PcdDeviceTreeInitialBaseAddress|0x40000000

  gEfiMdeModulePkgTokenSpaceGuid.PcdResetOnMemoryTypeInformationChange|FALSE
  gEfiMdeModulePkgTokenSpaceGuid.PcdBootManagerMenuFile|{ 0x21, 0xaa, 0x2c, 0x46, 0x14, 0x76, 0x03, 0x45, 0x83, 0x6e, 0x8a, 0xb6, 0xf4, 0x66, 0x23, 0x31 }

  #
  # The maximum physical I/O addressability of the processor, set with
  # BuildCpuHob().
  #
  gEmbeddedTokenSpaceGuid.PcdPrePiCpuIoSize|16

  #
  # RdkPkg Pcds
  #
  # system partition name is nothing but rootfs partition, used only in Http boot (DRI)
  gRdkTokenSpaceGuid.PcdRdkSystemPartitionName|"VenHw(837DCA9E-E874-4D82-B29A-23FE0E23D1E2,003E000A00000000)"
  gRdkTokenSpaceGuid.PcdRdkCmdLineArgs|"root=/dev/vda"
  gRdkTokenSpaceGuid.PcdRdkConfFileName|L"Rdk.conf"
  gRdkTokenSpaceGuid.PcdRdkConfFileDevicePath|L"PciRoot(0x0)/Pci(0x2,0x0)"

  gEfiMdePkgTokenSpaceGuid.PcdReportStatusCodePropertyMask|3

[PcdsFixedAtBuild.AARCH64]
  # Clearing BIT0 in this PCD prevents installing a 32-bit SMBIOS entry point,
  # if the entry point version is >= 3.0. AARCH64 OSes cannot assume the
  # presence of the 32-bit entry point anyway (because many AARCH64 systems
  # don't have 32-bit addressable physical RAM), and the additional allocations
  # below 4 GB needlessly fragment the memory map. So expose the 64-bit entry
  # point only, for entry point versions >= 3.0.
  gEfiMdeModulePkgTokenSpaceGuid.PcdSmbiosEntryPointProvideMethod|0x2

  # ACPI predates the AARCH64 architecture by 5 versions, so
  # we only target OSes that support ACPI v5.0 or later
  gEfiMdeModulePkgTokenSpaceGuid.PcdAcpiExposedTableVersions|0x20

[PcdsDynamicDefault.common]
  gEfiMdePkgTokenSpaceGuid.PcdPlatformBootTimeOut|3

  ## If TRUE, OvmfPkg/AcpiPlatformDxe will not wait for PCI
  #  enumeration to complete before installing ACPI tables.
  gEfiMdeModulePkgTokenSpaceGuid.PcdPciDisableBusEnumeration|TRUE

  # System Memory Size -- 1 MB initially, actual size will be fetched from DT
  gArmTokenSpaceGuid.PcdSystemMemorySize|0x00100000

  gArmTokenSpaceGuid.PcdArmArchTimerSecIntrNum|0x0
  gArmTokenSpaceGuid.PcdArmArchTimerIntrNum|0x0
  gArmTokenSpaceGuid.PcdArmArchTimerVirtIntrNum|0x0
  gArmTokenSpaceGuid.PcdArmArchTimerHypIntrNum|0x0

  #
  # ARM General Interrupt Controller
  #
  gArmTokenSpaceGuid.PcdGicDistributorBase|0x0
  gArmTokenSpaceGuid.PcdGicRedistributorsBase|0x0
  gArmTokenSpaceGuid.PcdGicInterruptInterfaceBase|0x0

  ## PL031 RealTimeClock
  gArmPlatformTokenSpaceGuid.PcdPL031RtcBase|0x0

  # set PcdPciExpressBaseAddress to MAX_UINT64, which signifies that this
  # PCD and PcdPciDisableBusEnumeration above have not been assigned yet
  gEfiMdePkgTokenSpaceGuid.PcdPciExpressBaseAddress|0xFFFFFFFFFFFFFFFF

  gArmTokenSpaceGuid.PcdPciIoTranslation|0x0

  #
  # Set video resolution for boot options and for text setup.
  # PlatformDxe can set the former at runtime.
  #
  gEfiMdeModulePkgTokenSpaceGuid.PcdVideoHorizontalResolution|800
  gEfiMdeModulePkgTokenSpaceGuid.PcdVideoVerticalResolution|600
  gEfiMdeModulePkgTokenSpaceGuid.PcdSetupVideoHorizontalResolution|640
  gEfiMdeModulePkgTokenSpaceGuid.PcdSetupVideoVerticalResolution|480

  #
  # SMBIOS entry point version
  #
  gEfiMdeModulePkgTokenSpaceGuid.PcdSmbiosVersion|0x0300
  gEfiMdeModulePkgTokenSpaceGuid.PcdSmbiosDocRev|0x0
  gUefiOvmfPkgTokenSpaceGuid.PcdQemuSmbiosValidated|FALSE

[PcdsDynamicHii]
  gArmVirtTokenSpaceGuid.PcdForceNoAcpi|L"ForceNoAcpi"|gArmVirtVariableGuid|0x0|FALSE|NV,BS

################################################################################
#
# Components Section - list of all EDK II Modules needed by this Platform
#
################################################################################
[Components.common]
  #
  # PEI Phase modules
  #
  ArmPlatformPkg/PrePeiCore/PrePeiCoreUniCore.inf
  MdeModulePkg/Core/Pei/PeiMain.inf
  MdeModulePkg/Universal/PCD/Pei/Pcd.inf {
    <LibraryClasses>
      PcdLib|MdePkg/Library/BasePcdLibNull/BasePcdLibNull.inf
  }
  ArmPlatformPkg/PlatformPei/PlatformPeim.inf
  ArmPlatformPkg/MemoryInitPei/MemoryInitPeim.inf
  ArmPkg/Drivers/CpuPei/CpuPei.inf

  MdeModulePkg/Universal/Variable/Pei/VariablePei.inf

  MdeModulePkg/Core/DxeIplPeim/DxeIpl.inf {
    <LibraryClasses>
      NULL|MdeModulePkg/Library/LzmaCustomDecompressLib/LzmaCustomDecompressLib.inf
  }

  #
  # DXE
  #
  MdeModulePkg/Core/Dxe/DxeMain.inf {
    <LibraryClasses>
      NULL|MdeModulePkg/Library/DxeCrc32GuidedSectionExtractLib/DxeCrc32GuidedSectionExtractLib.inf
      DevicePathLib|MdePkg/Library/UefiDevicePathLib/UefiDevicePathLib.inf
  }
  MdeModulePkg/Universal/PCD/Dxe/Pcd.inf {
    <LibraryClasses>
      PcdLib|MdePkg/Library/BasePcdLibNull/BasePcdLibNull.inf
  }

  #
  # Architectural Protocols
  #
  ArmPkg/Drivers/CpuDxe/CpuDxe.inf
  MdeModulePkg/Core/RuntimeDxe/RuntimeDxe.inf
  MdeModulePkg/Universal/Variable/RuntimeDxe/VariableRuntimeDxe.inf {
    <LibraryClasses>
      NULL|MdeModulePkg/Library/VarCheckUefiLib/VarCheckUefiLib.inf
      NULL|EmbeddedPkg/Library/NvVarStoreFormattedLib/NvVarStoreFormattedLib.inf
      # don't use unaligned CopyMem () on the UEFI varstore NOR flash region
      BaseMemoryLib|MdePkg/Library/BaseMemoryLib/BaseMemoryLib.inf
  }
!if $(SECURE_BOOT_ENABLE) == TRUE
  MdeModulePkg/Universal/SecurityStubDxe/SecurityStubDxe.inf {
    <LibraryClasses>
      NULL|SecurityPkg/Library/DxeImageVerificationLib/DxeImageVerificationLib.inf
  }
  SecurityPkg/VariableAuthenticated/SecureBootConfigDxe/SecureBootConfigDxe.inf
!else
  MdeModulePkg/Universal/SecurityStubDxe/SecurityStubDxe.inf
!endif
  MdeModulePkg/Universal/CapsuleRuntimeDxe/CapsuleRuntimeDxe.inf
  MdeModulePkg/Universal/FaultTolerantWriteDxe/FaultTolerantWriteDxe.inf
  MdeModulePkg/Universal/MonotonicCounterRuntimeDxe/MonotonicCounterRuntimeDxe.inf
  MdeModulePkg/Universal/ResetSystemRuntimeDxe/ResetSystemRuntimeDxe.inf
  EmbeddedPkg/RealTimeClockRuntimeDxe/RealTimeClockRuntimeDxe.inf {
    <LibraryClasses>
      NULL|ArmVirtPkg/Library/ArmVirtPL031FdtClientLib/ArmVirtPL031FdtClientLib.inf
  }
  EmbeddedPkg/MetronomeDxe/MetronomeDxe.inf

  MdeModulePkg/Universal/Console/ConPlatformDxe/ConPlatformDxe.inf
  MdeModulePkg/Universal/Console/ConSplitterDxe/ConSplitterDxe.inf
  MdeModulePkg/Universal/Console/GraphicsConsoleDxe/GraphicsConsoleDxe.inf
  MdeModulePkg/Universal/Console/TerminalDxe/TerminalDxe.inf
  MdeModulePkg/Universal/SerialDxe/SerialDxe.inf

  MdeModulePkg/Universal/HiiDatabaseDxe/HiiDatabaseDxe.inf

  ArmPkg/Drivers/ArmGic/ArmGicDxe.inf
  ArmPkg/Drivers/TimerDxe/TimerDxe.inf {
    <LibraryClasses>
      NULL|ArmVirtPkg/Library/ArmVirtTimerFdtClientLib/ArmVirtTimerFdtClientLib.inf
  }
  ArmPlatformPkg/Drivers/NorFlashDxe/NorFlashDxe.inf
  MdeModulePkg/Universal/WatchdogTimerDxe/WatchdogTimer.inf

  #
  # Platform Driver
  #
  ArmVirtPkg/VirtioFdtDxe/VirtioFdtDxe.inf
  ArmVirtPkg/FdtClientDxe/FdtClientDxe.inf
  ArmVirtPkg/HighMemDxe/HighMemDxe.inf
  OvmfPkg/VirtioBlkDxe/VirtioBlk.inf
  OvmfPkg/VirtioScsiDxe/VirtioScsi.inf
  OvmfPkg/VirtioNetDxe/VirtioNet.inf
  OvmfPkg/VirtioRngDxe/VirtioRng.inf

  #
  # FAT filesystem + GPT/MBR partitioning + UDF filesystem
  #
  MdeModulePkg/Universal/Disk/DiskIoDxe/DiskIoDxe.inf
  MdeModulePkg/Universal/Disk/PartitionDxe/PartitionDxe.inf
  MdeModulePkg/Universal/Disk/UnicodeCollation/EnglishDxe/EnglishDxe.inf
  FatPkg/EnhancedFatDxe/Fat.inf
  MdeModulePkg/Universal/Disk/UdfDxe/UdfDxe.inf

  #
  # Bds
  #
  MdeModulePkg/Universal/DevicePathDxe/DevicePathDxe.inf {
    <LibraryClasses>
      DevicePathLib|MdePkg/Library/UefiDevicePathLib/UefiDevicePathLib.inf
      PcdLib|MdePkg/Library/BasePcdLibNull/BasePcdLibNull.inf
  }
  MdeModulePkg/Universal/DisplayEngineDxe/DisplayEngineDxe.inf
  MdeModulePkg/Universal/SetupBrowserDxe/SetupBrowserDxe.inf
  MdeModulePkg/Universal/DriverHealthManagerDxe/DriverHealthManagerDxe.inf
  MdeModulePkg/Universal/BdsDxe/BdsDxe.inf
  MdeModulePkg/Logo/LogoDxe.inf
  MdeModulePkg/Application/UiApp/UiApp.inf {
    <LibraryClasses>
      NULL|MdeModulePkg/Library/DeviceManagerUiLib/DeviceManagerUiLib.inf
      NULL|MdeModulePkg/Library/BootManagerUiLib/BootManagerUiLib.inf
      NULL|MdeModulePkg/Library/BootMaintenanceManagerUiLib/BootMaintenanceManagerUiLib.inf
  }

  #
  # Networking stack
  #
!include NetworkPkg/Network.dsc.inc

  #
  # SCSI Bus and Disk Driver
  #
  MdeModulePkg/Bus/Scsi/ScsiBusDxe/ScsiBusDxe.inf
  MdeModulePkg/Bus/Scsi/ScsiDiskDxe/ScsiDiskDxe.inf

  #
  # SMBIOS Support
  #
  MdeModulePkg/Universal/SmbiosDxe/SmbiosDxe.inf {
    <LibraryClasses>
      NULL|OvmfPkg/Library/SmbiosVersionLib/DetectSmbiosVersionLib.inf
  }
  OvmfPkg/SmbiosPlatformDxe/SmbiosPlatformDxe.inf

  #
  # PCI support
  #
  ArmPkg/Drivers/ArmPciCpuIo2Dxe/ArmPciCpuIo2Dxe.inf {
    <LibraryClasses>
      NULL|ArmVirtPkg/Library/FdtPciPcdProducerLib/FdtPciPcdProducerLib.inf
  }
  MdeModulePkg/Bus/Pci/PciHostBridgeDxe/PciHostBridgeDxe.inf
  MdeModulePkg/Bus/Pci/PciBusDxe/PciBusDxe.inf {
    <LibraryClasses>
      NULL|ArmVirtPkg/Library/FdtPciPcdProducerLib/FdtPciPcdProducerLib.inf
  }
  OvmfPkg/VirtioPciDeviceDxe/VirtioPciDeviceDxe.inf
  OvmfPkg/Virtio10Dxe/Virtio10.inf

  #
  # Video support
  #
  OvmfPkg/QemuRamfbDxe/QemuRamfbDxe.inf
  OvmfPkg/VirtioGpuDxe/VirtioGpu.inf
  OvmfPkg/PlatformDxe/Platform.inf

  #
  # USB Support
  #
  MdeModulePkg/Bus/Pci/UhciDxe/UhciDxe.inf
  MdeModulePkg/Bus/Pci/EhciDxe/EhciDxe.inf
  MdeModulePkg/Bus/Pci/XhciDxe/XhciDxe.inf
  MdeModulePkg/Bus/Usb/UsbBusDxe/UsbBusDxe.inf
  MdeModulePkg/Bus/Usb/UsbKbDxe/UsbKbDxe.inf
  MdeModulePkg/Bus/Usb/UsbMassStorageDxe/UsbMassStorageDxe.inf

  #
  # ACPI Support
  #
  ArmVirtPkg/PlatformHasAcpiDtDxe/PlatformHasAcpiDtDxe.inf

  #
  # RdkPkg
  #
  Platform/Comcast/Application/Dri/Dri.inf
  Platform/Comcast/Application/SecureBoot/SecureBoot.inf
  Platform/Comcast/Application/DriSecureBoot/DriSecureBoot.inf

  # Status Code Routing
  #
  MdeModulePkg/Universal/ReportStatusCodeRouter/RuntimeDxe/ReportStatusCodeRouterRuntimeDxe.inf

[Components.AARCH64]
  MdeModulePkg/Universal/Acpi/BootGraphicsResourceTableDxe/BootGraphicsResourceTableDxe.inf
  OvmfPkg/AcpiPlatformDxe/QemuFwCfgAcpiPlatformDxe.inf {
    <LibraryClasses>
      NULL|ArmVirtPkg/Library/FdtPciPcdProducerLib/FdtPciPcdProducerLib.inf
  }
