##  @file  Vlv2DeviceRefCodePkg.dec
#
# Copyright (c) 2012  - 2019, Intel Corporation. All rights reserved
#
# SPDX-License-Identifier: BSD-2-Clause-Patent
#
#
##

[Defines]
  DEC_SPECIFICATION              = 0x00010005
  PACKAGE_NAME                   = Vlv2DeviceRefCodePkg
  PACKAGE_GUID                   = E4FA0DCA-91A3-4957-9344-C10BAA0BFE5F
  PACKAGE_VERSION                = 0.1

[Ppis]
  gVlvPolicyPpiGuid                                           = { 0x7D84B2C2, 0x22A1, 0x4372, {0xB1, 0x2C, 0xEB, 0xB2, 0x32, 0xD3, 0xA6, 0xA3}}
  gVlvMmioPolicyPpiGuid                                       = { 0xE767BF7F, 0x4DB6, 0x5B34, {0x10, 0x11, 0x4F, 0xBE, 0x4C, 0xA7, 0xAF, 0xD2}}
  gPeiSmbusPolicyPpiGuid                            = { 0x63b6e435, 0x32bc, 0x49c6, {0x81, 0xbd, 0xb7, 0xa1, 0xa0, 0xfe, 0x1a, 0x6c}}
  gSeCfTPMPpiGuid                       = { 0x10e26df1, 0x8775, 0x4ee1, {0xb5, 0x0a, 0x3a, 0xe8, 0x28, 0x93, 0x70, 0x3a}}
  gPchUsbPolicyPpiGuid                  = { 0xc02b0573, 0x2b4e, 0x4a31, {0xa3, 0x1a, 0x94, 0x56, 0x7b, 0x50, 0x44, 0x2c}}
  gPchInitPpiGuid                       = { 0x09ea894a, 0xbe0d, 0x4230, {0xa0, 0x03, 0xed, 0xc6, 0x93, 0xb4, 0x8e, 0x95}}
  gPchPlatformPolicyPpiGuid             = { 0x15344673, 0xD365, 0x4BE2, {0x85, 0x13, 0x14, 0x97, 0xCC, 0x07, 0x61, 0x1D}}
  gPeiSpiPpiGuid                        = { 0xA38C6898, 0x2B5C, 0x4FF6, {0x93, 0x26, 0x2E, 0x63, 0x21, 0x2E, 0x56, 0xC2}}
  gVlvPeiInitPpiGuid                    = { 0x09ea8911, 0xbe0d, 0x4230, {0xa0, 0x03, 0xed, 0xc6, 0x93, 0xb4, 0x8e, 0x11}}
  gSeCUmaPpiGuid                        = { 0xcbd86677, 0x362f, 0x4c04, {0x94, 0x59, 0xa7, 0x41, 0x32, 0x6e, 0x05, 0xcf}}
  gPeiSeCPlatformPolicyPpiGuid          = { 0x7ae3ceb7, 0x2ee2, 0x48fa, {0xaa, 0x49, 0x35, 0x10, 0xbc, 0x83, 0xca, 0xbf}}
  gPeiHeciPpiGuid                       = { 0xEE0EA811, 0xFBD9, 0x4777, {0xB9, 0x5A, 0xBA, 0x4F, 0x71, 0x10, 0x1F, 0x74}}
  gPeiSdhcPpiGuid                       = { 0xf4ef9d7a, 0x98c5, 0x4c1a, {0xb4, 0xd9, 0xd8, 0xd8, 0x72, 0x65, 0xbe, 0x0c}}
  gPeiBlockIoPpiGuid                    = { 0xbc5fa650, 0xedbb, 0x4d0d, {0xb3, 0xa3, 0xd9, 0x89, 0x07, 0xf8, 0x47, 0xdf}}
  gSeCfTPMPolicyPpiGuid                 = { 0x4fd1ba49, 0x8f90, 0x471a, {0xa2, 0xc9, 0x17, 0x3c, 0x7a, 0x73, 0x2f, 0xd0}}
  gEfiPeiReadOnlyVariable2PpiGuid       = { 0x2ab86ef5, 0xecb5, 0x4134, {0xb5, 0x56, 0x38, 0x54, 0xca, 0x1f, 0xe1, 0xb4}}
  gPchPeiInitPpiGuid                    = { 0xACB93B08, 0x5CDC, 0x4A8F, {0x93, 0xD4, 0x6, 0xE3, 0x42, 0xDF, 0x18, 0x2E}}
  gPttPassThruPpiGuid                   = { 0xc5068bac, 0xa7dc, 0x42f1, {0xae, 0x80, 0xca, 0xa2, 0x4b, 0xb4, 0x90, 0x4b}}

[Protocols]
  gEfiGlobalNvsAreaProtocolGuid         = { 0x074e1e48, 0x8132, 0x47a1, {0x8c, 0x2c, 0x3f, 0x14, 0xad, 0x9a, 0x66, 0xdc}}
  gPpmPlatformPolicyProtocolGuid        = { 0xddabfeac, 0xef63, 0x452c, {0x8f, 0x39, 0xed, 0x7f, 0xae, 0xd8, 0x26, 0x5e}}
  gEfiSpiProtocolGuid                   = { 0x1156efc6, 0xea32, 0x4396, {0xb5, 0xd5, 0x26, 0x93, 0x2e, 0x83, 0xc3, 0x13}}
  gMemInfoProtocolGuid                  = { 0x6f20f7c8, 0xe5ef, 0x4f21, {0x8d, 0x19, 0xed, 0xc5, 0xf0, 0xc4, 0x96, 0xae}}
  gEfiSdHostIoProtocolGuid              = { 0xb63f8ec7, 0xa9c9, 0x4472, {0xa4, 0xc0, 0x4d, 0x8b, 0xf3, 0x65, 0xcc, 0x51}}
  gEfiSmmSpiProtocolGuid                = { 0xD9072C35, 0xEB8F, 0x43AD, {0xA2, 0x20, 0x34, 0xD4, 0x0E, 0x2A, 0x82, 0x85}}
  gEfiSmmIchnDispatchProtocolGuid       = { 0xc50b323e, 0x9075, 0x4f2a, { 0xac, 0x8e, 0xd2, 0x59, 0x6a, 0x10, 0x85, 0xcc}}
  gEfiSmmIchnDispatchExProtocolGuid     = { 0x3920405B, 0xC897, 0x44DA, {0x88, 0xF3, 0x4C, 0x49, 0x8A, 0x6F, 0xF7, 0x36}}
  gEfiPchS3SupportProtocolGuid          = { 0xE287D20B, 0xD897, 0x4E1E, {0xA5, 0xD9, 0x97, 0x77, 0x63, 0x93, 0x6A, 0x04}}
  gPchResetProtocolGuid                 = { 0xDB63592C, 0xB8CC, 0x44C8, {0x91, 0x8C, 0x51, 0xF5, 0x34, 0x59, 0x8A, 0x5A}}
  gPchResetCallbackProtocolGuid         = { 0x3A3300AB, 0xC929, 0x487D, {0xAB, 0x34, 0x15, 0x9B, 0xC1, 0x35, 0x62, 0xC0}}
  gDxePchPlatformPolicyProtocolGuid     = { 0x4b0165a9, 0x61d6, 0x4e23, {0xa0, 0xb5, 0x3e, 0xc7, 0x9c, 0x2e, 0x30, 0xd5}}
  gEfiPchInfoProtocolGuid               = { 0xD31F0400, 0x7D16, 0x4316, {0xBF, 0x88, 0x60, 0x65, 0x88, 0x3B, 0x40, 0x2B}}
  gEfiPchExtendedResetProtocolGuid      = { 0xF0BBFCA0, 0x684E, 0x48B3, {0xBA, 0xE2, 0x6C, 0x84, 0xB8, 0x9E, 0x53, 0x39}}
  gEfiActiveBiosProtocolGuid            = { 0xEBBE2D1B, 0x1647, 0x4BDA, {0xAB, 0x9A, 0x78, 0x63, 0xE3, 0x96, 0xD4, 0x1A}}
  gDxeIchPlatformPolicyProtocolGuid     = { 0xf617b358, 0x12cf, 0x414a, {0xa0, 0x69, 0x60, 0x67, 0x7b, 0xda, 0x13, 0xb3}}
  gEfiIchInfoProtocolGuid               = { 0xd31f0400, 0x7d16, 0x4316, {0xbf, 0x88, 0x60, 0x65, 0x88, 0x3b, 0x40, 0x2b}}
  gEfiSmmIoTrapDispatchProtocolGuid     = { 0x58dc368d, 0x7bfa, 0x4e77, {0xab, 0xbc, 0x0e, 0x29, 0x41, 0x8d, 0xf9, 0x30}}
  gEfiSmmSmbusProtocolGuid              = { 0x72e40094, 0x2ee1, 0x497a, {0x8f, 0x33, 0x4c, 0x93, 0x4a, 0x9e, 0x9c, 0x0c}}
  gDxeVlvPlatformPolicyGuid             = { 0x5bab88ba, 0xe0e2, 0x4674, {0xb6, 0xad, 0xb8, 0x12, 0xf6, 0x88, 0x1c, 0xd6}}
  gIgdOpRegionProtocolGuid              = { 0xcdc5dddf, 0xe79d, 0x41ec, {0xa9, 0xb0, 0x65, 0x65, 0x49, 0x0d, 0xb9, 0xd3}}
  gEfiHeciProtocolGuid                  = { 0xcfb33810, 0x6e87, 0x4284, {0xb2, 0x03, 0xa6, 0x6a, 0xbe, 0x07, 0xf6, 0xe8}}
  gPlatformSeCHookProtocolGuid          = { 0xbc52476e, 0xf67e, 0x4301, {0xb2, 0x62, 0x36, 0x9c, 0x48, 0x78, 0xaa, 0xc2}}
  gEfiSeCRcInfoProtocolGuid             = { 0x11fbfdfb, 0x10d2, 0x43e6, {0xb5, 0xb1, 0xb4, 0x38, 0x6e, 0xdc, 0xcb, 0x9a}}
  gEfiTdtProtocolGuid                   = { 0x0bf70067, 0xd53b, 0x42df, {0xb7, 0x70, 0xe9, 0x2c, 0x91, 0xc6, 0x14, 0x11}}
  gDxePlatformSeCPolicyGuid             = { 0xf8bff014, 0x18fb, 0x4ef9, {0xb1, 0x0c, 0xae, 0x22, 0x73, 0x8d, 0xbe, 0xed}}
  gLpssDummyProtocolGuid                = { 0xaf4cc162, 0xd41c, 0x455a, {0xab, 0x45, 0x6d, 0xbc, 0xc1, 0xcd, 0x32, 0xf3}}
  gEfiEmmcCardInfoProtocolGuid          = { 0x1ebe5ab9, 0x2129, 0x49e7, {0x84, 0xd7, 0xee, 0xb9, 0xfc, 0xe5, 0xde, 0xdd}}
  gEfiTdtOperationProtocolGuid          = {0xfd301ba4, 0x5e62, 0x4679,{ 0xa0, 0x6f, 0xe0, 0x9a, 0xab, 0xdd, 0x2a, 0x91}}
  gEfiConfigFileNameGuid            = { 0x98B8D59B, 0xE8BA, 0x48EE, { 0x98, 0xDD, 0xC2, 0x95, 0x39, 0x2F, 0x1E, 0xDB }}
  gEfiDFUResultGuid                 = { 0x14a7c46f, 0xbc02, 0x4047, { 0x9f, 0x18, 0xa5, 0xd7, 0x25, 0xd8, 0xbd, 0x19 }}
  gPttPassThruProtocolGuid          = { 0x73e2576, 0xf6c1, 0x4b91, { 0x92, 0xa9, 0xd4, 0x67, 0x5d, 0xda, 0x34, 0xb1 } }
  
[Guids]
  gEfiCPTokenSpaceGuid                  = { 0x918211ce, 0xa1d2, 0x43a0, {0xa0, 0x4e, 0x75, 0xb5, 0xbf, 0x44, 0x50, 0x0E}}
  gEfiSmbusArpMapGuid                   = { 0x707BE83E, 0x0BF6, 0x40A5, {0xBE, 0x64, 0x34, 0xC0, 0x3A, 0xA0, 0xB8, 0xE2}}
  gEfiMemoryConfigDataGuid              = { 0x80dbd530, 0xb74c, 0x4f11, {0x8c, 0x03, 0x41, 0x86, 0x65, 0x53, 0x28, 0x31}}
  gEfiVLVTokenSpaceGuid                 = { 0xca452c68, 0xdf0c, 0x45c9, {0x82, 0xfb, 0xea, 0xe4, 0x2b, 0x31, 0x29, 0x46}}
  gSataControllerDriverGuid             = { 0xbb929da9, 0x68f7, 0x4035, {0xb2, 0x2c, 0xa3, 0xbb, 0x3f, 0x23, 0xda, 0x55}}
  gDxePchPolicyUpdateProtocolGuid       = { 0x1a819e49, 0xd8ee, 0x48cb, {0x9a, 0x9c, 0x0a, 0xa0, 0xd2, 0x81, 0x0a, 0x38}}
  gPowerManagementAcpiTableStorageGuid  = { 0x161be597, 0xe9c5, 0x49db, {0xae, 0x50, 0xc4, 0x62, 0xab, 0x54, 0xee, 0xda}}
  gEfiSetupVariableGuid                 = { 0xec87d643, 0xeba4, 0x4bb5, {0xa1, 0xe5, 0x3f, 0x3e, 0x36, 0xb2, 0x0d, 0xa9}}
  gBmpImageGuid                         = { 0x878AC2CC, 0x5343, 0x46F2, {0xB5, 0x63, 0x51, 0xF8, 0x9D, 0xAF, 0x56, 0xBA}}
  gPchInitVariableGuid                  = { 0xe6c2f70a, 0xb604, 0x4877, {0x85, 0xba, 0xde, 0xec, 0x89, 0xe1, 0x17, 0xeb}}
  gEfiMemoryConfigDataGuid              = { 0x80dbd530, 0xb74c, 0x4f11, {0x8c, 0x03, 0x41, 0x86, 0x65, 0x53, 0x28, 0x31}}
  gVlvRefCodePkgTokenSpaceGuid          = { 0x85768E4A, 0x6CDC, 0x444E, {0x93, 0xDF, 0x93, 0x66, 0x85, 0xB5, 0xDF, 0xCC}}
  gSeCPlatformReadyToBootGuid           = { 0x03fdf171, 0x1d67, 0x4ace, {0xa9, 0x04, 0x3e, 0x36, 0xd3, 0x38, 0xfa, 0x74}}
  gAmtReadyToBootGuid                   = { 0x40b09b5a, 0xf0ef, 0x4627, {0x93, 0xd5, 0x27, 0xf0, 0x4b, 0x75, 0x4d, 0x05}}
  #
  # According to UEFI 2.3.1 Errata C, 3.2 Globally Defined Variables.
  # To prevent name collisions with possible future globally defined variables,
  # other internal firmware data variables that are not defined in Table.10 must be saved with a unique VendorGuid other than EFI_GLOBAL_VARIABLE.
  #
  gEfiVlv2VariableGuid                  = { 0x10ba6bbe, 0xa97e, 0x41c3, {0x9a, 0x07, 0x60, 0x7a, 0xd9, 0xbd, 0x60, 0xe5}}

[Includes.common]
  .
  ValleyView2Soc/NorthCluster/Include
  ValleyView2Soc/SouthCluster/Include
  ValleyView2Soc/CPU/Include
  Include

[PcdsFixedAtBuild]
  gEfiVLVTokenSpaceGuid.PcdTCSmbaIoBaseAddress|0x1040|UINT16|0x10000207

[PcdsDynamic, PcdsDynamicEx]
  gEfiVLVTokenSpaceGuid.PcdTCSmbaIoBaseAddress|0x1040|UINT16|0x10000207
  gEfiVLVTokenSpaceGuid.PcdEmmcManufacturerId|0|UINT8|0x10000208
  gEfiVLVTokenSpaceGuid.PcdProductSerialNumber|0|UINT32|0x10000209
  gEfiVLVTokenSpaceGuid.PcdMeasuredBootEnable|TRUE|BOOLEAN|0x1000020A
  gEfiVLVTokenSpaceGuid.PcdFTPMErrorOccur|FALSE|BOOLEAN|0x1000020B
  gEfiVLVTokenSpaceGuid.PcdFTPMErrorSkip|FALSE|BOOLEAN|0x1000020C
  gEfiVLVTokenSpaceGuid.PcdFTPMCommand|0|UINT32|0x1000020D
  gEfiVLVTokenSpaceGuid.PcdFTPMResponse|0|UINT32|0x1000020E
  gEfiVLVTokenSpaceGuid.PcdFTPMNotRespond|FALSE|BOOLEAN|0x1000020F
  gEfiVLVTokenSpaceGuid.PcdFTPMStatus|0|UINT32|0x10000210
  gEfiVLVTokenSpaceGuid.PcdCpuLockBoxDataAddress|0x0|UINT64|0x10000211
  gEfiVLVTokenSpaceGuid.PcdCpuSmramCpuDataAddress|0x0|UINT64|0x10000212
  gEfiVLVTokenSpaceGuid.PcdCpuLockBoxSize|0x0|UINT64|0x10000213

[PcdsFeatureFlag]
  gVlvRefCodePkgTokenSpaceGuid.PcdCeAtaSupport|FALSE|BOOLEAN|0x12
  gVlvRefCodePkgTokenSpaceGuid.PcdMmcSdMultiBlockSupport|TRUE|BOOLEAN|0x13

[PcdsPatchableInModule]

  ## Memory Down or DIMM slot.<BR><BR>
  #  0 - DIMM<BR>
  #  1 - Memory Down<BR>
  # @Prompt Enable Memory Down
  # @ValidList 0x80000001 | 0, 1
  gVlvRefCodePkgTokenSpaceGuid.PcdEnableMemoryDown|1|UINT8|0x20000000
  
  ## Memory Parameter Patchable.<BR><BR>
  #  0 - Fixed Parameter for MinnowBoard Max<BR>
  #  1 - Patchable Parameter for Customization<BR>
  # @Prompt Memory Parameter Patchable.
  # @ValidList 0x80000001 | 0, 1  
  gVlvRefCodePkgTokenSpaceGuid.PcdMemoryParameterPatchable|FALSE|BOOLEAN|0x20000010
    
  ## The speed of DRAM.<BR><BR>
  #  0 - 800 MHz<BR>
  #  1 - 1066 MHz<BR>
  #  2 - 1333 MHz<BR>
  #  3 - 1600 MHz<BR>
  # @Prompt DRAM Speed
  # @ValidList 0x80000001 | 0, 1, 2, 3
  gVlvRefCodePkgTokenSpaceGuid.PcdDramSpeed|1|UINT8|0x20000001

  ## DRAM Type.<BR><BR>
  #  0 - DDR3<BR>
  #  1 - DDR3L<BR>
  #  2 - DDR3U<BR>
  #  3 - DDR3All<BR>
  #  4 - LPDDR2<BR>
  #  5 - LPDDR3<BR>
  #  6 - DDR4<BR>
  # @Prompt DRAM Type
  # @ValidList 0x80000001 | 0, 1, 2, 3, 4, 5, 6
  gVlvRefCodePkgTokenSpaceGuid.PcdDramType|1|UINT8|0x20000002
    
  ## Please populate DIMM slot 0 if only one DIMM is supported.<BR><BR>
  #  0 - Disable<BR>
  #  1 - Enable<BR>
  # @Prompt DIMM 0 Enable 
  # @ValidList 0x80000001 | 0, 1
  gVlvRefCodePkgTokenSpaceGuid.PcdEnableDimm0|1|UINT8|0x20000003

  ## DIMM 1 has to be identical to DIMM 0.<BR><BR>
  #  0 - Disable<BR>
  #  1 - Enable<BR>
  # @Prompt DIMM 1 Enable Type
  # @ValidList 0x80000001 | 0, 1
  gVlvRefCodePkgTokenSpaceGuid.PcdEnableDimm1|0|UINT8|0x20000004
  
  ## DRAM device data width.<BR><BR>
  #  0 - x8<BR>
  #  1 - x16<BR>
  #  2 - x32<BR>
  # @Prompt DIMM_DWIDTH
  # @ValidList 0x80000001 | 0, 1, 2
  gVlvRefCodePkgTokenSpaceGuid.PcdDimmDataWidth|1|UINT8|0x20000005

  ## DRAM device data density.<BR><BR>
  #  0 - 1 Gbit<BR>
  #  1 - 2 Gbit<BR>
  #  2 - 4 Gbit<BR>
  #  3 - 8 Gbit<BR>
  # @Prompt DIMM_Density
  # @ValidList 0x80000001 | 0, 1, 2, 3
  gVlvRefCodePkgTokenSpaceGuid.PcdDimmDensity|2|UINT8|0x20000006
  
  ## DRAM device data bus width.<BR><BR>
  #  0 - 8 bits<BR>
  #  1 - 16 bits<BR>
  #  2 - 32 bits<BR>
  #  3 - 64 bits<BR>
  # @Prompt DIMM_BusWidth
  # @ValidList 0x80000001 | 0, 1, 2, 3
  gVlvRefCodePkgTokenSpaceGuid.PcdDimmBusWidth|3|UINT8|0x20000007

  ## Ranks Per DIMM or Sides Per DIMM.<BR><BR>
  #  0 - 1 Rank<BR>
  #  1 - 2 Ranks<BR>
  # @Prompt DIMM_Sides
  # @ValidList 0x80000001 | 0, 1
  gVlvRefCodePkgTokenSpaceGuid.PcdRankPerDimm|0|UINT8|0x20000008

  ## tCL.<BR><BR>
  # @Prompt tCL
  gVlvRefCodePkgTokenSpaceGuid.PcdTcl|11|UINT8|0x20000009

  ## tRP and tRCD in DRAM clk - 5:12.5ns, 6:15ns, etc.<BR><BR>   
  # @Prompt tRP_tRCD 
  gVlvRefCodePkgTokenSpaceGuid.PcdTrpTrcd|11|UINT8|0x2000000A

  ## tWR in DRAM clk.<BR><BR>   
  # @Prompt tWR 
  gVlvRefCodePkgTokenSpaceGuid.PcdTwr|12|UINT8|0x2000000B
  
  ## tWTR in DRAM clk.<BR><BR>   
  # @Prompt tWTR 
  gVlvRefCodePkgTokenSpaceGuid.PcdTwtr|6|UINT8|0x2000000C
  
  ## tRRD in DRAM clk.<BR><BR>   
  # @Prompt tRRD 
  gVlvRefCodePkgTokenSpaceGuid.PcdTrrd|6|UINT8|0x2000000D
   
  ## tRTP in DRAM clk.<BR><BR>   
  # @Prompt tRTP 
  gVlvRefCodePkgTokenSpaceGuid.PcdTrtp|6|UINT8|0x2000000E

  ## tFAW in DRAM clk.<BR><BR>   
  # @Prompt tFAW 
  gVlvRefCodePkgTokenSpaceGuid.PcdTfaw|32|UINT8|0x2000000F
