/** @file
 * Copyright (c) 2018, Linaro Limited. All rights reserved.
 *
 * SPDX-License-Identifier: BSD-2-Clause-Patent
 */

#include "Secure96.h"

//
// Define a placeholder value for the GPIO phandle property cells appearing
// in this file. It is up to the driver code to discover the actual phandle
// value from the platform device tree and patch the overlay DTB before it
// can be applied.
//
#define GPIO_PARENT_PLACEHOLDER_PHANDLE     0x0

/dts-v1/;

/ {
    fragment@0 {
        target-path = "I2C_PARENT_PLACEHOLDER_STRING";
        __overlay__ {
            clock-frequency = <100000>;

            ATSHA204A_DT_NODENAME {
                compatible = "atmel,atsha204a";
                reg = <ATSHA204A_SLAVE_ADDRESS>;
            };

            ATECC508A_DT_NODENAME {
                compatible = "atmel,atecc508a";
                reg = <ATECC508A_SLAVE_ADDRESS>;
            };
        };
    };

    fragment@1 {
        target-path = "SPI_PARENT_PLACEHOLDER_STRING";
        __overlay__ {
            INFINEON_SLB9670_DT_NODENAME {
                compatible = "infineon,slb9670";
                reg = <SECURE96_SPI0_CS>;
                spi-max-frequency = <22500000>;
            };
        };
    };

    fragment@2 {
        target-path = "/";
        __overlay__ {
            gpio-leds {
                compatible = "gpio-leds";

                secure96-u1 {
                    gpios = <GPIO_PARENT_PLACEHOLDER_PHANDLE
                             FixedPcdGet32 (PcdGpioPinG)
                             FixedPcdGet32 (PcdGpioPolarity)>;
                };
                secure96-u2 {
                    gpios = <GPIO_PARENT_PLACEHOLDER_PHANDLE
                             FixedPcdGet32 (PcdGpioPinF)
                             FixedPcdGet32 (PcdGpioPolarity)>;
                };
                secure96-u3 {
                    gpios = <GPIO_PARENT_PLACEHOLDER_PHANDLE
                             FixedPcdGet32 (PcdGpioPinI)
                             FixedPcdGet32 (PcdGpioPolarity)>;
                };
                secure96-u4 {
                    gpios = <GPIO_PARENT_PLACEHOLDER_PHANDLE
                             FixedPcdGet32 (PcdGpioPinH)
                             FixedPcdGet32 (PcdGpioPolarity)>;
                };
            };
        };
    };
};
