#  Copyright (c) 2011, ARM Limited. All rights reserved.
#
#  SPDX-License-Identifier: BSD-2-Clause-Patent
#

[Defines]
  INF_VERSION                    = 0x00010005
  BASE_NAME                      = MMC
  FILE_GUID                      = 100c2cfa-b586-4198-9b4c-1683d195b1da
  MODULE_TYPE                    = DXE_DRIVER
  VERSION_STRING                 = 1.0

  ENTRY_POINT                    = MMCInitialize


[Sources.common]
  MmcHostDxe.c

[Packages]
  EmbeddedPkg/EmbeddedPkg.dec
  MdePkg/MdePkg.dec
  Silicon/TexasInstruments/Omap35xxPkg/Omap35xxPkg.dec

[LibraryClasses]
  PcdLib
  UefiLib
  UefiDriverEntryPoint
  MemoryAllocationLib
  IoLib
  OmapDmaLib
  DmaLib

[Guids]

[Protocols]
  gEfiBlockIoProtocolGuid
  gEfiCpuArchProtocolGuid
  gEfiDevicePathProtocolGuid
  gEmbeddedExternalDeviceProtocolGuid
  gEfiMmcHostProtocolGuid

[Pcd]
  gOmap35xxTokenSpaceGuid.PcdOmap35xxMMCHS1Base
  gOmap35xxTokenSpaceGuid.PcdMmchsTimerFreq100NanoSeconds

[depex]
  gEmbeddedExternalDeviceProtocolGuid
