## @file
# Firmware Boot Media Info Module
#
# This module publishes firmware boot media device information used in the boot flow for system initialization
# decisions dependent upon the firmware boot media.
#
# This module depends upon a library instance to actually perform firmware boot media device detection since the
# detection mechanism will vary across systems. In many cases, the media type may simply be set to a single firmware
# boot media device with no run-time logic required. In any case, this module should dispatch as early as possible in
# the system boot flow so the firmware boot media information is available for other modules. If any dependencies are
# required to dynamically determine the firmware boot media device, those should be in the DEPEX section of the active
# FirmwareBootMediaInfoLib such that this module will dispatch once those dependencies are satisfied.
#
# Copyright (c) 2019, Intel Corporation. All rights reserved.<BR>
#
#  SPDX-License-Identifier: BSD-2-Clause-Patent
#
##

[Defines]
  INF_VERSION       = 0x00010017
  BASE_NAME         = FirmwareBootMediaInfoPei
  FILE_GUID         = A8F14FA9-FC88-45F4-A622-F06E6C56E632
  VERSION_STRING    = 1.0
  MODULE_TYPE       = PEIM
  ENTRY_POINT       = FirmwareBootMediaInfoPeiEntry

[LibraryClasses]
  BaseLib
  DebugLib
  FirmwareBootMediaLib
  FirmwareBootMediaInfoLib
  HobLib
  PeimEntryPoint
  PeiServicesLib

[Packages]
  MdePkg/MdePkg.dec
  IntelSiliconPkg/IntelSiliconPkg.dec
  BoardModulePkg/BoardModulePkg.dec

[Sources]
  FirmwareBootMediaInfoPei.c

[Depex]
  TRUE
