// /** @file
// OEM Config Library used by UiApp
//
//
//  Copyright (c) 2018, Hisilicon Limited. All rights reserved.
//  Copyright (c) 2018, Linaro Limited. All rights reserved.
//
// SPDX-License-Identifier: BSD-2-Clause-Patent
//
// **/
#langdef   en-US "English"

#string STR_BMC_WATCHDOG_TIMER                      #language en-US  "iBMC WDT Support For POST"
#string STR_BMC_WATCHDOG_TIMER_HELP                 #language en-US  "Enable/Disable iBMC watchdog timer at start of POST."
#string STR_BMC_WATCHDOG_TIMER_TIMEOUT              #language en-US  "iBMC WDT TimeOut For POST"
#string STR_BMC_WATCHDOG_TIMER_TIMEOUT_C10_HELP     #language en-US  "Enter the number of minutes the system firmware has to boot the OS before it takes the Timeout Action. Valid values are from 15 to 25 minutes."
#string STR_BMC_WATCHDOG_TIMER_ACTION               #language en-US  "iBMC WDT Action For POST"
#string STR_BMC_WATCHDOG_TIMER_ACTION_HELP          #language en-US  "Timeout Action Choices: No Action, Hard Reset, Power Down or Power Cycle"
#string STR_BMC_WATCHDOG_TIMER_NO_ACTION            #language en-US  "No Action"
#string STR_BMC_WATCHDOG_TIMER_HARD_RESET           #language en-US  "Hard Reset"
#string STR_BMC_WATCHDOG_TIMER_POWER_DOWN           #language en-US  "Power Down"
#string STR_BMC_WATCHDOG_TIMER_POWER_CYCLE          #language en-US  "Power Cycle"
#string STR_BMC_OS_WATCHDOG_TIMER                   #language en-US  "iBMC WDT Support For OS"
#string STR_BMC_OS_WATCHDOG_TIMER_HELP              #language en-US  "Enable/Disable OS Watchdog Timer When OS Load"
#string STR_BMC_OS_WDT_TIMEOUT                      #language en-US  "iBMC WDT TimeOut For OS"
#string STR_BMC_OS_WDT_TIMEOUT_HELP                 #language en-US  "Enter the number of minutes the system firmware \n has to OS Load before it takes the Timeout Action. Valid values are from 5 to 8 minutes."
#string STR_BMC_OS_WDT_ACTION                       #language en-US  "iBMC WDT Action For OS"

