#/** @file
# Arm Versatile Express package.
#
#  Copyright (c) 2012-2018, ARM Limited. All rights reserved.
#
#  SPDX-License-Identifier: BSD-2-Clause-Patent
#
#**/

[Defines]
  DEC_SPECIFICATION              = 0x00010005
  PACKAGE_NAME                   = ArmVExpressPkg
  PACKAGE_GUID                   = 9c0aaed4-74c5-4043-b417-a3223814ce76
  PACKAGE_VERSION                = 0.1

################################################################################
#
# Include Section - list of Include Paths that are provided by this package.
#                   Comments are used for Keywords and Module Types.
#
# Supported Module Types:
#  BASE SEC PEI_CORE PEIM DXE_CORE DXE_DRIVER DXE_RUNTIME_DRIVER DXE_SMM_DRIVER DXE_SAL_DRIVER UEFI_DRIVER UEFI_APPLICATION
#
################################################################################
[Includes.common]
  Include                        # Root include for the package

[LibraryClasses]
  ArmPlatformSysConfigLib|Include/Library/ArmPlatformSysConfigLib.h
  LcdPlatformLib|Include/Library/LcdPlatformLib.h

[Guids.common]
  gArmVExpressTokenSpaceGuid    =  { 0x9c0aaed4, 0x74c5, 0x4043, { 0xb4, 0x17, 0xa3, 0x22, 0x38, 0x14, 0xce, 0x76 } }

[PcdsFeatureFlag.common]

[PcdsFixedAtBuild.common]
  #
  # MaxMode must be one number higher than the actual max mode,
  # i.e. for actual maximum mode 2, set the value to 3.
  #
  # For a list of mode numbers look in LcdArmVExpress.c
  #
  gArmVExpressTokenSpaceGuid.PcdPL111LcdMaxMode|3|UINT32|0x00000002
  gArmVExpressTokenSpaceGuid.PcdPL111LcdVideoModeOscId|1|UINT32|0x00000003

  gArmVExpressTokenSpaceGuid.PcdHdLcdVideoModeOscId|0|UINT32|0x00000005
  gArmVExpressTokenSpaceGuid.PcdArmMaliDpMaxMode|0|UINT32|0x00000008

  #
  # Device path of block device on which Fastboot will flash partitions
  #
  gArmVExpressTokenSpaceGuid.PcdAndroidFastbootNvmDevicePath|""|VOID*|0x00000006
  gArmVExpressTokenSpaceGuid.PcdAndroidFastbootProductName|""|VOID*|0x00000007
