## @file
# FDF file of Clanton Peak CRB platform with 32-bit DXE
#
# This package provides QuarkNcSocId platform specific modules.
# Copyright (c) 2013 - 2019 Intel Corporation.
#
# SPDX-License-Identifier: BSD-2-Clause-Patent
#
##

################################################################################
#
# Defines Section - statements that will be processed to create a Makefile.
#
################################################################################
[Defines]
#                  Address 0x100000000 (4 GB reset address)
#                                 Base                               Size
#                                      +---------------------------+
#                           FLASH_BASE | FD.Quark:                 | 0x800000 (8 MB)
#                           0xFF800000 | BaseAddress               |
#                                      +---------------------------+
#
# Flash offsets are 0 based, but are relative to FD.Quark BaseAddress, e.g. Payload Base is at 0x400000, Flash Base is at 0xFF800000 for 8 MB SPI part.
# 0xFF800000 + 0x400000 = 0xFFC00000.
#
#                          Address 0x0 (0xFF800000 for 8 MB SPI part)
#                                      +---------------------------+
#                FLASH_FV_PAYLOAD_BASE | Payload Image             | FLASH_FV_PAYLOAD_SIZE
#                           0x00400000 |                           | 0x00100000
#                                      +---------------------------+
#                   FLASH_FV_MAIN_BASE | FvMain Image (Compressed) | FLASH_FV_MAIN_SIZE
#                           0x00500000 |                           | 0x001E0000
#                                      +---------------------------+
#                      NVRAM_AREA_BASE | NVRAM Area=               | NVRAM_AREA_SIZE
#                           0x006E0000 | Variable + FTW Working +  |
#                                      | FTW Spare                 |
#                                      +---+-------------------+---+
#                 NVRAM_AREA_VARIABLE_BASE |                   | NVRAM_AREA_VARIABLE_SIZE
#                                          |                   |
#                                          +-------------------+
#                         FTW_WORKING_BASE |                   | FTW_WORKING_SIZE
#                                          |                   |
#                                          +-------------------+
#                           FTW_SPARE_BASE |                   | FTW_SPARE_SIZE
#                                          |                   |
#                                      +---+-------------------+---+
#                      RMU_BINARY_BASE | RMU Binary                | RMU_BINARY_SIZE
#                           0x00700000 |                           | 0x00008000
#                                      +---------------------------+
#                   PLATFORM_DATA_BASE | PlatformData Binary       | PLATFORM_DATA_SIZE
#                           0x00710000 |                           | 0x00001000
#                                      +---------------------------+
#                FVRECOVERY_IMAGE_BASE | FVRECOVERY Image          | FVRECOVERY_IMAGE_SIZE
#                             0x720000 |                           | 0x000E0000
#                                      +---------------------------+

  #
  # Define value used to compute FLASH regions below reset vector location just below 4GB
  #
  DEFINE RESET_ADDRESS                           = 0x100000000       # 4 GB

  #
  # Set size of FLASH to 8MB
  #
  DEFINE FLASH_SIZE                              = 0x800000
  DEFINE FLASH_BASE                              = $(RESET_ADDRESS) - $(FLASH_SIZE)                                                      # The base address of the Flash Device

  #
  # Set FLASH block size to 4KB
  #
  DEFINE FLASH_BLOCKSIZE                         = 0x1000            # 4 KB

  #
  # Misc settings
  #
  DEFINE FLASH_BLOCKSIZE_DATA                    = 0x00, 0x10, 0x00, 0x00                                                                # equivalent for DATA blocks

  #
  # Start PAYLOAD at 4MB into 8MB FLASH
  #
  DEFINE FLASH_FV_PAYLOAD_BASE                   = 0x00400000
  DEFINE FLASH_FV_PAYLOAD_SIZE                   = 0x00100000

  #
  # Put FVMAIN between PAYLOAD and RMU Binary
  #
  DEFINE FLASH_FV_MAIN_BASE                      = 0x00500000
  DEFINE FLASH_FV_MAIN_SIZE                      = 0x001E0000

  #
  # Place NV Storage just above Platform Data Base
  #
  DEFINE NVRAM_AREA_VARIABLE_BASE                = 0x006E0000
  DEFINE NVRAM_AREA_SIZE                         = 0x00020000

  DEFINE NVRAM_AREA_VARIABLE_SIZE                = 0x0000E000
  DEFINE FTW_WORKING_BASE                        = $(NVRAM_AREA_VARIABLE_BASE) + $(NVRAM_AREA_VARIABLE_SIZE)
  DEFINE FTW_WORKING_SIZE                        = 0x00002000
  DEFINE FTW_SPARE_BASE                          = $(FTW_WORKING_BASE) + $(FTW_WORKING_SIZE)
  DEFINE FTW_SPARE_SIZE                          = $(NVRAM_AREA_SIZE) - $(NVRAM_AREA_VARIABLE_SIZE) - $(FTW_WORKING_SIZE)

  #
  # RMU Binary must be at fixed address 1MB below 4GB (0xFFF00000)
  #
  DEFINE RMU_BINARY_BASE                         = 0x00700000  # HW fixed address
  DEFINE RMU_BINARY_SIZE                         = 0x00008000  # HW fixed address, so fixed size

  #
  # Platform Data Base must be 64KB above RMU
  #
  DEFINE VPD_BASE                                = 0x00708000
  DEFINE VPD_SIZE                                = 0x00001000

  #
  # Place FV Recovery above NV Storage
  #
  DEFINE FVRECOVERY_IMAGE_SIZE                   = 0x000F0000
  DEFINE FVRECOVERY_IMAGE_BASE                   = $(FLASH_SIZE) - $(FVRECOVERY_IMAGE_SIZE)

################################################################################
#
# FD Section
# The [FD] Section is made up of the definition statements and a
# description of what goes into  the Flash Device Image.  Each FD section
# defines one flash "device" image.  A flash device image may be one of
# the following: Removable media bootable image (like a boot floppy
# image,) an Option ROM image (that would be "flashed" into an add-in
# card,) a System "Flash"  image (that would be burned into a system's
# flash) or an Update ("Capsule") image that will be used to update and
# existing system flash.
#
################################################################################
[FD.Quark]
BaseAddress   = 0xFF800000                   #The base address of the Flash Device; set to same value as FLASH_BASE.
Size          = 0x800000                     #The size in bytes of the Flash Device; set to same value as FLASH_SIZE.
ErasePolarity = 1
BlockSize     = $(FLASH_BLOCKSIZE)
NumBlocks     = 0x800                        #The number of blocks for the Flash Device.

SET gQuarkPlatformTokenSpaceGuid.PcdFlashAreaBaseAddress = $(FLASH_BASE)
SET gQuarkPlatformTokenSpaceGuid.PcdFlashAreaSize        = $(FLASH_SIZE)

################################################################################
#
# Following are lists of FD Region layout which correspond to the locations of different
# images within the flash device.
#
# Regions must be defined in ascending order and may not overlap.
#
# A Layout Region start with a eight digit hex offset (leading "0x" required) followed by
# the pipe "|" character, followed by the size of the region, also in hex with the leading
# "0x" characters. Like:
# Offset|Size
# PcdOffsetCName|PcdSizeCName
# RegionType <FV, DATA, or FILE>
#
################################################################################

########################################################
# Quark Payload Image
########################################################
$(FLASH_FV_PAYLOAD_BASE)|$(FLASH_FV_PAYLOAD_SIZE)
gQuarkPlatformTokenSpaceGuid.PcdFlashFvPayloadBase|gQuarkPlatformTokenSpaceGuid.PcdFlashFvPayloadSize
FV = PAYLOAD

########################################################
# Quark FVMAIN Image (Compressed)
########################################################
$(FLASH_FV_MAIN_BASE)|$(FLASH_FV_MAIN_SIZE)
gQuarkPlatformTokenSpaceGuid.PcdFlashFvMainBase|gQuarkPlatformTokenSpaceGuid.PcdFlashFvMainSize
FV = FVMAIN_COMPACT

#############################################################################
# Quark NVRAM Area
# Quark NVRAM Area contains: Variable + FTW Working + FTW Spare
#############################################################################
$(NVRAM_AREA_VARIABLE_BASE)|$(NVRAM_AREA_VARIABLE_SIZE)
gEfiMdeModulePkgTokenSpaceGuid.PcdFlashNvStorageVariableBase|gEfiMdeModulePkgTokenSpaceGuid.PcdFlashNvStorageVariableSize
#NV_VARIABLE_STORE
DATA = {
  ## This is the EFI_FIRMWARE_VOLUME_HEADER
  # ZeroVector []
  0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00,
  0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00,
  # FileSystemGuid: gEfiSystemNvDataFvGuid         =
  #  { 0xFFF12B8D, 0x7696, 0x4C8B, { 0xA9, 0x85, 0x27, 0x47, 0x07, 0x5B, 0x4F, 0x50 }}
  0x8D, 0x2B, 0xF1, 0xFF, 0x96, 0x76, 0x8B, 0x4C,
  0xA9, 0x85, 0x27, 0x47, 0x07, 0x5B, 0x4F, 0x50,
  # FvLength: 0x20000
  0x00, 0x00, 0x02, 0x00, 0x00, 0x00, 0x00, 0x00,
  #Signature "_FVH"       #Attributes
  0x5f, 0x46, 0x56, 0x48, 0xff, 0xfe, 0x04, 0x00,
  #HeaderLength #CheckSum #ExtHeaderOffset #Reserved #Revision
  0x48, 0x00, 0x19, 0xF9, 0x00, 0x00, 0x00, 0x02,
  #Blockmap[0]: 32 Blocks * 0x1000 Bytes / Block
  0x20, 0x00, 0x00, 0x00, $(FLASH_BLOCKSIZE_DATA),
  #Blockmap[1]: End
  0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00,
  ## This is the VARIABLE_STORE_HEADER
  !if $(SECURE_BOOT_ENABLE)
    # Signature: gEfiAuthenticatedVariableGuid = { 0xaaf32c78, 0x947b, 0x439a, { 0xa1, 0x80, 0x2e, 0x14, 0x4e, 0xc3, 0x77, 0x92 } }
    0x78, 0x2c, 0xf3, 0xaa, 0x7b, 0x94, 0x9a, 0x43,
    0xa1, 0x80, 0x2e, 0x14, 0x4e, 0xc3, 0x77, 0x92,
  !else
    #  Signature: gEfiVariableGuid = { 0xddcf3616, 0x3275, 0x4164, { 0x98, 0xb6, 0xfe, 0x85, 0x70, 0x7f, 0xfe, 0x7d }}
    0x16, 0x36, 0xcf, 0xdd, 0x75, 0x32, 0x64, 0x41,
    0x98, 0xb6, 0xfe, 0x85, 0x70, 0x7f, 0xfe, 0x7d,
  !endif
  #Size: 0x0E000 (gEfiMdeModulePkgTokenSpaceGuid.PcdFlashNvStorageVariableSize) - 0x48 (size of EFI_FIRMWARE_VOLUME_HEADER) = 0x0DFB8
  # This can speed up the Variable Dispatch a bit.
  0xB8, 0xDF, 0x00, 0x00,
  #FORMATTED: 0x5A #HEALTHY: 0xFE #Reserved: UINT16 #Reserved1: UINT32
  0x5A, 0xFE, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00
}

$(FTW_WORKING_BASE)|$(FTW_WORKING_SIZE)
gEfiMdeModulePkgTokenSpaceGuid.PcdFlashNvStorageFtwWorkingBase|gEfiMdeModulePkgTokenSpaceGuid.PcdFlashNvStorageFtwWorkingSize
#NV_FTW_WORKING
DATA = {
  # EFI_FAULT_TOLERANT_WORKING_BLOCK_HEADER->Signature = gEdkiiWorkingBlockSignatureGuid         =
  #  { 0x9e58292b, 0x7c68, 0x497d, { 0xa0, 0xce, 0x65,  0x0, 0xfd, 0x9f, 0x1b, 0x95 }}
  0x2b, 0x29, 0x58, 0x9e, 0x68, 0x7c, 0x7d, 0x49,
  0xa0, 0xce, 0x65,  0x0, 0xfd, 0x9f, 0x1b, 0x95,
  # Crc:UINT32            #WorkingBlockValid:1, WorkingBlockInvalid:1, Reserved
  0xE2, 0x33, 0xF2, 0x03, 0xFE, 0xFF, 0xFF, 0xFF,
  # WriteQueueSize: UINT64 #Size: 0x2000 - 0x20 (FTW_WORKING_HEADER) = 0x1FE0
  0xE0, 0x1F, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00
}

$(FTW_SPARE_BASE)|$(FTW_SPARE_SIZE)
gEfiMdeModulePkgTokenSpaceGuid.PcdFlashNvStorageFtwSpareBase|gEfiMdeModulePkgTokenSpaceGuid.PcdFlashNvStorageFtwSpareSize
#NV_FTW_SPARE

#########################################################
# Quark Remote Management Unit Binary
#########################################################
$(RMU_BINARY_BASE)|$(RMU_BINARY_SIZE)
INF  QuarkSocBinPkg/QuarkNorthCluster/Binary/QuarkMicrocode/QuarkMicrocode.inf

#########################################################
# PlatformData Binary, default for standalone is none built-in so user selects.
#########################################################
$(VPD_BASE)|$(VPD_SIZE)
gEfiMdeModulePkgTokenSpaceGuid.PcdVpdBaseAddress
FILE = $(OUTPUT_DIRECTORY)/$(TARGET)_$(TOOL_CHAIN_TAG)/FV/8C3D856A-9BE6-468E-850A-24F7A8D38E08.bin

#######################
# Quark FVRECOVERY Image
#######################
$(FVRECOVERY_IMAGE_BASE)|$(FVRECOVERY_IMAGE_SIZE)
gQuarkPlatformTokenSpaceGuid.PcdFlashFvRecoveryBase|gQuarkPlatformTokenSpaceGuid.PcdFlashFvRecoverySize
FV = FVRECOVERY

################################################################################
#
# FV Section
#
# [FV] section is used to define what components or modules are placed within a flash
# device file.  This section also defines order the components and modules are positioned
# within the image.  The [FV] section consists of define statements, set statements and
# module statements.
#
################################################################################
[FV.FVRECOVERY]
BlockSize          = $(FLASH_BLOCKSIZE)
FvAlignment        = 16         #FV alignment and FV attributes setting.
ERASE_POLARITY     = 1
MEMORY_MAPPED      = TRUE
STICKY_WRITE       = TRUE
LOCK_CAP           = TRUE
LOCK_STATUS        = TRUE
WRITE_DISABLED_CAP = TRUE
WRITE_ENABLED_CAP  = TRUE
WRITE_STATUS       = TRUE
WRITE_LOCK_CAP     = TRUE
WRITE_LOCK_STATUS  = TRUE
READ_DISABLED_CAP  = TRUE
READ_ENABLED_CAP   = TRUE
READ_STATUS        = TRUE
READ_LOCK_CAP      = TRUE
READ_LOCK_STATUS   = TRUE
FvNameGuid         = 18D6D9F4-2EEF-4913-AEE6-BE61C6DA6CC8

################################################################################
#
# The INF statements point to EDK component and EDK II module INF files, which will be placed into this FV image.
# Parsing tools will scan the INF file to determine the type of component or module.
# The component or module type is used to reference the standard rules
# defined elsewhere in the FDF file.
#
# The format for INF statements is:
# INF $(PathAndInfFileName)
#
################################################################################

##
#  PEI Apriori file example, more PEIM module added later.
##
APRIORI PEI {
  INF  MdeModulePkg/Universal/PCD/Pei/Pcd.inf
  # PlatformConfigPei should be immediately after Pcd driver.
  INF  QuarkPlatformPkg/Platform/Pei/PlatformConfig/PlatformConfigPei.inf
  INF  MdeModulePkg/Universal/PcatSingleSegmentPciCfg2Pei/PcatSingleSegmentPciCfg2Pei.inf
  INF  MdeModulePkg/Universal/ReportStatusCodeRouter/Pei/ReportStatusCodeRouterPei.inf
  INF  MdeModulePkg/Universal/StatusCodeHandler/Pei/StatusCodeHandlerPei.inf
}

##
#  SEC Phase modules
##
INF  UefiCpuPkg/SecCore/SecCore.inf

!if $(CAPSULE_ENABLE) || $(RECOVERY_ENABLE)
  # FMP image decriptor
INF RuleOverride = FMP_IMAGE_DESC QuarkPlatformPkg/Feature/Capsule/SystemFirmwareDescriptor/SystemFirmwareDescriptor.inf
!endif

INF  MdeModulePkg/Core/Pei/PeiMain.inf

##
#  PEI Phase RAW Data files.
##
FILE FREEFORM = PCD(gEfiQuarkNcSocIdTokenSpaceGuid.PcdQuarkMicrocodeFile) {
  SECTION RAW = QuarkSocBinPkg/QuarkNorthCluster/Binary/QuarkMicrocode/RMU.bin
}

INF  RuleOverride = NORELOC  MdeModulePkg/Universal/PCD/Pei/Pcd.inf
INF  QuarkPlatformPkg/Platform/Pei/PlatformConfig/PlatformConfigPei.inf
INF  RuleOverride = NORELOC  MdeModulePkg/Universal/ReportStatusCodeRouter/Pei/ReportStatusCodeRouterPei.inf
INF  RuleOverride = NORELOC  MdeModulePkg/Universal/StatusCodeHandler/Pei/StatusCodeHandlerPei.inf
INF  RuleOverride = NORELOC  MdeModulePkg/Universal/FaultTolerantWritePei/FaultTolerantWritePei.inf
INF  RuleOverride = NORELOC  MdeModulePkg/Universal/Variable/Pei/VariablePei.inf
INF  RuleOverride = NORELOC  UefiCpuPkg/CpuMpPei/CpuMpPei.inf
INF  RuleOverride = NORELOC  MdeModulePkg/Universal/CapsulePei/CapsulePei.inf
INF  RuleOverride = NORELOC  QuarkSocPkg/QuarkNorthCluster/MemoryInit/Pei/MemoryInitPei.inf
INF  RuleOverride = NORELOC  QuarkSocPkg/QuarkNorthCluster/Smm/Pei/SmmAccessPei/SmmAccessPei.inf
INF  RuleOverride = NORELOC  QuarkSocPkg/QuarkNorthCluster/Smm/Pei/SmmControlPei/SmmControlPei.inf
INF  QuarkPlatformPkg/Platform/Pei/PlatformInit/PlatformEarlyInit.inf
INF  MdeModulePkg/Universal/PcatSingleSegmentPciCfg2Pei/PcatSingleSegmentPciCfg2Pei.inf
INF  MdeModulePkg/Core/DxeIplPeim/DxeIpl.inf
INF  UefiCpuPkg/PiSmmCommunication/PiSmmCommunicationPei.inf
INF  UefiCpuPkg/Universal/Acpi/S3Resume2Pei/S3Resume2Pei.inf
!if $(MEASURED_BOOT_ENABLE)
INF  SecurityPkg/Tcg/Tcg2Config/Tcg2ConfigPei.inf
INF  SecurityPkg/Tcg/TcgPei/TcgPei.inf
!endif

!if $(RECOVERY_ENABLE)
FILE FV_IMAGE = 1E9D7604-EF45-46a0-BD8A-71AC78C17AC1 {
  SECTION PEI_DEPEX_EXP = {gEfiPeiMemoryDiscoveredPpiGuid AND gEfiPeiBootInRecoveryModePpiGuid}
  SECTION GUIDED A31280AD-481E-41B6-95E8-127F4C984779 {    # TIANO COMPRESS GUID
    SECTION FV_IMAGE = FVRECOVERY_COMPONENTS
  }
}
!endif

!if $(RECOVERY_ENABLE)

################################################################################
#
# FV Section
#
# [FV] section is used to define what components or modules are placed within a flash
# device file.  This section also defines order the components and modules are positioned
# within the image.  The [FV] section consists of define statements, set statements and
# module statements.
#
################################################################################
[FV.FVRECOVERY_COMPONENTS]
BlockSize          = $(FLASH_BLOCKSIZE)
FvAlignment        = 16         #FV alignment and FV attributes setting.
ERASE_POLARITY     = 1
MEMORY_MAPPED      = TRUE
STICKY_WRITE       = TRUE
LOCK_CAP           = TRUE
LOCK_STATUS        = TRUE
WRITE_DISABLED_CAP = TRUE
WRITE_ENABLED_CAP  = TRUE
WRITE_STATUS       = TRUE
WRITE_LOCK_CAP     = TRUE
WRITE_LOCK_STATUS  = TRUE
READ_DISABLED_CAP  = TRUE
READ_ENABLED_CAP   = TRUE
READ_STATUS        = TRUE
READ_LOCK_CAP      = TRUE
READ_LOCK_STATUS   = TRUE

INF  QuarkSocPkg/QuarkSouthCluster/Usb/Common/Pei/UsbPei.inf
INF  MdeModulePkg/Bus/Pci/EhciPei/EhciPei.inf
INF  QuarkSocPkg/QuarkSouthCluster/Usb/Ohci/Pei/OhciPei.inf
INF  MdeModulePkg/Bus/Usb/UsbBusPei/UsbBusPei.inf
INF  MdeModulePkg/Bus/Usb/UsbBotPei/UsbBotPei.inf
INF  FatPkg/FatPei/FatPei.inf
INF  MdeModulePkg/Universal/Disk/CdExpressPei/CdExpressPei.inf
INF  SignedCapsulePkg/Universal/RecoveryModuleLoadPei/RecoveryModuleLoadPei.inf

!endif

################################################################################
#
# FV Section
#
# [FV] section is used to define what components or modules are placed within a flash
# device file.  This section also defines order the components and modules are positioned
# within the image.  The [FV] section consists of define statements, set statements and
# module statements.
#
################################################################################
[FV.FVMAIN]
BlockSize          = $(FLASH_BLOCKSIZE)
FvAlignment        = 16
ERASE_POLARITY     = 1
MEMORY_MAPPED      = TRUE
STICKY_WRITE       = TRUE
LOCK_CAP           = TRUE
LOCK_STATUS        = TRUE
WRITE_DISABLED_CAP = TRUE
WRITE_ENABLED_CAP  = TRUE
WRITE_STATUS       = TRUE
WRITE_LOCK_CAP     = TRUE
WRITE_LOCK_STATUS  = TRUE
READ_DISABLED_CAP  = TRUE
READ_ENABLED_CAP   = TRUE
READ_STATUS        = TRUE
READ_LOCK_CAP      = TRUE
READ_LOCK_STATUS   = TRUE
FvNameGuid         = 30D9ED01-38D2-418a-90D5-C561750BF80F

##
#  DXE Phase modules
##
INF  MdeModulePkg/Core/Dxe/DxeMain.inf
INF  MdeModulePkg/Universal/PCD/Dxe/Pcd.inf

!if $(SOURCE_DEBUG_ENABLE)
  INF  SourceLevelDebugPkg/DebugAgentDxe/DebugAgentDxe.inf
!endif

#
# Early SoC / Platform modules
#
INF  QuarkPlatformPkg/Platform/Dxe/PlatformInit/PlatformInitDxe.inf

##
#  EDK Core modules
##
INF  UefiCpuPkg/CpuIo2Dxe/CpuIo2Dxe.inf
INF  MdeModulePkg/Universal/ReportStatusCodeRouter/RuntimeDxe/ReportStatusCodeRouterRuntimeDxe.inf
INF  MdeModulePkg/Universal/StatusCodeHandler/RuntimeDxe/StatusCodeHandlerRuntimeDxe.inf
INF  MdeModulePkg/Universal/ReportStatusCodeRouter/Smm/ReportStatusCodeRouterSmm.inf
INF  MdeModulePkg/Universal/StatusCodeHandler/Smm/StatusCodeHandlerSmm.inf
INF  MdeModulePkg/Universal/SectionExtractionDxe/SectionExtractionDxe.inf

INF  MdeModulePkg/Universal/SecurityStubDxe/SecurityStubDxe.inf
INF  UefiCpuPkg/CpuDxe/CpuDxe.inf
INF  UefiCpuPkg/CpuS3DataDxe/CpuS3DataDxe.inf
INF  MdeModulePkg/Universal/Metronome/Metronome.inf
INF  MdeModulePkg/Universal/WatchdogTimerDxe/WatchdogTimer.inf
INF  MdeModulePkg/Core/RuntimeDxe/RuntimeDxe.inf
INF  MdeModulePkg/Universal/FaultTolerantWriteDxe/FaultTolerantWriteSmm.inf
!if $(SECURE_BOOT_ENABLE)
  INF  SecurityPkg/VariableAuthenticated/SecureBootConfigDxe/SecureBootConfigDxe.inf
!endif
INF  MdeModulePkg/Universal/Variable/RuntimeDxe/VariableSmmRuntimeDxe.inf
INF  MdeModulePkg/Universal/Variable/RuntimeDxe/VariableSmm.inf
INF  MdeModulePkg/Universal/CapsuleRuntimeDxe/CapsuleRuntimeDxe.inf
INF  MdeModulePkg/Universal/MonotonicCounterRuntimeDxe/MonotonicCounterRuntimeDxe.inf
INF  MdeModulePkg/Universal/ResetSystemRuntimeDxe/ResetSystemRuntimeDxe.inf
INF  PcAtChipsetPkg/PcatRealTimeClockRuntimeDxe/PcatRealTimeClockRuntimeDxe.inf
INF  MdeModulePkg/Universal/DevicePathDxe/DevicePathDxe.inf
INF  MdeModulePkg/Universal/MemoryTest/NullMemoryTestDxe/NullMemoryTestDxe.inf

#
# Platform
#
INF  MdeModulePkg/Universal/BdsDxe/BdsDxe.inf
INF  MdeModulePkg/Application/UiApp/UiApp.inf

INF  QuarkPlatformPkg/Pci/Dxe/PciHostBridge/PciHostBridge.inf
INF  QuarkPlatformPkg/Platform/SpiFvbServices/PlatformSpi.inf
INF  QuarkPlatformPkg/Platform/SpiFvbServices/PlatformSmmSpi.inf
INF  QuarkSocPkg/QuarkNorthCluster/QNCInit/Dxe/QNCInitDxe.inf
INF  PcAtChipsetPkg/HpetTimerDxe/HpetTimerDxe.inf
INF  QuarkSocPkg/QuarkNorthCluster/Smm/Dxe/SmmAccessDxe/SmmAccess.inf
INF  QuarkSocPkg/QuarkNorthCluster/S3Support/Dxe/QncS3Support.inf
INF  QuarkSocPkg/QuarkNorthCluster/Spi/PchSpiRuntime.inf
INF  QuarkSocPkg/QuarkNorthCluster/Spi/PchSpiSmm.inf
INF  QuarkPlatformPkg/Platform/Dxe/Setup/DxePlatform.inf

#
# ACPI
#
INF  QuarkPlatformPkg/Platform/Dxe/SaveMemoryConfig/SaveMemoryConfig.inf
INF  MdeModulePkg/Universal/Acpi/S3SaveStateDxe/S3SaveStateDxe.inf
INF  MdeModulePkg/Universal/Acpi/BootScriptExecutorDxe/BootScriptExecutorDxe.inf
INF  MdeModulePkg/Universal/Acpi/AcpiTableDxe/AcpiTableDxe.inf
INF  QuarkPlatformPkg/Acpi/Dxe/AcpiPlatform/AcpiPlatform.inf
INF  RuleOverride = ACPITABLE QuarkPlatformPkg/Acpi/AcpiTables/AcpiTables.inf

#
# SMM
#
INF  MdeModulePkg/Core/PiSmmCore/PiSmmIpl.inf
INF  MdeModulePkg/Core/PiSmmCore/PiSmmCore.inf
INF  UefiCpuPkg/PiSmmCpuDxeSmm/PiSmmCpuDxeSmm.inf
INF  UefiCpuPkg/CpuIo2Smm/CpuIo2Smm.inf
INF  QuarkSocPkg/QuarkNorthCluster/Smm/Dxe/SmmControlDxe/SmmControlDxe.inf
INF  QuarkSocPkg/QuarkNorthCluster/Smm/DxeSmm/QncSmmDispatcher/QNCSmmDispatcher.inf
INF  QuarkPlatformPkg/Acpi/DxeSmm/AcpiSmm/AcpiSmmPlatform.inf
INF  QuarkPlatformPkg/Acpi/DxeSmm/SmmPowerManagement/SmmPowerManagement.inf
INF  MdeModulePkg/Universal/LockBox/SmmLockBox/SmmLockBox.inf
INF  UefiCpuPkg/PiSmmCommunication/PiSmmCommunicationSmm.inf

#
# SMBIOS
#
INF   MdeModulePkg/Universal/SmbiosDxe/SmbiosDxe.inf
INF  QuarkPlatformPkg/Platform/Dxe/SmbiosMiscDxe/SmbiosMiscDxe.inf
INF  QuarkPlatformPkg/Platform/Dxe/MemorySubClass/MemorySubClass.inf

#
# PCI
#
INF  QuarkPlatformPkg/Pci/Dxe/PciPlatform/PciPlatform.inf
INF  MdeModulePkg/Bus/Pci/PciBusDxe/PciBusDxe.inf
INF  QuarkSocPkg/QuarkSouthCluster/IohInit/Dxe/IohInitDxe.inf
!if $(SOURCE_DEBUG_ENABLE)
!else
INF  MdeModulePkg/Bus/Pci/PciSioSerialDxe/PciSioSerialDxe.inf
!endif

#
# USB
#
!if $(PERFORMANCE_ENABLE)
!else
INF  MdeModulePkg/Bus/Pci/EhciDxe/EhciDxe.inf
INF  QuarkSocPkg/QuarkSouthCluster/Usb/Ohci/Dxe/OhciDxe.inf
INF  MdeModulePkg/Bus/Usb/UsbBusDxe/UsbBusDxe.inf
INF  MdeModulePkg/Bus/Usb/UsbKbDxe/UsbKbDxe.inf
INF  MdeModulePkg/Bus/Usb/UsbMouseDxe/UsbMouseDxe.inf
INF  MdeModulePkg/Bus/Usb/UsbMassStorageDxe/UsbMassStorageDxe.inf
!endif

#
# SDIO
#
!if $(PERFORMANCE_ENABLE)
!else
INF  QuarkSocPkg/QuarkSouthCluster/Sdio/Dxe/SDControllerDxe/SDControllerDxe.inf
INF  QuarkSocPkg/QuarkSouthCluster/Sdio/Dxe/SDMediaDeviceDxe/SDMediaDeviceDxe.inf
!endif

#
# Console
#
INF  MdeModulePkg/Universal/Console/ConPlatformDxe/ConPlatformDxe.inf
INF  MdeModulePkg/Universal/Console/ConSplitterDxe/ConSplitterDxe.inf
INF  MdeModulePkg/Universal/Console/TerminalDxe/TerminalDxe.inf

INF  MdeModulePkg/Universal/HiiDatabaseDxe/HiiDatabaseDxe.inf
INF  MdeModulePkg/Universal/DisplayEngineDxe/DisplayEngineDxe.inf
INF  MdeModulePkg/Universal/SetupBrowserDxe/SetupBrowserDxe.inf
INF  MdeModulePkg/Universal/Disk/UnicodeCollation/EnglishDxe/EnglishDxe.inf

#
# File System Modules
#
!if $(PERFORMANCE_ENABLE)
!else
INF  MdeModulePkg/Universal/Disk/DiskIoDxe/DiskIoDxe.inf
INF  MdeModulePkg/Universal/Disk/PartitionDxe/PartitionDxe.inf
INF  FatPkg/EnhancedFatDxe/Fat.inf
!endif

#
# Performance Application
#
!if $(PERFORMANCE_ENABLE)
INF  ShellPkg/DynamicCommand/DpDynamicCommand/DpDynamicCommand.inf
!endif

#
# Trusted Platform Module
#
!if $(MEASURED_BOOT_ENABLE)
INF  SecurityPkg/Tcg/MemoryOverwriteControl/TcgMor.inf
INF  SecurityPkg/Tcg/TcgDxe/TcgDxe.inf
INF  RuleOverride = DRIVER_ACPITABLE SecurityPkg/Tcg/TcgSmm/TcgSmm.inf
!endif

!if $(CAPSULE_ENABLE)
INF  MdeModulePkg/Universal/EsrtFmpDxe/EsrtFmpDxe.inf
INF  SignedCapsulePkg/Universal/SystemFirmwareUpdate/SystemFirmwareReportDxe.inf
!endif

!if $(RECOVERY_ENABLE)
FILE FREEFORM = PCD(gEfiSignedCapsulePkgTokenSpaceGuid.PcdEdkiiRsa2048Sha256TestPublicKeyFileGuid) {
     SECTION RAW = BaseTools/Source/Python/Rsa2048Sha256Sign/TestSigningPublicKey.bin
     SECTION UI = "Rsa2048Sha256TestSigningPublicKey"
     }
!endif

!if $(CAPSULE_ENABLE)
FILE FREEFORM = PCD(gEfiSignedCapsulePkgTokenSpaceGuid.PcdEdkiiPkcs7TestPublicKeyFileGuid) {
     SECTION RAW = BaseTools/Source/Python/Pkcs7Sign/TestRoot.cer
     SECTION UI = "Pkcs7TestRoot"
     }
!endif

################################################################################
#
# FV Section
#
# [FV] section is used to define what components or modules are placed within a flash
# device file.  This section also defines order the components and modules are positioned
# within the image.  The [FV] section consists of define statements, set statements and
# module statements.
#
################################################################################
[FV.FVMAIN_COMPACT]
FvAlignment        = 16
ERASE_POLARITY     = 1
MEMORY_MAPPED      = TRUE
STICKY_WRITE       = TRUE
LOCK_CAP           = TRUE
LOCK_STATUS        = TRUE
WRITE_DISABLED_CAP = TRUE
WRITE_ENABLED_CAP  = TRUE
WRITE_STATUS       = TRUE
WRITE_LOCK_CAP     = TRUE
WRITE_LOCK_STATUS  = TRUE
READ_DISABLED_CAP  = TRUE
READ_ENABLED_CAP   = TRUE
READ_STATUS        = TRUE
READ_LOCK_CAP      = TRUE
READ_LOCK_STATUS   = TRUE

FILE FV_IMAGE = 9E21FD93-9C72-4c15-8C4B-E77F1DB2D792 {
  SECTION GUIDED A31280AD-481E-41B6-95E8-127F4C984779 {    # TIANO COMPRESS GUID
    SECTION FV_IMAGE = FVMAIN
  }
}

################################################################################
#
# FV Section
#
# [FV] section is used to define what components or modules are placed within a flash
# device file.  This section also defines order the components and modules are positioned
# within the image.  The [FV] section consists of define statements, set statements and
# module statements.
#
################################################################################
[FV.PAYLOAD]
BlockSize          = $(FLASH_BLOCKSIZE)
FvAlignment        = 16         #FV alignment and FV attributes setting.
ERASE_POLARITY     = 1
MEMORY_MAPPED      = TRUE
STICKY_WRITE       = TRUE
LOCK_CAP           = TRUE
LOCK_STATUS        = TRUE
WRITE_DISABLED_CAP = TRUE
WRITE_ENABLED_CAP  = TRUE
WRITE_STATUS       = TRUE
WRITE_LOCK_CAP     = TRUE
WRITE_LOCK_STATUS  = TRUE
READ_DISABLED_CAP  = TRUE
READ_ENABLED_CAP   = TRUE
READ_STATUS        = TRUE
READ_LOCK_CAP      = TRUE
READ_LOCK_STATUS   = TRUE

#
# Shell and Applications
#
INF  RuleOverride = TIANOCOMPRESSED ShellPkg/Application/Shell/Shell.inf

!if $(CAPSULE_ENABLE) || $(RECOVERY_ENABLE)

[FV.CapsuleDispatchFv]
FvAlignment        = 16
ERASE_POLARITY     = 1
MEMORY_MAPPED      = TRUE
STICKY_WRITE       = TRUE
LOCK_CAP           = TRUE
LOCK_STATUS        = TRUE
WRITE_DISABLED_CAP = TRUE
WRITE_ENABLED_CAP  = TRUE
WRITE_STATUS       = TRUE
WRITE_LOCK_CAP     = TRUE
WRITE_LOCK_STATUS  = TRUE
READ_DISABLED_CAP  = TRUE
READ_ENABLED_CAP   = TRUE
READ_STATUS        = TRUE
READ_LOCK_CAP      = TRUE
READ_LOCK_STATUS   = TRUE

!if $(CAPSULE_ENABLE)
INF  SignedCapsulePkg/Universal/SystemFirmwareUpdate/SystemFirmwareUpdateDxe.inf
!endif

[FV.SystemFirmwareUpdateCargo]
FvAlignment        = 16
ERASE_POLARITY     = 1
MEMORY_MAPPED      = TRUE
STICKY_WRITE       = TRUE
LOCK_CAP           = TRUE
LOCK_STATUS        = TRUE
WRITE_DISABLED_CAP = TRUE
WRITE_ENABLED_CAP  = TRUE
WRITE_STATUS       = TRUE
WRITE_LOCK_CAP     = TRUE
WRITE_LOCK_STATUS  = TRUE
READ_DISABLED_CAP  = TRUE
READ_ENABLED_CAP   = TRUE
READ_STATUS        = TRUE
READ_LOCK_CAP      = TRUE
READ_LOCK_STATUS   = TRUE

FILE RAW = 14D83A59-A810-4556-8192-1C0A593C065C { # PcdEdkiiSystemFirmwareFileGuid
    FD = Quark
  }

FILE RAW = ce57b167-b0e4-41e8-a897-5f4feb781d40 { # gEdkiiSystemFmpCapsuleDriverFvFileGuid
    FV = CapsuleDispatchFv
  }

FILE RAW = 812136D3-4D3A-433A-9418-29BB9BF78F6E { # gEdkiiSystemFmpCapsuleConfigFileGuid
    QuarkPlatformPkg/Feature/Capsule/SystemFirmwareUpdateConfig/SystemFirmwareUpdateConfig.ini
  }

!endif

!if $(CAPSULE_ENABLE)
[FmpPayload.FmpPayloadSystemFirmwarePkcs7]
IMAGE_HEADER_INIT_VERSION = 0x02
IMAGE_TYPE_ID             = 62af20c0-7016-424a-9bf8-9ccc86584090 # PcdSystemFmpCapsuleImageTypeIdGuid
IMAGE_INDEX               = 0x1
HARDWARE_INSTANCE         = 0x0
MONOTONIC_COUNT           = 0x2
CERTIFICATE_GUID          = 4AAFD29D-68DF-49EE-8AA9-347D375665A7 # PKCS7

FV = SystemFirmwareUpdateCargo

[Capsule.QuarkFirmwareUpdateCapsuleFmpPkcs7]
CAPSULE_GUID                = 6dcbd5ed-e82d-4c44-bda1-7194199ad92a # gEfiFmpCapsuleGuid
CAPSULE_FLAGS               = PersistAcrossReset,InitiateReset
CAPSULE_HEADER_SIZE         = 0x20
CAPSULE_HEADER_INIT_VERSION = 0x1

FMP_PAYLOAD = FmpPayloadSystemFirmwarePkcs7
!endif

!if $(RECOVERY_ENABLE)
[FmpPayload.FmpPayloadSystemFirmwareRsa2048]
IMAGE_HEADER_INIT_VERSION = 0x02
IMAGE_TYPE_ID             = 62af20c0-7016-424a-9bf8-9ccc86584090 # PcdSystemFmpCapsuleImageTypeIdGuid
IMAGE_INDEX               = 0x1
HARDWARE_INSTANCE         = 0x0
MONOTONIC_COUNT           = 0x2
CERTIFICATE_GUID          = A7717414-C616-4977-9420-844712A735BF # RSA2048SHA256

FV = SystemFirmwareUpdateCargo

[Capsule.QuarkRec]
CAPSULE_GUID                = 6dcbd5ed-e82d-4c44-bda1-7194199ad92a # gEfiFmpCapsuleGuid
CAPSULE_FLAGS               = PersistAcrossReset,InitiateReset
CAPSULE_HEADER_SIZE         = 0x20
CAPSULE_HEADER_INIT_VERSION = 0x1

FMP_PAYLOAD = FmpPayloadSystemFirmwareRsa2048
!endif

################################################################################
#
# Rules are use with the [FV] section's module INF type to define
# how an FFS file is created for a given INF file. The following Rule are the default
# rules for the different module type. User can add the customized rules to define the
# content of the FFS file.
#
################################################################################
[Rule.Common.SEC]
  FILE SEC = $(NAMED_GUID) RELOCS_STRIPPED {
    TE  TE    Align = 8       $(INF_OUTPUT)/$(MODULE_NAME).efi
    RAW BIN   Align = 16      |.com
  }

[Rule.Common.PEI_CORE]
  FILE PEI_CORE = $(NAMED_GUID)            {
    TE       TE               $(INF_OUTPUT)/$(MODULE_NAME).efi
    UI       STRING="$(MODULE_NAME)" Optional
    VERSION  STRING="$(INF_VERSION)" Optional BUILD_NUM=$(BUILD_NUMBER)
  }

[Rule.Common.PEIM.NORELOC]
  FILE PEIM = $(NAMED_GUID) RELOCS_STRIPPED  {
     PEI_DEPEX PEI_DEPEX Optional        $(INF_OUTPUT)/$(MODULE_NAME).depex
     TE        TE                        $(INF_OUTPUT)/$(MODULE_NAME).efi
     UI        STRING="$(MODULE_NAME)" Optional
     VERSION   STRING="$(INF_VERSION)" Optional BUILD_NUM=$(BUILD_NUMBER)
  }

[Rule.Common.PEIM]
  FILE PEIM = $(NAMED_GUID)               {
     PEI_DEPEX PEI_DEPEX Optional        $(INF_OUTPUT)/$(MODULE_NAME).depex
     TE        TE                        $(INF_OUTPUT)/$(MODULE_NAME).efi
     UI        STRING="$(MODULE_NAME)" Optional
     VERSION   STRING="$(INF_VERSION)" Optional BUILD_NUM=$(BUILD_NUMBER)
  }

[Rule.Common.DXE_CORE]
  FILE DXE_CORE = $(NAMED_GUID) {
    PE32      PE32                     $(INF_OUTPUT)/$(MODULE_NAME).efi
    UI        STRING="$(MODULE_NAME)" Optional
    VERSION   STRING="$(INF_VERSION)" Optional BUILD_NUM=$(BUILD_NUMBER)
  }

[Rule.Common.UEFI_DRIVER]
  FILE DRIVER = $(NAMED_GUID) {
    DXE_DEPEX DXE_DEPEX Optional       $(INF_OUTPUT)/$(MODULE_NAME).depex
    PE32      PE32                     $(INF_OUTPUT)/$(MODULE_NAME).efi
    UI        STRING="$(MODULE_NAME)" Optional
    VERSION   STRING="$(INF_VERSION)" Optional BUILD_NUM=$(BUILD_NUMBER)
  }

[Rule.Common.DXE_DRIVER]
  FILE DRIVER = $(NAMED_GUID) {
    DXE_DEPEX DXE_DEPEX Optional       $(INF_OUTPUT)/$(MODULE_NAME).depex
    PE32      PE32                     $(INF_OUTPUT)/$(MODULE_NAME).efi
    UI        STRING="$(MODULE_NAME)" Optional
    VERSION   STRING="$(INF_VERSION)" Optional BUILD_NUM=$(BUILD_NUMBER)
  }

[Rule.Common.DXE_RUNTIME_DRIVER]
  FILE DRIVER = $(NAMED_GUID) {
    DXE_DEPEX DXE_DEPEX Optional       $(INF_OUTPUT)/$(MODULE_NAME).depex
    PE32      PE32                     $(INF_OUTPUT)/$(MODULE_NAME).efi
    UI        STRING="$(MODULE_NAME)" Optional
    VERSION   STRING="$(INF_VERSION)" Optional BUILD_NUM=$(BUILD_NUMBER)
  }

[Rule.Common.DXE_SMM_DRIVER]
  FILE SMM = $(NAMED_GUID) {
    SMM_DEPEX SMM_DEPEX Optional       $(INF_OUTPUT)/$(MODULE_NAME).depex
    PE32      PE32                     $(INF_OUTPUT)/$(MODULE_NAME).efi
    UI        STRING="$(MODULE_NAME)" Optional
    VERSION   STRING="$(INF_VERSION)" Optional BUILD_NUM=$(BUILD_NUMBER)
  }

[Rule.Common.DXE_SMM_DRIVER.DRIVER_ACPITABLE]
  FILE SMM = $(NAMED_GUID) {
    DXE_DEPEX DXE_DEPEX Optional       $(INF_OUTPUT)/$(MODULE_NAME).depex
    PE32      PE32                     $(INF_OUTPUT)/$(MODULE_NAME).efi
    RAW ACPI  Optional                |.acpi
    RAW ASL   Optional                |.aml
    UI        STRING="$(MODULE_NAME)" Optional
    VERSION   STRING="$(INF_VERSION)" Optional BUILD_NUM=$(BUILD_NUMBER)
  }

[Rule.Common.SMM_CORE]
  FILE SMM_CORE = $(NAMED_GUID) {
    PE32      PE32                     $(INF_OUTPUT)/$(MODULE_NAME).efi
    UI        STRING="$(MODULE_NAME)" Optional
    VERSION   STRING="$(INF_VERSION)" Optional BUILD_NUM=$(BUILD_NUMBER)
  }

[Rule.Common.UEFI_APPLICATION]
  FILE APPLICATION = $(NAMED_GUID) {
    PE32      PE32                     $(INF_OUTPUT)/$(MODULE_NAME).efi
    UI        STRING="$(MODULE_NAME)" Optional
    VERSION   STRING="$(INF_VERSION)" Optional BUILD_NUM=$(BUILD_NUMBER)
  }

[Rule.Common.UEFI_APPLICATION.TIANOCOMPRESSED]
  FILE APPLICATION = $(NAMED_GUID) {
    UI        STRING="$(MODULE_NAME)" Optional
    VERSION   STRING="$(INF_VERSION)" Optional BUILD_NUM=$(BUILD_NUMBER)
    SECTION GUIDED A31280AD-481E-41B6-95E8-127F4C984779 PROCESSING_REQUIRED = TRUE {  # TIANO COMPRESS GUID
      PE32      PE32                     $(INF_OUTPUT)/$(MODULE_NAME).efi
    }
  }

[Rule.Common.UEFI_APPLICATION.UI]
  FILE APPLICATION = $(NAMED_GUID) {
    PE32      PE32                     $(INF_OUTPUT)/$(MODULE_NAME).efi
    UI        STRING="Enter Setup"
    VERSION   STRING="$(INF_VERSION)" Optional BUILD_NUM=$(BUILD_NUMBER)
  }

[Rule.Common.USER_DEFINED.ACPITABLE]
  FILE FREEFORM = $(NAMED_GUID) {
    RAW ACPI               |.acpi
    RAW ASL                |.aml
  }

[Rule.Common.PEIM.FMP_IMAGE_DESC]
  FILE PEIM = $(NAMED_GUID) {
     RAW BIN                  |.acpi
     PEI_DEPEX PEI_DEPEX Optional        $(INF_OUTPUT)/$(MODULE_NAME).depex
     PE32      PE32    Align=4K          $(INF_OUTPUT)/$(MODULE_NAME).efi
     UI       STRING="$(MODULE_NAME)" Optional
     VERSION  STRING="$(INF_VERSION)" Optional BUILD_NUM=$(BUILD_NUMBER)
  }

