### @file
#
# Copyright (c) 2018, Intel Corporation. All rights reserved.<BR>
#
# SPDX-License-Identifier: BSD-2-Clause-Patent
#
###

[Defines]
  DEC_SPECIFICATION              = 0x00010005
  PACKAGE_NAME                   = PurleySktPkg
  PACKAGE_GUID                   = DD44D851-9A3E-46E8-A2Ef-D794D014ECC1
  PACKAGE_VERSION                = 0.91

[Includes]              
  Include
  Include/Library
  Include/Guid

  Library/ProcMemInit/Chip/Include
  Override/IA32FamilyCpuPkg
  Override/IA32FamilyCpuPkg/Include
  
  Iio/Include
  Iio/Include/Protocol
  
[Guids]
  gCpuUncoreTokenSpaceGuid                            = { 0x9044434c, 0x40e8, 0x47a1, { 0xa3, 0xba, 0x85, 0x07, 0xf3, 0xc0, 0xe2, 0x56 } }
  gProcessorProducerGuid                              = { 0x1bf06aea, 0x5bec, 0x4a8d, { 0x95, 0x76, 0x74, 0x9b, 0x09, 0x56, 0x2d, 0x30 } }
  gEfiCpuHtCapableGuid                                = { 0x0d1b9c8e, 0xf77b, 0x4632, { 0x83, 0x43, 0x91, 0xf4, 0x3d, 0x9a, 0x85, 0x60 } }
  gEfiMemoryConfigDataGuid                            = { 0x80dbd530, 0xb74c, 0x4f11, { 0x8c, 0x03, 0x41, 0x86, 0x65, 0x53, 0x28, 0x31 } }
  gEfiMemoryConfigDataHobGuid                         = { 0x1de25879, 0x6e2a, 0x4d72, { 0xa7, 0x68, 0x28, 0x8c, 0xcb, 0x9f, 0xa7, 0x19 } }
  gEfiMemorySetupGuid                                 = { 0x3eeff35f, 0x147c, 0x4cd1, { 0xa2, 0x34, 0x92, 0xa0, 0x69, 0x70, 0x0d, 0xb6 } }
  gEfiMemoryMapGuid                                   = { 0xf8870015, 0x6994, 0x4b98, { 0x95, 0xa2, 0xbd, 0x56, 0xda, 0x91, 0xc0, 0x7f } }
  gEfiMemoryMapDataHobBdatGuid                        = { 0x3417b225, 0x916a, 0x49f5, { 0x9a, 0xf5, 0xc9, 0xc7, 0xbf, 0x93, 0x7e, 0xa2 } }
  gEfiMpstNodeDataGuid                                = { 0x418bc604, 0xf15e, 0x4843, { 0x85, 0xd0, 0x2d, 0x24, 0x80, 0xb7, 0xe4, 0x88 } }
  gReadyForLockProtocolGuid                           = { 0x8d6f1add, 0x45a5, 0x45a8, { 0x8b, 0xb8, 0x0c, 0x3a, 0x95, 0x31, 0x48, 0xfa } }
  gPlatformTokenSpaceGuid                             = { 0x07dfa0d2, 0x2ac5, 0x4cab, { 0xac, 0x14, 0x30, 0x5c, 0x62, 0x48, 0x87, 0xe4 } }
  gEfiSocketIioVariableGuid                           = { 0xdd84017e, 0x7f52, 0x48f9, { 0xb1, 0x6e, 0x50, 0xed, 0x9e, 0x0d, 0xbe, 0x27 } }
  gEfiSocketCommonRcVariableGuid                      = { 0x4402ca38, 0x808f, 0x4279, { 0xbc, 0xec, 0x5b, 0xaf, 0x8d, 0x59, 0x09, 0x2f } }
  gEfiSocketMpLinkVariableGuid                        = { 0x2b9b22de, 0x2ad4, 0x4abc, { 0x95, 0x7d, 0x5f, 0x18, 0xc5, 0x04, 0xa0, 0x5c } }
  gEfiSocketPciResourceDataGuid                       = { 0xca3ff937, 0xd646, 0x4936, { 0x90, 0xe8, 0x1b, 0x95, 0x06, 0x49, 0xb3, 0x89 } }
  gEfiSocketMemoryVariableGuid                        = { 0x98cf19ed, 0x4109, 0x4681, { 0xb7, 0x9d, 0x91, 0x96, 0x75, 0x7c, 0x78, 0x24 } }
  gEfiSocketPowermanagementVarGuid                    = { 0xA1047342, 0xBDBA, 0x4DAE, { 0xA6, 0x7A, 0x40, 0x97, 0x9B, 0x65, 0xC7, 0xF8 } }
  gEfiSocketProcessorCoreVarGuid                      = { 0x07013588, 0xC789, 0x4E12, { 0xA7, 0xC3, 0x88, 0xFA, 0xFA, 0xE7, 0x9F, 0x7C } }
  gSocketPkgListGuid                                  = { 0x5c0083db, 0x3f7d, 0x4b20, { 0xac, 0x9b, 0x73, 0xfc, 0x65, 0x1b, 0x25, 0x03 } }
  gEfiVolatileMemModeVariableGuid                     = { 0x0633a0f1, 0x78fe, 0x4139, { 0xb8, 0x78, 0x00, 0x45, 0xe8, 0x1c, 0xb8, 0xab } }
  gEfiQpiRcParmGuid                                   = { 0x8149fbb8, 0xa2cf, 0x4234, { 0xb5, 0x06, 0xb7, 0x62, 0x55, 0xf7, 0xa3, 0x6d } }
  gAddressBasedMirrorGuid                             = { 0x7b9be2e0, 0xe28a, 0x4197, { 0xad, 0x3e, 0x32, 0xf0, 0x62, 0xf9, 0x46, 0x2c } }
  gClvBootTimeTestExecution                           = { 0x3ff7d152, 0xef86, 0x47c3, { 0x97, 0xb0, 0xce, 0xd9, 0xbb, 0x80, 0x9a, 0x67 } }
  gEfiRasClvTesterGuid                                = { 0x9bd36f4f, 0x08dc, 0x4eab, { 0x86, 0x37, 0x2b, 0xc1, 0xbd, 0x5e, 0x0d, 0x95 } }
  gSocketPkgFpgaGuid                                  = { 0x624b948f, 0x6eba, 0x4dfd, { 0x9d, 0xda, 0x10, 0xb0, 0x07, 0x3a, 0x37, 0x35 } }  # {624B948F-6EBA-4DFD-9DDA-10B0073A3735}
  gIioPolicyHobGuid                                   = { 0xcabb327,  0x11fe, 0x416b, { 0xae, 0x80, 0x2d, 0xe5, 0xdf, 0x60, 0xf7, 0x7d } }
  gEfiSmmPeiSmramMemoryReserveGuid                    = { 0x6dadf1d1, 0xd4cc, 0x4910, { 0xbb, 0x6e, 0x82, 0xb1, 0xfd, 0x80, 0xff, 0x3d } }

[Ppis]
  gPeiBaseMemoryTestPpiGuid                           = { 0xb6ec423c, 0x21d2, 0x490d, { 0x85, 0xc6, 0xdd, 0x58, 0x64, 0xea, 0xa6, 0x74 } }
  gPeiPlatformMemorySizePpiGuid                       = { 0x9a7ef41e, 0xc140, 0x4bd1, { 0xb8, 0x84, 0x1e, 0x11, 0x24, 0x0b, 0x4c, 0xe6 } }
  gPeiMpServicePpiGuid                                = { 0xee16160a, 0xe8be, 0x47a6, { 0x82, 0x0a, 0xc6, 0x90, 0x0d, 0xb0, 0x25, 0x0a } }

[Protocols]
  gEfiIioUdsProtocolGuid                              = { 0xa7ced760, 0xc71c, 0x4e1a, { 0xac, 0xb1, 0x89, 0x60, 0x4d, 0x52, 0x16, 0xcb } }
  gEfiIioSystemProtocolGuid                           = { 0xddc3080a, 0x2740, 0x4ec2, { 0x9a, 0xa5, 0xa0, 0xad, 0xef, 0xd6, 0xff, 0x9c } }
  gEfiCpuCsrAccessGuid                                = { 0x0067835f, 0x9a50, 0x433a, { 0x8c, 0xbb, 0x85, 0x20, 0x78, 0x19, 0x78, 0x14 } }
  gEfiQuiesceProtocolGuid                             = { 0x20d6e759, 0x4c4a, 0x40c0, { 0x95, 0x33, 0x2b, 0xf0, 0x06, 0x68, 0x50, 0xfd } }
  gEfiGlobalNvsAreaProtocolGuid                       = { 0x074e1e48, 0x8132, 0x47a1, { 0x8c, 0x2c, 0x3f, 0x14, 0xad, 0x9a, 0x66, 0xdc } }
  gEfiHpIoxAccessGuid                                 = { 0x62652b53, 0x79d9, 0x4cf2, { 0xb5, 0xaa, 0xad, 0x99, 0x81, 0x0a, 0x7f, 0x17 } }

  gEfiPciCallbackProtocolGuid                         = { 0x1ca0e202, 0xfe9e, 0x4776, { 0x9f, 0xaa, 0x57, 0xc, 0x19, 0x61, 0x7a, 0x06 }}

[PcdsFeatureFlag]
  gEfiCpuTokenSpaceGuid.PcdCpuIvyBridgeFamilyFlag|TRUE|BOOLEAN|0x10000031
  gPlatformTokenSpaceGuid.PcdLockCsrSsidSvidRegister|TRUE|BOOLEAN|0x10000001

### [PcdsFixedAtBuild, PcdsPatchableInModule]
[PcdsFixedAtBuild,PcdsPatchableInModule,PcdsDynamic]
  ## PCD for ServerCommonPkg\Override\IA32FamilyCpuPkg\CpuMpDxe.inf
  ## This PCD is the AP state on POST. The value is defined as below.
  #  1: ApInHltLoop,   AP is in the Hlt-Loop state.
  #  2: ApInMwaitLoop, AP is in the Mwait-Loop state.
  #  3: ApInRunLoop,   AP is in the Run-Loop state.
  gEfiCpuTokenSpaceGuid.PcdCpuApLoopMode|1|UINT8|0x10001004

[PcdsFixedAtBuild]
  gPlatformTokenSpaceGuid.PcdBusStack|0x06|UINT8|0x30000006
  gPlatformTokenSpaceGuid.PcdUboDev|0x08|UINT8|0x3000000D
  gPlatformTokenSpaceGuid.PcdUboFunc|0x02|UINT8|0x3000000E
  gPlatformTokenSpaceGuid.PcdUboCpuBusNo0|0xCC|UINT8|0x3000000F
  gCpuUncoreTokenSpaceGuid.PcdFlashSecCacheRegionBase|0x00FFD00000|UINT32|0x2000000D
  gCpuUncoreTokenSpaceGuid.PcdFlashSecCacheRegionSize|0x0000300000|UINT32|0x2000000E
  gCpuUncoreTokenSpaceGuid.PcdFlashNvStorageMicrocodeBase|0xFFFB0000|UINT32|0x30000004
  gCpuUncoreTokenSpaceGuid.PcdFlashNvStorageMicrocodeSize|0x00010000|UINT32|0x30000005
  gCpuUncoreTokenSpaceGuid.PcdWaSlowModeEnable|0|BOOLEAN|0x30000008

[PcdsDynamicEx]
  gPlatformTokenSpaceGuid.PcdFpgaSwSmiInputValue|0|UINT8|0x30000007
  gEfiCpuTokenSpaceGuid.PcdSbspSelection|0xFF|UINT8|0x6000801B
  gEfiCpuTokenSpaceGuid.PcdCpuCoreCStateValue|0x0|UINT8|0x60008009
  gEfiCpuTokenSpaceGuid.PcdCpuTurboOverride|0x0|UINT32|0x60008022
  gEfiCpuTokenSpaceGuid.PcdCpuProcessorMsrLockCtrl|0x0|UINT8|0x60008018
  gEfiCpuTokenSpaceGuid.PcdCpuIioLlcWaysBitMask|0x0|UINT64|0x60008019
  gEfiCpuTokenSpaceGuid.PcdCpuExpandedIioLlcWaysBitMask|0x0|UINT64|0x6000801C
  gEfiCpuTokenSpaceGuid.PcdCpuRemoteWaysBitMask|0x0|UINT64|0x60008023
  gEfiCpuTokenSpaceGuid.PcdPchTraceHubEn|0x0|UINT8|0x6000801D
  gEfiCpuTokenSpaceGuid.PcdCpuQlruCfgBitMask|0x0|UINT64|0x6000801A
  gEfiCpuTokenSpaceGuid.PcdCpuPmStructAddr|0x0|UINT64|0x60008020
  gEfiCpuTokenSpaceGuid.PcdCpuRRQCountThreshold|0x0|UINT64|0x60008024

[PcdsFeatureFlag]
  ## This PCD specifies whether StatusCode is reported via USB Serial port.
  gEfiCpuTokenSpaceGuid.PcdCpuSelectLfpAsBspFlag|TRUE|BOOLEAN|0x1000000F
