#
#  Copyright (c) 2018, ARM Limited. All rights reserved.
#
#  SPDX-License-Identifier: BSD-2-Clause-Patent
#

################################################################################
#
# FD Section
# The [FD] Section is made up of the definition statements and a
# description of what goes into  the Flash Device Image.  Each FD section
# defines one flash "device" image.  A flash device image may be one of
# the following: Removable media bootable image (like a boot floppy
# image,) an Option ROM image (that would be "flashed" into an add-in
# card,) a System "Flash"  image (that would be burned into a system's
# flash) or an Update ("Capsule") image that will be used to update and
# existing system flash.
#
################################################################################

[FD.BL32_AP_MM]
BaseAddress   = 0xff200000|gArmTokenSpaceGuid.PcdFdBaseAddress  # UEFI in DRAM + 128MB.
Size          = 0x00e00000|gArmTokenSpaceGuid.PcdFdSize         # The size in bytes of the device (64MiB).
ErasePolarity = 1

BlockSize     = 0x00001000
NumBlocks     = 0x0e00

0x00000000|0x00280000
gArmTokenSpaceGuid.PcdFvBaseAddress|gArmTokenSpaceGuid.PcdFvSize
FV = FVMAIN_COMPACT

[FV.FVMAIN_COMPACT]
FvAlignment        = 16
ERASE_POLARITY     = 1
MEMORY_MAPPED      = TRUE
STICKY_WRITE       = TRUE
LOCK_CAP           = TRUE
LOCK_STATUS        = TRUE
WRITE_DISABLED_CAP = TRUE
WRITE_ENABLED_CAP  = TRUE
WRITE_STATUS       = TRUE
WRITE_LOCK_CAP     = TRUE
WRITE_LOCK_STATUS  = TRUE
READ_DISABLED_CAP  = TRUE
READ_ENABLED_CAP   = TRUE
READ_STATUS        = TRUE
READ_LOCK_CAP      = TRUE
READ_LOCK_STATUS   = TRUE

  INF StandaloneMmPkg/Core/StandaloneMmCore.inf
  INF StandaloneMmPkg/Drivers/StandaloneMmCpu/AArch64/StandaloneMmCpu.inf

################################################################################
#
# Rules are use with the [FV] section's module INF type to define
# how an FFS file is created for a given INF file. The following Rule are the default
# rules for the different module type. User can add the customized rules to define the
# content of the FFS file.
#
################################################################################


############################################################################
# Example of a DXE_DRIVER FFS file with a Checksum encapsulation section   #
############################################################################
#
#[Rule.Common.DXE_DRIVER]
#  FILE DRIVER = $(NAMED_GUID) {
#    DXE_DEPEX    DXE_DEPEX               Optional $(INF_OUTPUT)/$(MODULE_NAME).depex
#    COMPRESS PI_STD {
#      GUIDED {
#        PE32     PE32                    $(INF_OUTPUT)/$(MODULE_NAME).efi
#        UI       STRING="$(MODULE_NAME)" Optional
#        VERSION  STRING="$(INF_VERSION)" Optional BUILD_NUM=$(BUILD_NUMBER)
#      }
#    }
#  }
#
############################################################################

[Rule.Common.MM_CORE_STANDALONE]
  FILE SEC = $(NAMED_GUID) RELOCS_STRIPPED FIXED {
    PE32  PE32 Align = Auto             $(INF_OUTPUT)/$(MODULE_NAME).efi
  }

[Rule.Common.MM_STANDALONE]
  FILE MM_STANDALONE = $(NAMED_GUID) {
    SMM_DEPEX SMM_DEPEX Optional       $(INF_OUTPUT)/$(MODULE_NAME).depex
    PE32      PE32                     $(INF_OUTPUT)/$(MODULE_NAME).efi
    UI        STRING="$(MODULE_NAME)" Optional
    VERSION   STRING="$(INF_VERSION)" Optional BUILD_NUM=$(BUILD_NUMBER)
  }
