/** @file
*  Multiple APIC Description Table (MADT)
*
*  Copyright (c) 2018, ARM Limited. All rights reserved.
*
*  SPDX-License-Identifier: BSD-2-Clause-Patent
*
**/

#include "SgiPlatform.h"
#include "SgiAcpiHeader.h"
#include <Library/AcpiLib.h>
#include <Library/ArmLib.h>
#include <Library/PcdLib.h>
#include <IndustryStandard/Acpi.h>

#define CORE_CNT   (FixedPcdGet32 (PcdClusterCount) * \
                    FixedPcdGet32 (PcdCoreCount))

// EFI_ACPI_6_2_GIC_STRUCTURE
#define EFI_ACPI_6_2_GICC_STRUCTURE_INIT(GicId, AcpiCpuUid, Mpidr, Flags,      \
  PmuIrq, GicBase, GicVBase, GicHBase, GsivId, GicRBase, Efficiency)           \
  {                                                                            \
    EFI_ACPI_6_2_GIC,                     /* Type */                           \
    sizeof (EFI_ACPI_6_2_GIC_STRUCTURE),  /* Length */                         \
    EFI_ACPI_RESERVED_WORD,               /* Reserved */                       \
    GicId,                                /* CPUInterfaceNumber */             \
    AcpiCpuUid,                           /* AcpiProcessorUid */               \
    Flags,                                /* Flags */                          \
    0,                                    /* ParkingProtocolVersion */         \
    PmuIrq,                               /* PerformanceInterruptGsiv */       \
    0,                                    /* ParkedAddress */                  \
    GicBase,                              /* PhysicalBaseAddress */            \
    GicVBase,                             /* GICV */                           \
    GicHBase,                             /* GICH */                           \
    GsivId,                               /* VGICMaintenanceInterrupt */       \
    GicRBase,                             /* GICRBaseAddress */                \
    Mpidr,                                /* MPIDR */                          \
    Efficiency,                           /* ProcessorPowerEfficiencyClass */  \
    {                                                                          \
      EFI_ACPI_RESERVED_BYTE,             /* Reserved2[0] */                   \
      EFI_ACPI_RESERVED_BYTE,             /* Reserved2[1] */                   \
      EFI_ACPI_RESERVED_BYTE              /* Reserved2[2] */                   \
    }                                                                          \
  }

// EFI_ACPI_6_2_GIC_DISTRIBUTOR_STRUCTURE
#define EFI_ACPI_6_2_GIC_DISTRIBUTOR_INIT(GicDistHwId, GicDistBase,            \
  GicDistVector, GicVersion)                                                   \
  {                                                                            \
    EFI_ACPI_6_2_GICD,                    /* Type */                           \
    sizeof (EFI_ACPI_6_2_GIC_DISTRIBUTOR_STRUCTURE),                           \
    EFI_ACPI_RESERVED_WORD,               /* Reserved1 */                      \
    GicDistHwId,                          /* GicId */                          \
    GicDistBase,                          /* PhysicalBaseAddress */            \
    GicDistVector,                        /* SystemVectorBase */               \
    GicVersion,                           /* GicVersion */                     \
    {                                                                          \
      EFI_ACPI_RESERVED_BYTE,             /* Reserved2[0] */                   \
      EFI_ACPI_RESERVED_BYTE,             /* Reserved2[1] */                   \
      EFI_ACPI_RESERVED_BYTE              /* Reserved2[2] */                   \
    }                                                                          \
  }

// EFI_ACPI_6_2_GICR_STRUCTURE
#define EFI_ACPI_6_2_GIC_REDISTRIBUTOR_INIT(RedisRegionAddr, RedisDiscLength)  \
  {                                                                            \
    EFI_ACPI_6_2_GICR,                    /* Type */                           \
    sizeof (EFI_ACPI_6_2_GICR_STRUCTURE), /* Length */                         \
    EFI_ACPI_RESERVED_WORD,               /* Reserved */                       \
    RedisRegionAddr,                      /* DiscoveryRangeBaseAddress */      \
    RedisDiscLength                       /* DiscoveryRangeLength */           \
  }

// EFI_ACPI_6_2_GIC_ITS_STRUCTURE
#define EFI_ACPI_6_2_GIC_ITS_INIT(GicItsId, GicItsBase)                        \
  {                                                                            \
    EFI_ACPI_6_2_GIC_ITS,                 /* Type */                           \
    sizeof (EFI_ACPI_6_2_GIC_ITS_STRUCTURE),                                   \
    EFI_ACPI_RESERVED_WORD,               /* Reserved */                       \
    GicItsId,                             /* GicItsId */                       \
    GicItsBase,                           /* PhysicalBaseAddress */            \
    EFI_ACPI_RESERVED_DWORD               /* DiscoveryRangeLength */           \
  }

// Multiple APIC Description Table
#pragma pack (1)

typedef struct {
  EFI_ACPI_6_2_MULTIPLE_APIC_DESCRIPTION_TABLE_HEADER   Header;
  EFI_ACPI_6_2_GIC_STRUCTURE                            GicInterfaces[CORE_CNT];
  EFI_ACPI_6_2_GIC_DISTRIBUTOR_STRUCTURE                GicDistributor;
  EFI_ACPI_6_2_GICR_STRUCTURE                           GicRedistributor;
  EFI_ACPI_6_2_GIC_ITS_STRUCTURE                        GicIts;
} EFI_ACPI_6_2_MULTIPLE_APIC_DESCRIPTION_TABLE;

#pragma pack ()

STATIC EFI_ACPI_6_2_MULTIPLE_APIC_DESCRIPTION_TABLE Madt = {
  {
    ARM_ACPI_HEADER (
      EFI_ACPI_6_2_MULTIPLE_APIC_DESCRIPTION_TABLE_SIGNATURE,
      EFI_ACPI_6_2_MULTIPLE_APIC_DESCRIPTION_TABLE,
      EFI_ACPI_6_2_MULTIPLE_APIC_DESCRIPTION_TABLE_REVISION
    ),
    // MADT specific fields
    0, // LocalApicAddress
    0  // Flags
  },
  {
    // Format: EFI_ACPI_6_2_GICC_STRUCTURE_INIT(GicId, AcpiCpuUid, Mpidr, Flags,
    //                                          PmuIrq, GicBase, GicVBase,
    //                                          GicHBase, GsivId, GicRBase,
    //                                          Efficiency)
    // Note: The GIC Structure of the primary CPU must be the first entry
    // (see note in 5.2.12.14 GICC Structure of ACPI v6.2).
    EFI_ACPI_6_2_GICC_STRUCTURE_INIT( // Neoverse-N1-0
      0, 0, GET_MPID(0x0, 0x0), EFI_ACPI_6_2_GIC_ENABLED, 23,
      FixedPcdGet32 (PcdGicDistributorBase),
      0x2c020000, 0x2c010000, 25, 0 /* GicRBase */, 0 /* Efficiency */),
    EFI_ACPI_6_2_GICC_STRUCTURE_INIT( // Neoverse-N1-1
      0, 1, GET_MPID(0x0, 0x100), EFI_ACPI_6_2_GIC_ENABLED, 23,
      FixedPcdGet32 (PcdGicDistributorBase),
      0x2c020000, 0x2c010000, 25, 0 /* GicRBase */, 0 /* Efficiency */),
    EFI_ACPI_6_2_GICC_STRUCTURE_INIT( // Neoverse-N1-2
      0, 2, GET_MPID(0x0, 0x200), EFI_ACPI_6_2_GIC_ENABLED, 23,
      FixedPcdGet32 (PcdGicDistributorBase),
      0x2c020000, 0x2c010000, 25, 0 /* GicRBase */, 0 /* Efficiency */),
    EFI_ACPI_6_2_GICC_STRUCTURE_INIT( // Neoverse-N1-3
      0, 3, GET_MPID(0x0, 0x300), EFI_ACPI_6_2_GIC_ENABLED, 23,
      FixedPcdGet32 (PcdGicDistributorBase),
      0x2c020000, 0x2c010000, 25, 0 /* GicRBase */, 0 /* Efficiency */),

    EFI_ACPI_6_2_GICC_STRUCTURE_INIT( // Neoverse-N1-4
      0, 4, GET_MPID(0x100, 0x00), EFI_ACPI_6_2_GIC_ENABLED, 23,
      FixedPcdGet32 (PcdGicDistributorBase),
      0x2c020000, 0x2c010000, 25, 0 /* GicRBase */, 0 /* Efficiency */),
    EFI_ACPI_6_2_GICC_STRUCTURE_INIT( // Neoverse-N1-5
      0, 5, GET_MPID(0x100, 0x100), EFI_ACPI_6_2_GIC_ENABLED, 23,
      FixedPcdGet32 (PcdGicDistributorBase),
      0x2c020000, 0x2c010000, 25, 0 /* GicRBase */, 0 /* Efficiency */),
    EFI_ACPI_6_2_GICC_STRUCTURE_INIT( // Neoverse-N1-6
      0, 6, GET_MPID(0x100, 0x200), EFI_ACPI_6_2_GIC_ENABLED, 23,
      FixedPcdGet32 (PcdGicDistributorBase),
      0x2c020000, 0x2c010000, 25, 0 /* GicRBase */, 0 /* Efficiency */),
    EFI_ACPI_6_2_GICC_STRUCTURE_INIT( // Neoverse-N1-7
      0, 7, GET_MPID(0x100, 0x300), EFI_ACPI_6_2_GIC_ENABLED, 23,
      FixedPcdGet32 (PcdGicDistributorBase),
      0x2c020000, 0x2c010000, 25, 0 /* GicRBase */, 0 /* Efficiency */)
  },
  // GIC Distributor Entry
  EFI_ACPI_6_2_GIC_DISTRIBUTOR_INIT(0, FixedPcdGet32 (PcdGicDistributorBase),
                                    0, 3),
  // GIC Redistributor
  EFI_ACPI_6_2_GIC_REDISTRIBUTOR_INIT(FixedPcdGet32 (PcdGicRedistributorsBase),
                                      SIZE_1MB),
  // GIC ITS
  EFI_ACPI_6_2_GIC_ITS_INIT(0, 0x30040000)
};

//
// Reference the table being generated to prevent the optimizer from removing
// the data structure from the executable
//
VOID* CONST ReferenceAcpiTable = &Madt;
