# @file
#
#  Copyright (c) 2011-2015, ARM Limited. All rights reserved.
#  Copyright (c) 2014, Linaro Limited. All rights reserved.
#  Copyright (c) 2015 - 2016, Intel Corporation. All rights reserved.
#  Copyright (c) 2017 - 2018, Andrei Warkentin <andrey.warkentin@gmail.com>
#
#  SPDX-License-Identifier: BSD-2-Clause-Patent
#
##

################################################################################
#
# Defines Section - statements that will be processed to create a Makefile.
#
################################################################################
[Defines]
  PLATFORM_NAME                  = RPi3
  PLATFORM_GUID                  = 5d30c4fc-93cf-40c9-8486-3badc0410816
  PLATFORM_VERSION               = 1.0
  DSC_SPECIFICATION              = 0x0001001A
  OUTPUT_DIRECTORY               = Build/$(PLATFORM_NAME)
  SUPPORTED_ARCHITECTURES        = AARCH64
  BUILD_TARGETS                  = DEBUG|RELEASE|NOOPT
  SKUID_IDENTIFIER               = DEFAULT
  FLASH_DEFINITION               = Platform/RaspberryPi/$(PLATFORM_NAME)/$(PLATFORM_NAME).fdf

  #
  # Network definition
  #
  DEFINE NETWORK_TLS_ENABLE       = FALSE
  DEFINE NETWORK_HTTP_BOOT_ENABLE = FALSE

  #
  # Defines for default states.  These can be changed on the command line.
  # -D FLAG=VALUE
  #
  DEFINE SECURE_BOOT_ENABLE      = FALSE
  DEFINE DEBUG_PRINT_ERROR_LEVEL = 0x8000004F

################################################################################
#
# Library Class section - list of all Library Classes needed by this Platform.
#
################################################################################
[LibraryClasses.common]
!if $(TARGET) == RELEASE
  DebugLib|MdePkg/Library/BaseDebugLibNull/BaseDebugLibNull.inf
!else
  DebugLib|MdePkg/Library/BaseDebugLibSerialPort/BaseDebugLibSerialPort.inf
!endif
  DebugPrintErrorLevelLib|MdePkg/Library/BaseDebugPrintErrorLevelLib/BaseDebugPrintErrorLevelLib.inf

  BaseLib|MdePkg/Library/BaseLib/BaseLib.inf
  SafeIntLib|MdePkg/Library/BaseSafeIntLib/BaseSafeIntLib.inf
  BmpSupportLib|MdeModulePkg/Library/BaseBmpSupportLib/BaseBmpSupportLib.inf
  SynchronizationLib|MdePkg/Library/BaseSynchronizationLib/BaseSynchronizationLib.inf
  PerformanceLib|MdePkg/Library/BasePerformanceLibNull/BasePerformanceLibNull.inf
  ReportStatusCodeLib|MdePkg/Library/BaseReportStatusCodeLibNull/BaseReportStatusCodeLibNull.inf
  PrintLib|MdePkg/Library/BasePrintLib/BasePrintLib.inf
  PeCoffGetEntryPointLib|MdePkg/Library/BasePeCoffGetEntryPointLib/BasePeCoffGetEntryPointLib.inf
  PeCoffLib|MdePkg/Library/BasePeCoffLib/BasePeCoffLib.inf
  IoLib|MdePkg/Library/BaseIoLibIntrinsic/BaseIoLibIntrinsic.inf
  UefiDecompressLib|MdePkg/Library/BaseUefiDecompressLib/BaseUefiDecompressLib.inf
  CpuLib|MdePkg/Library/BaseCpuLib/BaseCpuLib.inf

  UefiLib|MdePkg/Library/UefiLib/UefiLib.inf
  HobLib|MdePkg/Library/DxeHobLib/DxeHobLib.inf
  UefiRuntimeServicesTableLib|MdePkg/Library/UefiRuntimeServicesTableLib/UefiRuntimeServicesTableLib.inf
  DevicePathLib|MdePkg/Library/UefiDevicePathLib/UefiDevicePathLib.inf
  UefiBootServicesTableLib|MdePkg/Library/UefiBootServicesTableLib/UefiBootServicesTableLib.inf
  DxeServicesTableLib|MdePkg/Library/DxeServicesTableLib/DxeServicesTableLib.inf
  DxeServicesLib|MdePkg/Library/DxeServicesLib/DxeServicesLib.inf
  UefiDriverEntryPoint|MdePkg/Library/UefiDriverEntryPoint/UefiDriverEntryPoint.inf
  UefiApplicationEntryPoint|MdePkg/Library/UefiApplicationEntryPoint/UefiApplicationEntryPoint.inf
  HiiLib|MdeModulePkg/Library/UefiHiiLib/UefiHiiLib.inf
  UefiHiiServicesLib|MdeModulePkg/Library/UefiHiiServicesLib/UefiHiiServicesLib.inf
  SortLib|MdeModulePkg/Library/UefiSortLib/UefiSortLib.inf

  UefiRuntimeLib|MdePkg/Library/UefiRuntimeLib/UefiRuntimeLib.inf
  OrderedCollectionLib|MdePkg/Library/BaseOrderedCollectionRedBlackTreeLib/BaseOrderedCollectionRedBlackTreeLib.inf

  #
  # Ramdisk Requirements
  #
  FileExplorerLib|MdeModulePkg/Library/FileExplorerLib/FileExplorerLib.inf

  # Allow dynamic PCDs
  #
  PcdLib|MdePkg/Library/DxePcdLib/DxePcdLib.inf

  # use the accelerated BaseMemoryLibOptDxe by default, overrides for SEC/PEI below
  BaseMemoryLib|MdePkg/Library/BaseMemoryLibOptDxe/BaseMemoryLibOptDxe.inf

  #
  # It is not possible to prevent the ARM compiler from inserting calls to intrinsic functions.
  # This library provides the instrinsic functions such a compiler may generate calls to.
  #
  NULL|ArmPkg/Library/CompilerIntrinsicsLib/CompilerIntrinsicsLib.inf

  # Add support for GCC stack protector
  NULL|MdePkg/Library/BaseStackCheckLib/BaseStackCheckLib.inf

  # ARM Architectural Libraries
  CacheMaintenanceLib|ArmPkg/Library/ArmCacheMaintenanceLib/ArmCacheMaintenanceLib.inf
  DefaultExceptionHandlerLib|ArmPkg/Library/DefaultExceptionHandlerLib/DefaultExceptionHandlerLib.inf
  CpuExceptionHandlerLib|ArmPkg/Library/ArmExceptionLib/ArmExceptionLib.inf
  ArmDisassemblerLib|ArmPkg/Library/ArmDisassemblerLib/ArmDisassemblerLib.inf
  DmaLib|EmbeddedPkg/Library/NonCoherentDmaLib/NonCoherentDmaLib.inf
  TimeBaseLib|EmbeddedPkg/Library/TimeBaseLib/TimeBaseLib.inf
  ArmPlatformStackLib|ArmPlatformPkg/Library/ArmPlatformStackLib/ArmPlatformStackLib.inf
  ArmSmcLib|ArmPkg/Library/ArmSmcLib/ArmSmcLib.inf
  ArmHvcLib|ArmPkg/Library/ArmHvcLib/ArmHvcLib.inf
  ArmGenericTimerCounterLib|ArmPkg/Library/ArmGenericTimerPhyCounterLib/ArmGenericTimerPhyCounterLib.inf

  PciCf8Lib|MdePkg/Library/BasePciCf8Lib/BasePciCf8Lib.inf
  PciLib|MdePkg/Library/BasePciLibCf8/BasePciLibCf8.inf
  PlatformHookLib|MdeModulePkg/Library/BasePlatformHookLibNull/BasePlatformHookLibNull.inf
  SerialPortLib|MdeModulePkg/Library/BaseSerialPortLib16550/BaseSerialPortLib16550.inf

  # Cryptographic libraries
  IntrinsicLib|CryptoPkg/Library/IntrinsicLib/IntrinsicLib.inf
  BaseCryptLib|CryptoPkg/Library/BaseCryptLib/BaseCryptLib.inf
  OpensslLib|CryptoPkg/Library/OpensslLib/OpensslLib.inf

  #
  # Uncomment (and comment out the next line) For RealView Debugger. The Standard IO window
  # in the debugger will show load and unload commands for symbols. You can cut and paste this
  # into the command window to load symbols. We should be able to use a script to do this, but
  # the version of RVD I have does not support scripts accessing system memory.
  #
  #PeCoffExtraActionLib|ArmPkg/Library/RvdPeCoffExtraActionLib/RvdPeCoffExtraActionLib.inf
  PeCoffExtraActionLib|ArmPkg/Library/DebugPeCoffExtraActionLib/DebugPeCoffExtraActionLib.inf
  #PeCoffExtraActionLib|MdePkg/Library/BasePeCoffExtraActionLibNull/BasePeCoffExtraActionLibNull.inf

  DebugAgentLib|MdeModulePkg/Library/DebugAgentLibNull/DebugAgentLibNull.inf
  DebugAgentTimerLib|EmbeddedPkg/Library/DebugAgentTimerLibNull/DebugAgentTimerLibNull.inf

  # Flattened Device Tree (FDT) access library
  FdtLib|EmbeddedPkg/Library/FdtLib/FdtLib.inf

  # USB Libraries
  UefiUsbLib|MdePkg/Library/UefiUsbLib/UefiUsbLib.inf

  #
  # Secure Boot dependencies
  #
!if $(SECURE_BOOT_ENABLE) == TRUE
  TpmMeasurementLib|SecurityPkg/Library/DxeTpmMeasurementLib/DxeTpmMeasurementLib.inf
  AuthVariableLib|SecurityPkg/Library/AuthVariableLib/AuthVariableLib.inf

  # re-use the UserPhysicalPresent() dummy implementation from the ovmf tree
  PlatformSecureLib|OvmfPkg/Library/PlatformSecureLib/PlatformSecureLib.inf
!else
  TpmMeasurementLib|MdeModulePkg/Library/TpmMeasurementLibNull/TpmMeasurementLibNull.inf
  AuthVariableLib|MdeModulePkg/Library/AuthVariableLibNull/AuthVariableLibNull.inf
!endif
  VarCheckLib|MdeModulePkg/Library/VarCheckLib/VarCheckLib.inf
  GpioLib|Silicon/Broadcom/Bcm283x/Library/GpioLib/GpioLib.inf

[LibraryClasses.common.SEC]
  PcdLib|MdePkg/Library/BasePcdLibNull/BasePcdLibNull.inf
  BaseMemoryLib|MdePkg/Library/BaseMemoryLib/BaseMemoryLib.inf
  MemoryInitPeiLib|Platform/RaspberryPi/$(PLATFORM_NAME)/Library/MemoryInitPeiLib/MemoryInitPeiLib.inf
  PlatformPeiLib|ArmPlatformPkg/PlatformPei/PlatformPeiLib.inf
  ExtractGuidedSectionLib|EmbeddedPkg/Library/PrePiExtractGuidedSectionLib/PrePiExtractGuidedSectionLib.inf
  LzmaDecompressLib|MdeModulePkg/Library/LzmaCustomDecompressLib/LzmaCustomDecompressLib.inf
  PrePiLib|EmbeddedPkg/Library/PrePiLib/PrePiLib.inf
  HobLib|EmbeddedPkg/Library/PrePiHobLib/PrePiHobLib.inf
  PrePiHobListPointerLib|ArmPlatformPkg/Library/PrePiHobListPointerLib/PrePiHobListPointerLib.inf
  MemoryAllocationLib|EmbeddedPkg/Library/PrePiMemoryAllocationLib/PrePiMemoryAllocationLib.inf

[LibraryClasses.common.DXE_CORE]
  HobLib|MdePkg/Library/DxeCoreHobLib/DxeCoreHobLib.inf
  MemoryAllocationLib|MdeModulePkg/Library/DxeCoreMemoryAllocationLib/DxeCoreMemoryAllocationLib.inf
  DxeCoreEntryPoint|MdePkg/Library/DxeCoreEntryPoint/DxeCoreEntryPoint.inf
  ExtractGuidedSectionLib|MdePkg/Library/DxeExtractGuidedSectionLib/DxeExtractGuidedSectionLib.inf
  PerformanceLib|MdeModulePkg/Library/DxeCorePerformanceLib/DxeCorePerformanceLib.inf

[LibraryClasses.common.DXE_DRIVER]
  SecurityManagementLib|MdeModulePkg/Library/DxeSecurityManagementLib/DxeSecurityManagementLib.inf
  PerformanceLib|MdeModulePkg/Library/DxePerformanceLib/DxePerformanceLib.inf
  MemoryAllocationLib|MdePkg/Library/UefiMemoryAllocationLib/UefiMemoryAllocationLib.inf

[LibraryClasses.common.UEFI_APPLICATION]
  PerformanceLib|MdeModulePkg/Library/DxePerformanceLib/DxePerformanceLib.inf
  MemoryAllocationLib|MdePkg/Library/UefiMemoryAllocationLib/UefiMemoryAllocationLib.inf
  HiiLib|MdeModulePkg/Library/UefiHiiLib/UefiHiiLib.inf
  ShellLib|ShellPkg/Library/UefiShellLib/UefiShellLib.inf
  FileHandleLib|MdePkg/Library/UefiFileHandleLib/UefiFileHandleLib.inf

[LibraryClasses.common.UEFI_DRIVER]
  ExtractGuidedSectionLib|MdePkg/Library/DxeExtractGuidedSectionLib/DxeExtractGuidedSectionLib.inf
  PerformanceLib|MdeModulePkg/Library/DxePerformanceLib/DxePerformanceLib.inf
  MemoryAllocationLib|MdePkg/Library/UefiMemoryAllocationLib/UefiMemoryAllocationLib.inf

[LibraryClasses.common.DXE_RUNTIME_DRIVER]
  MemoryAllocationLib|MdePkg/Library/UefiMemoryAllocationLib/UefiMemoryAllocationLib.inf
  CapsuleLib|MdeModulePkg/Library/DxeCapsuleLibNull/DxeCapsuleLibNull.inf
  EfiResetSystemLib|Platform/RaspberryPi/$(PLATFORM_NAME)/Library/ResetLib/ResetLib.inf
  ArmSmcLib|ArmPkg/Library/ArmSmcLib/ArmSmcLib.inf

!if $(SECURE_BOOT_ENABLE) == TRUE
  BaseCryptLib|CryptoPkg/Library/BaseCryptLib/RuntimeCryptLib.inf
!endif

###################################################################################################
# BuildOptions Section - Define the module specific tool chain flags that should be used as
#                        the default flags for a module. These flags are appended to any
#                        standard flags that are defined by the build process.
###################################################################################################

[BuildOptions]
  GCC:*_*_AARCH64_DLINK_FLAGS = -Wl,--fix-cortex-a53-843419
  GCC:RELEASE_*_*_CC_FLAGS    = -DMDEPKG_NDEBUG -DNDEBUG

[BuildOptions.common.EDKII.DXE_RUNTIME_DRIVER]
  GCC:*_*_AARCH64_DLINK_FLAGS = -z common-page-size=0x10000

################################################################################
#
# Pcd Section - list of all EDK II PCD Entries defined by this Platform
#
################################################################################

[PcdsFeatureFlag.common]
  # Use the Vector Table location in CpuDxe. We will not copy the Vector Table at PcdCpuVectorBaseAddress
  gArmTokenSpaceGuid.PcdRelocateVectorTable|FALSE

  gEmbeddedTokenSpaceGuid.PcdPrePiProduceMemoryTypeInformationHob|TRUE
  gEfiMdeModulePkgTokenSpaceGuid.PcdTurnOffUsbLegacySupport|TRUE

  ## If TRUE, Graphics Output Protocol will be installed on virtual handle created by ConsplitterDxe.
  #  It could be set FALSE to save size.
  gEfiMdeModulePkgTokenSpaceGuid.PcdConOutGopSupport|TRUE
  gEfiMdeModulePkgTokenSpaceGuid.PcdConOutUgaSupport|FALSE

[PcdsFixedAtBuild.common]
  gEfiMdePkgTokenSpaceGuid.PcdMaximumUnicodeStringLength|1000000
  gEfiMdePkgTokenSpaceGuid.PcdMaximumAsciiStringLength|1000000
  gEfiMdePkgTokenSpaceGuid.PcdMaximumLinkedListLength|1000000
  gEfiMdePkgTokenSpaceGuid.PcdSpinLockTimeout|10000000
  gEfiMdePkgTokenSpaceGuid.PcdDebugClearMemoryValue|0xAF
  gEfiMdePkgTokenSpaceGuid.PcdPerformanceLibraryPropertyMask|1
  gEfiMdePkgTokenSpaceGuid.PcdPostCodePropertyMask|0
  gEfiMdePkgTokenSpaceGuid.PcdUefiLibMaxPrintBufferSize|320

  # DEBUG_ASSERT_ENABLED       0x01
  # DEBUG_PRINT_ENABLED        0x02
  # DEBUG_CODE_ENABLED         0x04
  # CLEAR_MEMORY_ENABLED       0x08
  # ASSERT_BREAKPOINT_ENABLED  0x10
  # ASSERT_DEADLOOP_ENABLED    0x20
!if $(TARGET) == RELEASE
  gEfiMdePkgTokenSpaceGuid.PcdDebugPropertyMask|0x21
!else
  gEfiMdePkgTokenSpaceGuid.PcdDebugPropertyMask|0x2f
!endif

  #  DEBUG_INIT      0x00000001  // Initialization
  #  DEBUG_WARN      0x00000002  // Warnings
  #  DEBUG_LOAD      0x00000004  // Load events
  #  DEBUG_FS        0x00000008  // EFI File system
  #  DEBUG_POOL      0x00000010  // Alloc & Free (pool)
  #  DEBUG_PAGE      0x00000020  // Alloc & Free (page)
  #  DEBUG_INFO      0x00000040  // Informational debug messages
  #  DEBUG_DISPATCH  0x00000080  // PEI/DXE/SMM Dispatchers
  #  DEBUG_VARIABLE  0x00000100  // Variable
  #  DEBUG_BM        0x00000400  // Boot Manager
  #  DEBUG_BLKIO     0x00001000  // BlkIo Driver
  #  DEBUG_NET       0x00004000  // SNP Driver
  #  DEBUG_UNDI      0x00010000  // UNDI Driver
  #  DEBUG_LOADFILE  0x00020000  // LoadFile
  #  DEBUG_EVENT     0x00080000  // Event messages
  #  DEBUG_GCD       0x00100000  // Global Coherency Database changes
  #  DEBUG_CACHE     0x00200000  // Memory range cachability changes
  #  DEBUG_VERBOSE   0x00400000  // Detailed debug messages that may
  #                              // significantly impact boot performance
  #  DEBUG_ERROR     0x80000000  // Error
  gEfiMdePkgTokenSpaceGuid.PcdDebugPrintErrorLevel|$(DEBUG_PRINT_ERROR_LEVEL)

  gEfiMdePkgTokenSpaceGuid.PcdReportStatusCodePropertyMask|0x07

  #
  # Optional feature to help prevent EFI memory map fragments
  # Turned on and off via: PcdPrePiProduceMemoryTypeInformationHob
  # Values are in EFI Pages (4K). DXE Core will make sure that
  # at least this much of each type of memory can be allocated
  # from a single memory range. This way you only end up with
  # maximum of two fragments for each type in the memory map
  # (the memory used, and the free memory that was prereserved
  # but not used).
  #
  gEmbeddedTokenSpaceGuid.PcdMemoryTypeEfiACPIReclaimMemory|0
  gEmbeddedTokenSpaceGuid.PcdMemoryTypeEfiACPIMemoryNVS|0
  gEmbeddedTokenSpaceGuid.PcdMemoryTypeEfiReservedMemoryType|0
!if $(SECURE_BOOT_ENABLE) == TRUE
  gEmbeddedTokenSpaceGuid.PcdMemoryTypeEfiRuntimeServicesData|600
  gEmbeddedTokenSpaceGuid.PcdMemoryTypeEfiRuntimeServicesCode|400
  gEmbeddedTokenSpaceGuid.PcdMemoryTypeEfiBootServicesCode|1500
!else
  gEmbeddedTokenSpaceGuid.PcdMemoryTypeEfiRuntimeServicesData|300
  gEmbeddedTokenSpaceGuid.PcdMemoryTypeEfiRuntimeServicesCode|150
  gEmbeddedTokenSpaceGuid.PcdMemoryTypeEfiBootServicesCode|1000
!endif
  gEmbeddedTokenSpaceGuid.PcdMemoryTypeEfiBootServicesData|12000
  gEmbeddedTokenSpaceGuid.PcdMemoryTypeEfiLoaderCode|20
  gEmbeddedTokenSpaceGuid.PcdMemoryTypeEfiLoaderData|0

  gEmbeddedTokenSpaceGuid.PcdDmaDeviceOffset|0xc0000000

  gEfiMdeModulePkgTokenSpaceGuid.PcdFirmwareVersionString|L"edk2-1.0"

!if $(SECURE_BOOT_ENABLE) == TRUE
  # override the default values from SecurityPkg to ensure images from all sources are verified in secure boot
  gEfiSecurityPkgTokenSpaceGuid.PcdOptionRomImageVerificationPolicy|0x04
  gEfiSecurityPkgTokenSpaceGuid.PcdFixedMediaImageVerificationPolicy|0x04
  gEfiSecurityPkgTokenSpaceGuid.PcdRemovableMediaImageVerificationPolicy|0x04
!endif

  gEmbeddedTokenSpaceGuid.PcdInterruptBaseAddress|0x40000000
  gArmTokenSpaceGuid.PcdArmArchTimerSecIntrNum|0x0
  gArmTokenSpaceGuid.PcdArmArchTimerIntrNum|0x1
  gArmTokenSpaceGuid.PcdArmArchTimerVirtIntrNum|0x2
  gArmTokenSpaceGuid.PcdArmArchTimerHypIntrNum|0x3

[LibraryClasses.common]
  ArmLib|ArmPkg/Library/ArmLib/ArmBaseLib.inf
  ArmMmuLib|ArmPkg/Library/ArmMmuLib/ArmMmuBaseLib.inf
  ArmPlatformLib|Platform/RaspberryPi/$(PLATFORM_NAME)/Library/PlatformLib/PlatformLib.inf
  TimerLib|ArmPkg/Library/ArmArchTimerLib/ArmArchTimerLib.inf
  CapsuleLib|MdeModulePkg/Library/DxeCapsuleLibNull/DxeCapsuleLibNull.inf
  UefiBootManagerLib|MdeModulePkg/Library/UefiBootManagerLib/UefiBootManagerLib.inf
  BootLogoLib|MdeModulePkg/Library/BootLogoLib/BootLogoLib.inf
  PlatformBootManagerLib|Platform/RaspberryPi/$(PLATFORM_NAME)/Library/PlatformBootManagerLib/PlatformBootManagerLib.inf
  CustomizedDisplayLib|MdeModulePkg/Library/CustomizedDisplayLib/CustomizedDisplayLib.inf
  FileExplorerLib|MdeModulePkg/Library/FileExplorerLib/FileExplorerLib.inf

[LibraryClasses.common.UEFI_DRIVER]
  UefiScsiLib|MdePkg/Library/UefiScsiLib/UefiScsiLib.inf

################################################################################
#
# Pcd Section - list of all EDK II PCD Entries defined by this Platform
#
################################################################################

[PcdsFeatureFlag.common]
  gEfiMdeModulePkgTokenSpaceGuid.PcdConOutGopSupport|TRUE
  gEfiMdeModulePkgTokenSpaceGuid.PcdConOutUgaSupport|FALSE
  gEfiMdeModulePkgTokenSpaceGuid.PcdInstallAcpiSdtProtocol|TRUE

[PcdsFixedAtBuild.common]
  gArmPlatformTokenSpaceGuid.PcdCoreCount|4
  gArmTokenSpaceGuid.PcdVFPEnabled|1

  gArmPlatformTokenSpaceGuid.PcdCPUCorePrimaryStackSize|0x4000
  gEfiMdeModulePkgTokenSpaceGuid.PcdMaxVariableSize|0x2000
  gEfiMdeModulePkgTokenSpaceGuid.PcdMaxAuthVariableSize|0x2800

  # Size of the region used by UEFI in permanent memory (Reserved 64MB)
  gArmPlatformTokenSpaceGuid.PcdSystemMemoryUefiRegionSize|0x04000000
  #
  # This matches PcdFvBaseAddress, since everything less is ATF, and
  # will be reserved away.
  #
  gArmTokenSpaceGuid.PcdSystemMemoryBase|0x00400000
  gArmTokenSpaceGuid.PcdSystemMemorySize|0x3FC00000

  ## NS16550 compatible UART
  gEfiMdeModulePkgTokenSpaceGuid.PcdSerialRegisterBase|0x3f215040
  gEfiMdeModulePkgTokenSpaceGuid.PcdSerialUseMmio|TRUE
  gEfiMdeModulePkgTokenSpaceGuid.PcdSerialRegisterStride|4
  gEfiMdeModulePkgTokenSpaceGuid.PcdSerialClockRate|500000000
  gEfiMdeModulePkgTokenSpaceGuid.PcdSerialFifoControl|0x27
  gEfiMdeModulePkgTokenSpaceGuid.PcdSerialExtendedTxFifoSize|8
  gEfiMdePkgTokenSpaceGuid.PcdUartDefaultBaudRate|115200

  ## Default Terminal Type
  ## 0-PCANSI, 1-VT100, 2-VT00+, 3-UTF8, 4-TTYTERM
  gEfiMdePkgTokenSpaceGuid.PcdDefaultTerminalType|4

  gEfiMdeModulePkgTokenSpaceGuid.PcdResetOnMemoryTypeInformationChange|FALSE
  gEfiMdeModulePkgTokenSpaceGuid.PcdBootManagerMenuFile|{ 0x21, 0xaa, 0x2c, 0x46, 0x14, 0x76, 0x03, 0x45, 0x83, 0x6e, 0x8a, 0xb6, 0xf4, 0x66, 0x23, 0x31 }

  gEfiMdeModulePkgTokenSpaceGuid.PcdFirmwareVendor|L"Raspberry Pi 3 64-bit UEFI"
  gEfiMdeModulePkgTokenSpaceGuid.PcdSetNxForStack|TRUE

[PcdsDynamicHii.common.DEFAULT]

  #
  # Clock overrides.
  #

  gRaspberryPiTokenSpaceGuid.PcdCpuClock|L"CpuClock"|gConfigDxeFormSetGuid|0x0|0
  gRaspberryPiTokenSpaceGuid.PcdCustomCpuClock|L"CustomCpuClock"|gConfigDxeFormSetGuid|0x0|600

  #
  # SD-related.
  #

  gRaspberryPiTokenSpaceGuid.PcdSdIsArasan|L"SdIsArasan"|gConfigDxeFormSetGuid|0x0|0
  gRaspberryPiTokenSpaceGuid.PcdMmcForce1Bit|L"MmcForce1Bit"|gConfigDxeFormSetGuid|0x0|0
  gRaspberryPiTokenSpaceGuid.PcdMmcForceDefaultSpeed|L"MmcForceDefaultSpeed"|gConfigDxeFormSetGuid|0x0|0
  gRaspberryPiTokenSpaceGuid.PcdMmcSdDefaultSpeedMHz|L"MmcSdDefaultSpeedMHz"|gConfigDxeFormSetGuid|0x0|25
  gRaspberryPiTokenSpaceGuid.PcdMmcSdHighSpeedMHz|L"MmcSdHighSpeedMHz"|gConfigDxeFormSetGuid|0x0|50
  gRaspberryPiTokenSpaceGuid.PcdMmcDisableMulti|L"MmcDisableMulti"|gConfigDxeFormSetGuid|0x0|0

  #
  # Debug-related.
  #

  gRaspberryPiTokenSpaceGuid.PcdDebugEnableJTAG|L"DebugEnableJTAG"|gConfigDxeFormSetGuid|0x0|0
  gRaspberryPiTokenSpaceGuid.PcdDebugShowUEFIExit|L"DebugShowUEFIExit"|gConfigDxeFormSetGuid|0x0|0

  #
  # Display-related.
  #
  gRaspberryPiTokenSpaceGuid.PcdDisplayEnableVModes|L"DisplayEnableVModes"|gConfigDxeFormSetGuid|0x0|0
  gRaspberryPiTokenSpaceGuid.PcdDisplayEnableSShot|L"DisplayEnableSShot"|gConfigDxeFormSetGuid|0x0|1

  #
  # Common UEFI ones.
  #

  gEfiMdePkgTokenSpaceGuid.PcdPlatformBootTimeOut|L"Timeout"|gEfiGlobalVariableGuid|0x0|5
  #
  # This is silly, but by pointing SetupConXXX and ConXXX PCDs to
  # the same variables, I can use the graphical configuration to
  # change the mode used by ConSplitter.
  #
  gEfiMdeModulePkgTokenSpaceGuid.PcdSetupConOutColumn|L"Columns"|gRaspberryPiTokenSpaceGuid|0x0|80
  gEfiMdeModulePkgTokenSpaceGuid.PcdConOutColumn|L"Columns"|gRaspberryPiTokenSpaceGuid|0x0|80
  gEfiMdeModulePkgTokenSpaceGuid.PcdSetupConOutRow|L"Rows"|gRaspberryPiTokenSpaceGuid|0x0|25
  gEfiMdeModulePkgTokenSpaceGuid.PcdConOutRow|L"Rows"|gRaspberryPiTokenSpaceGuid|0x0|25

[PcdsDynamicDefault.common]
  #
  # Set video resolution for boot options and for text setup.
  #
  gEfiMdeModulePkgTokenSpaceGuid.PcdVideoHorizontalResolution|0
  gEfiMdeModulePkgTokenSpaceGuid.PcdVideoVerticalResolution|0
  gEfiMdeModulePkgTokenSpaceGuid.PcdSetupVideoHorizontalResolution|640
  gEfiMdeModulePkgTokenSpaceGuid.PcdSetupVideoVerticalResolution|480
  gEfiMdeModulePkgTokenSpaceGuid.PcdFlashNvStorageVariableBase64|0
  gEfiMdeModulePkgTokenSpaceGuid.PcdFlashNvStorageFtwWorkingBase|0
  gEfiMdeModulePkgTokenSpaceGuid.PcdFlashNvStorageFtwSpareBase|0

################################################################################
#
# Components Section - list of all EDK II Modules needed by this Platform
#
################################################################################
[Components.common]
  #
  # PEI Phase modules
  #
  ArmPlatformPkg/PrePi/PeiUniCore.inf

  #
  # DXE
  #
  MdeModulePkg/Core/Dxe/DxeMain.inf {
    <LibraryClasses>
      NULL|MdeModulePkg/Library/DxeCrc32GuidedSectionExtractLib/DxeCrc32GuidedSectionExtractLib.inf
  }
  MdeModulePkg/Universal/PCD/Dxe/Pcd.inf {
    <LibraryClasses>
      PcdLib|MdePkg/Library/BasePcdLibNull/BasePcdLibNull.inf
  }

  #
  # Architectural Protocols
  #
  ArmPkg/Drivers/CpuDxe/CpuDxe.inf
  MdeModulePkg/Core/RuntimeDxe/RuntimeDxe.inf
  Platform/RaspberryPi/$(PLATFORM_NAME)/Drivers/VarBlockServiceDxe/VarBlockServiceDxe.inf
  MdeModulePkg/Universal/FaultTolerantWriteDxe/FaultTolerantWriteDxe.inf
  MdeModulePkg/Universal/Variable/RuntimeDxe/VariableRuntimeDxe.inf {
    <LibraryClasses>
      NULL|MdeModulePkg/Library/VarCheckUefiLib/VarCheckUefiLib.inf
      DebugLib|MdePkg/Library/BaseDebugLibNull/BaseDebugLibNull.inf
  }
!if $(SECURE_BOOT_ENABLE) == TRUE
  MdeModulePkg/Universal/SecurityStubDxe/SecurityStubDxe.inf {
    <LibraryClasses>
      NULL|SecurityPkg/Library/DxeImageVerificationLib/DxeImageVerificationLib.inf
  }
  SecurityPkg/VariableAuthenticated/SecureBootConfigDxe/SecureBootConfigDxe.inf
!else
  MdeModulePkg/Universal/SecurityStubDxe/SecurityStubDxe.inf
!endif
  MdeModulePkg/Universal/CapsuleRuntimeDxe/CapsuleRuntimeDxe.inf
  MdeModulePkg/Universal/MonotonicCounterRuntimeDxe/MonotonicCounterRuntimeDxe.inf
  EmbeddedPkg/ResetRuntimeDxe/ResetRuntimeDxe.inf
  EmbeddedPkg/RealTimeClockRuntimeDxe/RealTimeClockRuntimeDxe.inf {
    <LibraryClasses>
      RealTimeClockLib|EmbeddedPkg/Library/VirtualRealTimeClockLib/VirtualRealTimeClockLib.inf
  }
  EmbeddedPkg/MetronomeDxe/MetronomeDxe.inf

  MdeModulePkg/Universal/Console/ConPlatformDxe/ConPlatformDxe.inf
  MdeModulePkg/Universal/Console/ConSplitterDxe/ConSplitterDxe.inf
  Platform/RaspberryPi/$(PLATFORM_NAME)/Drivers/GraphicsConsoleDxe/GraphicsConsoleDxe.inf
  MdeModulePkg/Universal/Console/TerminalDxe/TerminalDxe.inf
  MdeModulePkg/Universal/SerialDxe/SerialDxe.inf
  Platform/RaspberryPi/$(PLATFORM_NAME)/Drivers/DisplayDxe/DisplayDxe.inf

  MdeModulePkg/Universal/HiiDatabaseDxe/HiiDatabaseDxe.inf

  UefiCpuPkg/CpuIo2Dxe/CpuIo2Dxe.inf
  Silicon/Broadcom/Bcm283x/Drivers/InterruptDxe/InterruptDxe.inf
  Platform/RaspberryPi/$(PLATFORM_NAME)/Drivers/RpiFirmwareDxe/RpiFirmwareDxe.inf
  Platform/RaspberryPi/$(PLATFORM_NAME)/Drivers/FdtDxe/FdtDxe.inf
  Platform/RaspberryPi/$(PLATFORM_NAME)/Drivers/ConfigDxe/ConfigDxe.inf
  ArmPkg/Drivers/TimerDxe/TimerDxe.inf
  MdeModulePkg/Universal/WatchdogTimerDxe/WatchdogTimer.inf
  MdeModulePkg/Universal/EbcDxe/EbcDxe.inf

  #
  # FAT filesystem + GPT/MBR partitioning
  #
  MdeModulePkg/Universal/Disk/DiskIoDxe/DiskIoDxe.inf
  MdeModulePkg/Universal/Disk/PartitionDxe/PartitionDxe.inf
  MdeModulePkg/Universal/Disk/UnicodeCollation/EnglishDxe/EnglishDxe.inf
  FatPkg/EnhancedFatDxe/Fat.inf

  #
  # ACPI Support
  #
  MdeModulePkg/Universal/Acpi/AcpiTableDxe/AcpiTableDxe.inf
  MdeModulePkg/Universal/Acpi/AcpiPlatformDxe/AcpiPlatformDxe.inf
  MdeModulePkg/Universal/Acpi/BootGraphicsResourceTableDxe/BootGraphicsResourceTableDxe.inf
  Platform/RaspberryPi/$(PLATFORM_NAME)/AcpiTables/AcpiTables.inf

  #
  # SMBIOS Support
  #
  Platform/RaspberryPi/$(PLATFORM_NAME)/Drivers/PlatformSmbiosDxe/PlatformSmbiosDxe.inf
  MdeModulePkg/Universal/SmbiosDxe/SmbiosDxe.inf

  #
  # RAM Disk Support
  #
  MdeModulePkg/Universal/Disk/RamDiskDxe/RamDiskDxe.inf

  #
  # Bds
  #
  MdeModulePkg/Universal/DevicePathDxe/DevicePathDxe.inf
  MdeModulePkg/Universal/DisplayEngineDxe/DisplayEngineDxe.inf
  MdeModulePkg/Universal/SetupBrowserDxe/SetupBrowserDxe.inf
  MdeModulePkg/Universal/DriverHealthManagerDxe/DriverHealthManagerDxe.inf
  MdeModulePkg/Universal/BdsDxe/BdsDxe.inf
  Platform/RaspberryPi/$(PLATFORM_NAME)/Drivers/LogoDxe/LogoDxe.inf
  MdeModulePkg/Application/UiApp/UiApp.inf {
    <LibraryClasses>
      NULL|MdeModulePkg/Library/DeviceManagerUiLib/DeviceManagerUiLib.inf
      NULL|MdeModulePkg/Library/BootManagerUiLib/BootManagerUiLib.inf
      NULL|Platform/RaspberryPi/$(PLATFORM_NAME)/Library/PlatformUiAppLib/PlatformUiAppLib.inf
      NULL|MdeModulePkg/Library/BootMaintenanceManagerUiLib/BootMaintenanceManagerUiLib.inf
  }

  #
  # SCSI Bus and Disk Driver
  #
  MdeModulePkg/Bus/Scsi/ScsiBusDxe/ScsiBusDxe.inf
  MdeModulePkg/Bus/Scsi/ScsiDiskDxe/ScsiDiskDxe.inf

  #
  # USB Support
  #
  Platform/RaspberryPi/$(PLATFORM_NAME)/Drivers/DwUsbHostDxe/DwUsbHostDxe.inf
  MdeModulePkg/Bus/Usb/UsbBusDxe/UsbBusDxe.inf
  MdeModulePkg/Bus/Usb/UsbKbDxe/UsbKbDxe.inf
  MdeModulePkg/Bus/Usb/UsbMassStorageDxe/UsbMassStorageDxe.inf
  Drivers/OptionRomPkg/Bus/Usb/UsbNetworking/Ax88772b/Ax88772b.inf

  #
  # SD/MMC support
  #
  Platform/RaspberryPi/$(PLATFORM_NAME)/Drivers/SdHostDxe/SdHostDxe.inf
  Platform/RaspberryPi/$(PLATFORM_NAME)/Drivers/ArasanMmcHostDxe/ArasanMmcHostDxe.inf
  Platform/RaspberryPi/$(PLATFORM_NAME)/Drivers/MmcDxe/MmcDxe.inf

  #
  # Networking stack
  #
!include NetworkPkg/Network.dsc.inc

  #
  # RNG
  #
  Silicon/Broadcom/Bcm283x/Drivers/RngDxe/RngDxe.inf

  #
  # UEFI application (Shell Embedded Boot Loader)
  #
  ShellPkg/Application/Shell/Shell.inf {
    <LibraryClasses>
      ShellCommandLib|ShellPkg/Library/UefiShellCommandLib/UefiShellCommandLib.inf
      NULL|ShellPkg/Library/UefiShellLevel2CommandsLib/UefiShellLevel2CommandsLib.inf
      NULL|ShellPkg/Library/UefiShellLevel1CommandsLib/UefiShellLevel1CommandsLib.inf
      NULL|ShellPkg/Library/UefiShellLevel3CommandsLib/UefiShellLevel3CommandsLib.inf
      NULL|ShellPkg/Library/UefiShellDriver1CommandsLib/UefiShellDriver1CommandsLib.inf
      NULL|ShellPkg/Library/UefiShellDebug1CommandsLib/UefiShellDebug1CommandsLib.inf
      NULL|ShellPkg/Library/UefiShellInstall1CommandsLib/UefiShellInstall1CommandsLib.inf
      NULL|ShellPkg/Library/UefiShellNetwork1CommandsLib/UefiShellNetwork1CommandsLib.inf
      HandleParsingLib|ShellPkg/Library/UefiHandleParsingLib/UefiHandleParsingLib.inf
      PrintLib|MdePkg/Library/BasePrintLib/BasePrintLib.inf
      BcfgCommandLib|ShellPkg/Library/UefiShellBcfgCommandLib/UefiShellBcfgCommandLib.inf

    <PcdsFixedAtBuild>
      gEfiMdePkgTokenSpaceGuid.PcdDebugPropertyMask|0xFF
      gEfiShellPkgTokenSpaceGuid.PcdShellLibAutoInitialize|FALSE
      gEfiMdePkgTokenSpaceGuid.PcdUefiLibMaxPrintBufferSize|8000
      gEfiShellPkgTokenSpaceGuid.PcdShellFileOperationSize|0x200000
  }
