#
#  Copyright (C) Marvell International Ltd. and its affiliates
#
#  SPDX-License-Identifier: BSD-2-Clause-Patent
#

[FD.Armada_Capsule]
BaseAddress   = 0x00000000 #|gArmTokenSpaceGuid.PcdFdBaseAddress  # The base address of the Firmware in NOR Flash.
Size          = 0x00400000 #|gArmTokenSpaceGuid.PcdFdSize         # The size in bytes of the FLASH Device
ErasePolarity = 1

0x00000000|0x00010000
FILE = $(WORKSPACE)/$(OUTPUT_DIRECTORY)/$(TARGET)_$(TOOL_CHAIN_TAG)/FV/SYSTEMFIRMWAREDESCRIPTOR.Fv

0x00100000|0x00300000
FILE = $(FIRMWARE_IMAGE)

[FV.SystemFirmwareUpdateCargo]
FvAlignment        = 8
ERASE_POLARITY     = 1
MEMORY_MAPPED      = TRUE
STICKY_WRITE       = TRUE
LOCK_CAP           = TRUE
LOCK_STATUS        = TRUE
WRITE_DISABLED_CAP = TRUE
WRITE_ENABLED_CAP  = TRUE
WRITE_STATUS       = TRUE
WRITE_LOCK_CAP     = TRUE
WRITE_LOCK_STATUS  = TRUE
READ_DISABLED_CAP  = TRUE
READ_ENABLED_CAP   = TRUE
READ_STATUS        = TRUE
READ_LOCK_CAP      = TRUE
READ_LOCK_STATUS   = TRUE

  FILE RAW = b3890e02-c46b-4970-9536-57787a9e06c7 { # PcdEdkiiSystemFirmwareFileGuid
     FD = Armada_Capsule
  }

  FILE RAW = ce57b167-b0e4-41e8-a897-5f4feb781d40 { # gEdkiiSystemFmpCapsuleDriverFvFileGuid
    $(WORKSPACE)/$(OUTPUT_DIRECTORY)/$(TARGET)_$(TOOL_CHAIN_TAG)/FV/CAPSULEDISPATCHFV.Fv
  }

  FILE RAW = 812136D3-4D3A-433A-9418-29BB9BF78F6E { # gEdkiiSystemFmpCapsuleConfigFileGuid
    Silicon/Marvell/Armada7k8k/Feature/Capsule/SystemFirmwareUpdateConfig/SystemFirmwareUpdateConfig.ini
  }

[FmpPayload.FmpPayloadSystemFirmwarePkcs7]
IMAGE_HEADER_INIT_VERSION = 0x02
IMAGE_TYPE_ID             = 757fc475-6b22-4482-868e-ded286f30940 # PcdSystemFmpCapsuleImageTypeIdGuid
IMAGE_INDEX               = 0x1
HARDWARE_INSTANCE         = 0x0
MONOTONIC_COUNT           = 0x1
CERTIFICATE_GUID          = 4AAFD29D-68DF-49EE-8AA9-347D375665A7 # PKCS7

  FV = SystemFirmwareUpdateCargo

[Capsule.MvFirmwareUpdateCapsuleFmpPkcs7]
CAPSULE_GUID                = 6dcbd5ed-e82d-4c44-bda1-7194199ad92a # gEfiFmpCapsuleGuid
CAPSULE_HEADER_SIZE         = 0x20
CAPSULE_HEADER_INIT_VERSION = 0x1

  FMP_PAYLOAD = FmpPayloadSystemFirmwarePkcs7

