#
#  Copyright (c) 2018, Linaro Limited. All rights reserved.
#
#  SPDX-License-Identifier: BSD-2-Clause-Patent
#

################################################################################
#
# FD Section
# The [FD] Section is made up of the definition statements and a
# description of what goes into  the Flash Device Image.  Each FD section
# defines one flash "device" image.  A flash device image may be one of
# the following: Removable media bootable image (like a boot floppy
# image,) an Option ROM image (that would be "flashed" into an add-in
# card,) a System "Flash"  image (that would be burned into a system's
# flash) or an Update ("Capsule") image that will be used to update and
# existing system flash.
#
################################################################################

[FD.BL33_AP_UEFI]
BaseAddress   = 0x1AC98000|gArmTokenSpaceGuid.PcdFdBaseAddress  # The base address of the Firmware in NOR Flash.
Size          = 0x000F0000|gArmTokenSpaceGuid.PcdFdSize         # The size in bytes of the FLASH Device
ErasePolarity = 1

# This one is tricky, it must be: BlockSize * NumBlocks = Size
BlockSize     = 0x00001000
NumBlocks     = 0xF0

################################################################################
#
# Following are lists of FD Region layout which correspond to the locations of different
# images within the flash device.
#
# Regions must be defined in ascending order and may not overlap.
#
# A Layout Region start with a eight digit hex offset (leading "0x" required) followed by
# the pipe "|" character, followed by the size of the region, also in hex with the leading
# "0x" characters. Like:
# Offset|Size
# PcdOffsetCName|PcdSizeCName
# RegionType <FV, DATA, or FILE>
#
################################################################################

0x00000000|0x000F0000
gArmTokenSpaceGuid.PcdFvBaseAddress|gArmTokenSpaceGuid.PcdFvSize
FV = FVMAIN_COMPACT


################################################################################
#
# FV Section
#
# [FV] section is used to define what components or modules are placed within a flash
# device file.  This section also defines order the components and modules are positioned
# within the image.  The [FV] section consists of define statements, set statements and
# module statements.
#
################################################################################

[FV.FvMain]
BlockSize          = 0x40
NumBlocks          = 0         # This FV gets compressed so make it just big enough
FvAlignment        = 8         # FV alignment and FV attributes setting.
ERASE_POLARITY     = 1
MEMORY_MAPPED      = TRUE
STICKY_WRITE       = TRUE
LOCK_CAP           = TRUE
LOCK_STATUS        = TRUE
WRITE_DISABLED_CAP = TRUE
WRITE_ENABLED_CAP  = TRUE
WRITE_STATUS       = TRUE
WRITE_LOCK_CAP     = TRUE
WRITE_LOCK_STATUS  = TRUE
READ_DISABLED_CAP  = TRUE
READ_ENABLED_CAP   = TRUE
READ_STATUS        = TRUE
READ_LOCK_CAP      = TRUE
READ_LOCK_STATUS   = TRUE

  APRIORI DXE {
    INF MdeModulePkg/Universal/PCD/Dxe/Pcd.inf
  }

  INF MdeModulePkg/Core/Dxe/DxeMain.inf

  #
  # PI DXE Drivers producing Architectural Protocols (EFI Services)
  #
  INF ArmPkg/Drivers/CpuDxe/CpuDxe.inf
  INF MdeModulePkg/Core/RuntimeDxe/RuntimeDxe.inf
  INF MdeModulePkg/Universal/SecurityStubDxe/SecurityStubDxe.inf
  INF MdeModulePkg/Universal/CapsuleRuntimeDxe/CapsuleRuntimeDxe.inf
  INF EmbeddedPkg/EmbeddedMonotonicCounter/EmbeddedMonotonicCounter.inf
  INF MdeModulePkg/Universal/ResetSystemRuntimeDxe/ResetSystemRuntimeDxe.inf
  INF EmbeddedPkg/RealTimeClockRuntimeDxe/RealTimeClockRuntimeDxe.inf
  INF EmbeddedPkg/MetronomeDxe/MetronomeDxe.inf

  #
  # Multiple Console IO support
  #
  INF MdeModulePkg/Universal/Console/ConPlatformDxe/ConPlatformDxe.inf
  INF MdeModulePkg/Universal/Console/TerminalDxe/TerminalDxe.inf
  INF MdeModulePkg/Universal/SerialDxe/SerialDxe.inf

  INF ArmPkg/Drivers/ArmGic/ArmGicDxe.inf
  INF ArmPkg/Drivers/TimerDxe/TimerDxe.inf

  INF MdeModulePkg/Universal/WatchdogTimerDxe/WatchdogTimer.inf

  INF MdeModulePkg/Universal/PCD/Dxe/Pcd.inf

  #
  # GPIO
  #
  INF Platform/Hisilicon/HiKey960/HiKey960GpioDxe/HiKey960GpioDxe.inf
  INF ArmPlatformPkg/Drivers/PL061GpioDxe/PL061GpioDxe.inf

  #
  # Virtual Keyboard
  #
  INF EmbeddedPkg/Drivers/VirtualKeyboardDxe/VirtualKeyboardDxe.inf

  INF Platform/Hisilicon/HiKey960/HiKey960Dxe/HiKey960Dxe.inf

  #
  # USB Host Support
  #
  INF MdeModulePkg/Bus/Usb/UsbBusDxe/UsbBusDxe.inf

  #
  # USB Mass Storage Support
  #
  INF MdeModulePkg/Bus/Usb/UsbMassStorageDxe/UsbMassStorageDxe.inf

  #
  # USB Peripheral Support
  #
  INF EmbeddedPkg/Drivers/AndroidFastbootTransportUsbDxe/FastbootTransportUsbDxe.inf

  #
  # Fastboot
  #
  INF EmbeddedPkg/Application/AndroidFastboot/AndroidFastbootApp.inf

  #
  # UEFI Network Stack
  #
!include NetworkPkg/Network.fdf.inc
  #
  # FAT filesystem + GPT/MBR partitioning
  #
  INF MdeModulePkg/Universal/Disk/DiskIoDxe/DiskIoDxe.inf
  INF MdeModulePkg/Universal/Disk/PartitionDxe/PartitionDxe.inf
  INF FatPkg/EnhancedFatDxe/Fat.inf
  INF MdeModulePkg/Universal/Disk/UnicodeCollation/EnglishDxe/EnglishDxe.inf

  INF MdeModulePkg/Universal/Variable/RuntimeDxe/VariableRuntimeDxe.inf

  INF MdeModulePkg/Universal/HiiDatabaseDxe/HiiDatabaseDxe.inf

  #
  # UEFI applications
  #
  INF ShellPkg/Application/Shell/Shell.inf
!ifdef $(INCLUDE_TFTP_COMMAND)
  INF ShellPkg/DynamicCommand/TftpDynamicCommand/TftpDynamicCommand.inf
!endif #$(INCLUDE_TFTP_COMMAND)

  #
  # Bds
  #
  INF MdeModulePkg/Universal/DevicePathDxe/DevicePathDxe.inf
  INF MdeModulePkg/Universal/SetupBrowserDxe/SetupBrowserDxe.inf
  INF MdeModulePkg/Universal/DisplayEngineDxe/DisplayEngineDxe.inf
  INF MdeModulePkg/Universal/BdsDxe/BdsDxe.inf
  INF MdeModulePkg/Application/UiApp/UiApp.inf

[FV.FVMAIN_COMPACT]
FvAlignment        = 8
ERASE_POLARITY     = 1
MEMORY_MAPPED      = TRUE
STICKY_WRITE       = TRUE
LOCK_CAP           = TRUE
LOCK_STATUS        = TRUE
WRITE_DISABLED_CAP = TRUE
WRITE_ENABLED_CAP  = TRUE
WRITE_STATUS       = TRUE
WRITE_LOCK_CAP     = TRUE
WRITE_LOCK_STATUS  = TRUE
READ_DISABLED_CAP  = TRUE
READ_ENABLED_CAP   = TRUE
READ_STATUS        = TRUE
READ_LOCK_CAP      = TRUE
READ_LOCK_STATUS   = TRUE

  INF ArmPlatformPkg/PrePi/PeiUniCore.inf

  FILE FV_IMAGE = 9E21FD93-9C72-4c15-8C4B-E77F1DB2D792 {
    SECTION GUIDED EE4E5898-3914-4259-9D6E-DC7BD79403CF PROCESSING_REQUIRED = TRUE {
      SECTION FV_IMAGE = FVMAIN
    }
  }

!include Silicon/Hisilicon/Hisilicon.fdf.inc
