/** @file

Copyright (c) 2018, Intel Corporation. All rights reserved.<BR>
SPDX-License-Identifier: BSD-2-Clause-Patent

**/

//
// Define bits in LPC bridge config space
//  (\_SB.PCI0.LPC0)
//
OperationRegion (LPCB, PCI_Config, 0x00, 0x100)
Field (LPCB, DWordAcc, NoLock, Preserve)
{
	Offset (0xAC),
	, 16,
	XSMB, 1					// set when OS routes USB ports to xHCI in SmartAuto mode so next POST will know
}

#include "IrqLink.asl"       // PCI routing control methods
#include "Mother.asi"        // Static motherboard device resource declaration

