## @file
# Package for support of Clanton Peak CRB platform
#
# This package provides QuarkNcSocId platform specific modules.
# Copyright (c) 2013-2019 Intel Corporation.
#
# SPDX-License-Identifier: BSD-2-Clause-Patent
#
##


################################################################################
#
# Defines Section - statements that will be processed to create a Makefile.
#
################################################################################

[Defines]
  DEC_SPECIFICATION              = 0x00010005
  PACKAGE_NAME                   = QuarkPlatformPkg
  PACKAGE_GUID                   = 46C1F476-A85E-49a8-B258-DD4396B87FEF
  PACKAGE_VERSION                = 0.1


################################################################################
#
# Include Section - list of Include Paths that are provided by this package.
#                   Comments are used for Keywords and Module Types.
#
# Supported Module Types:
#  SEC PEIM DXE_DRIVER DXE_RUNTIME_DRIVER DXE_SMM_DRIVER DXE_SAL_DRIVER UEFI_DRIVER
#
################################################################################
[Includes]
  Include

################################################################################
#
# Library Class Header section - list of Library Class header files that are
#                                provided by this package.
#
################################################################################
[LibraryClasses]

################################################################################
#
# Global Guid Definition section - list of Global Guid C Name Data Structures
#                                  that are provided by this package.
#
################################################################################
[Guids]
  gQuarkPlatformTokenSpaceGuid      = { 0x199c1ef0, 0x6400, 0x41c5, { 0xb0, 0xa4, 0xff, 0xbf, 0x21, 0x9d, 0xcb, 0xae }}
  gEfiMemoryConfigDataGuid       = { 0x80dbd530, 0xb74c, 0x4f11, { 0x8c, 0x03, 0x41, 0x86, 0x65, 0x53, 0x28, 0x31 }}
  gPowerManagementAcpiTableStorageGuid = { 0xc0cc43bd, 0xc920, 0x4064, { 0x93, 0x5b, 0x93, 0xb4, 0x47, 0x37, 0x94, 0x70 }}
  gPeiCapsuleOnFatFloppyDiskGuid = {0x2e3d2e75, 0x9b2e, 0x412d, {0xb4, 0xb1, 0x70, 0x41, 0x6b, 0x87, 0x0, 0xff }}
  gPeiCapsuleOnFatIdeDiskGuid = {0xb38573b6, 0x6200, 0x4ac5, {0xb5, 0x1d, 0x82, 0xe6, 0x59, 0x38, 0xd7, 0x83 }}
  gPeiCapsuleOnFatUsbDiskGuid = {0x0ffbce19, 0x324c, 0x4690, {0xa0, 0x09, 0x98, 0xc6, 0xae, 0x2e, 0xb1, 0x86 }}
  gPeiCapsuleOnDataCDGuid = {0x5cac0099, 0x0dc9, 0x48e5, {0x80, 0x68, 0xbb, 0x95, 0xf5, 0x40, 0x0a, 0x9f }}
  gEfiQuarkCapsuleGuid = { 0xd400d1e4, 0xa314, 0x442b, { 0x89, 0xed, 0xa9, 0x2e, 0x4c, 0x81, 0x97, 0xcb } }
  gQuarkVariableLockGuid      = { 0xeef749c2, 0xc047, 0x4d6e, { 0xb1, 0xbc, 0xd3, 0x6e, 0xb3, 0xa5, 0x55, 0x9c }}

################################################################################
#
# Global Protocols Definition section - list of Global Protocols C Name Data
#                                  Structures that are provided by this package.
#
################################################################################
[Protocols]
  gEfiGlobalNvsAreaProtocolGuid  = { 0x074E1E48, 0x8132, 0x47A1, { 0x8C, 0x2C, 0x3F, 0x14, 0xAD, 0x9A, 0x66, 0xDC }}
  gEfiSmmSpiReadyProtocolGuid    = { 0x7a5dbc75, 0x5b2b, 0x4e67, { 0xbd, 0xe1, 0xd4, 0x8e, 0xee, 0x76, 0x15, 0x62 }}
  gEfiIioUdsProtocolGuid        = { 0xa7ced760, 0xc71c, 0x4e1a, { 0xac, 0xb1, 0x89, 0x60, 0x4d, 0x52, 0x16, 0xcb }}

################################################################################
#
# PCD Declarations section - list of all PCDs Declared by this Package
#                            Only this package should be providing the
#                            declaration, other packages should not.
#
################################################################################

[PcdsFeatureFlag]
  gQuarkPlatformTokenSpaceGuid.WaitIfResetDueToError|FALSE|BOOLEAN|0x2000000F

[PcdsFixedAtBuild]
  gQuarkPlatformTokenSpaceGuid.PcdFlashAreaBaseAddress|0xFF800000|UINT32|0x20000001
  gQuarkPlatformTokenSpaceGuid.PcdFlashAreaSize|0x800000|UINT32|0x20000002
  gQuarkPlatformTokenSpaceGuid.PcdFlashNvStorageBase|0xFFF30000|UINT32|0x20000003
  gQuarkPlatformTokenSpaceGuid.PcdFlashNvStorageSize|0x00020000|UINT32|0x20000004
  gQuarkPlatformTokenSpaceGuid.PcdFlashFvRecovery2Base|0xFFEF0400|UINT32|0x2000001C
  gQuarkPlatformTokenSpaceGuid.PcdFlashFvRecovery2Size|0x00007000|UINT32|0x2000001D
  gQuarkPlatformTokenSpaceGuid.PcdFlashQNCMicrocodeSize|0x00004000|UINT32|0x2000000C
  gQuarkPlatformTokenSpaceGuid.PcdPlatformDataBaseAddress|0xFFF10000|UINT32|0x2000001E
  gQuarkPlatformTokenSpaceGuid.PcdPlatformDataMaxLen|0x20000|UINT32|0x2000001F
  gQuarkPlatformTokenSpaceGuid.PcdHpetEnable|TRUE|BOOLEAN|0x20000018

  gQuarkPlatformTokenSpaceGuid.PcdFlashFvDefaultPayloadBase|0xFFC00400|UINT32|0x20000020
  gQuarkPlatformTokenSpaceGuid.PcdFlashFvDefaultPayloadSize|0x000F0000|UINT32|0x20000021
  gQuarkPlatformTokenSpaceGuid.PcdFlashFvDefaultMainBase|0xFFD00400|UINT32|0x20000022
  gQuarkPlatformTokenSpaceGuid.PcdFlashFvDefaultMainSize|0x000D0000|UINT32|0x20000023

  gQuarkPlatformTokenSpaceGuid.PcdMemorySize|0x80000000|UINT32|0x20000032
  # ECC scrub interval in miliseconds 1..255 (0 works as feature disable)
  gQuarkPlatformTokenSpaceGuid.PcdEccScrubInterval|0x00|UINT8|0x20000037
  # Number of 32B blocks read for ECC scrub 2..16
  gQuarkPlatformTokenSpaceGuid.PcdEccScrubBlkSize|0x02|UINT8|0x20000038
  gQuarkPlatformTokenSpaceGuid.PcdFlashNvMfh|0xFFF08000|UINT32|0x20000039
  gQuarkPlatformTokenSpaceGuid.PcdFlashFvFixedStage1AreaBase|0xFFF90000|UINT32|0x2000003A
  gQuarkPlatformTokenSpaceGuid.PcdFlashFvFixedStage1AreaSize|0x00040000|UINT32|0x2000003B
  gQuarkPlatformTokenSpaceGuid.PcdEsramStage1Base|0x80000000|UINT32|0x2000003C

  # Legacy Bridge protected BIOS range register configs, if == 0 then do nothing since register default.
  gQuarkPlatformTokenSpaceGuid.PcdLegacyProtectedBIOSRange0Pei|0x00000000|UINT32|0x2000003D
  gQuarkPlatformTokenSpaceGuid.PcdLegacyProtectedBIOSRange1Pei|0x00000000|UINT32|0x2000003E
  gQuarkPlatformTokenSpaceGuid.PcdLegacyProtectedBIOSRange2Pei|0x00000000|UINT32|0x2000004F

  # ACPI Power management settings.

  # Power Management flags.
  # PpmFlags[5] = PPM_C2      = C2 Capable, Enabled.
  gQuarkPlatformTokenSpaceGuid.PcdPpmFlags|0x00000020|UINT32|0xA00000CF

  # Madt Table Initialize settings.
  # Defines a flag to Enable/Disable interrupt override setting table0,
  # and the source Irq, Polarity, Triger Mode and global Irq of interrupt override setting table0
  gQuarkPlatformTokenSpaceGuid.PcdInterruptOverrideSettingTable0Enable|0x01|UINT8|0xA0000100
  gQuarkPlatformTokenSpaceGuid.PcdInterruptOverrideSettingTable0SourceIrq|0x00|UINT8|0xA0000101
  gQuarkPlatformTokenSpaceGuid.PcdInterruptOverrideSettingTable0Polarity|0x00|UINT8|0xA0000102
  gQuarkPlatformTokenSpaceGuid.PcdInterruptOverrideSettingTable0TrigerMode|0x00|UINT8|0xA0000103
  gQuarkPlatformTokenSpaceGuid.PcdInterruptOverrideSettingTable0GlobalIrq|0x02|UINT32|0xA0000104

  # Madt Table Initialize settings.
  # Defines a flag to Enable/Disable interrupt override setting table1,
  # and the source Irq, Polarity, Triger Mode and global Irq of interrupt override setting table1
  gQuarkPlatformTokenSpaceGuid.PcdInterruptOverrideSettingTable1Enable|0x01|UINT8|0xA0000105
  gQuarkPlatformTokenSpaceGuid.PcdInterruptOverrideSettingTable1SourceIrq|0x09|UINT8|0xA0000106
  gQuarkPlatformTokenSpaceGuid.PcdInterruptOverrideSettingTable1Polarity|0x01|UINT8|0xA0000107
  gQuarkPlatformTokenSpaceGuid.PcdInterruptOverrideSettingTable1TrigerMode|0x03|UINT8|0xA0000108
  gQuarkPlatformTokenSpaceGuid.PcdInterruptOverrideSettingTable1GlobalIrq|0x09|UINT32|0xA0000109

  # Madt Table Initialize settings.
  # Defines a flag to Enable/Disable interrupt override setting table2,
  # and the source Irq, Polarity, Triger Mode and global Irq of interrupt override setting table2
  gQuarkPlatformTokenSpaceGuid.PcdInterruptOverrideSettingTable2Enable|0x0|UINT8|0xA000010F
  gQuarkPlatformTokenSpaceGuid.PcdInterruptOverrideSettingTable2SourceIrq|0x0|UINT8|0xA0000110
  gQuarkPlatformTokenSpaceGuid.PcdInterruptOverrideSettingTable2Polarity|0x0|UINT8|0xA0000111
  gQuarkPlatformTokenSpaceGuid.PcdInterruptOverrideSettingTable2TrigerMode|0x0|UINT8|0xA0000112
  gQuarkPlatformTokenSpaceGuid.PcdInterruptOverrideSettingTable2GlobalIrq|0x0|UINT32|0xA0000113

  # Madt Table Initialize settings.
  # Defines a flag to Enable/Disable interrupt override setting table3,
  # and the source Irq, Polarity, Triger Mode and global Irq of interrupt override setting table3
  gQuarkPlatformTokenSpaceGuid.PcdInterruptOverrideSettingTable3Enable|0x0|UINT8|0xA0000114
  gQuarkPlatformTokenSpaceGuid.PcdInterruptOverrideSettingTable3SourceIrq|0x0|UINT8|0xA0000115
  gQuarkPlatformTokenSpaceGuid.PcdInterruptOverrideSettingTable3Polarity|0x0|UINT8|0xA0000116
  gQuarkPlatformTokenSpaceGuid.PcdInterruptOverrideSettingTable3TrigerMode|0x0|UINT8|0xA0000117
  gQuarkPlatformTokenSpaceGuid.PcdInterruptOverrideSettingTable3GlobalIrq|0x0|UINT32|0xA0000118

  # Madt Table Initialize settings.
  # Defines a flag to Enable/Disable interrupt override setting table4,
  # and the source Irq, Polarity, Triger Mode and global Irq of interrupt override setting table4
  gQuarkPlatformTokenSpaceGuid.PcdInterruptOverrideSettingTable4Enable|0x0|UINT8|0xA0000119
  gQuarkPlatformTokenSpaceGuid.PcdInterruptOverrideSettingTable4SourceIrq|0x0|UINT8|0xA000011A
  gQuarkPlatformTokenSpaceGuid.PcdInterruptOverrideSettingTable4Polarity|0x0|UINT8|0xA0000120
  gQuarkPlatformTokenSpaceGuid.PcdInterruptOverrideSettingTable4TrigerMode|0x0|UINT8|0xA0000121
  gQuarkPlatformTokenSpaceGuid.PcdInterruptOverrideSettingTable4GlobalIrq|0x0|UINT32|0xA0000122

  # Madt Table Initialize settings.
  # Defines a flag to Enable/Disable interrupt override setting table5,
  # and the source Irq, Polarity, Triger Mode and global Irq of interrupt override setting table5
  gQuarkPlatformTokenSpaceGuid.PcdInterruptOverrideSettingTable5Enable|0x0|UINT8|0xA0000123
  gQuarkPlatformTokenSpaceGuid.PcdInterruptOverrideSettingTable5SourceIrq|0x0|UINT8|0xA0000124
  gQuarkPlatformTokenSpaceGuid.PcdInterruptOverrideSettingTable5Polarity|0x0|UINT8|0xA0000125
  gQuarkPlatformTokenSpaceGuid.PcdInterruptOverrideSettingTable5TrigerMode|0x0|UINT8|0xA0000126
  gQuarkPlatformTokenSpaceGuid.PcdInterruptOverrideSettingTable5GlobalIrq|0x0|UINT32|0xA0000127

  # Madt Table Initialize settings.
  # Defines a flag to Enable/Disable interrupt override setting table6,
  # and the source Irq, Polarity, Triger Mode and global Irq of interrupt override setting table6
  gQuarkPlatformTokenSpaceGuid.PcdInterruptOverrideSettingTable6Enable|0x0|UINT8|0xA0000128
  gQuarkPlatformTokenSpaceGuid.PcdInterruptOverrideSettingTable6SourceIrq|0x0|UINT8|0xA0000129
  gQuarkPlatformTokenSpaceGuid.PcdInterruptOverrideSettingTable6Polarity|0x0|UINT8|0xA000012A
  gQuarkPlatformTokenSpaceGuid.PcdInterruptOverrideSettingTable6TrigerMode|0x0|UINT8|0xA000012B
  gQuarkPlatformTokenSpaceGuid.PcdInterruptOverrideSettingTable6GlobalIrq|0x0|UINT32|0xA000012C

  # Madt Table Initialize settings.
  # Defines a flag to Enable/Disable interrupt override setting table7,
  # and the source Irq, Polarity, Triger Mode and global Irq of interrupt override setting table7
  gQuarkPlatformTokenSpaceGuid.PcdInterruptOverrideSettingTable7Enable|0x0|UINT8|0xA000012D
  gQuarkPlatformTokenSpaceGuid.PcdInterruptOverrideSettingTable7SourceIrq|0x0|UINT8|0xA000012E
  gQuarkPlatformTokenSpaceGuid.PcdInterruptOverrideSettingTable7Polarity|0x0|UINT8|0xA000012F
  gQuarkPlatformTokenSpaceGuid.PcdInterruptOverrideSettingTable7TrigerMode|0x0|UINT8|0xA0000130
  gQuarkPlatformTokenSpaceGuid.PcdInterruptOverrideSettingTable7GlobalIrq|0x0|UINT32|0xA0000131

  # Madt Table Initialize settings.
  # Defines a flag to Enable/Disable interrupt override setting table8,
  # and the source Irq, Polarity, Triger Mode and global Irq of interrupt override setting table8
  gQuarkPlatformTokenSpaceGuid.PcdInterruptOverrideSettingTable8Enable|0x0|UINT8|0xA0000132
  gQuarkPlatformTokenSpaceGuid.PcdInterruptOverrideSettingTable8SourceIrq|0x0|UINT8|0xA0000133
  gQuarkPlatformTokenSpaceGuid.PcdInterruptOverrideSettingTable8Polarity|0x0|UINT8|0xA0000134
  gQuarkPlatformTokenSpaceGuid.PcdInterruptOverrideSettingTable8TrigerMode|0x0|UINT8|0xA0000135
  gQuarkPlatformTokenSpaceGuid.PcdInterruptOverrideSettingTable8GlobalIrq|0x0|UINT32|0xA0000136

  # Madt Table Initialize settings.
  # Defines a flag to Enable/Disable interrupt override setting table9,
  # and the source Irq, Polarity, Triger Mode and global Irq of interrupt override setting table9
  gQuarkPlatformTokenSpaceGuid.PcdInterruptOverrideSettingTable9Enable|0x0|UINT8|0xA0000137
  gQuarkPlatformTokenSpaceGuid.PcdInterruptOverrideSettingTable9SourceIrq|0x0|UINT8|0xA0000138
  gQuarkPlatformTokenSpaceGuid.PcdInterruptOverrideSettingTable9Polarity|0x0|UINT8|0xA0000139
  gQuarkPlatformTokenSpaceGuid.PcdInterruptOverrideSettingTable9TrigerMode|0x0|UINT8|0xA000013A
  gQuarkPlatformTokenSpaceGuid.PcdInterruptOverrideSettingTable9GlobalIrq|0x0|UINT32|0xA000013B

  # Madt Table Initialize settings.
  # Defines a flag to Enable/Disable interrupt override setting table10,
  # and the source Irq, Polarity, Triger Mode and global Irq of interrupt override setting table10
  gQuarkPlatformTokenSpaceGuid.PcdInterruptOverrideSettingTable10Enable|0x0|UINT8|0xA000013C
  gQuarkPlatformTokenSpaceGuid.PcdInterruptOverrideSettingTable10SourceIrq|0x0|UINT8|0xA000013D
  gQuarkPlatformTokenSpaceGuid.PcdInterruptOverrideSettingTable10Polarity|0x0|UINT8|0xA000013E
  gQuarkPlatformTokenSpaceGuid.PcdInterruptOverrideSettingTable10TrigerMode|0x0|UINT8|0xA000013F
  gQuarkPlatformTokenSpaceGuid.PcdInterruptOverrideSettingTable10GlobalIrq|0x0|UINT32|0xA0000140

  # Madt Table Initialize settings.
  # Defines a flag to Enable/Disable interrupt override setting table11,
  # and the source Irq, Polarity, Triger Mode and global Irq of interrupt override setting table11
  gQuarkPlatformTokenSpaceGuid.PcdInterruptOverrideSettingTable11Enable|0x0|UINT8|0xA0000141
  gQuarkPlatformTokenSpaceGuid.PcdInterruptOverrideSettingTable11SourceIrq|0x0|UINT8|0xA0000142
  gQuarkPlatformTokenSpaceGuid.PcdInterruptOverrideSettingTable11Polarity|0x0|UINT8|0xA0000143
  gQuarkPlatformTokenSpaceGuid.PcdInterruptOverrideSettingTable11TrigerMode|0x0|UINT8|0xA0000144
  gQuarkPlatformTokenSpaceGuid.PcdInterruptOverrideSettingTable11GlobalIrq|0x0|UINT32|0xA0000145

  # Madt Table Initialize settings.
  # Defines a flag to Enable/Disable interrupt override setting table12,
  # and the source Irq, Polarity, Triger Mode and global Irq of interrupt override setting table12
  gQuarkPlatformTokenSpaceGuid.PcdInterruptOverrideSettingTable12Enable|0x0|UINT8|0xA0000146
  gQuarkPlatformTokenSpaceGuid.PcdInterruptOverrideSettingTable12SourceIrq|0x0|UINT8|0xA0000147
  gQuarkPlatformTokenSpaceGuid.PcdInterruptOverrideSettingTable12Polarity|0x0|UINT8|0xA0000148
  gQuarkPlatformTokenSpaceGuid.PcdInterruptOverrideSettingTable12TrigerMode|0x0|UINT8|0xA0000149
  gQuarkPlatformTokenSpaceGuid.PcdInterruptOverrideSettingTable12GlobalIrq|0x0|UINT32|0xA000014A

  # Madt Table Initialize settings.
  # Defines a flag to Enable/Disable interrupt override setting table13,
  # and the source Irq, Polarity, Triger Mode and global Irq of interrupt override setting table13
  gQuarkPlatformTokenSpaceGuid.PcdInterruptOverrideSettingTable13Enable|0x0|UINT8|0xA000014B
  gQuarkPlatformTokenSpaceGuid.PcdInterruptOverrideSettingTable13SourceIrq|0x0|UINT8|0xA000014C
  gQuarkPlatformTokenSpaceGuid.PcdInterruptOverrideSettingTable13Polarity|0x0|UINT8|0xA000014D
  gQuarkPlatformTokenSpaceGuid.PcdInterruptOverrideSettingTable13TrigerMode|0x0|UINT8|0xA000014E
  gQuarkPlatformTokenSpaceGuid.PcdInterruptOverrideSettingTable13GlobalIrq|0x0|UINT32|0xA000014F

  # Madt Table Initialize settings.
  # Defines a flag to Enable/Disable interrupt override setting table14,
  # and the source Irq, Polarity, Triger Mode and global Irq of interrupt override setting table14
  gQuarkPlatformTokenSpaceGuid.PcdInterruptOverrideSettingTable14Enable|0x0|UINT8|0xA0000150
  gQuarkPlatformTokenSpaceGuid.PcdInterruptOverrideSettingTable14SourceIrq|0x0|UINT8|0xA0000151
  gQuarkPlatformTokenSpaceGuid.PcdInterruptOverrideSettingTable14Polarity|0x0|UINT8|0xA0000152
  gQuarkPlatformTokenSpaceGuid.PcdInterruptOverrideSettingTable14TrigerMode|0x0|UINT8|0xA0000153
  gQuarkPlatformTokenSpaceGuid.PcdInterruptOverrideSettingTable14GlobalIrq|0x0|UINT32|0xA0000154

  # Madt Table Initialize settings.
  # Defines a flag to Enable/Disable interrupt override setting table15,
  # and the source Irq, Polarity, Triger Mode and global Irq of interrupt override setting table15
  gQuarkPlatformTokenSpaceGuid.PcdInterruptOverrideSettingTable15Enable|0x0|UINT8|0xA0000155
  gQuarkPlatformTokenSpaceGuid.PcdInterruptOverrideSettingTable15SourceIrq|0x0|UINT8|0xA0000156
  gQuarkPlatformTokenSpaceGuid.PcdInterruptOverrideSettingTable15Polarity|0x0|UINT8|0xA0000157
  gQuarkPlatformTokenSpaceGuid.PcdInterruptOverrideSettingTable15TrigerMode|0x0|UINT8|0xA0000158
  gQuarkPlatformTokenSpaceGuid.PcdInterruptOverrideSettingTable15GlobalIrq|0x0|UINT32|0xA0000159

  # Madt Table Initialize settings.
  # Defines a bunch of Pcds for IO APIC setting:
  # IoApicAddress, GlobalInterruptBase, IoApicId, NmiEnable, NmiSource, Polarity and TrigerMode
  gQuarkPlatformTokenSpaceGuid.PcdIoApicSettingIoApicAddress|0xFEC00000|UINT32|0xA0000170
  gQuarkPlatformTokenSpaceGuid.PcdIoApicSettingGlobalInterruptBase|0x0|UINT32|0xA0000171
  gQuarkPlatformTokenSpaceGuid.PcdIoApicSettingIoApicId|0x01|UINT8|0xA0000172
  gQuarkPlatformTokenSpaceGuid.PcdIoApicSettingNmiEnable|0x0|UINT8|0xA0000173
  gQuarkPlatformTokenSpaceGuid.PcdIoApicSettingNmiSource|0x0|UINT8|0xA0000174
  gQuarkPlatformTokenSpaceGuid.PcdIoApicSettingPolarity|0x0|UINT8|0xA0000175
  gQuarkPlatformTokenSpaceGuid.PcdIoApicSettingTrigerMode|0x0|UINT8|0xA0000176

  # Madt Table Initialize settings.
  # Defines a bunch of Pcds for Local APIC setting:
  # NmiEnabelApicIdMask, AddressOverrideEnable, Polarity, TrigerMode, LocalApicLint, LocalApicAddress and LocalApicAddressOverride
  gQuarkPlatformTokenSpaceGuid.PcdLocalApicSettingNmiEnabelApicIdMask|0x03|UINT8|0xA0000177
  gQuarkPlatformTokenSpaceGuid.PcdLocalApicSettingAddressOverrideEnable|0x00|UINT8|0xA0000178
  gQuarkPlatformTokenSpaceGuid.PcdLocalApicSettingPolarity|0x01|UINT8|0xA0000179
  gQuarkPlatformTokenSpaceGuid.PcdLocalApicSettingTrigerMode|0x01|UINT8|0xA000017A
  gQuarkPlatformTokenSpaceGuid.PcdLocalApicSettingLocalApicLint|0x01|UINT8|0xA000017B
  gQuarkPlatformTokenSpaceGuid.PcdLocalApicAddressOverride|0x00|UINT64|0xA000017C

  # PCDs for auto provisioning of UEFI SecureBoot.
  gQuarkPlatformTokenSpaceGuid.PcdPkX509File |{ 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00 }|VOID*|0xA0000180
  gQuarkPlatformTokenSpaceGuid.PcdKekX509File |{ 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00 }|VOID*|0xA0000181
  gQuarkPlatformTokenSpaceGuid.PcdKekRsa2048File |{ 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00 }|VOID*|0xA0000182
  gQuarkPlatformTokenSpaceGuid.PcdDbX509File |{ 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00 }|VOID*|0xA0000183
  gQuarkPlatformTokenSpaceGuid.PcdDbxX509File |{ 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00 }|VOID*|0xA0000184

[PcdsFixedAtBuild, PcdsPatchableInModule]
  ## This PCD points to the file name GUID of the BootManagerMenuApp
  #  Platform can customize the PCD to point to different application for Boot Manager Menu
  gQuarkPlatformTokenSpaceGuid.PcdBootManagerMenuFile|{ 0xdc, 0x5b, 0xc2, 0xee, 0xf2, 0x67, 0x95, 0x4d, 0xb1, 0xd5, 0xf8, 0x1b, 0x20, 0x39, 0xd1, 0x1d }|VOID*|0x00000003

  #BIOS Information (Type 0), please refer spec SMBIOS 2.4, section 3.3.1 ,for following SMBIOS relates comments.

  # String number of the BIOS Vendors Name
  gQuarkPlatformTokenSpaceGuid.PcdSMBIOSBiosVendor|"Intel Corp."|VOID*|0xA0000033
  # String number of the BIOS Release Data
  gQuarkPlatformTokenSpaceGuid.PcdSMBIOSBiosReleaseDate|"01/01/2014"|VOID*|0xA0000035
  # Segment location of BIOS starting address.
  # Note: The size of the runtime BIOS image can be computed by subtracting the Starting Address Segment from 10000h and multiplying the result by 16.
  gQuarkPlatformTokenSpaceGuid.PcdSMBIOSBiosStartAddress|0xE000|UINT16|0xA0000036
  #Defines which functions the BIOS supports. PCI, PCMCIA, Flash, etc. See 3.3.1.1.
  gQuarkPlatformTokenSpaceGuid.PcdSMBIOSBiosChar|0x03037C099880|UINT64|0xA0000037
  #Defines which functions the BIOS supports. etc.See 3.3.1.2.1.
  gQuarkPlatformTokenSpaceGuid.PcdSMBIOSBiosCharEx1|0x03|UINT8|0xA0000038
  #Defines which functions the BIOS supports. etc.See 3.3.1.2.2.
  gQuarkPlatformTokenSpaceGuid.PcdSMBIOSBiosCharEx2|0x03|UINT8|0xA0000039

  # System Information (Type 1), Section 3.3.2
  # System Manufacturer String
  gQuarkPlatformTokenSpaceGuid.PcdSMBIOSSystemManufacturer|"Intel Corp."|VOID*|0xA000003A
  # System Product String
  gQuarkPlatformTokenSpaceGuid.PcdSMBIOSSystemProductName|"QUARK"|VOID*|0xA000003B
  # System Version
  gQuarkPlatformTokenSpaceGuid.PcdSMBIOSSystemVersion|"1.0"|VOID*|0xA000003C
  # System SerialNumber String
  gQuarkPlatformTokenSpaceGuid.PcdSMBIOSSystemSerialNumber|"Unknown"|VOID*|0xA000003D
  # System UUID
  gQuarkPlatformTokenSpaceGuid.PcdSMBIOSSystemUuid|{0x23, 0xef, 0xff, 0x13,0x54, 0x86, 0xda, 0x46, 0xa4, 0x7, 0x39, 0xc9, 0x12, 0x2, 0xd3, 0x56}|VOID*|0xA000003E
  # Manufacturer String
  gQuarkPlatformTokenSpaceGuid.PcdSMBIOSSystemSKUNumber|"System SKUNumber"|VOID*|0xA000003F
  # System Family String
  gQuarkPlatformTokenSpaceGuid.PcdSMBIOSSystemFamily|"X1000"|VOID*|0xA0000040

  # Base Board (or Module) Information (Type 2), Section 3.3.3
  # Board Manufacturer String
  gQuarkPlatformTokenSpaceGuid.PcdSMBIOSBoardManufacturer|"Intel Corp."|VOID*|0xA0000041
  # Board Product Name| String
  gQuarkPlatformTokenSpaceGuid.PcdSMBIOSBoardProductName|"QUARK"|VOID*|0xA0000042
  # Board Version String
  gQuarkPlatformTokenSpaceGuid.PcdSMBIOSBoardVersion|"FAB-D"|VOID*|0xA0000043
  # Board Serial Number
  gQuarkPlatformTokenSpaceGuid.PcdSMBIOSBoardSerialNumber|"3"|VOID*|0xA0000044
  # System Enclosure or Chassis(Type 3) Section 3.3.4
  # Chassis Manufacturer String
  gQuarkPlatformTokenSpaceGuid.PcdSMBIOSChassisManufacturer|"Chassis Manufacturer"|VOID*|0xA0000045
  # ChassisVersion
  gQuarkPlatformTokenSpaceGuid.PcdSMBIOSChassisVersion|"Chassis Version"|VOID*|0xA0000046
  # Chassis SerialNumber String
  gQuarkPlatformTokenSpaceGuid.PcdSMBIOSChassisSerialNumber|"Chassis Serial Number"|VOID*|0xA0000047
  # Chassis Asset Tag
  gQuarkPlatformTokenSpaceGuid.PcdSMBIOSChassisAssetTag|"Chassis Asset Tag"|VOID*|0xA0000051
  # Chassis Type
  gQuarkPlatformTokenSpaceGuid.PcdSMBIOSChassisType|0x00000003|UINT8|0xA0000048
  # Identifies the state of the enclosure when it was last booted. See 3.3.4.2 for definitions.
  gQuarkPlatformTokenSpaceGuid.PcdSMBIOSChassisBootupState|0x03|UINT8|0xA0000049
  # Identifies the state of the enclosures power supply (or supplies) when last booted. See 3.3.4.2 for definitions.
  gQuarkPlatformTokenSpaceGuid.PcdSMBIOSChassisPowerSupplyState|0x03|UINT8|0xA000004A
  # Identifies the enclosures physical security status when last booted. See 3.3.4.3 for definitions.
  gQuarkPlatformTokenSpaceGuid.PcdSMBIOSChassisSecurityState|0x01|UINT8|0xA000004B
  # Contains OEM- or BIOS vendor-specific information.
  gQuarkPlatformTokenSpaceGuid.PcdSMBIOSChassisOemDefined|0x0|UINT32|0xA000004C
  # The height of the enclosure, in 'U's. A U is a standard unit of measure for the height of a rack or rack-mountable component
  # and is equal to 1.75 inches or 4.445 cm. A value of 00h indicates that the enclosure height is unspecified.
  gQuarkPlatformTokenSpaceGuid.PcdSMBIOSChassisHeight|0x0|UINT8|0xA000004D
  # Identifies the number of power cords associated with the enclosure or chassis. A value of 00h indicates that the number is unspecified.
  gQuarkPlatformTokenSpaceGuid.PcdSMBIOSChassisNumberPowerCords|0x0|UINT8|0xA000004E
  # Identifies the number of Contained Element records that follow, in the range 0 to 255.
  # Each Contained Element group comprises m bytes, as specified by the Contained Element Record Length field that follows.
  # If no Contained Elements are included, this field is set to 0.
  gQuarkPlatformTokenSpaceGuid.PcdSMBIOSChassisElementCount|0x0|UINT8|0xA000004F
  # Identifies the byte length of each Contained Element record that follow, in the range 0 to 255.
  # If no Contained Elements are included, this field is set to 0. For v2.3.2 and later of this specification,
  # this field is set to at least 03h when Contained Elements are specified.
  gQuarkPlatformTokenSpaceGuid.PcdSMBIOSChassisElementRecordLength|0x0|UINT8|0xA0000050

  # Defines the number of connectors existent on the board
  # The valid range is between 0 and 16
  gQuarkPlatformTokenSpaceGuid.PcdSMBIOSConnectorNumber|16|UINT8|0xA0000060

  # Defines the designator of port1 internal connector
  gQuarkPlatformTokenSpaceGuid.PcdSMBIOSPort1InternalConnectorDesignator|"X14 "|VOID*|0xA0000061
  # Defines the designator of port1 external connector
  gQuarkPlatformTokenSpaceGuid.PcdSMBIOSPort1ExternalConnectorDesignator|"Keyboard"|VOID*|0xA0000062
  # Defines the type of port1 internal connector
  # The valid range is between 0 to 0xFF, and 0 here means EfiPortConnectorTypeNone
  gQuarkPlatformTokenSpaceGuid.PcdSMBIOSPort1InternalConnectorType|0x0F|UINT8|0xA0000063
  # Defines the type of port1 external connector
  # The valid range is between 0 to 0xFF, and 0x0F here means EfiPortConnectorTypePS2
  gQuarkPlatformTokenSpaceGuid.PcdSMBIOSPort1ExternalConnectorType|0x0F|UINT8|0xA0000064
  # Defines the type of port1
  # The valid range is between 0 to 0xFF, and 0x0D here means EfiPortTypeKeyboard
  gQuarkPlatformTokenSpaceGuid.PcdSMBIOSPort1Type|0x0D|UINT8|0xA0000065

  # Defines the designator of port2 internal connector
  gQuarkPlatformTokenSpaceGuid.PcdSMBIOSPort2InternalConnectorDesignator|"X15 "|VOID*|0xA0000066
  # Defines the designator of port2 external connector
  gQuarkPlatformTokenSpaceGuid.PcdSMBIOSPort2ExternalConnectorDesignator|"Mouse"|VOID*|0xA0000067
  # Defines the type of port2 internal connector
  # The valid range is between 0 to 0xFF, and 0 here means EfiPortConnectorTypeNone
  gQuarkPlatformTokenSpaceGuid.PcdSMBIOSPort2InternalConnectorType|0x0F|UINT8|0xA0000068
  # Defines the type of port2 external connector
  # The valid range is between 0 to 0xFF, and 0x0F here means EfiPortConnectorTypePS2
  gQuarkPlatformTokenSpaceGuid.PcdSMBIOSPort2ExternalConnectorType|0x0F|UINT8|0xA0000069
  # Defines the type of port2
  # The valid range is between 0 to 0xFF, and 0x0E here means EfiPortTypeMouse
  gQuarkPlatformTokenSpaceGuid.PcdSMBIOSPort2Type|0x0E|UINT8|0xA000006A

  # Defines the designator of port3 internal connector
  gQuarkPlatformTokenSpaceGuid.PcdSMBIOSPort3InternalConnectorDesignator|"X16 "|VOID*|0xA000006B
  # Defines the designator of port3 external connector
  gQuarkPlatformTokenSpaceGuid.PcdSMBIOSPort3ExternalConnectorDesignator|"COM 1"|VOID*|0xA000006C
  # Defines the type of port3 internal connector
  # The valid range is between 0 to 0xFF, and 0xFF here means EfiPortConnectorTypeOther
  gQuarkPlatformTokenSpaceGuid.PcdSMBIOSPort3InternalConnectorType|0xFF|UINT8|0xA000006D
  # Defines the type of port3 external connector
  # The valid range is between 0 to 0xFF, and 0 here means EfiPortConnectorTypeNone
  gQuarkPlatformTokenSpaceGuid.PcdSMBIOSPort3ExternalConnectorType|0x0|UINT8|0xA000006E
  # Defines the type of port3
  # The valid range is between 0 to 0xFF, and 0x09 here means EfiPortTypeSerial16550ACompatible
  gQuarkPlatformTokenSpaceGuid.PcdSMBIOSPort3Type|0x09|UINT8|0xA000006F

  # Defines the designator of port4 internal connector
  gQuarkPlatformTokenSpaceGuid.PcdSMBIOSPort4InternalConnectorDesignator|"X17 "|VOID*|0xA0000070
  # Defines the designator of port4 external connector
  gQuarkPlatformTokenSpaceGuid.PcdSMBIOSPort4ExternalConnectorDesignator|"COM 2"|VOID*|0xA0000071
  # Defines the type of port4 internal connector
  # The valid range is between 0 to 0xFF, and 0xFF here means EfiPortConnectorTypeOther
  gQuarkPlatformTokenSpaceGuid.PcdSMBIOSPort4InternalConnectorType|0xFF|UINT8|0xA0000072
  # Defines the type of port4 external connector
  # The valid range is between 0 to 0xFF, and 0 here means EfiPortConnectorTypeNone
  gQuarkPlatformTokenSpaceGuid.PcdSMBIOSPort4ExternalConnectorType|0x0|UINT8|0xA0000073
  # Defines the type of port4
  # The valid range is between 0 to 0xFF, and 0x09 here means EfiPortTypeSerial16550ACompatible
  gQuarkPlatformTokenSpaceGuid.PcdSMBIOSPort4Type|0x09|UINT8|0xA0000074

  # Defines the designator of port5 internal connector
  gQuarkPlatformTokenSpaceGuid.PcdSMBIOSPort5InternalConnectorDesignator|"X18 "|VOID*|0xA0000075
  # Defines the designator of port5 external connector
  gQuarkPlatformTokenSpaceGuid.PcdSMBIOSPort5ExternalConnectorDesignator|"COM 3"|VOID*|0xA0000076
  # Defines the type of port5 internal connector
  # The valid range is between 0 to 0xFF, and 0xFF here means EfiPortConnectorTypeOther
  gQuarkPlatformTokenSpaceGuid.PcdSMBIOSPort5InternalConnectorType|0xFF|UINT8|0xA0000077
  # Defines the type of port5 external connector
  # The valid range is between 0 to 0xFF, and 0 here means EfiPortConnectorTypeNone
  gQuarkPlatformTokenSpaceGuid.PcdSMBIOSPort5ExternalConnectorType|0x0|UINT8|0xA0000078
  # Defines the type of port5
  # The valid range is between 0 to 0xFF, and 0x09 here means EfiPortTypeSerial16550ACompatible
  gQuarkPlatformTokenSpaceGuid.PcdSMBIOSPort5Type|0x09|UINT8|0xA0000079

  # Defines the designator of port6 internal connector
  gQuarkPlatformTokenSpaceGuid.PcdSMBIOSPort6InternalConnectorDesignator|"X19 "|VOID*|0xA000007A
  # Defines the designator of port6 external connector
  gQuarkPlatformTokenSpaceGuid.PcdSMBIOSPort6ExternalConnectorDesignator|"COM 4"|VOID*|0xA000007B
  # Defines the type of port6 internal connector
  # The valid range is between 0 to 0xFF, and 0xFF here means EfiPortConnectorTypeOther
  gQuarkPlatformTokenSpaceGuid.PcdSMBIOSPort6InternalConnectorType|0xFF|UINT8|0xA000007C
  # Defines the type of port6 external connector
  # The valid range is between 0 to 0xFF, and 0 here means EfiPortConnectorTypeNone
  gQuarkPlatformTokenSpaceGuid.PcdSMBIOSPort6ExternalConnectorType|0x0|UINT8|0xA000007D
  # Defines the type of port6
  # The valid range is between 0 to 0xFF, and 0x09 here means EfiPortTypeSerial16550ACompatible
  gQuarkPlatformTokenSpaceGuid.PcdSMBIOSPort6Type|0x09|UINT8|0xA000007E

  # Defines the designator of port7 internal connector
  gQuarkPlatformTokenSpaceGuid.PcdSMBIOSPort7InternalConnectorDesignator|"J4A2"|VOID*|0xA000007F
  # Defines the designator of port7 external connector
  gQuarkPlatformTokenSpaceGuid.PcdSMBIOSPort7ExternalConnectorDesignator|"LPT 1"|VOID*|0xA0000080
  # Defines the type of port7 internal connector
  # The valid range is between 0 to 0xFF, and 0 here means EfiPortConnectorTypeNone
  gQuarkPlatformTokenSpaceGuid.PcdSMBIOSPort7InternalConnectorType|0x0|UINT8|0xA0000081
  # Defines the type of port7 external connector
  # The valid range is between 0 to 0xFF, and 0x12 here means EfiPortConnectorTypeDB25Male
  gQuarkPlatformTokenSpaceGuid.PcdSMBIOSPort7ExternalConnectorType|0x04|UINT8|0xA0000082
  # Defines the type of port7
  # The valid range is between 0 to 0xFF, and 0x10 here means EfiPortTypeEcpEpp
  gQuarkPlatformTokenSpaceGuid.PcdSMBIOSPort7Type|0x05|UINT8|0xA0000083

  # Defines the designator of port8 internal connector
  gQuarkPlatformTokenSpaceGuid.PcdSMBIOSPort8InternalConnectorDesignator|"X20 "|VOID*|0xA0000084
  # Defines the designator of port8 external connector
  gQuarkPlatformTokenSpaceGuid.PcdSMBIOSPort8ExternalConnectorDesignator|"USB1"|VOID*|0xA0000085
  # Defines the type of port8 internal connector
  # The valid range is between 0 to 0xFF, and 0 here means EfiPortConnectorTypeNone
  gQuarkPlatformTokenSpaceGuid.PcdSMBIOSPort8InternalConnectorType|0x0|UINT8|0xA0000086
  # Defines the type of port8 external connector
  # The valid range is between 0 to 0xFF, and 0x12 here means EfiPortConnectorTypeUsb
  gQuarkPlatformTokenSpaceGuid.PcdSMBIOSPort8ExternalConnectorType|0x12|UINT8|0xA0000087
  # Defines the type of port8
  # The valid range is between 0 to 0xFF, and 0x10 here means EfiPortTypeUsb
  gQuarkPlatformTokenSpaceGuid.PcdSMBIOSPort8Type|0x10|UINT8|0xA0000088

  # Defines the designator of port9 internal connector
  gQuarkPlatformTokenSpaceGuid.PcdSMBIOSPort9InternalConnectorDesignator|"X21 "|VOID*|0xA0000089
  # Defines the designator of port9 external connector
  gQuarkPlatformTokenSpaceGuid.PcdSMBIOSPort9ExternalConnectorDesignator|"USB2"|VOID*|0xA000008A
  # Defines the type of port9 internal connector
  # The valid range is between 0 to 0xFF, and 0 here means EfiPortConnectorTypeNone
  gQuarkPlatformTokenSpaceGuid.PcdSMBIOSPort9InternalConnectorType|0x0|UINT8|0xA000008B
  # Defines the type of port9 external connector
  # The valid range is between 0 to 0xFF, and 0x12 here means EfiPortConnectorTypeUsb
  gQuarkPlatformTokenSpaceGuid.PcdSMBIOSPort9ExternalConnectorType|0x12|UINT8|0xA000008C
  # Defines the type of port9
  # The valid range is between 0 to 0xFF, and 0x10 here means EfiPortTypeUsb
  gQuarkPlatformTokenSpaceGuid.PcdSMBIOSPort9Type|0x10|UINT8|0xA000008D

  # Defines the designator of port10 internal connector
  gQuarkPlatformTokenSpaceGuid.PcdSMBIOSPort10InternalConnectorDesignator|"X22 "|VOID*|0xA000008E
  # Defines the designator of port10 external connector
  gQuarkPlatformTokenSpaceGuid.PcdSMBIOSPort10ExternalConnectorDesignator|"USB3"|VOID*|0xA000008F
  # Defines the type of port10 internal connector
  # The valid range is between 0 to 0xFF, and 0 here means EfiPortConnectorTypeNone
  gQuarkPlatformTokenSpaceGuid.PcdSMBIOSPort10InternalConnectorType|0x0|UINT8|0xA0000090
  # Defines the type of port10 external connector
  # The valid range is between 0 to 0xFF, and 0x12 here means EfiPortConnectorTypeUsb
  gQuarkPlatformTokenSpaceGuid.PcdSMBIOSPort10ExternalConnectorType|0x12|UINT8|0xA0000091
  # Defines the type of port10
  # The valid range is between 0 to 0xFF, and 0x10 here means EfiPortTypeUsb
  gQuarkPlatformTokenSpaceGuid.PcdSMBIOSPort10Type|0x10|UINT8|0xA0000092

  # Defines the designator of port11 internal connector
  gQuarkPlatformTokenSpaceGuid.PcdSMBIOSPort11InternalConnectorDesignator|"X23 "|VOID*|0xA0000093
  # Defines the designator of port11 external connector
  gQuarkPlatformTokenSpaceGuid.PcdSMBIOSPort11ExternalConnectorDesignator|"USB4"|VOID*|0xA0000094
  # Defines the type of port11 internal connector
  # The valid range is between 0 to 0xFF, and 0 here means EfiPortConnectorTypeNone
  gQuarkPlatformTokenSpaceGuid.PcdSMBIOSPort11InternalConnectorType|0x0|UINT8|0xA0000095
  # Defines the type of port11 external connector
  # The valid range is between 0 to 0xFF, and 0x12 here means EfiPortConnectorTypeUsb
  gQuarkPlatformTokenSpaceGuid.PcdSMBIOSPort11ExternalConnectorType|0x12|UINT8|0xA0000096
  # Defines the type of port11
  # The valid range is between 0 to 0xFF, and 0x10 here means EfiPortTypeUsb
  gQuarkPlatformTokenSpaceGuid.PcdSMBIOSPort11Type|0x10|UINT8|0xA0000097

  # Defines the designator of port12 internal connector
  gQuarkPlatformTokenSpaceGuid.PcdSMBIOSPort12InternalConnectorDesignator|"X28 "|VOID*|0xA0000098
  # Defines the designator of port12 external connector
  gQuarkPlatformTokenSpaceGuid.PcdSMBIOSPort12ExternalConnectorDesignator|"RJ-45 Type"|VOID*|0xA0000099
  # Defines the type of port12 internal connector
  # The valid range is between 0 to 0xFF, and 0 here means EfiPortConnectorTypeNone
  gQuarkPlatformTokenSpaceGuid.PcdSMBIOSPort12InternalConnectorType|0x0|UINT8|0xA000009A
  # Defines the type of port12 external connector
  # The valid range is between 0 to 0xFF, and 0x0B here means EfiPortConnectorTypeRJ45
  gQuarkPlatformTokenSpaceGuid.PcdSMBIOSPort12ExternalConnectorType|0x0B|UINT8|0xA000009B
  # Defines the type of port12
  # The valid range is between 0 to 0xFF, and 0x1F here means EfiPortTypeNetworkPort
  gQuarkPlatformTokenSpaceGuid.PcdSMBIOSPort12Type|0x1F|UINT8|0xA000009C

  # Defines the designator of port13 internal connector
  gQuarkPlatformTokenSpaceGuid.PcdSMBIOSPort13InternalConnectorDesignator|"J1G1"|VOID*|0xA000009D
  # Defines the designator of port13 external connector
  gQuarkPlatformTokenSpaceGuid.PcdSMBIOSPort13ExternalConnectorDesignator|"Floppy"|VOID*|0xA000009E
  # Defines the type of port13 internal connector
  # The valid range is between 0 to 0xFF, and 0x16 here means EfiPortConnectorTypeOnboardFloppy
  gQuarkPlatformTokenSpaceGuid.PcdSMBIOSPort13InternalConnectorType|0x17|UINT8|0xA000009F
  # Defines the type of port13 external connector
  # The valid range is between 0 to 0xFF, and 0 here means EfiPortConnectorTypeNone
  gQuarkPlatformTokenSpaceGuid.PcdSMBIOSPort13ExternalConnectorType|0x0|UINT8|0xA00000A0
  # Defines the type of port13
  # The valid range is between 0 to 0xFF, and 0xFF here means EfiPortTypeOther
  gQuarkPlatformTokenSpaceGuid.PcdSMBIOSPort13Type|0xFF|UINT8|0xA00000A1

  # Defines the designator of port14 internal connector
  gQuarkPlatformTokenSpaceGuid.PcdSMBIOSPort14InternalConnectorDesignator|"J2H2"|VOID*|0xA00000A2
  # Defines the designator of port14 external connector
  gQuarkPlatformTokenSpaceGuid.PcdSMBIOSPort14ExternalConnectorDesignator|"IDE"|VOID*|0xA00000A3
  # Defines the type of port14 internal connector
  # The valid range is between 0 to 0xFF, and 0x16 here means EfiPortConnectorTypeOnboardIde
  gQuarkPlatformTokenSpaceGuid.PcdSMBIOSPort14InternalConnectorType|0x16|UINT8|0xA00000A4
  # Defines the type of port14 external connector
  # The valid range is between 0 to 0xFF, and 0 here means EfiPortConnectorTypeNone
  gQuarkPlatformTokenSpaceGuid.PcdSMBIOSPort14ExternalConnectorType|0x0|UINT8|0xA00000A5
  # Defines the type of port14
  # The valid range is between 0 to 0xFF, and 0xFF here means EfiPortTypeOther
  gQuarkPlatformTokenSpaceGuid.PcdSMBIOSPort14Type|0xFF|UINT8|0xA00000A6

  # Defines the designator of port15 internal connector
  gQuarkPlatformTokenSpaceGuid.PcdSMBIOSPort15InternalConnectorDesignator|"X29 "|VOID*|0xA00000A7
  # Defines the designator of port15 external connector

  # Defines the type of port15 internal connector
  # The valid range is between 0 to 0xFF, and 0x16 here means EfiPortConnectorTypeOnboardIde
  gQuarkPlatformTokenSpaceGuid.PcdSMBIOSPort15InternalConnectorType|0x16|UINT8|0xA00000A9
  # Defines the type of port15 external connector
  # The valid range is between 0 to 0xFF, and 0 here means EfiPortConnectorTypeNone
  gQuarkPlatformTokenSpaceGuid.PcdSMBIOSPort15ExternalConnectorType|0x0|UINT8|0xA00000AA
  # Defines the type of port15
  # The valid range is between 0 to 0xFF, and 0xFF here means EfiPortTypeOther
  gQuarkPlatformTokenSpaceGuid.PcdSMBIOSPort15Type|0xFF|UINT8|0xA00000AB

  # Defines the designator of port16 internal connector
  gQuarkPlatformTokenSpaceGuid.PcdSMBIOSPort16InternalConnectorDesignator|"X30 "|VOID*|0xA00000AC
  # Defines the designator of port16 external connector

  # Defines the type of port16 internal connector
  # The valid range is between 0 to 0xFF, and 0x16 here means EfiPortConnectorTypeOnboardIde
  gQuarkPlatformTokenSpaceGuid.PcdSMBIOSPort16InternalConnectorType|0x16|UINT8|0xA00000AE
  # Defines the type of port16 external connector
  # The valid range is between 0 to 0xFF, and 0 here means EfiPortConnectorTypeNone
  gQuarkPlatformTokenSpaceGuid.PcdSMBIOSPort16ExternalConnectorType|0x0|UINT8|0xA00000AF
  # Defines the type of port16
  # The valid range is between 0 to 0xFF, and 0xFF here means EfiPortTypeOther
  gQuarkPlatformTokenSpaceGuid.PcdSMBIOSPort16Type|0xFF|UINT8|0xA00000B0

  # Defines the number of the slots existent on board
  # The valid range is between 0 and 14
  gQuarkPlatformTokenSpaceGuid.PcdSMBIOSSystemSlotNumber|5|UINT8|0xA000023F
  # Defines the designation of system slot1
  gQuarkPlatformTokenSpaceGuid.PcdSMBIOSSystemSlot1Designation|"PCI SLOT1"|VOID*|0xA0000240
  # Defines the type of system slot1
  # The valid range is between 0x01 to 0xA5, and 0x06 here means EfiSlotTypePci
  gQuarkPlatformTokenSpaceGuid.PcdSMBIOSSystemSlot1Type|0x6|UINT8|0xA0000241
  # Defines the data bus width of system slot1
  # The valid range is between 0x01 to 0x07, and 0x05 here means EfiSlotDataBusWidth32Bit
  gQuarkPlatformTokenSpaceGuid.PcdSMBIOSSystemSlot1DataBusWidth|0x5|UINT8|0xA0000242
  # Defines the usage of system slot1
  # The valid range is between 0x01 to 0x04, and 0x03 here means EfiSlotUsageAvailable
  gQuarkPlatformTokenSpaceGuid.PcdSMBIOSSystemSlot1Usage|0x3|UINT8|0xA0000243
  # Defines the length of system slot1
  # The valid range is between 0x01 to 0x04, and 0x04 here means EfiSlotLengthLong
  gQuarkPlatformTokenSpaceGuid.PcdSMBIOSSystemSlot1Length|0x4|UINT8|0xA0000244
  # Defines the ID of system slot1, a number of UINT16
  gQuarkPlatformTokenSpaceGuid.PcdSMBIOSSystemSlot1Id|0x01|UINT16|0xA0000245
  # Defines the characteristics of system slot1 , a bit mask of EFI_MISC_SLOT_CHARACTERISTICS
  # typedef struct {
  #   UINT32  CharacteristicsUnknown  :1;
  #   UINT32  Provides50Volts         :1;
  #   UINT32  Provides33Volts         :1;
  #   UINT32  SharedSlot              :1;
  #   UINT32  PcCard16Supported       :1;
  #   UINT32  CardBusSupported        :1;
  #   UINT32  ZoomVideoSupported      :1;
  #   UINT32  ModemRingResumeSupported:1;
  #   UINT32  PmeSignalSupported      :1;
  #   UINT32  HotPlugDevicesSupported :1;
  #   UINT32  SmbusSignalSupported    :1;
  #   UINT32  Reserved                :21;
  # } EFI_MISC_SLOT_CHARACTERISTICS;
  gQuarkPlatformTokenSpaceGuid.PcdSMBIOSSystemSlot1Characteristics|0x504|UINT32|0xA0000246

  # Defines the designation of system slot2
  gQuarkPlatformTokenSpaceGuid.PcdSMBIOSSystemSlot2Designation|"PCI-Express 1"|VOID*|0xA0000247

  # Defines the type of system slot2
  # The valid range is between 0x01 to 0xA5, and 0x06 here means EfiSlotTypePci
  gQuarkPlatformTokenSpaceGuid.PcdSMBIOSSystemSlot2Type|0xA5|UINT8|0xA0000248
  # Defines the data bus width of system slot2
  # The valid range is between 0x01 to 0x07, and 0x05 here means EfiSlotDataBusWidth32Bit
  gQuarkPlatformTokenSpaceGuid.PcdSMBIOSSystemSlot2DataBusWidth|0x5|UINT8|0xA0000249
  # Defines the usage of system slot2
  # The valid range is between 0x01 to 0x04, and 0x03 here means EfiSlotUsageAvailable
  gQuarkPlatformTokenSpaceGuid.PcdSMBIOSSystemSlot2Usage|0x3|UINT8|0xA000024A
  # Defines the length of system slot2
  # The valid range is between 0x01 to 0x04, and 0x04 here means EfiSlotLengthLong
  gQuarkPlatformTokenSpaceGuid.PcdSMBIOSSystemSlot2Length|0x4|UINT8|0xA000024B
  # Defines the ID of system slot2, a number of UINT16
  gQuarkPlatformTokenSpaceGuid.PcdSMBIOSSystemSlot2Id|0x02|UINT16|0xA000024C
  # Defines the characteristics of system slot2 , a bit mask of EFI_MISC_SLOT_CHARACTERISTICS
  gQuarkPlatformTokenSpaceGuid.PcdSMBIOSSystemSlot2Characteristics|0x504|UINT32|0xA000024D

  # Defines the designation of system slot3
  gQuarkPlatformTokenSpaceGuid.PcdSMBIOSSystemSlot3Designation|"PCI-Express 2"|VOID*|0xA000024E
  # Defines the type of system slot3
  # The valid range is between 0x01 to 0xA5, and 0x06 here means EfiSlotTypePci
  gQuarkPlatformTokenSpaceGuid.PcdSMBIOSSystemSlot3Type|0xA5|UINT8|0xA000024F
  # Defines the data bus width of system slot3
  # The valid range is between 0x01 to 0x07, and 0x05 here means EfiSlotDataBusWidth32Bit
  gQuarkPlatformTokenSpaceGuid.PcdSMBIOSSystemSlot3DataBusWidth|0x5|UINT8|0xA0000250
  # Defines the usage of system slot3
  # The valid range is between 0x01 to 0x04, and 0x03 here means EfiSlotUsageAvailable
  gQuarkPlatformTokenSpaceGuid.PcdSMBIOSSystemSlot3Usage|0x3|UINT8|0xA0000251
  # Defines the length of system slot3
  # The valid range is between 0x01 to 0x04, and 0x04 here means EfiSlotLengthLong
  gQuarkPlatformTokenSpaceGuid.PcdSMBIOSSystemSlot3Length|0x4|UINT8|0xA0000252
  # Defines the ID of system slot3, a number of UINT16
  gQuarkPlatformTokenSpaceGuid.PcdSMBIOSSystemSlot3Id|0x03|UINT16|0xA0000253
  # Defines the characteristics of system slot3 , a bit mask of EFI_MISC_SLOT_CHARACTERISTICS
  gQuarkPlatformTokenSpaceGuid.PcdSMBIOSSystemSlot3Characteristics|0x504|UINT32|0xA000254

  # Defines the designation of system slot4
  gQuarkPlatformTokenSpaceGuid.PcdSMBIOSSystemSlot4Designation|"PCI-Express 3"|VOID*|0xA0000255
  # Defines the type of system slot4
  # The valid range is between 0x01 to 0xA5, and 0xA5 here means EfiSlotTypePciExpress
  gQuarkPlatformTokenSpaceGuid.PcdSMBIOSSystemSlot4Type|0xA5|UINT8|0xA0000256
  # Defines the data bus width of system slot4
  # The valid range is between 0x01 to 0x07, and 0x05 here means EfiSlotDataBusWidth32Bit
  gQuarkPlatformTokenSpaceGuid.PcdSMBIOSSystemSlot4DataBusWidth|0x5|UINT8|0xA0000257
  # Defines the usage of system slot4
  # The valid range is between 0x01 to 0x04, and 0x03 here means EfiSlotUsageAvailable
  gQuarkPlatformTokenSpaceGuid.PcdSMBIOSSystemSlot4Usage|0x3|UINT8|0xA0000258
  # Defines the length of system slot4
  # The valid range is between 0x01 to 0x04, and 0x04 here means EfiSlotLengthLong
  gQuarkPlatformTokenSpaceGuid.PcdSMBIOSSystemSlot4Length|0x4|UINT8|0xA0000259
  # Defines the ID of system slot4, a number of UINT16
  gQuarkPlatformTokenSpaceGuid.PcdSMBIOSSystemSlot4Id|0x04|UINT16|0xA0000260
  # Defines the characteristics of system slot4 , a bit mask of EFI_MISC_SLOT_CHARACTERISTICS
  gQuarkPlatformTokenSpaceGuid.PcdSMBIOSSystemSlot4Characteristics|0x504|UINT32|0xA0000261

  # Defines the designation of system slot5
  gQuarkPlatformTokenSpaceGuid.PcdSMBIOSSystemSlot5Designation|"Mini PCI-E"|VOID*|0xA0000262
  # Defines the type of system slot5
  # The valid range is between 0x01 to 0xA5, and 0xA5 here means EfiSlotTypePciExpress
  gQuarkPlatformTokenSpaceGuid.PcdSMBIOSSystemSlot5Type|0xA5|UINT8|0xA0000263
  # Defines the data bus width of system slot5
  # The valid range is between 0x01 to 0x07, and 0x05 here means EfiSlotDataBusWidth32Bit
  gQuarkPlatformTokenSpaceGuid.PcdSMBIOSSystemSlot5DataBusWidth|0x5|UINT8|0xA0000264
  # Defines the usage of system slot5
  # The valid range is between 0x01 to 0x04, and 0x03 here means EfiSlotUsageAvailable
  gQuarkPlatformTokenSpaceGuid.PcdSMBIOSSystemSlot5Usage|0x3|UINT8|0xA0000265
  # Defines the length of system slot5
  # The valid range is between 0x01 to 0x04, and 0x04 here means EfiSlotLengthLong
  gQuarkPlatformTokenSpaceGuid.PcdSMBIOSSystemSlot5Length|0x4|UINT8|0xA0000266
  # Defines the ID of system slot5, a number of UINT16
  gQuarkPlatformTokenSpaceGuid.PcdSMBIOSSystemSlot5Id|0x05|UINT16|0xA0000267
  # Defines the characteristics of system slot5 , a bit mask of EFI_MISC_SLOT_CHARACTERISTICS
  gQuarkPlatformTokenSpaceGuid.PcdSMBIOSSystemSlot5Characteristics|0x504|UINT32|0xA0000268

  # Defines the designation of system slot6
  gQuarkPlatformTokenSpaceGuid.PcdSMBIOSSystemSlot6Designation|"NONE"|VOID*|0xA0000269
  # Defines the type of system slot6
  # The valid range is between 0x01 to 0xA5, and 0x02 here means EfiSlotTypeUnknown
  gQuarkPlatformTokenSpaceGuid.PcdSMBIOSSystemSlot6Type|0x2|UINT8|0xA000026A
  # Defines the data bus width of system slot6
  # The valid range is between 0x01 to 0x07, and 0x02 here means EfiSlotDataBusWidthUnknown
  gQuarkPlatformTokenSpaceGuid.PcdSMBIOSSystemSlot6DataBusWidth|0x2|UINT8|0xA000026B
  # Defines the usage of system slot6
  # The valid range is between 0x01 to 0x04, and 0x02 here means EfiSlotUsageUnknown
  gQuarkPlatformTokenSpaceGuid.PcdSMBIOSSystemSlot6Usage|0x2|UINT8|0xA000026C
  # Defines the length of system slot6
  # The valid range is between 0x01 to 0x04, and 0x02 here means EfiSlotLengthUnknown
  gQuarkPlatformTokenSpaceGuid.PcdSMBIOSSystemSlot6Length|0x2|UINT8|0xA000026D
  # Defines the ID of system slot6, a number of UINT16
  gQuarkPlatformTokenSpaceGuid.PcdSMBIOSSystemSlot6Id|0x0|UINT16|0xA000026E
  # Defines the characteristics of system slot6 , a bit mask of EFI_MISC_SLOT_CHARACTERISTICS
  gQuarkPlatformTokenSpaceGuid.PcdSMBIOSSystemSlot6Characteristics|0x0|UINT32|0xA000026F

  # Defines the designation of system slot7
  gQuarkPlatformTokenSpaceGuid.PcdSMBIOSSystemSlot7Designation|"NONE"|VOID*|0xA0000270
  # Defines the type of system slot7
  # The valid range is between 0x01 to 0xA5, and 0x02 here means EfiSlotTypeUnknown
  gQuarkPlatformTokenSpaceGuid.PcdSMBIOSSystemSlot7Type|0x2|UINT8|0xA0000271
  # Defines the data bus width of system slot7
  # The valid range is between 0x01 to 0x07, and 0x02 here means EfiSlotDataBusWidthUnknown
  gQuarkPlatformTokenSpaceGuid.PcdSMBIOSSystemSlot7DataBusWidth|0x2|UINT8|0xA0000272
  # Defines the usage of system slot7
  # The valid range is between 0x01 to 0x04, and 0x02 here means EfiSlotUsageUnknown
  gQuarkPlatformTokenSpaceGuid.PcdSMBIOSSystemSlot7Usage|0x2|UINT8|0xA0000273
  # Defines the length of system slot7
  # The valid range is between 0x01 to 0x04, and 0x02 here means EfiSlotLengthUnknown
  gQuarkPlatformTokenSpaceGuid.PcdSMBIOSSystemSlot7Length|0x2|UINT8|0xA0000274
  # Defines the ID of system slot7, a number of UINT16
  gQuarkPlatformTokenSpaceGuid.PcdSMBIOSSystemSlot7Id|0x0|UINT16|0xA0000275
  # Defines the characteristics of system slot7 , a bit mask of EFI_MISC_SLOT_CHARACTERISTICS
  gQuarkPlatformTokenSpaceGuid.PcdSMBIOSSystemSlot7Characteristics|0x0|UINT32|0xA0000276

  # Defines the designation of system slot8
  gQuarkPlatformTokenSpaceGuid.PcdSMBIOSSystemSlot8Designation|"NONE"|VOID*|0xA0000277
  # Defines the type of system slot8
  # The valid range is between 0x01 to 0xA5, and 0x02 here means EfiSlotTypeUnknown
  gQuarkPlatformTokenSpaceGuid.PcdSMBIOSSystemSlot8Type|0x2|UINT8|0xA0000278
  # Defines the data bus width of system slot8
  # The valid range is between 0x01 to 0x07, and 0x02 here means EfiSlotDataBusWidthUnknown
  gQuarkPlatformTokenSpaceGuid.PcdSMBIOSSystemSlot8DataBusWidth|0x2|UINT8|0xA0000279
  # Defines the usage of system slot8
  # The valid range is between 0x01 to 0x04, and 0x02 here means EfiSlotUsageUnknown
  gQuarkPlatformTokenSpaceGuid.PcdSMBIOSSystemSlot8Usage|0x2|UINT8|0xA000027A
  # Defines the length of system slot8
  # The valid range is between 0x01 to 0x04, and 0x02 here means EfiSlotLengthUnknown
  gQuarkPlatformTokenSpaceGuid.PcdSMBIOSSystemSlot8Length|0x2|UINT8|0xA000027B
  # Defines the ID of system slot8, a number of UINT16
  gQuarkPlatformTokenSpaceGuid.PcdSMBIOSSystemSlot8Id|0x0|UINT16|0xA000027C
  # Defines the characteristics of system slot8 , a bit mask of EFI_MISC_SLOT_CHARACTERISTICS
  gQuarkPlatformTokenSpaceGuid.PcdSMBIOSSystemSlot8Characteristics|0x0|UINT32|0xA000027D

  # Defines the designation of system slot9
  gQuarkPlatformTokenSpaceGuid.PcdSMBIOSSystemSlot9Designation|"NONE"|VOID*|0xA000027E
  # Defines the type of system slot9
  # The valid range is between 0x01 to 0xA5, and 0x02 here means EfiSlotTypeUnknown
  gQuarkPlatformTokenSpaceGuid.PcdSMBIOSSystemSlot9Type|0x2|UINT8|0xA000027F
  # Defines the data bus width of system slot9
  # The valid range is between 0x01 to 0x07, and 0x02 here means EfiSlotDataBusWidthUnknown
  gQuarkPlatformTokenSpaceGuid.PcdSMBIOSSystemSlot9DataBusWidth|0x2|UINT8|0xA0000280
  # Defines the usage of system slot9
  # The valid range is between 0x01 to 0x04, and 0x02 here means EfiSlotUsageUnknown
  gQuarkPlatformTokenSpaceGuid.PcdSMBIOSSystemSlot9Usage|0x2|UINT8|0xA0000281
  # Defines the length of system slot9
  # The valid range is between 0x01 to 0x04, and 0x02 here means EfiSlotLengthUnknown
  gQuarkPlatformTokenSpaceGuid.PcdSMBIOSSystemSlot9Length|0x2|UINT8|0xA0000282
  # Defines the ID of system slot9, a number of UINT16
  gQuarkPlatformTokenSpaceGuid.PcdSMBIOSSystemSlot9Id|0x0|UINT16|0xA0000283
  # Defines the characteristics of system slot9 , a bit mask of EFI_MISC_SLOT_CHARACTERISTICS
  gQuarkPlatformTokenSpaceGuid.PcdSMBIOSSystemSlot9Characteristics|0x0|UINT32|0xA0000284

  # Defines the designation of system slot10
  gQuarkPlatformTokenSpaceGuid.PcdSMBIOSSystemSlot10Designation|"None"|VOID*|0xA0000285
  # Defines the type of system slot10
  # The valid range is between 0x01 to 0xA5, and 0x02 here means EfiSlotTypeUnknown
  gQuarkPlatformTokenSpaceGuid.PcdSMBIOSSystemSlot10Type|0x2|UINT8|0xA0000286
  # Defines the data bus width of system slot10
  # The valid range is between 0x01 to 0x07, and 0x02 here means EfiSlotDataBusWidthUnknown
  gQuarkPlatformTokenSpaceGuid.PcdSMBIOSSystemSlot10DataBusWidth|0x2|UINT8|0xA0000287
  # Defines the usage of system slot10
  # The valid range is between 0x01 to 0x04, and 0x02 here means EfiSlotUsageUnknown
  gQuarkPlatformTokenSpaceGuid.PcdSMBIOSSystemSlot10Usage|0x2|UINT8|0xA0000288
  # Defines the length of system slot10
  # The valid range is between 0x01 to 0x04, and 0x02 here means EfiSlotLengthUnknown
  gQuarkPlatformTokenSpaceGuid.PcdSMBIOSSystemSlot10Length|0x2|UINT8|0xA0000289
  # Defines the ID of system slot10, a number of UINT16
  gQuarkPlatformTokenSpaceGuid.PcdSMBIOSSystemSlot10Id|0x0|UINT16|0xA000028A
  # Defines the characteristics of system slot10 , a bit mask of EFI_MISC_SLOT_CHARACTERISTICS
  gQuarkPlatformTokenSpaceGuid.PcdSMBIOSSystemSlot10Characteristics|0x0|UINT32|0xA000028B

  # Defines the designation of system slot11
  gQuarkPlatformTokenSpaceGuid.PcdSMBIOSSystemSlot11Designation|"None"|VOID*|0xA000028C
  # Defines the type of system slot11
  # The valid range is between 0x01 to 0xA5, and 0x02 here means EfiSlotTypeUnknown
  gQuarkPlatformTokenSpaceGuid.PcdSMBIOSSystemSlot11Type|0x2|UINT8|0xA000028D
  # Defines the data bus width of system slot11
  # The valid range is between 0x01 to 0x07, and 0x02 here means EfiSlotDataBusWidthUnknown
  gQuarkPlatformTokenSpaceGuid.PcdSMBIOSSystemSlot11DataBusWidth|0x2|UINT8|0xA000028E
  # Defines the usage of system slot11
  # The valid range is between 0x01 to 0x04, and 0x02 here means EfiSlotUsageUnknown
  gQuarkPlatformTokenSpaceGuid.PcdSMBIOSSystemSlot11Usage|0x2|UINT8|0xA000028F
  # Defines the length of system slot11
  # The valid range is between 0x01 to 0x04, and 0x02 here means EfiSlotLengthUnknown
  gQuarkPlatformTokenSpaceGuid.PcdSMBIOSSystemSlot11Length|0x2|UINT8|0xA0000290
  # Defines the ID of system slot11, a number of UINT16
  gQuarkPlatformTokenSpaceGuid.PcdSMBIOSSystemSlot11Id|0x0|UINT16|0xA00000EE
  # Defines the characteristics of system slot11 , a bit mask of EFI_MISC_SLOT_CHARACTERISTICS
  gQuarkPlatformTokenSpaceGuid.PcdSMBIOSSystemSlot11Characteristics|0x0|UINT32|0xA0000291

  # Defines the designation of system slot12
  gQuarkPlatformTokenSpaceGuid.PcdSMBIOSSystemSlot12Designation|"None"|VOID*|0xA0000292
  # Defines the type of system slot12
  # The valid range is between 0x01 to 0xA5, and 0x02 here means EfiSlotTypeUnknown
  gQuarkPlatformTokenSpaceGuid.PcdSMBIOSSystemSlot12Type|0x2|UINT8|0xA0000293
  # Defines the data bus width of system slot12
  # The valid range is between 0x01 to 0x07, and 0x02 here means EfiSlotDataBusWidthUnknown
  gQuarkPlatformTokenSpaceGuid.PcdSMBIOSSystemSlot12DataBusWidth|0x2|UINT8|0xA0000294
  # Defines the usage of system slot12
  # The valid range is between 0x01 to 0x04, and 0x02 here means EfiSlotUsageUnknown
  gQuarkPlatformTokenSpaceGuid.PcdSMBIOSSystemSlot12Usage|0x2|UINT8|0xA0000295
  # Defines the length of system slot12
  # The valid range is between 0x01 to 0x04, and 0x02 here means EfiSlotLengthUnknown
  gQuarkPlatformTokenSpaceGuid.PcdSMBIOSSystemSlot12Length|0x2|UINT8|0xA0000296
  # Defines the ID of system slot12, a number of UINT16
  gQuarkPlatformTokenSpaceGuid.PcdSMBIOSSystemSlot12Id|0x0|UINT16|0xA0000297
  # Defines the characteristics of system slot12 , a bit mask of EFI_MISC_SLOT_CHARACTERISTICS
  gQuarkPlatformTokenSpaceGuid.PcdSMBIOSSystemSlot12Characteristics|0x0|UINT32|0xA0000298

  # Defines the designation of system slot13
  gQuarkPlatformTokenSpaceGuid.PcdSMBIOSSystemSlot13Designation|"None"|VOID*|0xA0000299
  # Defines the type of system slot13
  # The valid range is between 0x01 to 0xA5, and 0x02 here means EfiSlotTypeUnknown
  gQuarkPlatformTokenSpaceGuid.PcdSMBIOSSystemSlot13Type|0x2|UINT8|0xA000029A
  # Defines the data bus width of system slot13
  # The valid range is between 0x01 to 0x07, and 0x02 here means EfiSlotDataBusWidthUnknown
  gQuarkPlatformTokenSpaceGuid.PcdSMBIOSSystemSlot13DataBusWidth|0x2|UINT8|0xA000029B
  # Defines the usage of system slot13
  # The valid range is between 0x01 to 0x04, and 0x02 here means EfiSlotUsageUnknown
  gQuarkPlatformTokenSpaceGuid.PcdSMBIOSSystemSlot13Usage|0x2|UINT8|0xA000029C
  # Defines the length of system slot13
  # The valid range is between 0x01 to 0x04, and 0x02 here means EfiSlotLengthUnknown
  gQuarkPlatformTokenSpaceGuid.PcdSMBIOSSystemSlot13Length|0x2|UINT8|0xA000029D
  # Defines the ID of system slot13, a number of UINT16
  gQuarkPlatformTokenSpaceGuid.PcdSMBIOSSystemSlot13Id|0x0|UINT16|0xA000029E
  # Defines the characteristics of system slot13 , a bit mask of EFI_MISC_SLOT_CHARACTERISTICS
  gQuarkPlatformTokenSpaceGuid.PcdSMBIOSSystemSlot13Characteristics|0x0|UINT32|0xA000029F

  # Defines the designation of system slot14
  gQuarkPlatformTokenSpaceGuid.PcdSMBIOSSystemSlot14Designation|"None"|VOID*|0xA00002A0
  # Defines the type of system slot14
  # The valid range is between 0x01 to 0xA5, and 0x02 here means EfiSlotTypeUnknown
  gQuarkPlatformTokenSpaceGuid.PcdSMBIOSSystemSlot14Type|0x2|UINT8|0xA00002A1
  # Defines the data bus width of system slot14
  # The valid range is between 0x01 to 0x07, and 0x02 here means EfiSlotDataBusWidthUnknown
  gQuarkPlatformTokenSpaceGuid.PcdSMBIOSSystemSlot14DataBusWidth|0x2|UINT8|0xA00002A2
  # Defines the usage of system slot14
  # The valid range is between 0x01 to 0x04, and 0x02 here means EfiSlotUsageUnknown
  gQuarkPlatformTokenSpaceGuid.PcdSMBIOSSystemSlot14Usage|0x2|UINT8|0xA00002A3
  # Defines the length of system slot14
  # The valid range is between 0x01 to 0x04, and 0x02 here means EfiSlotLengthUnknown
  gQuarkPlatformTokenSpaceGuid.PcdSMBIOSSystemSlot14Length|0x2|UINT8|0xA00002A4
  # Defines the ID of system slot14, a number of UINT16
  gQuarkPlatformTokenSpaceGuid.PcdSMBIOSSystemSlot14Id|0x0|UINT16|0xA00002A5
  # Defines the characteristics of system slot14 , a bit mask of EFI_MISC_SLOT_CHARACTERISTICS
  gQuarkPlatformTokenSpaceGuid.PcdSMBIOSSystemSlot14Characteristics|0x0|UINT32|0xA00002A6

  gQuarkPlatformTokenSpaceGuid.PcdFlashFvPayloadBase|0xFFC00400|UINT32|0xA00002A7
  gQuarkPlatformTokenSpaceGuid.PcdFlashFvPayloadSize|0x000F0000|UINT32|0xA00002A8
  gQuarkPlatformTokenSpaceGuid.PcdFlashFvMainBase|0xFFD00400|UINT32|0xA00002A9
  gQuarkPlatformTokenSpaceGuid.PcdFlashFvMainSize|0x000D0000|UINT32|0xA00002AA
  gQuarkPlatformTokenSpaceGuid.PcdFlashFvRecoveryBase|0xFFEC0400|UINT32|0xA00002AB
  gQuarkPlatformTokenSpaceGuid.PcdFlashFvRecoverySize|0x0003F000|UINT32|0xA00002AC

[PcdsDynamic, PcdsDynamicEx]
  ## Provides the ability to enable the Fast Boot feature of the BIOS.  This
  #  enables the system to boot faster but may only enumerate the hardware
  #  that is required to boot the system.<BR>
  #
  # @Prompt Fast Boot Support
  #
  gQuarkPlatformTokenSpaceGuid.PcdEnableFastBoot|FALSE|BOOLEAN|0xB000004

  ## Determines if the user is physically present.  This information is collected and shared
  #  with all other modules using a dynamic PCD.<BR>
  #
  # @Prompt The User is Physically Present
  #
  gQuarkPlatformTokenSpaceGuid.PcdUserIsPhysicallyPresent|FALSE|BOOLEAN|0xB000006

  ## The Quark SOC X1000 Based Platform Type.<BR>
  #   0x0000 - Unknown<BR>
  #   0x0001 - Quark Emulation<BR>
  #   0x0002 - ClantonPeak SVP<BR>
  #   0x0003 - KipsBay<BR>
  #   0x0004 - CrossHill<BR>
  #   0x0005 - ClantonHill<BR>
  #   0x0006 - Galileo Gen 1<BR>
  #   0x0007 - Reserved<BR>
  #   0x0008 - Galileo Gen 2<BR>
  #
  # @Prompt The Quark SOC X1000 Based Platform Type
  #
  gQuarkPlatformTokenSpaceGuid.PcdPlatformType|0x0008|UINT16|0xB000007

  ## The Quark SOC X1000 Based Platform Type Name.<BR>
  #
  # @Prompt The Quark SOC X1000 Based Platform Type Name
  #
  gQuarkPlatformTokenSpaceGuid.PcdPlatformTypeName|L"GalileoGen2"|VOID*|0xB000008

  ## The size, in bytes, of the SPI FLASH part attached to Quark SOC X1000
  #
  # @Prompt The SPI FALSH Part Size
  #
  gQuarkPlatformTokenSpaceGuid.PcdSpiFlashDeviceSize|0|UINT32|0xB000009

  ## Indicates if the machine has completed one boot cycle before.
  #  After the complete boot, BootState will be set to FALSE.<BR><BR>
  #   TRUE  - The complete boot cycle has not happened before.<BR>
  #   FALSE - The complete boot cycle has happened before.<BR>
  # @Prompt Boot State Flag
  gQuarkPlatformTokenSpaceGuid.PcdBootState|TRUE|BOOLEAN|0xB00000A

[PcdsFixedAtBuild, PcdsDynamic, PcdsDynamicEx, PcdsPatchableInModule]
  ## Specify memory size with page number for a pre-allocated reserved memory to be used
  #  by PEI in S3 phase. The default size 32K. When changing the value make sure the memory size
  #  is large enough to meet PEI requirement in the S3 phase.
  # @Prompt Reserved S3 Boot ACPI Memory Size
  gQuarkPlatformTokenSpaceGuid.PcdS3AcpiReservedMemorySize|0x8000|UINT32|0xB00000B
