#
#  Copyright (c) 2014 - 2016, AMD Incorporated. All rights reserved.
#
#  SPDX-License-Identifier: BSD-2-Clause-Patent
#

################################################################################
#
# FD Section
# The [FD] Section is made up of the definition statements and a
# description of what goes into  the Flash Device Image.  Each FD section
# defines one flash "device" image.  A flash device image may be one of
# the following: Removable media bootable image (like a boot floppy
# image,) an Option ROM image (that would be "flashed" into an add-in
# card,) a System "Flash"  image (that would be burned into a system's
# flash) or an Update ("Capsule") image that will be used to update and
# existing system flash.
#
################################################################################

[FD.STYX_ROM]
BaseAddress   = 0x8000C80000|gArmTokenSpaceGuid.PcdFdBaseAddress  # The base address of the Firmware in NOR Flash.
Size          = 0x00500000|gArmTokenSpaceGuid.PcdFdSize         # The size in bytes of the FLASH Device
ErasePolarity = 1

# This one is tricky, it must be: BlockSize * NumBlocks = Size
BlockSize     = 0x00001000
NumBlocks     = 0x500

################################################################################
#
# Following are lists of FD Region layout which correspond to the locations of different
# images within the flash device.
#
# Regions must be defined in ascending order and may not overlap.
#
# A Layout Region start with a eight digit hex offset (leading "0x" required) followed by
# the pipe "|" character, followed by the size of the region, also in hex with the leading
# "0x" characters. Like:
# Offset|Size
# PcdOffsetCName|PcdSizeCName
# RegionType <FV, DATA, or FILE>
#
################################################################################

0x00000000|0x0004bb00
FILE = Platform/AMD/OverdriveBoard/ScpFirmware.bin

0x0004bb00|0x00020000
FILE = Silicon/AMD/Styx/ArmTrustedFirmware.bin

0x00200000|0x00260000
gArmTokenSpaceGuid.PcdFvBaseAddress|gArmTokenSpaceGuid.PcdFvSize
FV = STYX_EFI

!include Silicon/AMD/Styx/Common/Varstore.fdf.inc

################################################################################
#
# FV Section
#
# [FV] section is used to define what components or modules are placed within a flash
# device file.  This section also defines order the components and modules are positioned
# within the image.  The [FV] section consists of define statements, set statements and
# module statements.
#
################################################################################

[FV.FvMain]
FvNameGuid         = 94f067ae-2aa6-4b30-aa07-4e47fe518bb8
BlockSize          = 0x40
NumBlocks          = 0         # This FV gets compressed so make it just big enough
FvAlignment        = 16        # FV alignment and FV attributes setting.
ERASE_POLARITY     = 1
MEMORY_MAPPED      = TRUE
STICKY_WRITE       = TRUE
LOCK_CAP           = TRUE
LOCK_STATUS        = TRUE
WRITE_DISABLED_CAP = TRUE
WRITE_ENABLED_CAP  = TRUE
WRITE_STATUS       = TRUE
WRITE_LOCK_CAP     = TRUE
WRITE_LOCK_STATUS  = TRUE
READ_DISABLED_CAP  = TRUE
READ_ENABLED_CAP   = TRUE
READ_STATUS        = TRUE
READ_LOCK_CAP      = TRUE
READ_LOCK_STATUS   = TRUE

  INF MdeModulePkg/Core/Dxe/DxeMain.inf
  INF MdeModulePkg/Universal/PCD/Dxe/Pcd.inf

  #
  # PI DXE Drivers producing Architectural Protocols (EFI Services)
  #
  INF ArmPkg/Drivers/CpuDxe/CpuDxe.inf
  INF MdeModulePkg/Core/RuntimeDxe/RuntimeDxe.inf
  INF MdeModulePkg/Universal/SecurityStubDxe/SecurityStubDxe.inf
  INF MdeModulePkg/Universal/CapsuleRuntimeDxe/CapsuleRuntimeDxe.inf
  INF MdeModulePkg/Universal/FaultTolerantWriteDxe/FaultTolerantWriteDxe.inf
  INF MdeModulePkg/Universal/MonotonicCounterRuntimeDxe/MonotonicCounterRuntimeDxe.inf
  INF MdeModulePkg/Universal/ResetSystemRuntimeDxe/ResetSystemRuntimeDxe.inf
  INF EmbeddedPkg/RealTimeClockRuntimeDxe/RealTimeClockRuntimeDxe.inf
  INF EmbeddedPkg/MetronomeDxe/MetronomeDxe.inf
  INF MdeModulePkg/Universal/EbcDxe/EbcDxe.inf

  INF MdeModulePkg/Universal/HiiDatabaseDxe/HiiDatabaseDxe.inf
  INF MdeModulePkg/Universal/WatchdogTimerDxe/WatchdogTimer.inf

  #
  # Console IO support
  #
  INF MdeModulePkg/Universal/Console/ConPlatformDxe/ConPlatformDxe.inf
  INF MdeModulePkg/Universal/Console/ConSplitterDxe/ConSplitterDxe.inf
  INF MdeModulePkg/Universal/Console/GraphicsConsoleDxe/GraphicsConsoleDxe.inf
  INF MdeModulePkg/Universal/Console/TerminalDxe/TerminalDxe.inf
  INF MdeModulePkg/Universal/SerialDxe/SerialDxe.inf
  INF EmbeddedPkg/Drivers/ConsolePrefDxe/ConsolePrefDxe.inf

  INF ArmPkg/Drivers/ArmGic/ArmGicDxe.inf
  INF ArmPkg/Drivers/TimerDxe/TimerDxe.inf

  #
  # FAT filesystem + GPT/MBR partitioning
  #
  INF MdeModulePkg/Universal/Disk/DiskIoDxe/DiskIoDxe.inf
  INF MdeModulePkg/Universal/Disk/PartitionDxe/PartitionDxe.inf
  INF FatPkg/EnhancedFatDxe/Fat.inf
  INF MdeModulePkg/Universal/Disk/UnicodeCollation/EnglishDxe/EnglishDxe.inf

  #
  # Environment Variables Protocol
  #
  INF MdeModulePkg/Universal/Variable/RuntimeDxe/VariableRuntimeDxe.inf
  INF Silicon/AMD/Styx/Drivers/StyxSpiFvDxe/StyxSpiFvDxe.inf

  #
  # Iscp support
  #
  INF Silicon/AMD/Styx/AmdModulePkg/Iscp/IscpDxe.inf

  #
  # FDT support
  #
  INF EmbeddedPkg/Drivers/DtPlatformDxe/DtPlatformDxe.inf
  INF RuleOverride = DTB Platform/AMD/OverdriveBoard/DeviceTree/OverdriveBoard.inf

  #
  # PCI support
  #
  INF Silicon/AMD/Styx/AmdModulePkg/Gionb/Gionb.inf
  INF ArmPkg/Drivers/ArmPciCpuIo2Dxe/ArmPciCpuIo2Dxe.inf
  INF MdeModulePkg/Bus/Pci/PciHostBridgeDxe/PciHostBridgeDxe.inf
  INF MdeModulePkg/Bus/Pci/PciBusDxe/PciBusDxe.inf
  INF MdeModulePkg/Bus/Pci/NvmExpressDxe/NvmExpressDxe.inf
!if $(X64EMU_ENABLE) == TRUE
  INF Emulator/X86EmulatorDxe/X86EmulatorDxe.inf
!endif

  #
  # AHCI Support
  #
  INF MdeModulePkg/Bus/Ata/AtaAtapiPassThru/AtaAtapiPassThru.inf
  INF MdeModulePkg/Bus/Ata/AtaBusDxe/AtaBusDxe.inf
  INF MdeModulePkg/Bus/Scsi/ScsiBusDxe/ScsiBusDxe.inf
  INF MdeModulePkg/Bus/Scsi/ScsiDiskDxe/ScsiDiskDxe.inf
  INF MdeModulePkg/Bus/Pci/SataControllerDxe/SataControllerDxe.inf
  INF MdeModulePkg/Bus/Pci/NonDiscoverablePciDeviceDxe/NonDiscoverablePciDeviceDxe.inf
  INF Silicon/AMD/Styx/Drivers/StyxSataPlatformDxe/StyxSataPlatformDxe.inf

  #
  # USB Support
  #
  INF MdeModulePkg/Bus/Pci/UhciDxe/UhciDxe.inf
  INF MdeModulePkg/Bus/Pci/EhciDxe/EhciDxe.inf
  INF MdeModulePkg/Bus/Pci/XhciDxe/XhciDxe.inf
  INF MdeModulePkg/Bus/Usb/UsbBusDxe/UsbBusDxe.inf
  INF MdeModulePkg/Bus/Usb/UsbMassStorageDxe/UsbMassStorageDxe.inf
  INF MdeModulePkg/Bus/Usb/UsbKbDxe/UsbKbDxe.inf

  #
  # SNP support
  #
  INF Silicon/AMD/Styx/AmdModulePkg/SnpDxe/SnpDxePort0.inf
  INF Silicon/AMD/Styx/AmdModulePkg/SnpDxe/SnpDxePort1.inf

  #
  # Networking stack
  #
!include NetworkPkg/Network.fdf.inc
  INF MdeModulePkg/Universal/Disk/RamDiskDxe/RamDiskDxe.inf

  #
  # Core Info
  #
  INF Silicon/AMD/Styx/Drivers/PlatInitDxe/PlatInitDxe.inf

  #
  # ACPI Support
  #
  INF MdeModulePkg/Universal/Acpi/AcpiTableDxe/AcpiTableDxe.inf
  INF Silicon/AMD/Styx/Drivers/AcpiPlatformDxe/AcpiPlatformDxe.inf
  INF MdeModulePkg/Universal/Acpi/BootGraphicsResourceTableDxe/BootGraphicsResourceTableDxe.inf

  #
  # SMBIOS Support
  #
  INF MdeModulePkg/Universal/SmbiosDxe/SmbiosDxe.inf
  INF Silicon/AMD/Styx/Drivers/PlatformSmbiosDxe/PlatformSmbiosDxe.inf

  #
  # UEFI application (Shell Embedded Boot Loader)
  #
  INF ShellPkg/Application/Shell/Shell.inf

  #
  # Bds
  #
  INF MdeModulePkg/Universal/DevicePathDxe/DevicePathDxe.inf
  INF MdeModulePkg/Universal/DisplayEngineDxe/DisplayEngineDxe.inf
  INF MdeModulePkg/Universal/SetupBrowserDxe/SetupBrowserDxe.inf
  INF MdeModulePkg/Universal/BdsDxe/BdsDxe.inf
  INF MdeModulePkg/Application/UiApp/UiApp.inf
  INF MdeModulePkg/Logo/LogoDxe.inf

  #
  # Crypto Accelerator support (RNG only)
  #
  INF Silicon/AMD/Styx/Drivers/StyxRngDxe/StyxRngDxe.inf

  #
  # Firmware update
  #
  INF MdeModulePkg/Universal/EsrtDxe/EsrtDxe.inf
  INF SignedCapsulePkg/Universal/SystemFirmwareUpdate/SystemFirmwareReportDxe.inf

[FV.STYX_EFI]
FvAlignment        = 16
ERASE_POLARITY     = 1
MEMORY_MAPPED      = TRUE
STICKY_WRITE       = TRUE
LOCK_CAP           = TRUE
LOCK_STATUS        = TRUE
WRITE_DISABLED_CAP = TRUE
WRITE_ENABLED_CAP  = TRUE
WRITE_STATUS       = TRUE
WRITE_LOCK_CAP     = TRUE
WRITE_LOCK_STATUS  = TRUE
READ_DISABLED_CAP  = TRUE
READ_ENABLED_CAP   = TRUE
READ_STATUS        = TRUE
READ_LOCK_CAP      = TRUE
READ_LOCK_STATUS   = TRUE

  INF ArmPlatformPkg/PrePeiCore/PrePeiCoreUniCore.inf
  INF MdeModulePkg/Core/Pei/PeiMain.inf
  INF ArmPlatformPkg/PlatformPei/PlatformPeim.inf
  INF Silicon/AMD/Styx/AmdModulePkg/Iscp/IscpPei.inf
  INF Silicon/AMD/Styx/Drivers/PlatInitPei/PlatInitPei.inf
  INF ArmPlatformPkg/MemoryInitPei/MemoryInitPeim.inf
  INF ArmPkg/Drivers/CpuPei/CpuPei.inf
  INF MdeModulePkg/Universal/PCD/Pei/Pcd.inf
  INF MdeModulePkg/Universal/Variable/Pei/VariablePei.inf
  INF MdeModulePkg/Core/DxeIplPeim/DxeIpl.inf
  INF RuleOverride = FMP_IMAGE_DESC Platform/AMD/OverdriveBoard/SystemFirmwareDescriptor/SystemFirmwareDescriptor.inf

  FILE FV_IMAGE = 9E21FD93-9C72-4c15-8C4B-E77F1DB2D792 {
    SECTION GUIDED EE4E5898-3914-4259-9D6E-DC7BD79403CF PROCESSING_REQUIRED = TRUE {
      SECTION FV_IMAGE = FVMAIN
    }
  }

[FV.CapsuleDispatchFv]
FvAlignment        = 16
ERASE_POLARITY     = 1
MEMORY_MAPPED      = TRUE
STICKY_WRITE       = TRUE
LOCK_CAP           = TRUE
LOCK_STATUS        = TRUE
WRITE_DISABLED_CAP = TRUE
WRITE_ENABLED_CAP  = TRUE
WRITE_STATUS       = TRUE
WRITE_LOCK_CAP     = TRUE
WRITE_LOCK_STATUS  = TRUE
READ_DISABLED_CAP  = TRUE
READ_ENABLED_CAP   = TRUE
READ_STATUS        = TRUE
READ_LOCK_CAP      = TRUE
READ_LOCK_STATUS   = TRUE

  INF  SignedCapsulePkg/Universal/SystemFirmwareUpdate/SystemFirmwareUpdateDxe.inf

[FV.SystemFirmwareUpdateCargo]
FvAlignment        = 16
ERASE_POLARITY     = 1
MEMORY_MAPPED      = TRUE
STICKY_WRITE       = TRUE
LOCK_CAP           = TRUE
LOCK_STATUS        = TRUE
WRITE_DISABLED_CAP = TRUE
WRITE_ENABLED_CAP  = TRUE
WRITE_STATUS       = TRUE
WRITE_LOCK_CAP     = TRUE
WRITE_LOCK_STATUS  = TRUE
READ_DISABLED_CAP  = TRUE
READ_ENABLED_CAP   = TRUE
READ_STATUS        = TRUE
READ_LOCK_CAP      = TRUE
READ_LOCK_STATUS   = TRUE

  FILE RAW = 642e4fcf-2df7-4415-8b70-a03909c57b55 { # PcdEdkiiSystemFirmwareFileGuid
    FD = STYX_ROM
  }

  FILE RAW = ce57b167-b0e4-41e8-a897-5f4feb781d40 { # gEdkiiSystemFmpCapsuleDriverFvFileGuid
    FV = CapsuleDispatchFv
  }

  FILE RAW = 812136D3-4D3A-433A-9418-29BB9BF78F6E { # gEdkiiSystemFmpCapsuleConfigFileGuid
    Platform/AMD/OverdriveBoard/SystemFirmwareUpdateConfig/SystemFirmwareUpdateConfig.ini
  }
  INF RuleOverride = FMP_IMAGE_DESC Platform/AMD/OverdriveBoard/SystemFirmwareDescriptor/SystemFirmwareDescriptor.inf

[FmpPayload.FmpPayloadSystemFirmwarePkcs7]
IMAGE_HEADER_INIT_VERSION = 0x02
IMAGE_TYPE_ID             = d34b3d29-0085-4ab3-8be8-84188cc50489 # PcdSystemFmpCapsuleImageTypeIdGuid
IMAGE_INDEX               = 0x1
HARDWARE_INSTANCE         = 0x0
MONOTONIC_COUNT           = 0x1
CERTIFICATE_GUID          = 4AAFD29D-68DF-49EE-8AA9-347D375665A7 # PKCS7

  FV = SystemFirmwareUpdateCargo

[Capsule.StyxFirmwareUpdateCapsuleFmpPkcs7]
CAPSULE_GUID                = 6dcbd5ed-e82d-4c44-bda1-7194199ad92a # gEfiFmpCapsuleGuid
CAPSULE_HEADER_SIZE         = 0x20
CAPSULE_HEADER_INIT_VERSION = 0x1

  FMP_PAYLOAD = FmpPayloadSystemFirmwarePkcs7

################################################################################
#
# Rules are use with the [FV] section's module INF type to define
# how an FFS file is created for a given INF file. The following Rule are the default
# rules for the different module type. User can add the customized rules to define the
# content of the FFS file.
#
################################################################################


############################################################################
# Example of a DXE_DRIVER FFS file with a Checksum encapsulation section   #
############################################################################
#
#[Rule.Common.DXE_DRIVER]
#  FILE DRIVER = $(NAMED_GUID) {
#    DXE_DEPEX    DXE_DEPEX               Optional $(INF_OUTPUT)/$(MODULE_NAME).depex
#    COMPRESS PI_STD {
#      GUIDED {
#        PE32     PE32                    $(INF_OUTPUT)/$(MODULE_NAME).efi
#        UI       STRING="$(MODULE_NAME)" Optional
#        VERSION  STRING="$(INF_VERSION)" Optional BUILD_NUM=$(BUILD_NUMBER)
#      }
#    }
#  }
#
############################################################################

[Rule.Common.SEC]
  FILE SEC = $(NAMED_GUID) RELOCS_STRIPPED {
    TE  TE Align = 4K                   $(INF_OUTPUT)/$(MODULE_NAME).efi
  }

[Rule.Common.PEI_CORE]
  FILE PEI_CORE = $(NAMED_GUID) {
    TE     TE Align = Auto              $(INF_OUTPUT)/$(MODULE_NAME).efi
    UI     STRING ="$(MODULE_NAME)" Optional
  }

[Rule.Common.PEIM]
  FILE PEIM = $(NAMED_GUID) {
     PEI_DEPEX PEI_DEPEX Optional       $(INF_OUTPUT)/$(MODULE_NAME).depex
     TE       TE Align = Auto           $(INF_OUTPUT)/$(MODULE_NAME).efi
     UI       STRING="$(MODULE_NAME)" Optional
  }

[Rule.Common.PEIM.Binary]
  FILE PEIM = $(NAMED_GUID) {
     PEI_DEPEX PEI_DEPEX Optional       |.depex
     TE       TE Align = Auto           |.efi
     UI       STRING="$(MODULE_NAME)" Optional
  }

[Rule.Common.DXE_CORE]
  FILE DXE_CORE = $(NAMED_GUID) {
    PE32     PE32                       $(INF_OUTPUT)/$(MODULE_NAME).efi
    UI       STRING="$(MODULE_NAME)" Optional
  }

[Rule.Common.UEFI_DRIVER]
  FILE DRIVER = $(NAMED_GUID) {
    DXE_DEPEX    DXE_DEPEX              Optional $(INF_OUTPUT)/$(MODULE_NAME).depex
    PE32         PE32                   $(INF_OUTPUT)/$(MODULE_NAME).efi
    UI           STRING="$(MODULE_NAME)" Optional
  }

[Rule.Common.UEFI_DRIVER.Binary]
  FILE DRIVER = $(NAMED_GUID) {
    PE32         PE32                   |.efi
    UI           STRING="$(MODULE_NAME)" Optional
  }

[Rule.Common.DXE_DRIVER]
  FILE DRIVER = $(NAMED_GUID) {
    DXE_DEPEX    DXE_DEPEX              Optional $(INF_OUTPUT)/$(MODULE_NAME).depex
    PE32         PE32                   $(INF_OUTPUT)/$(MODULE_NAME).efi
    UI           STRING="$(MODULE_NAME)" Optional
    RAW          ASL                    Optional    |.aml
    RAW          ACPI                   Optional    |.acpi
  }

[Rule.Common.DXE_RUNTIME_DRIVER]
  FILE DRIVER = $(NAMED_GUID) {
    DXE_DEPEX    DXE_DEPEX              Optional $(INF_OUTPUT)/$(MODULE_NAME).depex
    PE32         PE32                   $(INF_OUTPUT)/$(MODULE_NAME).efi
    UI           STRING="$(MODULE_NAME)" Optional
  }

[Rule.Common.DXE_RUNTIME_DRIVER.Binary]
  FILE DRIVER = $(NAMED_GUID) {
    DXE_DEPEX    DXE_DEPEX              Optional |.depex
    PE32         PE32                   |.efi
    UI           STRING="$(MODULE_NAME)" Optional
  }

[Rule.Common.UEFI_APPLICATION]
  FILE APPLICATION = $(NAMED_GUID) {
    UI     STRING ="$(MODULE_NAME)"     Optional
    PE32   PE32                         $(INF_OUTPUT)/$(MODULE_NAME).efi
  }

[Rule.Common.UEFI_DRIVER.BINARY]
  FILE DRIVER = $(NAMED_GUID) {
    DXE_DEPEX DXE_DEPEX Optional      |.depex
    PE32      PE32                    |.efi
    UI        STRING="$(MODULE_NAME)" Optional
    VERSION   STRING="$(INF_VERSION)" Optional BUILD_NUM=$(BUILD_NUMBER)
  }

[Rule.Common.UEFI_APPLICATION.BINARY]
  FILE APPLICATION = $(NAMED_GUID) {
    PE32      PE32                    |.efi
    UI        STRING="$(MODULE_NAME)" Optional
    VERSION   STRING="$(INF_VERSION)" Optional BUILD_NUM=$(BUILD_NUMBER)
  }

[Rule.Common.USER_DEFINED.ACPITABLE]
  FILE FREEFORM = $(NAMED_GUID) {
    RAW ASL                |.aml
  }

[Rule.Common.PEIM.FMP_IMAGE_DESC]
  FILE PEIM = $(NAMED_GUID) {
     RAW BIN                  |.acpi
     PEI_DEPEX PEI_DEPEX Optional        $(INF_OUTPUT)/$(MODULE_NAME).depex
     PE32      PE32    Align=4K          $(INF_OUTPUT)/$(MODULE_NAME).efi
     UI       STRING="$(MODULE_NAME)" Optional
     VERSION  STRING="$(INF_VERSION)" Optional BUILD_NUM=$(BUILD_NUMBER)
  }

[Rule.Common.USER_DEFINED.DTB]
  FILE FREEFORM = $(NAMED_GUID) {
    RAW BIN                |.dtb
  }
