// SPDX-License-Identifier: (GPL-2.0+ OR MIT)
/*
 * Copyright (C) 2016 Marvell Technology Group Ltd.
 *
 * Device Tree file for the Armada 8020 SoC, made of an AP806 Dual and
 * two CP110.
 */

#include "armada-ap806-dual.dtsi"
#include "armada-80x0.dtsi"

/ {
        model = "Marvell Armada 8020";
        compatible = "marvell,armada8020", "marvell,armada-ap806-dual",
                     "marvell,armada-ap806";
};

/* The RTC requires external oscillator. But on Aramda 80x0, the RTC clock
 * in CP master is not connected (by package) to the oscillator. So
 * disable it. However, the RTC clock in CP slave is connected to the
 * oscillator so this one is let enabled.
 */

&cp0_rtc {
        status = "disabled";
};
