#
#  Copyright (c) 2018, ARM Limited. All rights reserved.
#
#  SPDX-License-Identifier: BSD-2-Clause-Patent
#

################################################################################
#
# FD Section
# The [FD] Section is made up of the definition statements and a
# description of what goes into  the Flash Device Image.  Each FD section
# defines one flash "device" image.  A flash device image may be one of
# the following: Removable media bootable image (like a boot floppy
# image,) an Option ROM image (that would be "flashed" into an add-in
# card,) a System "Flash"  image (that would be burned into a system's
# flash) or an Update ("Capsule") image that will be used to update and
# existing system flash.
#
################################################################################

[FD.BL33_AP_UEFI]
BaseAddress   = 0xE0000000|gArmTokenSpaceGuid.PcdFdBaseAddress
Size          = 0x00200000|gArmTokenSpaceGuid.PcdFdSize
ErasePolarity = 1

# This one is tricky, it must be: BlockSize * NumBlocks = Size
BlockSize     = 0x00001000
NumBlocks     = 0x200

################################################################################
#
# Following are lists of FD Region layout which correspond to the locations of
# different images within the flash device.
#
# Regions must be defined in ascending order and may not overlap.
#
# A Layout Region start with a eight digit hex offset (leading "0x" required)
# followed by the pipe "|" character, followed by the size of the region, also
# in hex with the leading "0x" characters. Like:
# Offset|Size
# PcdOffsetCName|PcdSizeCName
# RegionType <FV, DATA, or FILE>
#
################################################################################

0x00000000|0x00200000
gArmTokenSpaceGuid.PcdFvBaseAddress|gArmTokenSpaceGuid.PcdFvSize
FV = FVMAIN_COMPACT

################################################################################
#
# FV Section
#
# [FV] section is used to define what components or modules are placed within a
# flash device file. This section also defines order the components and modules
# are positioned within the image. The [FV] section consists of define
# statements, set statements and module statements.
#
################################################################################

[FV.FvMain]
FvNameGuid         = 89cc2ab6-b847-475f-93e2-819603c3d15a
BlockSize          = 0x40
NumBlocks          = 0      # This FV gets compressed so make it just big enough
FvAlignment        = 8      # FV alignment and FV attributes setting.
ERASE_POLARITY     = 1
MEMORY_MAPPED      = TRUE
STICKY_WRITE       = TRUE
LOCK_CAP           = TRUE
LOCK_STATUS        = TRUE
WRITE_DISABLED_CAP = TRUE
WRITE_ENABLED_CAP  = TRUE
WRITE_STATUS       = TRUE
WRITE_LOCK_CAP     = TRUE
WRITE_LOCK_STATUS  = TRUE
READ_DISABLED_CAP  = TRUE
READ_ENABLED_CAP   = TRUE
READ_STATUS        = TRUE
READ_LOCK_CAP      = TRUE
READ_LOCK_STATUS   = TRUE

  INF MdeModulePkg/Core/Dxe/DxeMain.inf

  #
  # PI DXE Drivers producing Architectural Protocols (EFI Services)
  #
  INF ArmPkg/Drivers/CpuDxe/CpuDxe.inf
  INF EmbeddedPkg/MetronomeDxe/MetronomeDxe.inf
  INF EmbeddedPkg/RealTimeClockRuntimeDxe/RealTimeClockRuntimeDxe.inf
  INF EmbeddedPkg/ResetRuntimeDxe/ResetRuntimeDxe.inf
  INF MdeModulePkg/Core/RuntimeDxe/RuntimeDxe.inf
  INF MdeModulePkg/Universal/CapsuleRuntimeDxe/CapsuleRuntimeDxe.inf
  INF MdeModulePkg/Universal/FaultTolerantWriteDxe/FaultTolerantWriteDxe.inf
  INF MdeModulePkg/Universal/MonotonicCounterRuntimeDxe/MonotonicCounterRuntimeDxe.inf
  INF MdeModulePkg/Universal/SecurityStubDxe/SecurityStubDxe.inf
  INF MdeModulePkg/Universal/Variable/RuntimeDxe/VariableRuntimeDxe.inf

  #
  # ACPI Support
  #
  INF MdeModulePkg/Universal/Acpi/AcpiTableDxe/AcpiTableDxe.inf
  INF RuleOverride=ACPITABLE Platform/ARM/SgiPkg/AcpiTables/Sgi575AcpiTables.inf
  INF RuleOverride=ACPITABLE Platform/ARM/SgiPkg/AcpiTables/RdN1EdgeAcpiTables.inf
  INF RuleOverride=ACPITABLE Platform/ARM/SgiPkg/AcpiTables/RdE1EdgeAcpiTables.inf
  INF MdeModulePkg/Universal/HiiDatabaseDxe/HiiDatabaseDxe.inf

  # Required by PCI
  INF ArmPkg/Drivers/ArmPciCpuIo2Dxe/ArmPciCpuIo2Dxe.inf

  #
  # PCI Support
  #
  INF MdeModulePkg/Bus/Pci/PciBusDxe/PciBusDxe.inf
  INF MdeModulePkg/Bus/Pci/PciHostBridgeDxe/PciHostBridgeDxe.inf

  #
  # AHCI Support
  #
  INF MdeModulePkg/Bus/Ata/AtaAtapiPassThru/AtaAtapiPassThru.inf
  INF MdeModulePkg/Bus/Ata/AtaBusDxe/AtaBusDxe.inf

  #
  # SATA Controller
  #
  INF MdeModulePkg/Bus/Pci/SataControllerDxe/SataControllerDxe.inf

  #
  # Multiple Console IO support
  #
  INF MdeModulePkg/Universal/Console/ConPlatformDxe/ConPlatformDxe.inf
  INF MdeModulePkg/Universal/Console/ConSplitterDxe/ConSplitterDxe.inf
  INF MdeModulePkg/Universal/Console/GraphicsConsoleDxe/GraphicsConsoleDxe.inf
  INF MdeModulePkg/Universal/Console/TerminalDxe/TerminalDxe.inf
  INF MdeModulePkg/Universal/SerialDxe/SerialDxe.inf

  INF ArmPkg/Drivers/ArmGic/ArmGicDxe.inf
  INF ArmPkg/Drivers/GenericWatchdogDxe/GenericWatchdogDxe.inf
  INF ArmPkg/Drivers/TimerDxe/TimerDxe.inf

  # NOR Flash driver
  INF ArmPlatformPkg/Drivers/NorFlashDxe/NorFlashDxe.inf
  INF OvmfPkg/VirtioBlkDxe/VirtioBlk.inf

  # Graphics Output Protocol
  INF ArmPlatformPkg/Drivers/LcdGraphicsOutputDxe/LcdGraphicsOutputDxe.inf

  INF Platform/ARM/Drivers/BootMonFs/BootMonFs.inf
  INF MdeModulePkg/Universal/PCD/Dxe/Pcd.inf

  #
  # FAT filesystem + GPT/MBR partitioning
  #
  INF MdeModulePkg/Universal/Disk/DiskIoDxe/DiskIoDxe.inf
  INF MdeModulePkg/Universal/Disk/PartitionDxe/PartitionDxe.inf
  INF FatPkg/EnhancedFatDxe/Fat.inf
  INF MdeModulePkg/Universal/Disk/UnicodeCollation/EnglishDxe/EnglishDxe.inf

  # FV FileSystem
  INF MdeModulePkg/Universal/FvSimpleFileSystemDxe/FvSimpleFileSystemDxe.inf

  #
  # UEFI applications
  #
  INF  ShellPkg/Application/Shell/Shell.inf

  # MM Communicate
  INF ArmPkg/Drivers/MmCommunicationDxe/MmCommunication.inf

  #
  # Platform driver
  #
  INF Platform/ARM/SgiPkg/Drivers/PlatformDxe/PlatformDxe.inf

  #
  # Bds
  #
  INF MdeModulePkg/Application/UiApp/UiApp.inf
  INF MdeModulePkg/Universal/DevicePathDxe/DevicePathDxe.inf
  INF MdeModulePkg/Universal/DisplayEngineDxe/DisplayEngineDxe.inf
  INF MdeModulePkg/Universal/SetupBrowserDxe/SetupBrowserDxe.inf
  INF MdeModulePkg/Universal/BdsDxe/BdsDxe.inf

  #
  # Networking stack
  #
!include NetworkPkg/Network.fdf.inc

!ifdef EDK2_ENABLE_SMSC_91X
  INF EmbeddedPkg/Drivers/Lan91xDxe/Lan91xDxe.inf
!endif
  INF OvmfPkg/VirtioNetDxe/VirtioNet.inf

[FV.FVMAIN_COMPACT]
FvAlignment        = 16
BlockSize          = 0x1000
NumBlocks          = 0x200
ERASE_POLARITY     = 1
MEMORY_MAPPED      = TRUE
STICKY_WRITE       = TRUE
LOCK_CAP           = TRUE
LOCK_STATUS        = TRUE
WRITE_DISABLED_CAP = TRUE
WRITE_ENABLED_CAP  = TRUE
WRITE_STATUS       = TRUE
WRITE_LOCK_CAP     = TRUE
WRITE_LOCK_STATUS  = TRUE
READ_DISABLED_CAP  = TRUE
READ_ENABLED_CAP   = TRUE
READ_STATUS        = TRUE
READ_LOCK_CAP      = TRUE
READ_LOCK_STATUS   = TRUE

  INF ArmPkg/Drivers/CpuPei/CpuPei.inf
  INF ArmPlatformPkg/MemoryInitPei/MemoryInitPeim.inf
  INF ArmPlatformPkg/PlatformPei/PlatformPeim.inf
  INF ArmPlatformPkg/PrePeiCore/PrePeiCoreUniCore.inf
  INF MdeModulePkg/Core/DxeIplPeim/DxeIpl.inf
  INF MdeModulePkg/Core/Pei/PeiMain.inf
  INF MdeModulePkg/Universal/FaultTolerantWritePei/FaultTolerantWritePei.inf
  INF MdeModulePkg/Universal/PCD/Pei/Pcd.inf
  INF MdeModulePkg/Universal/Variable/Pei/VariablePei.inf
  INF Platform/ARM/SgiPkg/Library/SgiPlatformPei/SgiPlatformPei.inf

  FILE FV_IMAGE = 9E21FD93-9C72-4c15-8C4B-E77F1DB2D792 {
    SECTION GUIDED EE4E5898-3914-4259-9D6E-DC7BD79403CF PROCESSING_REQUIRED = TRUE {
      SECTION FV_IMAGE = FVMAIN
    }
  }

################################################################################
#
# Rules are use with the [FV] section's module INF type to define
# how an FFS file is created for a given INF file. The following Rule are the default
# rules for the different module type. User can add the customized rules to define the
# content of the FFS file.
#
################################################################################

############################################################################
# Example of a DXE_DRIVER FFS file with a Checksum encapsulation section   #
############################################################################
#
#[Rule.Common.DXE_DRIVER]
#  FILE DRIVER = $(NAMED_GUID) {
#    DXE_DEPEX    DXE_DEPEX               Optional $(INF_OUTPUT)/$(MODULE_NAME).depex
#    COMPRESS PI_STD {
#      GUIDED {
#        PE32     PE32                    $(INF_OUTPUT)/$(MODULE_NAME).efi
#        UI       STRING="$(MODULE_NAME)" Optional
#        VERSION  STRING="$(INF_VERSION)" Optional BUILD_NUM=$(BUILD_NUMBER)
#      }
#    }
#  }
#
############################################################################

#
# These SEC rules are used for ArmPlatformPkg/PrePeiCore module.
# ArmPlatformPkg/PrePeiCore is declared as a SEC module to make GenFv patch
# the UEFI Firmware to jump to ArmPlatformPkg/PrePeiCore entrypoint
#

[Rule.Common.SEC]
  FILE SEC = $(NAMED_GUID) RELOCS_STRIPPED FIXED {
    TE  TE Align = Auto                 $(INF_OUTPUT)/$(MODULE_NAME).efi
  }

[Rule.Common.PEI_CORE]
  FILE PEI_CORE = $(NAMED_GUID) FIXED {
    TE  TE Align = Auto                 $(INF_OUTPUT)/$(MODULE_NAME).efi
    UI  STRING ="$(MODULE_NAME)" Optional
  }

[Rule.Common.PEIM]
  FILE PEIM = $(NAMED_GUID) FIXED {
     PEI_DEPEX PEI_DEPEX Optional       $(INF_OUTPUT)/$(MODULE_NAME).depex
     TE  TE Align = Auto                $(INF_OUTPUT)/$(MODULE_NAME).efi
     UI  STRING="$(MODULE_NAME)" Optional
  }

[Rule.Common.DXE_CORE]
  FILE DXE_CORE = $(NAMED_GUID) {
    PE32     PE32                       $(INF_OUTPUT)/$(MODULE_NAME).efi
    UI       STRING="$(MODULE_NAME)" Optional
  }

[Rule.Common.UEFI_DRIVER]
  FILE DRIVER = $(NAMED_GUID) {
    DXE_DEPEX    DXE_DEPEX              Optional $(INF_OUTPUT)/$(MODULE_NAME).depex
    PE32         PE32                   $(INF_OUTPUT)/$(MODULE_NAME).efi
    UI           STRING="$(MODULE_NAME)" Optional
  }

[Rule.Common.DXE_DRIVER]
  FILE DRIVER = $(NAMED_GUID) {
    DXE_DEPEX    DXE_DEPEX              Optional $(INF_OUTPUT)/$(MODULE_NAME).depex
    PE32         PE32                   $(INF_OUTPUT)/$(MODULE_NAME).efi
    UI           STRING="$(MODULE_NAME)" Optional
  }

[Rule.Common.DXE_RUNTIME_DRIVER]
  FILE DRIVER = $(NAMED_GUID) {
    DXE_DEPEX    DXE_DEPEX              Optional $(INF_OUTPUT)/$(MODULE_NAME).depex
    PE32         PE32                   $(INF_OUTPUT)/$(MODULE_NAME).efi
    UI           STRING="$(MODULE_NAME)" Optional
  }

[Rule.Common.UEFI_APPLICATION]
  FILE APPLICATION = $(NAMED_GUID) {
    UI     STRING ="$(MODULE_NAME)" Optional
    PE32   PE32                         $(INF_OUTPUT)/$(MODULE_NAME).efi
  }

[Rule.Common.UEFI_DRIVER.BINARY]
  FILE DRIVER = $(NAMED_GUID) {
    DXE_DEPEX DXE_DEPEX Optional      |.depex
    PE32      PE32                    |.efi
    UI        STRING="$(MODULE_NAME)" Optional
    VERSION   STRING="$(INF_VERSION)" Optional BUILD_NUM=$(BUILD_NUMBER)
  }

[Rule.Common.UEFI_APPLICATION.BINARY]
  FILE APPLICATION = $(NAMED_GUID) {
    PE32      PE32                    |.efi
    UI        STRING="$(MODULE_NAME)" Optional
    VERSION   STRING="$(INF_VERSION)" Optional BUILD_NUM=$(BUILD_NUMBER)
  }

[Rule.Common.USER_DEFINED.ACPITABLE]
  FILE FREEFORM = $(NAMED_GUID) {
    RAW ACPI               |.acpi
    RAW ASL                |.aml
  }
