#/** @file
#
#  WARNING:
#  This driver fails to follow the UEFI driver model without a good
#  reason, and only remains in the tree because it is still used by
#  a small number of platforms. It will be removed when no longer used.
#  New platforms should not use it, and no one should use this as
#  reference code for developing new drivers.
#
#  Copyright (c) 2013-2015, ARM Ltd. All rights reserved.<BR>
#
#  SPDX-License-Identifier: BSD-2-Clause-Patent
#
#
#**/

[Defines]
  INF_VERSION                    = 0x00010005
  BASE_NAME                      = Isp1761PeriphDxe
  FILE_GUID                      = 72d78ea6-4dee-11e3-8100-f3842a48d0a0
  MODULE_TYPE                    = UEFI_DRIVER
  VERSION_STRING                 = 1.0
  ENTRY_POINT                    = Isp1761PeriphEntryPoint

[Sources.common]
  Isp1761UsbDxe.c

[LibraryClasses]
  DebugLib
  IoLib
  MemoryAllocationLib
  UefiBootServicesTableLib
  UefiDriverEntryPoint

[Protocols]
  gEfiDriverBindingProtocolGuid
  gUsbDeviceProtocolGuid

[Packages]
  EmbeddedPkg/EmbeddedPkg.dec
  MdePkg/MdePkg.dec
  MdeModulePkg/MdeModulePkg.dec
  Platform/ARM/VExpressPkg/ArmVExpressPkg.dec

[Pcd]
  gArmVExpressTokenSpaceGuid.PcdIsp1761BaseAddress
