/** @file
  Differentiated System Description Table Fields (DSDT)

  Copyright (c) 2014, ARM Ltd. All rights reserved.<BR>
  Copyright (c) 2018, Hisilicon Limited. All rights reserved.<BR>
  Copyright (c) 2015, Linaro Limited. All rights reserved.<BR>
    SPDX-License-Identifier: BSD-2-Clause-Patent

  Based on the files under ArmPlatformPkg/ArmJunoPkg/AcpiTables/

**/

Scope(_SB)
{
  Device(RDE0) {
    Name(_HID, "HISI0201")
    Name(_UID, 0)
    Name(_CCA, 1)
    Name (_CRS, ResourceTemplate ()  {
      //Memory32Fixed (ReadWrite, 0x602E0000, 0x10000)
      QWordMemory (
        ResourceConsumer,
        ,
        MinFixed,
        MaxFixed,
        NonCacheable,
        ReadWrite,
        0x0,
        0x209000000,
        0x209ffffff,
        0x0,
        0x01000000
      )

      Interrupt (ResourceConsumer, Edge, ActiveHigh, Exclusive, 0, "\\_SB.MBI2")
      { 586,587,588,589,590,591,592,593,594,595,596,597,598,599,600,601,
        602,603,604,605,606,607,608,609,610,611,612,613,614,615,616,617
      }
    })
  }
}
