From 7b27b6134f9a2ca4730a6081af8b5331c7a64f63 Mon Sep 17 00:00:00 2001
From: Clement <clement@starfivetech.com>
Date: Thu, 8 Jun 2023 01:33:10 -0400
Subject: [PATCH 1/1] Add sf-extra folder

Signed-off-by: Clement <clement@starfivetech.com>
---
 sf-extra/omx-il/OMX_Audio.h        | 1310 +++++++++++++++++++++++++
 sf-extra/omx-il/OMX_Component.h    |  569 +++++++++++
 sf-extra/omx-il/OMX_ComponentExt.h |   61 ++
 sf-extra/omx-il/OMX_ContentPipe.h  |  193 ++++
 sf-extra/omx-il/OMX_Core.h         | 1422 ++++++++++++++++++++++++++++
 sf-extra/omx-il/OMX_CoreExt.h      |   73 ++
 sf-extra/omx-il/OMX_IVCommon.h     |  993 +++++++++++++++++++
 sf-extra/omx-il/OMX_Image.h        |  328 +++++++
 sf-extra/omx-il/OMX_ImageExt.h     |   55 ++
 sf-extra/omx-il/OMX_Index.h        |  260 +++++
 sf-extra/omx-il/OMX_IndexExt.h     |  105 ++
 sf-extra/omx-il/OMX_Other.h        |  366 +++++++
 sf-extra/omx-il/OMX_Types.h        |  361 +++++++
 sf-extra/omx-il/OMX_Video.h        | 1141 ++++++++++++++++++++++
 sf-extra/omx-il/OMX_VideoExt.h     |  401 ++++++++
 15 files changed, 7638 insertions(+)
 create mode 100644 sf-extra/omx-il/OMX_Audio.h
 create mode 100644 sf-extra/omx-il/OMX_Component.h
 create mode 100644 sf-extra/omx-il/OMX_ComponentExt.h
 create mode 100644 sf-extra/omx-il/OMX_ContentPipe.h
 create mode 100644 sf-extra/omx-il/OMX_Core.h
 create mode 100644 sf-extra/omx-il/OMX_CoreExt.h
 create mode 100644 sf-extra/omx-il/OMX_IVCommon.h
 create mode 100644 sf-extra/omx-il/OMX_Image.h
 create mode 100644 sf-extra/omx-il/OMX_ImageExt.h
 create mode 100644 sf-extra/omx-il/OMX_Index.h
 create mode 100644 sf-extra/omx-il/OMX_IndexExt.h
 create mode 100644 sf-extra/omx-il/OMX_Other.h
 create mode 100644 sf-extra/omx-il/OMX_Types.h
 create mode 100644 sf-extra/omx-il/OMX_Video.h
 create mode 100644 sf-extra/omx-il/OMX_VideoExt.h

diff --git a/sf-extra/omx-il/OMX_Audio.h b/sf-extra/omx-il/OMX_Audio.h
new file mode 100644
index 00000000..72053193
--- /dev/null
+++ b/sf-extra/omx-il/OMX_Audio.h
@@ -0,0 +1,1310 @@
+/*
+ * Copyright (c) 2008 The Khronos Group Inc.
+ *
+ * Permission is hereby granted, free of charge, to any person obtaining
+ * a copy of this software and associated documentation files (the
+ * "Software"), to deal in the Software without restriction, including
+ * without limitation the rights to use, copy, modify, merge, publish,
+ * distribute, sublicense, and/or sell copies of the Software, and to
+ * permit persons to whom the Software is furnished to do so, subject
+ * to the following conditions:
+ * The above copyright notice and this permission notice shall be included
+ * in all copies or substantial portions of the Software.
+ *
+ * THE SOFTWARE IS PROVIDED "AS IS", WITHOUT WARRANTY OF ANY KIND, EXPRESS
+ * OR IMPLIED, INCLUDING BUT NOT LIMITED TO THE WARRANTIES OF
+ * MERCHANTABILITY, FITNESS FOR A PARTICULAR PURPOSE AND NONINFRINGEMENT.
+ * IN NO EVENT SHALL THE AUTHORS OR COPYRIGHT HOLDERS BE LIABLE FOR ANY
+ * CLAIM, DAMAGES OR OTHER LIABILITY, WHETHER IN AN ACTION OF CONTRACT,
+ * TORT OR OTHERWISE, ARISING FROM, OUT OF OR IN CONNECTION WITH THE
+ * SOFTWARE OR THE USE OR OTHER DEALINGS IN THE SOFTWARE.
+ *
+ */
+
+/** @file OMX_Audio.h - OpenMax IL version 1.1.2
+ *  The structures needed by Audio components to exchange
+ *  parameters and configuration data with the componenmilts.
+ */
+
+#ifndef OMX_Audio_h
+#define OMX_Audio_h
+
+#ifdef __cplusplus
+extern "C" {
+#endif /* __cplusplus */
+
+
+/* Each OMX header must include all required header files to allow the
+ *  header to compile without errors.  The includes below are required
+ *  for this header file to compile successfully
+ */
+
+#include <OMX_Core.h>
+
+/** @defgroup midi MIDI
+ * @ingroup audio
+ */
+
+/** @defgroup effects Audio effects
+ * @ingroup audio
+ */
+
+/** @defgroup audio OpenMAX IL Audio Domain
+ * Structures for OpenMAX IL Audio domain
+ * @{
+ */
+
+/** Enumeration used to define the possible audio codings.
+ *  If "OMX_AUDIO_CodingUnused" is selected, the coding selection must
+ *  be done in a vendor specific way.  Since this is for an audio
+ *  processing element this enum is relevant.  However, for another
+ *  type of component other enums would be in this area.
+ */
+typedef enum OMX_AUDIO_CODINGTYPE {
+    OMX_AUDIO_CodingUnused = 0,  /**< Placeholder value when coding is N/A  */
+    OMX_AUDIO_CodingAutoDetect,  /**< auto detection of audio format */
+    OMX_AUDIO_CodingPCM,         /**< Any variant of PCM coding */
+    OMX_AUDIO_CodingADPCM,       /**< Any variant of ADPCM encoded data */
+    OMX_AUDIO_CodingAMR,         /**< Any variant of AMR encoded data */
+    OMX_AUDIO_CodingGSMFR,       /**< Any variant of GSM fullrate (i.e. GSM610) */
+    OMX_AUDIO_CodingGSMEFR,      /**< Any variant of GSM Enhanced Fullrate encoded data*/
+    OMX_AUDIO_CodingGSMHR,       /**< Any variant of GSM Halfrate encoded data */
+    OMX_AUDIO_CodingPDCFR,       /**< Any variant of PDC Fullrate encoded data */
+    OMX_AUDIO_CodingPDCEFR,      /**< Any variant of PDC Enhanced Fullrate encoded data */
+    OMX_AUDIO_CodingPDCHR,       /**< Any variant of PDC Halfrate encoded data */
+    OMX_AUDIO_CodingTDMAFR,      /**< Any variant of TDMA Fullrate encoded data (TIA/EIA-136-420) */
+    OMX_AUDIO_CodingTDMAEFR,     /**< Any variant of TDMA Enhanced Fullrate encoded data (TIA/EIA-136-410) */
+    OMX_AUDIO_CodingQCELP8,      /**< Any variant of QCELP 8kbps encoded data */
+    OMX_AUDIO_CodingQCELP13,     /**< Any variant of QCELP 13kbps encoded data */
+    OMX_AUDIO_CodingEVRC,        /**< Any variant of EVRC encoded data */
+    OMX_AUDIO_CodingSMV,         /**< Any variant of SMV encoded data */
+    OMX_AUDIO_CodingG711,        /**< Any variant of G.711 encoded data */
+    OMX_AUDIO_CodingG723,        /**< Any variant of G.723 dot 1 encoded data */
+    OMX_AUDIO_CodingG726,        /**< Any variant of G.726 encoded data */
+    OMX_AUDIO_CodingG729,        /**< Any variant of G.729 encoded data */
+    OMX_AUDIO_CodingAAC,         /**< Any variant of AAC encoded data */
+    OMX_AUDIO_CodingMP3,         /**< Any variant of MP3 encoded data */
+    OMX_AUDIO_CodingSBC,         /**< Any variant of SBC encoded data */
+    OMX_AUDIO_CodingVORBIS,      /**< Any variant of VORBIS encoded data */
+    OMX_AUDIO_CodingWMA,         /**< Any variant of WMA encoded data */
+    OMX_AUDIO_CodingRA,          /**< Any variant of RA encoded data */
+    OMX_AUDIO_CodingMIDI,        /**< Any variant of MIDI encoded data */
+    OMX_AUDIO_CodingKhronosExtensions = 0x6F000000, /**< Reserved region for introducing Khronos Standard Extensions */
+    OMX_AUDIO_CodingVendorStartUnused = 0x7F000000, /**< Reserved region for introducing Vendor Extensions */
+    OMX_AUDIO_CodingMax = 0x7FFFFFFF
+} OMX_AUDIO_CODINGTYPE;
+
+
+/** The PortDefinition structure is used to define all of the parameters
+ *  necessary for the compliant component to setup an input or an output audio
+ *  path.  If additional information is needed to define the parameters of the
+ *  port (such as frequency), additional structures must be sent such as the
+ *  OMX_AUDIO_PARAM_PCMMODETYPE structure to supply the extra parameters for the port.
+ */
+typedef struct OMX_AUDIO_PORTDEFINITIONTYPE {
+    OMX_STRING cMIMEType;            /**< MIME type of data for the port */
+    OMX_NATIVE_DEVICETYPE pNativeRender; /** < platform specific reference
+                                               for an output device,
+                                               otherwise this field is 0 */
+    OMX_BOOL bFlagErrorConcealment;  /**< Turns on error concealment if it is
+                                          supported by the OMX component */
+    OMX_AUDIO_CODINGTYPE eEncoding;  /**< Type of data expected for this
+                                          port (e.g. PCM, AMR, MP3, etc) */
+} OMX_AUDIO_PORTDEFINITIONTYPE;
+
+
+/**  Port format parameter.  This structure is used to enumerate
+  *  the various data input/output format supported by the port.
+  */
+typedef struct OMX_AUDIO_PARAM_PORTFORMATTYPE {
+    OMX_U32 nSize;                  /**< size of the structure in bytes */
+    OMX_VERSIONTYPE nVersion;       /**< OMX specification version information */
+    OMX_U32 nPortIndex;             /**< Indicates which port to set */
+    OMX_U32 nIndex;                 /**< Indicates the enumeration index for the format from 0x0 to N-1 */
+    OMX_AUDIO_CODINGTYPE eEncoding; /**< Type of data expected for this port (e.g. PCM, AMR, MP3, etc) */
+} OMX_AUDIO_PARAM_PORTFORMATTYPE;
+
+
+/** PCM mode type  */
+typedef enum OMX_AUDIO_PCMMODETYPE {
+    OMX_AUDIO_PCMModeLinear = 0,  /**< Linear PCM encoded data */
+    OMX_AUDIO_PCMModeALaw,        /**< A law PCM encoded data (G.711) */
+    OMX_AUDIO_PCMModeMULaw,       /**< Mu law PCM encoded data (G.711)  */
+    OMX_AUDIO_PCMModeKhronosExtensions = 0x6F000000, /**< Reserved region for introducing Khronos Standard Extensions */
+    OMX_AUDIO_PCMModeVendorStartUnused = 0x7F000000, /**< Reserved region for introducing Vendor Extensions */
+    OMX_AUDIO_PCMModeMax = 0x7FFFFFFF
+} OMX_AUDIO_PCMMODETYPE;
+
+
+typedef enum OMX_AUDIO_CHANNELTYPE {
+    OMX_AUDIO_ChannelNone = 0x0,    /**< Unused or empty */
+    OMX_AUDIO_ChannelLF   = 0x1,    /**< Left front */
+    OMX_AUDIO_ChannelRF   = 0x2,    /**< Right front */
+    OMX_AUDIO_ChannelCF   = 0x3,    /**< Center front */
+    OMX_AUDIO_ChannelLS   = 0x4,    /**< Left surround */
+    OMX_AUDIO_ChannelRS   = 0x5,    /**< Right surround */
+    OMX_AUDIO_ChannelLFE  = 0x6,    /**< Low frequency effects */
+    OMX_AUDIO_ChannelCS   = 0x7,    /**< Back surround */
+    OMX_AUDIO_ChannelLR   = 0x8,    /**< Left rear. */
+    OMX_AUDIO_ChannelRR   = 0x9,    /**< Right rear. */
+    OMX_AUDIO_ChannelKhronosExtensions = 0x6F000000, /**< Reserved region for introducing Khronos Standard Extensions */
+    OMX_AUDIO_ChannelVendorStartUnused = 0x7F000000, /**< Reserved region for introducing Vendor Extensions */
+    OMX_AUDIO_ChannelMax  = 0x7FFFFFFF
+} OMX_AUDIO_CHANNELTYPE;
+
+#define OMX_AUDIO_MAXCHANNELS 16  /**< maximum number distinct audio channels that a buffer may contain */
+#define OMX_MIN_PCMPAYLOAD_MSEC 5 /**< Minimum audio buffer payload size for uncompressed (PCM) audio */
+
+/** PCM format description */
+typedef struct OMX_AUDIO_PARAM_PCMMODETYPE {
+    OMX_U32 nSize;                    /**< Size of this structure, in Bytes */
+    OMX_VERSIONTYPE nVersion;         /**< OMX specification version information */
+    OMX_U32 nPortIndex;               /**< port that this structure applies to */
+    OMX_U32 nChannels;                /**< Number of channels (e.g. 2 for stereo) */
+    OMX_NUMERICALDATATYPE eNumData;   /**< indicates PCM data as signed or unsigned */
+    OMX_ENDIANTYPE eEndian;           /**< indicates PCM data as little or big endian */
+    OMX_BOOL bInterleaved;            /**< True for normal interleaved data; false for
+                                           non-interleaved data (e.g. block data) */
+    OMX_U32 nBitPerSample;            /**< Bit per sample */
+    OMX_U32 nSamplingRate;            /**< Sampling rate of the source data.  Use 0 for
+                                           variable or unknown sampling rate. */
+    OMX_AUDIO_PCMMODETYPE ePCMMode;   /**< PCM mode enumeration */
+    OMX_AUDIO_CHANNELTYPE eChannelMapping[OMX_AUDIO_MAXCHANNELS]; /**< Slot i contains channel defined by eChannelMap[i] */
+
+} OMX_AUDIO_PARAM_PCMMODETYPE;
+
+
+/** Audio channel mode.  This is used by both AAC and MP3, although the names are more appropriate
+ * for the MP3.  For example, JointStereo for MP3 is CouplingChannels for AAC.
+ */
+typedef enum OMX_AUDIO_CHANNELMODETYPE {
+    OMX_AUDIO_ChannelModeStereo = 0,  /**< 2 channels, the bitrate allocation between those
+                                          two channels changes accordingly to each channel information */
+    OMX_AUDIO_ChannelModeJointStereo, /**< mode that takes advantage of what is common between
+                                           2 channels for higher compression gain */
+    OMX_AUDIO_ChannelModeDual,        /**< 2 mono-channels, each channel is encoded with half
+                                           the bitrate of the overall bitrate */
+    OMX_AUDIO_ChannelModeMono,        /**< Mono channel mode */
+    OMX_AUDIO_ChannelModeKhronosExtensions = 0x6F000000, /**< Reserved region for introducing Khronos Standard Extensions */
+    OMX_AUDIO_ChannelModeVendorStartUnused = 0x7F000000, /**< Reserved region for introducing Vendor Extensions */
+    OMX_AUDIO_ChannelModeMax = 0x7FFFFFFF
+} OMX_AUDIO_CHANNELMODETYPE;
+
+
+typedef enum OMX_AUDIO_MP3STREAMFORMATTYPE {
+    OMX_AUDIO_MP3StreamFormatMP1Layer3 = 0, /**< MP3 Audio MPEG 1 Layer 3 Stream format */
+    OMX_AUDIO_MP3StreamFormatMP2Layer3,     /**< MP3 Audio MPEG 2 Layer 3 Stream format */
+    OMX_AUDIO_MP3StreamFormatMP2_5Layer3,   /**< MP3 Audio MPEG2.5 Layer 3 Stream format */
+    OMX_AUDIO_MP3StreamFormatKhronosExtensions = 0x6F000000, /**< Reserved region for introducing Khronos Standard Extensions */
+    OMX_AUDIO_MP3StreamFormatVendorStartUnused = 0x7F000000, /**< Reserved region for introducing Vendor Extensions */
+    OMX_AUDIO_MP3StreamFormatMax = 0x7FFFFFFF
+} OMX_AUDIO_MP3STREAMFORMATTYPE;
+
+/** MP3 params */
+typedef struct OMX_AUDIO_PARAM_MP3TYPE {
+    OMX_U32 nSize;                 /**< size of the structure in bytes */
+    OMX_VERSIONTYPE nVersion;      /**< OMX specification version information */
+    OMX_U32 nPortIndex;            /**< port that this structure applies to */
+    OMX_U32 nChannels;             /**< Number of channels */
+    OMX_U32 nBitRate;              /**< Bit rate of the input data.  Use 0 for variable
+                                        rate or unknown bit rates */
+    OMX_U32 nSampleRate;           /**< Sampling rate of the source data.  Use 0 for
+                                        variable or unknown sampling rate. */
+    OMX_U32 nAudioBandWidth;       /**< Audio band width (in Hz) to which an encoder should
+                                        limit the audio signal. Use 0 to let encoder decide */
+    OMX_AUDIO_CHANNELMODETYPE eChannelMode;   /**< Channel mode enumeration */
+    OMX_AUDIO_MP3STREAMFORMATTYPE eFormat;  /**< MP3 stream format */
+} OMX_AUDIO_PARAM_MP3TYPE;
+
+
+typedef enum OMX_AUDIO_AACSTREAMFORMATTYPE {
+    OMX_AUDIO_AACStreamFormatMP2ADTS = 0, /**< AAC Audio Data Transport Stream 2 format */
+    OMX_AUDIO_AACStreamFormatMP4ADTS,     /**< AAC Audio Data Transport Stream 4 format */
+    OMX_AUDIO_AACStreamFormatMP4LOAS,     /**< AAC Low Overhead Audio Stream format */
+    OMX_AUDIO_AACStreamFormatMP4LATM,     /**< AAC Low overhead Audio Transport Multiplex */
+    OMX_AUDIO_AACStreamFormatADIF,        /**< AAC Audio Data Interchange Format */
+    OMX_AUDIO_AACStreamFormatMP4FF,       /**< AAC inside MPEG-4/ISO File Format */
+    OMX_AUDIO_AACStreamFormatRAW,         /**< AAC Raw Format */
+    OMX_AUDIO_AACStreamFormatKhronosExtensions = 0x6F000000, /**< Reserved region for introducing Khronos Standard Extensions */
+    OMX_AUDIO_AACStreamFormatVendorStartUnused = 0x7F000000, /**< Reserved region for introducing Vendor Extensions */
+    OMX_AUDIO_AACStreamFormatMax = 0x7FFFFFFF
+} OMX_AUDIO_AACSTREAMFORMATTYPE;
+
+
+/** AAC mode type.  Note that the term profile is used with the MPEG-2
+ * standard and the term object type and profile is used with MPEG-4 */
+typedef enum OMX_AUDIO_AACPROFILETYPE {
+    OMX_AUDIO_AACObjectNull = 0,      /**< Null, not used */
+    OMX_AUDIO_AACObjectMain = 1,      /**< AAC Main object */
+    OMX_AUDIO_AACObjectLC,            /**< AAC Low Complexity object (AAC profile) */
+    OMX_AUDIO_AACObjectSSR,           /**< AAC Scalable Sample Rate object */
+    OMX_AUDIO_AACObjectLTP,           /**< AAC Long Term Prediction object */
+    OMX_AUDIO_AACObjectHE,            /**< AAC High Efficiency (object type SBR, HE-AAC profile) */
+    OMX_AUDIO_AACObjectScalable,      /**< AAC Scalable object */
+    OMX_AUDIO_AACObjectERLC = 17,     /**< ER AAC Low Complexity object (Error Resilient AAC-LC) */
+    OMX_AUDIO_AACObjectLD = 23,       /**< AAC Low Delay object (Error Resilient) */
+    OMX_AUDIO_AACObjectHE_PS = 29,    /**< AAC High Efficiency with Parametric Stereo coding (HE-AAC v2, object type PS) */
+    OMX_AUDIO_AACObjectKhronosExtensions = 0x6F000000, /**< Reserved region for introducing Khronos Standard Extensions */
+    OMX_AUDIO_AACObjectVendorStartUnused = 0x7F000000, /**< Reserved region for introducing Vendor Extensions */
+    OMX_AUDIO_AACObjectMax = 0x7FFFFFFF
+} OMX_AUDIO_AACPROFILETYPE;
+
+
+/** AAC tool usage (for nAACtools in OMX_AUDIO_PARAM_AACPROFILETYPE).
+ * Required for encoder configuration and optional as decoder info output.
+ * For MP3, OMX_AUDIO_CHANNELMODETYPE is sufficient. */
+#define OMX_AUDIO_AACToolNone 0x00000000 /**< no AAC tools allowed (encoder config) or active (decoder info output) */
+#define OMX_AUDIO_AACToolMS   0x00000001 /**< MS: Mid/side joint coding tool allowed or active */
+#define OMX_AUDIO_AACToolIS   0x00000002 /**< IS: Intensity stereo tool allowed or active */
+#define OMX_AUDIO_AACToolTNS  0x00000004 /**< TNS: Temporal Noise Shaping tool allowed or active */
+#define OMX_AUDIO_AACToolPNS  0x00000008 /**< PNS: MPEG-4 Perceptual Noise substitution tool allowed or active */
+#define OMX_AUDIO_AACToolLTP  0x00000010 /**< LTP: MPEG-4 Long Term Prediction tool allowed or active */
+#define OMX_AUDIO_AACToolAll  0x7FFFFFFF /**< all AAC tools allowed or active (*/
+
+/** MPEG-4 AAC error resilience (ER) tool usage (for nAACERtools in OMX_AUDIO_PARAM_AACPROFILETYPE).
+ * Required for ER encoder configuration and optional as decoder info output */
+#define OMX_AUDIO_AACERNone  0x00000000  /**< no AAC ER tools allowed/used */
+#define OMX_AUDIO_AACERVCB11 0x00000001  /**< VCB11: Virtual Code Books for AAC section data */
+#define OMX_AUDIO_AACERRVLC  0x00000002  /**< RVLC: Reversible Variable Length Coding */
+#define OMX_AUDIO_AACERHCR   0x00000004  /**< HCR: Huffman Codeword Reordering */
+#define OMX_AUDIO_AACERAll   0x7FFFFFFF  /**< all AAC ER tools allowed/used */
+
+
+/** AAC params */
+typedef struct OMX_AUDIO_PARAM_AACPROFILETYPE {
+    OMX_U32 nSize;                 /**< Size of this structure, in Bytes */
+    OMX_VERSIONTYPE nVersion;      /**< OMX specification version information */
+    OMX_U32 nPortIndex;            /**< Port that this structure applies to */
+    OMX_U32 nChannels;             /**< Number of channels */
+    OMX_U32 nSampleRate;           /**< Sampling rate of the source data.  Use 0 for
+                                        variable or unknown sampling rate. */
+    OMX_U32 nBitRate;              /**< Bit rate of the input data.  Use 0 for variable
+                                        rate or unknown bit rates */
+    OMX_U32 nAudioBandWidth;       /**< Audio band width (in Hz) to which an encoder should
+                                        limit the audio signal. Use 0 to let encoder decide */
+    OMX_U32 nFrameLength;          /**< Frame length (in audio samples per channel) of the codec.
+                                        Can be 1024 or 960 (AAC-LC), 2048 (HE-AAC), 480 or 512 (AAC-LD).
+                                        Use 0 to let encoder decide */
+    OMX_U32 nAACtools;             /**< AAC tool usage */
+    OMX_U32 nAACERtools;           /**< MPEG-4 AAC error resilience tool usage */
+    OMX_AUDIO_AACPROFILETYPE eAACProfile;   /**< AAC profile enumeration */
+    OMX_AUDIO_AACSTREAMFORMATTYPE eAACStreamFormat; /**< AAC stream format enumeration */
+    OMX_AUDIO_CHANNELMODETYPE eChannelMode;   /**< Channel mode enumeration */
+} OMX_AUDIO_PARAM_AACPROFILETYPE;
+
+
+/** VORBIS params */
+typedef struct OMX_AUDIO_PARAM_VORBISTYPE {
+    OMX_U32 nSize;            /**< size of the structure in bytes */
+    OMX_VERSIONTYPE nVersion; /**< OMX specification version information */
+    OMX_U32 nPortIndex;       /**< port that this structure applies to */
+    OMX_U32 nChannels;        /**< Number of channels */
+    OMX_U32 nBitRate;         /**< Bit rate of the encoded data data.  Use 0 for variable
+                                   rate or unknown bit rates. Encoding is set to the
+                                   bitrate closest to specified  value (in bps) */
+    OMX_U32 nMinBitRate;      /**< Sets minimum bitrate (in bps). */
+    OMX_U32 nMaxBitRate;      /**< Sets maximum bitrate (in bps). */
+
+    OMX_U32 nSampleRate;      /**< Sampling rate of the source data.  Use 0 for
+                                   variable or unknown sampling rate. */
+    OMX_U32 nAudioBandWidth;  /**< Audio band width (in Hz) to which an encoder should
+                                   limit the audio signal. Use 0 to let encoder decide */
+    OMX_S32 nQuality;         /**< Sets encoding quality to n, between -1 (low) and 10 (high).
+                                   In the default mode of operation, teh quality level is 3.
+                                   Normal quality range is 0 - 10. */
+    OMX_BOOL bManaged;        /**< Set  bitrate  management  mode. This turns off the
+                                   normal VBR encoding, but allows hard or soft bitrate
+                                   constraints to be enforced by the encoder. This mode can
+                                   be slower, and may also be lower quality. It is
+                                   primarily useful for streaming. */
+    OMX_BOOL bDownmix;        /**< Downmix input from stereo to mono (has no effect on
+                                   non-stereo streams). Useful for lower-bitrate encoding. */
+} OMX_AUDIO_PARAM_VORBISTYPE;
+
+
+/** WMA Version */
+typedef enum OMX_AUDIO_WMAFORMATTYPE {
+    OMX_AUDIO_WMAFormatUnused = 0, /**< format unused or unknown */
+    OMX_AUDIO_WMAFormat7,          /**< Windows Media Audio format 7 */
+    OMX_AUDIO_WMAFormat8,          /**< Windows Media Audio format 8 */
+    OMX_AUDIO_WMAFormat9,          /**< Windows Media Audio format 9 */
+    OMX_AUDIO_WMAFormatKhronosExtensions = 0x6F000000, /**< Reserved region for introducing Khronos Standard Extensions */
+    OMX_AUDIO_WMAFormatVendorStartUnused = 0x7F000000, /**< Reserved region for introducing Vendor Extensions */
+    OMX_AUDIO_WMAFormatMax = 0x7FFFFFFF
+} OMX_AUDIO_WMAFORMATTYPE;
+
+
+/** WMA Profile */
+typedef enum OMX_AUDIO_WMAPROFILETYPE {
+    OMX_AUDIO_WMAProfileUnused = 0,  /**< profile unused or unknown */
+    OMX_AUDIO_WMAProfileL1,          /**< Windows Media audio version 9 profile L1 */
+    OMX_AUDIO_WMAProfileL2,          /**< Windows Media audio version 9 profile L2 */
+    OMX_AUDIO_WMAProfileL3,          /**< Windows Media audio version 9 profile L3 */
+    OMX_AUDIO_WMAProfileKhronosExtensions = 0x6F000000, /**< Reserved region for introducing Khronos Standard Extensions */
+    OMX_AUDIO_WMAProfileVendorStartUnused = 0x7F000000, /**< Reserved region for introducing Vendor Extensions */
+    OMX_AUDIO_WMAProfileMax = 0x7FFFFFFF
+} OMX_AUDIO_WMAPROFILETYPE;
+
+
+/** WMA params */
+typedef struct OMX_AUDIO_PARAM_WMATYPE {
+    OMX_U32 nSize;            /**< size of the structure in bytes */
+    OMX_VERSIONTYPE nVersion; /**< OMX specification version information */
+    OMX_U32 nPortIndex;       /**< port that this structure applies to */
+    OMX_U16 nChannels;        /**< Number of channels */
+    OMX_U32 nBitRate;         /**< Bit rate of the input data.  Use 0 for variable
+                                   rate or unknown bit rates */
+    OMX_AUDIO_WMAFORMATTYPE eFormat; /**< Version of WMA stream / data */
+    OMX_AUDIO_WMAPROFILETYPE eProfile;  /**< Profile of WMA stream / data */
+    OMX_U32 nSamplingRate;    /**< Sampling rate of the source data */
+    OMX_U16 nBlockAlign;      /**< is the block alignment, or block size, in bytes of the audio codec */
+    OMX_U16 nEncodeOptions;   /**< WMA Type-specific data */
+    OMX_U32 nSuperBlockAlign; /**< WMA Type-specific data */
+} OMX_AUDIO_PARAM_WMATYPE;
+
+/**
+ * RealAudio format
+ */
+typedef enum OMX_AUDIO_RAFORMATTYPE {
+    OMX_AUDIO_RAFormatUnused = 0, /**< Format unused or unknown */
+    OMX_AUDIO_RA8,                /**< RealAudio 8 codec */
+    OMX_AUDIO_RA9,                /**< RealAudio 9 codec */
+    OMX_AUDIO_RA10_AAC,           /**< MPEG-4 AAC codec for bitrates of more than 128kbps */
+    OMX_AUDIO_RA10_CODEC,         /**< RealAudio codec for bitrates less than 128 kbps */
+    OMX_AUDIO_RA10_LOSSLESS,      /**< RealAudio Lossless */
+    OMX_AUDIO_RA10_MULTICHANNEL,  /**< RealAudio Multichannel */
+    OMX_AUDIO_RA10_VOICE,         /**< RealAudio Voice for bitrates below 15 kbps */
+    OMX_AUDIO_RAFormatKhronosExtensions = 0x6F000000, /**< Reserved region for introducing Khronos Standard Extensions */
+    OMX_AUDIO_RAFormatVendorStartUnused = 0x7F000000, /**< Reserved region for introducing Vendor Extensions */
+    OMX_VIDEO_RAFormatMax = 0x7FFFFFFF
+} OMX_AUDIO_RAFORMATTYPE;
+
+/** RA (Real Audio) params */
+typedef struct OMX_AUDIO_PARAM_RATYPE {
+    OMX_U32 nSize;              /**< Size of this structure, in Bytes */
+    OMX_VERSIONTYPE nVersion;   /**< OMX specification version information */
+    OMX_U32 nPortIndex;         /**< Port that this structure applies to */
+    OMX_U32 nChannels;          /**< Number of channels */
+    OMX_U32 nSamplingRate;      /**< is the sampling rate of the source data */
+    OMX_U32 nBitsPerFrame;      /**< is the value for bits per frame  */
+    OMX_U32 nSamplePerFrame;    /**< is the value for samples per frame */
+    OMX_U32 nCouplingQuantBits; /**< is the number of coupling quantization bits in the stream */
+    OMX_U32 nCouplingStartRegion;   /**< is the coupling start region in the stream  */
+    OMX_U32 nNumRegions;        /**< is the number of regions value */
+    OMX_AUDIO_RAFORMATTYPE eFormat; /**< is the RealAudio audio format */
+} OMX_AUDIO_PARAM_RATYPE;
+
+
+/** SBC Allocation Method Type */
+typedef enum OMX_AUDIO_SBCALLOCMETHODTYPE {
+    OMX_AUDIO_SBCAllocMethodLoudness, /**< Loudness allocation method */
+    OMX_AUDIO_SBCAllocMethodSNR,      /**< SNR allocation method */
+    OMX_AUDIO_SBCAllocMethodKhronosExtensions = 0x6F000000, /**< Reserved region for introducing Khronos Standard Extensions */
+    OMX_AUDIO_SBCAllocMethodVendorStartUnused = 0x7F000000, /**< Reserved region for introducing Vendor Extensions */
+    OMX_AUDIO_SBCAllocMethodMax = 0x7FFFFFFF
+} OMX_AUDIO_SBCALLOCMETHODTYPE;
+
+
+/** SBC params */
+typedef struct OMX_AUDIO_PARAM_SBCTYPE {
+    OMX_U32 nSize;             /**< size of the structure in bytes */
+    OMX_VERSIONTYPE nVersion;  /**< OMX specification version information */
+    OMX_U32 nPortIndex;        /**< port that this structure applies to */
+    OMX_U32 nChannels;         /**< Number of channels */
+    OMX_U32 nBitRate;          /**< Bit rate of the input data.  Use 0 for variable
+                                    rate or unknown bit rates */
+    OMX_U32 nSampleRate;       /**< Sampling rate of the source data.  Use 0 for
+                                    variable or unknown sampling rate. */
+    OMX_U32 nBlocks;           /**< Number of blocks */
+    OMX_U32 nSubbands;         /**< Number of subbands */
+    OMX_U32 nBitPool;          /**< Bitpool value */
+    OMX_BOOL bEnableBitrate;   /**< Use bitrate value instead of bitpool */
+    OMX_AUDIO_CHANNELMODETYPE eChannelMode; /**< Channel mode enumeration */
+    OMX_AUDIO_SBCALLOCMETHODTYPE eSBCAllocType;   /**< SBC Allocation method type */
+} OMX_AUDIO_PARAM_SBCTYPE;
+
+
+/** ADPCM stream format parameters */
+typedef struct OMX_AUDIO_PARAM_ADPCMTYPE {
+    OMX_U32 nSize;              /**< size of the structure in bytes */
+    OMX_VERSIONTYPE nVersion;   /**< OMX specification version information */
+    OMX_U32 nPortIndex;         /**< port that this structure applies to */
+    OMX_U32 nChannels;          /**< Number of channels in the data stream (not
+                                     necessarily the same as the number of channels
+                                     to be rendered. */
+    OMX_U32 nBitsPerSample;     /**< Number of bits in each sample */
+    OMX_U32 nSampleRate;        /**< Sampling rate of the source data.  Use 0 for
+                                    variable or unknown sampling rate. */
+} OMX_AUDIO_PARAM_ADPCMTYPE;
+
+
+/** G723 rate */
+typedef enum OMX_AUDIO_G723RATE {
+    OMX_AUDIO_G723ModeUnused = 0,  /**< AMRNB Mode unused / unknown */
+    OMX_AUDIO_G723ModeLow,         /**< 5300 bps */
+    OMX_AUDIO_G723ModeHigh,        /**< 6300 bps */
+    OMX_AUDIO_G723ModeKhronosExtensions = 0x6F000000, /**< Reserved region for introducing Khronos Standard Extensions */
+    OMX_AUDIO_G723ModeVendorStartUnused = 0x7F000000, /**< Reserved region for introducing Vendor Extensions */
+    OMX_AUDIO_G723ModeMax = 0x7FFFFFFF
+} OMX_AUDIO_G723RATE;
+
+
+/** G723 - Sample rate must be 8 KHz */
+typedef struct OMX_AUDIO_PARAM_G723TYPE {
+    OMX_U32 nSize;                /**< size of the structure in bytes */
+    OMX_VERSIONTYPE nVersion;     /**< OMX specification version information */
+    OMX_U32 nPortIndex;           /**< port that this structure applies to */
+    OMX_U32 nChannels;            /**< Number of channels in the data stream (not
+                                       necessarily the same as the number of channels
+                                       to be rendered. */
+    OMX_BOOL bDTX;                /**< Enable Discontinuous Transmisssion */
+    OMX_AUDIO_G723RATE eBitRate;  /**< todo: Should this be moved to a config? */
+    OMX_BOOL bHiPassFilter;       /**< Enable High Pass Filter */
+    OMX_BOOL bPostFilter;         /**< Enable Post Filter */
+} OMX_AUDIO_PARAM_G723TYPE;
+
+
+/** ITU G726 (ADPCM) rate */
+typedef enum OMX_AUDIO_G726MODE {
+    OMX_AUDIO_G726ModeUnused = 0,  /**< G726 Mode unused / unknown */
+    OMX_AUDIO_G726Mode16,          /**< 16 kbps */
+    OMX_AUDIO_G726Mode24,          /**< 24 kbps */
+    OMX_AUDIO_G726Mode32,          /**< 32 kbps, most common rate, also G721 */
+    OMX_AUDIO_G726Mode40,          /**< 40 kbps */
+    OMX_AUDIO_G726ModeKhronosExtensions = 0x6F000000, /**< Reserved region for introducing Khronos Standard Extensions */
+    OMX_AUDIO_G726ModeVendorStartUnused = 0x7F000000, /**< Reserved region for introducing Vendor Extensions */
+    OMX_AUDIO_G726ModeMax = 0x7FFFFFFF
+} OMX_AUDIO_G726MODE;
+
+
+/** G.726 stream format parameters - must be at 8KHz */
+typedef struct OMX_AUDIO_PARAM_G726TYPE {
+    OMX_U32 nSize;              /**< size of the structure in bytes */
+    OMX_VERSIONTYPE nVersion;   /**< OMX specification version information */
+    OMX_U32 nPortIndex;         /**< port that this structure applies to */
+    OMX_U32 nChannels;          /**< Number of channels in the data stream (not
+                                     necessarily the same as the number of channels
+                                     to be rendered. */
+    OMX_AUDIO_G726MODE eG726Mode;
+} OMX_AUDIO_PARAM_G726TYPE;
+
+
+/** G729 coder type */
+typedef enum OMX_AUDIO_G729TYPE {
+    OMX_AUDIO_G729 = 0,           /**< ITU G.729  encoded data */
+    OMX_AUDIO_G729A,              /**< ITU G.729 annex A  encoded data */
+    OMX_AUDIO_G729B,              /**< ITU G.729 with annex B encoded data */
+    OMX_AUDIO_G729AB,             /**< ITU G.729 annexes A and B encoded data */
+    OMX_AUDIO_G729KhronosExtensions = 0x6F000000, /**< Reserved region for introducing Khronos Standard Extensions */
+    OMX_AUDIO_G729VendorStartUnused = 0x7F000000, /**< Reserved region for introducing Vendor Extensions */
+    OMX_AUDIO_G729Max = 0x7FFFFFFF
+} OMX_AUDIO_G729TYPE;
+
+
+/** G729 stream format parameters - fixed 6KHz sample rate */
+typedef struct OMX_AUDIO_PARAM_G729TYPE {
+    OMX_U32 nSize;            /**< size of the structure in bytes */
+    OMX_VERSIONTYPE nVersion; /**< OMX specification version information */
+    OMX_U32 nPortIndex;       /**< port that this structure applies to */
+    OMX_U32 nChannels;        /**< Number of channels in the data stream (not
+                                   necessarily the same as the number of channels
+                                   to be rendered. */
+    OMX_BOOL bDTX;            /**< Enable Discontinuous Transmisssion */
+    OMX_AUDIO_G729TYPE eBitType;
+} OMX_AUDIO_PARAM_G729TYPE;
+
+
+/** AMR Frame format */
+typedef enum OMX_AUDIO_AMRFRAMEFORMATTYPE {
+    OMX_AUDIO_AMRFrameFormatConformance = 0,  /**< Frame Format is AMR Conformance
+                                                   (Standard) Format */
+    OMX_AUDIO_AMRFrameFormatIF1,              /**< Frame Format is AMR Interface
+                                                   Format 1 */
+    OMX_AUDIO_AMRFrameFormatIF2,              /**< Frame Format is AMR Interface
+                                                   Format 2*/
+    OMX_AUDIO_AMRFrameFormatFSF,              /**< Frame Format is AMR File Storage
+                                                   Format */
+    OMX_AUDIO_AMRFrameFormatRTPPayload,       /**< Frame Format is AMR Real-Time
+                                                   Transport Protocol Payload Format */
+    OMX_AUDIO_AMRFrameFormatITU,              /**< Frame Format is ITU Format (added at Motorola request) */
+    OMX_AUDIO_AMRFrameFormatKhronosExtensions = 0x6F000000, /**< Reserved region for introducing Khronos Standard Extensions */
+    OMX_AUDIO_AMRFrameFormatVendorStartUnused = 0x7F000000, /**< Reserved region for introducing Vendor Extensions */
+    OMX_AUDIO_AMRFrameFormatMax = 0x7FFFFFFF
+} OMX_AUDIO_AMRFRAMEFORMATTYPE;
+
+
+/** AMR band mode */
+typedef enum OMX_AUDIO_AMRBANDMODETYPE {
+    OMX_AUDIO_AMRBandModeUnused = 0,          /**< AMRNB Mode unused / unknown */
+    OMX_AUDIO_AMRBandModeNB0,                 /**< AMRNB Mode 0 =  4750 bps */
+    OMX_AUDIO_AMRBandModeNB1,                 /**< AMRNB Mode 1 =  5150 bps */
+    OMX_AUDIO_AMRBandModeNB2,                 /**< AMRNB Mode 2 =  5900 bps */
+    OMX_AUDIO_AMRBandModeNB3,                 /**< AMRNB Mode 3 =  6700 bps */
+    OMX_AUDIO_AMRBandModeNB4,                 /**< AMRNB Mode 4 =  7400 bps */
+    OMX_AUDIO_AMRBandModeNB5,                 /**< AMRNB Mode 5 =  7950 bps */
+    OMX_AUDIO_AMRBandModeNB6,                 /**< AMRNB Mode 6 = 10200 bps */
+    OMX_AUDIO_AMRBandModeNB7,                 /**< AMRNB Mode 7 = 12200 bps */
+    OMX_AUDIO_AMRBandModeWB0,                 /**< AMRWB Mode 0 =  6600 bps */
+    OMX_AUDIO_AMRBandModeWB1,                 /**< AMRWB Mode 1 =  8850 bps */
+    OMX_AUDIO_AMRBandModeWB2,                 /**< AMRWB Mode 2 = 12650 bps */
+    OMX_AUDIO_AMRBandModeWB3,                 /**< AMRWB Mode 3 = 14250 bps */
+    OMX_AUDIO_AMRBandModeWB4,                 /**< AMRWB Mode 4 = 15850 bps */
+    OMX_AUDIO_AMRBandModeWB5,                 /**< AMRWB Mode 5 = 18250 bps */
+    OMX_AUDIO_AMRBandModeWB6,                 /**< AMRWB Mode 6 = 19850 bps */
+    OMX_AUDIO_AMRBandModeWB7,                 /**< AMRWB Mode 7 = 23050 bps */
+    OMX_AUDIO_AMRBandModeWB8,                 /**< AMRWB Mode 8 = 23850 bps */
+    OMX_AUDIO_AMRBandModeKhronosExtensions = 0x6F000000, /**< Reserved region for introducing Khronos Standard Extensions */
+    OMX_AUDIO_AMRBandModeVendorStartUnused = 0x7F000000, /**< Reserved region for introducing Vendor Extensions */
+    OMX_AUDIO_AMRBandModeMax = 0x7FFFFFFF
+} OMX_AUDIO_AMRBANDMODETYPE;
+
+
+/** AMR Discontinuous Transmission mode */
+typedef enum OMX_AUDIO_AMRDTXMODETYPE {
+    OMX_AUDIO_AMRDTXModeOff = 0,        /**< AMR Discontinuous Transmission Mode is disabled */
+    OMX_AUDIO_AMRDTXModeOnVAD1,         /**< AMR Discontinuous Transmission Mode using
+                                             Voice Activity Detector 1 (VAD1) is enabled */
+    OMX_AUDIO_AMRDTXModeOnVAD2,         /**< AMR Discontinuous Transmission Mode using
+                                             Voice Activity Detector 2 (VAD2) is enabled */
+    OMX_AUDIO_AMRDTXModeOnAuto,         /**< The codec will automatically select between
+                                             Off, VAD1 or VAD2 modes */
+
+    OMX_AUDIO_AMRDTXasEFR,             /**< DTX as EFR instead of AMR standard (3GPP 26.101, frame type =8,9,10) */
+
+    OMX_AUDIO_AMRDTXModeKhronosExtensions = 0x6F000000, /**< Reserved region for introducing Khronos Standard Extensions */
+    OMX_AUDIO_AMRDTXModeVendorStartUnused = 0x7F000000, /**< Reserved region for introducing Vendor Extensions */
+    OMX_AUDIO_AMRDTXModeMax = 0x7FFFFFFF
+} OMX_AUDIO_AMRDTXMODETYPE;
+
+
+/** AMR params */
+typedef struct OMX_AUDIO_PARAM_AMRTYPE {
+    OMX_U32 nSize;                          /**< size of the structure in bytes */
+    OMX_VERSIONTYPE nVersion;               /**< OMX specification version information */
+    OMX_U32 nPortIndex;                     /**< port that this structure applies to */
+    OMX_U32 nChannels;                      /**< Number of channels */
+    OMX_U32 nBitRate;                       /**< Bit rate read only field */
+    OMX_AUDIO_AMRBANDMODETYPE eAMRBandMode; /**< AMR Band Mode enumeration */
+    OMX_AUDIO_AMRDTXMODETYPE  eAMRDTXMode;  /**< AMR DTX Mode enumeration */
+    OMX_AUDIO_AMRFRAMEFORMATTYPE eAMRFrameFormat; /**< AMR frame format enumeration */
+} OMX_AUDIO_PARAM_AMRTYPE;
+
+
+/** GSM_FR (ETSI 06.10, 3GPP 46.010) stream format parameters */
+typedef struct OMX_AUDIO_PARAM_GSMFRTYPE {
+    OMX_U32 nSize;            /**< size of the structure in bytes */
+    OMX_VERSIONTYPE nVersion; /**< OMX specification version information */
+    OMX_U32 nPortIndex;       /**< port that this structure applies to */
+    OMX_BOOL bDTX;            /**< Enable Discontinuous Transmisssion */
+    OMX_BOOL bHiPassFilter;   /**< Enable High Pass Filter */
+} OMX_AUDIO_PARAM_GSMFRTYPE;
+
+
+/** GSM-HR (ETSI 06.20, 3GPP 46.020) stream format parameters */
+typedef struct OMX_AUDIO_PARAM_GSMHRTYPE {
+    OMX_U32 nSize;            /**< size of the structure in bytes */
+    OMX_VERSIONTYPE nVersion; /**< OMX specification version information */
+    OMX_U32 nPortIndex;       /**< port that this structure applies to */
+    OMX_BOOL bDTX;            /**< Enable Discontinuous Transmisssion */
+    OMX_BOOL bHiPassFilter;   /**< Enable High Pass Filter */
+} OMX_AUDIO_PARAM_GSMHRTYPE;
+
+
+/** GSM-EFR (ETSI 06.60, 3GPP 46.060) stream format parameters */
+typedef struct OMX_AUDIO_PARAM_GSMEFRTYPE {
+    OMX_U32 nSize;            /**< size of the structure in bytes */
+    OMX_VERSIONTYPE nVersion; /**< OMX specification version information */
+    OMX_U32 nPortIndex;       /**< port that this structure applies to */
+    OMX_BOOL bDTX;            /**< Enable Discontinuous Transmisssion */
+    OMX_BOOL bHiPassFilter;   /**< Enable High Pass Filter */
+} OMX_AUDIO_PARAM_GSMEFRTYPE;
+
+
+/** TDMA FR (TIA/EIA-136-420, VSELP 7.95kbps coder) stream format parameters */
+typedef struct OMX_AUDIO_PARAM_TDMAFRTYPE {
+    OMX_U32 nSize;                /**< size of the structure in bytes */
+    OMX_VERSIONTYPE nVersion;     /**< OMX specification version information */
+    OMX_U32 nPortIndex;           /**< port that this structure applies to */
+    OMX_U32 nChannels;            /**< Number of channels in the data stream (not
+                                       necessarily the same as the number of channels
+                                       to be rendered. */
+    OMX_BOOL bDTX;                /**< Enable Discontinuous Transmisssion */
+    OMX_BOOL bHiPassFilter;       /**< Enable High Pass Filter */
+} OMX_AUDIO_PARAM_TDMAFRTYPE;
+
+
+/** TDMA EFR (TIA/EIA-136-410, ACELP 7.4kbps coder) stream format parameters */
+typedef struct OMX_AUDIO_PARAM_TDMAEFRTYPE {
+    OMX_U32 nSize;                /**< size of the structure in bytes */
+    OMX_VERSIONTYPE nVersion;     /**< OMX specification version information */
+    OMX_U32 nPortIndex;           /**< port that this structure applies to */
+    OMX_U32 nChannels;            /**< Number of channels in the data stream (not
+                                       necessarily the same as the number of channels
+                                       to be rendered. */
+    OMX_BOOL bDTX;                /**< Enable Discontinuous Transmisssion */
+    OMX_BOOL bHiPassFilter;       /**< Enable High Pass Filter */
+} OMX_AUDIO_PARAM_TDMAEFRTYPE;
+
+
+/** PDC FR ( RCR-27, VSELP 6.7kbps coder) stream format parameters */
+typedef struct OMX_AUDIO_PARAM_PDCFRTYPE {
+    OMX_U32 nSize;                /**< size of the structure in bytes */
+    OMX_VERSIONTYPE nVersion;     /**< OMX specification version information */
+    OMX_U32 nPortIndex;           /**< port that this structure applies to */
+    OMX_U32 nChannels;            /**< Number of channels in the data stream (not
+                                       necessarily the same as the number of channels
+                                       to be rendered. */
+    OMX_BOOL bDTX;                /**< Enable Discontinuous Transmisssion */
+    OMX_BOOL bHiPassFilter;       /**< Enable High Pass Filter */
+} OMX_AUDIO_PARAM_PDCFRTYPE;
+
+
+/** PDC EFR ( RCR-27, ACELP 6.7kbps coder) stream format parameters */
+typedef struct OMX_AUDIO_PARAM_PDCEFRTYPE {
+    OMX_U32 nSize;                /**< size of the structure in bytes */
+    OMX_VERSIONTYPE nVersion;     /**< OMX specification version information */
+    OMX_U32 nPortIndex;           /**< port that this structure applies to */
+    OMX_U32 nChannels;            /**< Number of channels in the data stream (not
+                                       necessarily the same as the number of channels
+                                       to be rendered. */
+    OMX_BOOL bDTX;                /**< Enable Discontinuous Transmisssion */
+    OMX_BOOL bHiPassFilter;       /**< Enable High Pass Filter */
+} OMX_AUDIO_PARAM_PDCEFRTYPE;
+
+/** PDC HR ( RCR-27, PSI-CELP 3.45kbps coder) stream format parameters */
+typedef struct OMX_AUDIO_PARAM_PDCHRTYPE {
+    OMX_U32 nSize;                /**< size of the structure in bytes */
+    OMX_VERSIONTYPE nVersion;     /**< OMX specification version information */
+    OMX_U32 nPortIndex;           /**< port that this structure applies to */
+    OMX_U32 nChannels;            /**< Number of channels in the data stream (not
+                                       necessarily the same as the number of channels
+                                       to be rendered. */
+    OMX_BOOL bDTX;                /**< Enable Discontinuous Transmisssion */
+    OMX_BOOL bHiPassFilter;       /**< Enable High Pass Filter */
+} OMX_AUDIO_PARAM_PDCHRTYPE;
+
+
+/** CDMA Rate types */
+typedef enum OMX_AUDIO_CDMARATETYPE {
+    OMX_AUDIO_CDMARateBlank = 0,          /**< CDMA encoded frame is blank */
+    OMX_AUDIO_CDMARateFull,               /**< CDMA encoded frame in full rate */
+    OMX_AUDIO_CDMARateHalf,               /**< CDMA encoded frame in half rate */
+    OMX_AUDIO_CDMARateQuarter,            /**< CDMA encoded frame in quarter rate */
+    OMX_AUDIO_CDMARateEighth,             /**< CDMA encoded frame in eighth rate (DTX)*/
+    OMX_AUDIO_CDMARateErasure,            /**< CDMA erasure frame */
+    OMX_AUDIO_CDMARateKhronosExtensions = 0x6F000000, /**< Reserved region for introducing Khronos Standard Extensions */
+    OMX_AUDIO_CDMARateVendorStartUnused = 0x7F000000, /**< Reserved region for introducing Vendor Extensions */
+    OMX_AUDIO_CDMARateMax = 0x7FFFFFFF
+} OMX_AUDIO_CDMARATETYPE;
+
+
+/** QCELP8 (TIA/EIA-96, up to 8kbps coder) stream format parameters */
+typedef struct OMX_AUDIO_PARAM_QCELP8TYPE {
+    OMX_U32 nSize;                /**< size of the structure in bytes */
+    OMX_VERSIONTYPE nVersion;     /**< OMX specification version information */
+    OMX_U32 nPortIndex;           /**< port that this structure applies to */
+    OMX_U32 nChannels;            /**< Number of channels in the data stream (not
+                                       necessarily the same as the number of channels
+                                       to be rendered. */
+    OMX_U32 nBitRate;             /**< Bit rate of the input data.  Use 0 for variable
+                                       rate or unknown bit rates */
+    OMX_AUDIO_CDMARATETYPE eCDMARate; /**< Frame rate */
+    OMX_U32 nMinBitRate;          /**< minmal rate for the encoder = 1,2,3,4, default = 1 */
+    OMX_U32 nMaxBitRate;          /**< maximal rate for the encoder = 1,2,3,4, default = 4 */
+} OMX_AUDIO_PARAM_QCELP8TYPE;
+
+
+/** QCELP13 ( CDMA, EIA/TIA-733, 13.3kbps coder) stream format parameters */
+typedef struct OMX_AUDIO_PARAM_QCELP13TYPE {
+    OMX_U32 nSize;                /**< size of the structure in bytes */
+    OMX_VERSIONTYPE nVersion;     /**< OMX specification version information */
+    OMX_U32 nPortIndex;           /**< port that this structure applies to */
+    OMX_U32 nChannels;            /**< Number of channels in the data stream (not
+                                       necessarily the same as the number of channels
+                                       to be rendered. */
+    OMX_AUDIO_CDMARATETYPE eCDMARate; /**< Frame rate */
+    OMX_U32 nMinBitRate;          /**< minmal rate for the encoder = 1,2,3,4, default = 1 */
+    OMX_U32 nMaxBitRate;          /**< maximal rate for the encoder = 1,2,3,4, default = 4 */
+} OMX_AUDIO_PARAM_QCELP13TYPE;
+
+
+/** EVRC ( CDMA, EIA/TIA-127, RCELP up to 8.55kbps coder) stream format parameters */
+typedef struct OMX_AUDIO_PARAM_EVRCTYPE {
+    OMX_U32 nSize;                /**< size of the structure in bytes */
+    OMX_VERSIONTYPE nVersion;     /**< OMX specification version information */
+    OMX_U32 nPortIndex;           /**< port that this structure applies to */
+    OMX_U32 nChannels;            /**< Number of channels in the data stream (not
+                                       necessarily the same as the number of channels
+                                       to be rendered. */
+    OMX_AUDIO_CDMARATETYPE eCDMARate; /**< actual Frame rate */
+    OMX_BOOL bRATE_REDUCon;       /**< RATE_REDUCtion is requested for this frame */
+    OMX_U32 nMinBitRate;          /**< minmal rate for the encoder = 1,2,3,4, default = 1 */
+    OMX_U32 nMaxBitRate;          /**< maximal rate for the encoder = 1,2,3,4, default = 4 */
+    OMX_BOOL bHiPassFilter;       /**< Enable encoder's High Pass Filter */
+    OMX_BOOL bNoiseSuppressor;    /**< Enable encoder's noise suppressor pre-processing */
+    OMX_BOOL bPostFilter;         /**< Enable decoder's post Filter */
+} OMX_AUDIO_PARAM_EVRCTYPE;
+
+
+/** SMV ( up to 8.55kbps coder) stream format parameters */
+typedef struct OMX_AUDIO_PARAM_SMVTYPE {
+    OMX_U32 nSize;                /**< size of the structure in bytes */
+    OMX_VERSIONTYPE nVersion;     /**< OMX specification version information */
+    OMX_U32 nPortIndex;           /**< port that this structure applies to */
+    OMX_U32 nChannels;            /**< Number of channels in the data stream (not
+                                       necessarily the same as the number of channels
+                                       to be rendered. */
+    OMX_AUDIO_CDMARATETYPE eCDMARate; /**< Frame rate */
+    OMX_BOOL bRATE_REDUCon;           /**< RATE_REDUCtion is requested for this frame */
+    OMX_U32 nMinBitRate;          /**< minmal rate for the encoder = 1,2,3,4, default = 1 ??*/
+    OMX_U32 nMaxBitRate;          /**< maximal rate for the encoder = 1,2,3,4, default = 4 ??*/
+    OMX_BOOL bHiPassFilter;       /**< Enable encoder's High Pass Filter ??*/
+    OMX_BOOL bNoiseSuppressor;    /**< Enable encoder's noise suppressor pre-processing */
+    OMX_BOOL bPostFilter;         /**< Enable decoder's post Filter ??*/
+} OMX_AUDIO_PARAM_SMVTYPE;
+
+
+/** MIDI Format
+ * @ingroup midi
+ */
+typedef enum OMX_AUDIO_MIDIFORMATTYPE {
+    OMX_AUDIO_MIDIFormatUnknown = 0, /**< MIDI Format unknown or don't care */
+    OMX_AUDIO_MIDIFormatSMF0,        /**< Standard MIDI File Type 0 */
+    OMX_AUDIO_MIDIFormatSMF1,        /**< Standard MIDI File Type 1 */
+    OMX_AUDIO_MIDIFormatSMF2,        /**< Standard MIDI File Type 2 */
+    OMX_AUDIO_MIDIFormatSPMIDI,      /**< SP-MIDI */
+    OMX_AUDIO_MIDIFormatXMF0,        /**< eXtensible Music Format type 0 */
+    OMX_AUDIO_MIDIFormatXMF1,        /**< eXtensible Music Format type 1 */
+    OMX_AUDIO_MIDIFormatMobileXMF,   /**< Mobile XMF (eXtensible Music Format type 2) */
+    OMX_AUDIO_MIDIFormatKhronosExtensions = 0x6F000000, /**< Reserved region for introducing Khronos Standard Extensions */
+    OMX_AUDIO_MIDIFormatVendorStartUnused = 0x7F000000, /**< Reserved region for introducing Vendor Extensions */
+    OMX_AUDIO_MIDIFormatMax = 0x7FFFFFFF
+} OMX_AUDIO_MIDIFORMATTYPE;
+
+
+/** MIDI params
+ * @ingroup midi
+ */
+typedef struct OMX_AUDIO_PARAM_MIDITYPE {
+    OMX_U32 nSize;                 /**< size of the structure in bytes */
+    OMX_VERSIONTYPE nVersion;      /**< OMX specification version information */
+    OMX_U32 nPortIndex;            /**< port that this structure applies to */
+    OMX_U32 nFileSize;             /**< size of the MIDI file in bytes, where the entire
+                                        MIDI file passed in, otherwise if 0x0, the MIDI data
+                                        is merged and streamed (instead of passed as an
+                                        entire MIDI file) */
+    OMX_BU32 sMaxPolyphony;        /**< Specifies the maximum simultaneous polyphonic
+                                        voices. A value of zero indicates that the default
+                                        polyphony of the device is used  */
+    OMX_BOOL bLoadDefaultSound;    /**< Whether to load default sound
+                                        bank at initialization */
+    OMX_AUDIO_MIDIFORMATTYPE eMidiFormat; /**< Version of the MIDI file */
+} OMX_AUDIO_PARAM_MIDITYPE;
+
+
+/** Type of the MIDI sound bank
+ * @ingroup midi
+ */
+typedef enum OMX_AUDIO_MIDISOUNDBANKTYPE {
+    OMX_AUDIO_MIDISoundBankUnused = 0,           /**< unused/unknown soundbank type */
+    OMX_AUDIO_MIDISoundBankDLS1,                 /**< DLS version 1 */
+    OMX_AUDIO_MIDISoundBankDLS2,                 /**< DLS version 2 */
+    OMX_AUDIO_MIDISoundBankMobileDLSBase,        /**< Mobile DLS, using the base functionality */
+    OMX_AUDIO_MIDISoundBankMobileDLSPlusOptions, /**< Mobile DLS, using the specification-defined optional feature set */
+    OMX_AUDIO_MIDISoundBankKhronosExtensions = 0x6F000000, /**< Reserved region for introducing Khronos Standard Extensions */
+    OMX_AUDIO_MIDISoundBankVendorStartUnused = 0x7F000000, /**< Reserved region for introducing Vendor Extensions */
+    OMX_AUDIO_MIDISoundBankMax = 0x7FFFFFFF
+} OMX_AUDIO_MIDISOUNDBANKTYPE;
+
+
+/** Bank Layout describes how bank MSB & LSB are used in the DLS instrument definitions sound bank
+ * @ingroup midi
+ */
+typedef enum OMX_AUDIO_MIDISOUNDBANKLAYOUTTYPE {
+    OMX_AUDIO_MIDISoundBankLayoutUnused = 0,   /**< unused/unknown soundbank type */
+    OMX_AUDIO_MIDISoundBankLayoutGM,           /**< GS layout (based on bank MSB 0x00) */
+    OMX_AUDIO_MIDISoundBankLayoutGM2,          /**< General MIDI 2 layout (using MSB 0x78/0x79, LSB 0x00) */
+    OMX_AUDIO_MIDISoundBankLayoutUser,         /**< Does not conform to any bank numbering standards */
+    OMX_AUDIO_MIDISoundBankLayoutKhronosExtensions = 0x6F000000, /**< Reserved region for introducing Khronos Standard Extensions */
+    OMX_AUDIO_MIDISoundBankLayoutVendorStartUnused = 0x7F000000, /**< Reserved region for introducing Vendor Extensions */
+    OMX_AUDIO_MIDISoundBankLayoutMax = 0x7FFFFFFF
+} OMX_AUDIO_MIDISOUNDBANKLAYOUTTYPE;
+
+
+/** MIDI params to load/unload user soundbank
+ * @ingroup midi
+ */
+typedef struct OMX_AUDIO_PARAM_MIDILOADUSERSOUNDTYPE {
+    OMX_U32 nSize;            /**< size of the structure in bytes */
+    OMX_VERSIONTYPE nVersion; /**< OMX specification version information */
+    OMX_U32 nPortIndex;       /**< port that this structure applies to */
+    OMX_U32 nDLSIndex;        /**< DLS file index to be loaded */
+    OMX_U32 nDLSSize;         /**< Size in bytes */
+    OMX_PTR pDLSData;         /**< Pointer to DLS file data */
+    OMX_AUDIO_MIDISOUNDBANKTYPE eMidiSoundBank;   /**< Midi sound bank type enumeration */
+    OMX_AUDIO_MIDISOUNDBANKLAYOUTTYPE eMidiSoundBankLayout; /**< Midi sound bank layout enumeration */
+} OMX_AUDIO_PARAM_MIDILOADUSERSOUNDTYPE;
+
+
+/** Structure for Live MIDI events and MIP messages.
+ * (MIP = Maximum Instantaneous Polyphony; part of the SP-MIDI standard.)
+ * @ingroup midi
+ */
+typedef struct OMX_AUDIO_CONFIG_MIDIIMMEDIATEEVENTTYPE {
+    OMX_U32 nSize;            /**< size of the structure in bytes */
+    OMX_VERSIONTYPE nVersion; /**< OMX specification version information */
+    OMX_U32 nPortIndex;       /**< Port that this structure applies to */
+    OMX_U32 nMidiEventSize;   /**< Size of immediate MIDI events or MIP message in bytes  */
+    OMX_U8 nMidiEvents[1];    /**< MIDI event array to be rendered immediately, or an
+                                   array for the MIP message buffer, where the size is
+                                   indicated by nMidiEventSize */
+} OMX_AUDIO_CONFIG_MIDIIMMEDIATEEVENTTYPE;
+
+
+/** MIDI sound bank/ program pair in a given channel
+ * @ingroup midi
+ */
+typedef struct OMX_AUDIO_CONFIG_MIDISOUNDBANKPROGRAMTYPE {
+    OMX_U32 nSize;              /**< size of the structure in bytes */
+    OMX_VERSIONTYPE nVersion;   /**< OMX specification version information */
+    OMX_U32 nPortIndex;         /**< Port that this structure applies to */
+    OMX_U32 nChannel;           /**< Valid channel values range from 1 to 16 */
+    OMX_U16 nIDProgram;         /**< Valid program ID range is 1 to 128 */
+    OMX_U16 nIDSoundBank;       /**< Sound bank ID */
+    OMX_U32 nUserSoundBankIndex;/**< User soundbank index, easier to access soundbanks
+                                     by index if multiple banks are present */
+} OMX_AUDIO_CONFIG_MIDISOUNDBANKPROGRAMTYPE;
+
+
+/** MIDI control
+ * @ingroup midi
+ */
+typedef struct OMX_AUDIO_CONFIG_MIDICONTROLTYPE {
+    OMX_U32 nSize;                /**< size of the structure in bytes */
+    OMX_VERSIONTYPE nVersion;     /**< OMX specification version information */
+    OMX_U32 nPortIndex;           /**< port that this structure applies to */
+    OMX_BS32 sPitchTransposition; /**< Pitch transposition in semitones, stored as Q22.10
+                                       format based on JAVA MMAPI (JSR-135) requirement */
+    OMX_BU32 sPlayBackRate;       /**< Relative playback rate, stored as Q14.17 fixed-point
+                                       number based on JSR-135 requirement */
+    OMX_BU32 sTempo ;             /**< Tempo in beats per minute (BPM), stored as Q22.10
+                                       fixed-point number based on JSR-135 requirement */
+    OMX_U32 nMaxPolyphony;        /**< Specifies the maximum simultaneous polyphonic
+                                       voices. A value of zero indicates that the default
+                                       polyphony of the device is used  */
+    OMX_U32 nNumRepeat;           /**< Number of times to repeat playback */
+    OMX_U32 nStopTime;            /**< Time in milliseconds to indicate when playback
+                                       will stop automatically.  Set to zero if not used */
+    OMX_U16 nChannelMuteMask;     /**< 16 bit mask for channel mute status */
+    OMX_U16 nChannelSoloMask;     /**< 16 bit mask for channel solo status */
+    OMX_U32 nTrack0031MuteMask;   /**< 32 bit mask for track mute status. Note: This is for tracks 0-31 */
+    OMX_U32 nTrack3263MuteMask;   /**< 32 bit mask for track mute status. Note: This is for tracks 32-63 */
+    OMX_U32 nTrack0031SoloMask;   /**< 32 bit mask for track solo status. Note: This is for tracks 0-31 */
+    OMX_U32 nTrack3263SoloMask;   /**< 32 bit mask for track solo status. Note: This is for tracks 32-63 */
+
+} OMX_AUDIO_CONFIG_MIDICONTROLTYPE;
+
+
+/** MIDI Playback States
+ * @ingroup midi
+ */
+typedef enum OMX_AUDIO_MIDIPLAYBACKSTATETYPE {
+    OMX_AUDIO_MIDIPlayBackStateUnknown = 0,      /**< Unknown state or state does not map to
+                                                    other defined states */
+    OMX_AUDIO_MIDIPlayBackStateClosedEngaged,    /**< No MIDI resource is currently open.
+                                                    The MIDI engine is currently processing
+                                                    MIDI events. */
+    OMX_AUDIO_MIDIPlayBackStateParsing,          /**< A MIDI resource is open and is being
+                                                    primed. The MIDI engine is currently
+                                                    processing MIDI events. */
+    OMX_AUDIO_MIDIPlayBackStateOpenEngaged,      /**< A MIDI resource is open and primed but
+                                                    not playing. The MIDI engine is currently
+                                                    processing MIDI events. The transition to
+                                                    this state is only possible from the
+                                                    OMX_AUDIO_MIDIPlayBackStatePlaying state,
+                                                    when the 'playback head' reaches the end
+                                                    of media data or the playback stops due
+                                                    to stop time set.*/
+    OMX_AUDIO_MIDIPlayBackStatePlaying,          /**< A MIDI resource is open and currently
+                                                    playing. The MIDI engine is currently
+                                                    processing MIDI events.*/
+    OMX_AUDIO_MIDIPlayBackStatePlayingPartially, /**< Best-effort playback due to SP-MIDI/DLS
+                                                    resource constraints */
+    OMX_AUDIO_MIDIPlayBackStatePlayingSilently,  /**< Due to system resource constraints and
+                                                    SP-MIDI content constraints, there is
+                                                    no audible MIDI content during playback
+                                                    currently. The situation may change if
+                                                    resources are freed later.*/
+    OMX_AUDIO_MIDIPlayBackStateKhronosExtensions = 0x6F000000, /**< Reserved region for introducing Khronos Standard Extensions */
+    OMX_AUDIO_MIDIPlayBackStateVendorStartUnused = 0x7F000000, /**< Reserved region for introducing Vendor Extensions */
+    OMX_AUDIO_MIDIPlayBackStateMax = 0x7FFFFFFF
+} OMX_AUDIO_MIDIPLAYBACKSTATETYPE;
+
+
+/** MIDI status
+ * @ingroup midi
+ */
+typedef struct OMX_AUDIO_CONFIG_MIDISTATUSTYPE {
+    OMX_U32 nSize;              /**< size of the structure in bytes */
+    OMX_VERSIONTYPE nVersion;   /**< OMX specification version information */
+    OMX_U32 nPortIndex;         /**< port that this structure applies to */
+    OMX_U16 nNumTracks;         /**< Number of MIDI tracks in the file, read only field.
+                                     NOTE: May not return a meaningful value until the entire
+                                     file is parsed and buffered.  */
+    OMX_U32 nDuration;          /**< The length of the currently open MIDI resource
+                                     in milliseconds. NOTE: May not return a meaningful value
+                                     until the entire file is parsed and buffered.  */
+    OMX_U32 nPosition;          /**< Current Position of the MIDI resource being played
+                                     in milliseconds */
+    OMX_BOOL bVibra;            /**< Does Vibra track exist? NOTE: May not return a meaningful
+                                     value until the entire file is parsed and buffered. */
+    OMX_U32 nNumMetaEvents;     /**< Total number of MIDI Meta Events in the currently
+                                     open MIDI resource. NOTE: May not return a meaningful value
+                                     until the entire file is parsed and buffered.  */
+    OMX_U32 nNumActiveVoices;   /**< Number of active voices in the currently playing
+                                     MIDI resource. NOTE: May not return a meaningful value until
+                                     the entire file is parsed and buffered. */
+    OMX_AUDIO_MIDIPLAYBACKSTATETYPE eMIDIPlayBackState;  /**< MIDI playback state enumeration, read only field */
+} OMX_AUDIO_CONFIG_MIDISTATUSTYPE;
+
+
+/** MIDI Meta Event structure one per Meta Event.
+ *  MIDI Meta Events are like audio metadata, except that they are interspersed
+ *  with the MIDI content throughout the file and are not localized in the header.
+ *  As such, it is necessary to retrieve information about these Meta Events from
+ *  the engine, as it encounters these Meta Events within the MIDI content.
+ *  For example, SMF files can have up to 14 types of MIDI Meta Events (copyright,
+ *  author, default tempo, etc.) scattered throughout the file.
+ *  @ingroup midi
+ */
+typedef struct OMX_AUDIO_CONFIG_MIDIMETAEVENTTYPE {
+    OMX_U32 nSize;            /**< size of the structure in bytes */
+    OMX_VERSIONTYPE nVersion; /**< OMX specification version information */
+    OMX_U32 nPortIndex;       /**< port that this structure applies to */
+    OMX_U32 nIndex;           /**< Index of Meta Event */
+    OMX_U8 nMetaEventType;    /**< Meta Event Type, 7bits (i.e. 0 - 127) */
+    OMX_U32 nMetaEventSize;   /**< size of the Meta Event in bytes */
+    OMX_U32 nTrack;           /**< track number for the meta event */
+    OMX_U32 nPosition;        /**< Position of the meta-event in milliseconds */
+} OMX_AUDIO_CONFIG_MIDIMETAEVENTTYPE;
+
+
+/** MIDI Meta Event Data structure - one per Meta Event.
+ * @ingroup midi
+ */
+typedef struct OMX_AUDIO_CONFIG_MIDIMETAEVENTDATATYPE {
+    OMX_U32 nSize;            /**< size of the structure in bytes */
+    OMX_VERSIONTYPE nVersion; /**< OMX specification version information */
+    OMX_U32 nPortIndex;       /**< port that this structure applies to */
+    OMX_U32 nIndex;           /**< Index of Meta Event */
+    OMX_U32 nMetaEventSize;   /**< size of the Meta Event in bytes */
+    OMX_U8 nData[1];          /**< array of one or more bytes of meta data
+                                   as indicated by the nMetaEventSize field */
+} OMX_AUDIO_CONFIG__MIDIMETAEVENTDATATYPE;
+
+
+/** Audio Volume adjustment for a port */
+typedef struct OMX_AUDIO_CONFIG_VOLUMETYPE {
+    OMX_U32 nSize;              /**< size of the structure in bytes */
+    OMX_VERSIONTYPE nVersion;   /**< OMX specification version information */
+    OMX_U32 nPortIndex;         /**< Port index indicating which port to
+                                     set.  Select the input port to set
+                                     just that port's volume.  Select the
+                                     output port to adjust the master
+                                     volume. */
+    OMX_BOOL bLinear;           /**< Is the volume to be set in linear (0.100)
+                                     or logarithmic scale (mB) */
+    OMX_BS32 sVolume;           /**< Volume linear setting in the 0..100 range, OR
+                                     Volume logarithmic setting for this port.  The values
+                                     for volume are in mB (millibels = 1/100 dB) relative
+                                     to a gain of 1 (e.g. the output is the same as the
+                                     input level).  Values are in mB from nMax
+                                     (maximum volume) to nMin mB (typically negative).
+                                     Since the volume is "voltage"
+                                     and not a "power", it takes a setting of
+                                     -600 mB to decrease the volume by 1/2.  If
+                                     a component cannot accurately set the
+                                     volume to the requested value, it must
+                                     set the volume to the closest value BELOW
+                                     the requested value.  When getting the
+                                     volume setting, the current actual volume
+                                     must be returned. */
+} OMX_AUDIO_CONFIG_VOLUMETYPE;
+
+
+/** Audio Volume adjustment for a channel */
+typedef struct OMX_AUDIO_CONFIG_CHANNELVOLUMETYPE {
+    OMX_U32 nSize;              /**< size of the structure in bytes */
+    OMX_VERSIONTYPE nVersion;   /**< OMX specification version information */
+    OMX_U32 nPortIndex;         /**< Port index indicating which port to
+                                     set.  Select the input port to set
+                                     just that port's volume.  Select the
+                                     output port to adjust the master
+                                     volume. */
+    OMX_U32 nChannel;           /**< channel to select from 0 to N-1,
+                                     using OMX_ALL to apply volume settings
+                                     to all channels */
+    OMX_BOOL bLinear;           /**< Is the volume to be set in linear (0.100) or
+                                     logarithmic scale (mB) */
+    OMX_BS32 sVolume;           /**< Volume linear setting in the 0..100 range, OR
+                                     Volume logarithmic setting for this port.
+                                     The values for volume are in mB
+                                     (millibels = 1/100 dB) relative to a gain
+                                     of 1 (e.g. the output is the same as the
+                                     input level).  Values are in mB from nMax
+                                     (maximum volume) to nMin mB (typically negative).
+                                     Since the volume is "voltage"
+                                     and not a "power", it takes a setting of
+                                     -600 mB to decrease the volume by 1/2.  If
+                                     a component cannot accurately set the
+                                     volume to the requested value, it must
+                                     set the volume to the closest value BELOW
+                                     the requested value.  When getting the
+                                     volume setting, the current actual volume
+                                     must be returned. */
+    OMX_BOOL bIsMIDI;           /**< TRUE if nChannel refers to a MIDI channel,
+                                     FALSE otherwise */
+} OMX_AUDIO_CONFIG_CHANNELVOLUMETYPE;
+
+
+/** Audio balance setting */
+typedef struct OMX_AUDIO_CONFIG_BALANCETYPE {
+    OMX_U32 nSize;              /**< size of the structure in bytes */
+    OMX_VERSIONTYPE nVersion;   /**< OMX specification version information */
+    OMX_U32 nPortIndex;         /**< Port index indicating which port to
+                                     set.  Select the input port to set
+                                     just that port's balance.  Select the
+                                     output port to adjust the master
+                                     balance. */
+    OMX_S32 nBalance;           /**< balance setting for this port
+                                     (-100 to 100, where -100 indicates
+                                     all left, and no right */
+} OMX_AUDIO_CONFIG_BALANCETYPE;
+
+
+/** Audio Port mute */
+typedef struct OMX_AUDIO_CONFIG_MUTETYPE {
+    OMX_U32 nSize;              /**< size of the structure in bytes */
+    OMX_VERSIONTYPE nVersion;   /**< OMX specification version information */
+    OMX_U32 nPortIndex;         /**< Port index indicating which port to
+                                     set.  Select the input port to set
+                                     just that port's mute.  Select the
+                                     output port to adjust the master
+                                     mute. */
+    OMX_BOOL bMute;             /**< Mute setting for this port */
+} OMX_AUDIO_CONFIG_MUTETYPE;
+
+
+/** Audio Channel mute */
+typedef struct OMX_AUDIO_CONFIG_CHANNELMUTETYPE {
+    OMX_U32 nSize;              /**< size of the structure in bytes */
+    OMX_VERSIONTYPE nVersion;   /**< OMX specification version information */
+    OMX_U32 nPortIndex;         /**< port that this structure applies to */
+    OMX_U32 nChannel;           /**< channel to select from 0 to N-1,
+                                     using OMX_ALL to apply mute settings
+                                     to all channels */
+    OMX_BOOL bMute;             /**< Mute setting for this channel */
+    OMX_BOOL bIsMIDI;           /**< TRUE if nChannel refers to a MIDI channel,
+                                     FALSE otherwise */
+} OMX_AUDIO_CONFIG_CHANNELMUTETYPE;
+
+
+
+/** Enable / Disable for loudness control, which boosts bass and to a
+ *  smaller extent high end frequencies to compensate for hearing
+ *  ability at the extreme ends of the audio spectrum
+ */
+typedef struct OMX_AUDIO_CONFIG_LOUDNESSTYPE {
+    OMX_U32 nSize;             /**< size of the structure in bytes */
+    OMX_VERSIONTYPE nVersion;  /**< OMX specification version information */
+    OMX_U32 nPortIndex;        /**< port that this structure applies to */
+    OMX_BOOL bLoudness;        /**< Enable/disable for loudness */
+} OMX_AUDIO_CONFIG_LOUDNESSTYPE;
+
+
+/** Enable / Disable for bass, which controls low frequencies
+ */
+typedef struct OMX_AUDIO_CONFIG_BASSTYPE {
+    OMX_U32 nSize;             /**< size of the structure in bytes */
+    OMX_VERSIONTYPE nVersion;  /**< OMX specification version information */
+    OMX_U32 nPortIndex;        /**< port that this structure applies to */
+    OMX_BOOL bEnable;          /**< Enable/disable for bass control */
+    OMX_S32 nBass;             /**< bass setting for the port, as a
+                                    continuous value from -100 to 100
+                                    (0 means no change in bass level)*/
+} OMX_AUDIO_CONFIG_BASSTYPE;
+
+
+/** Enable / Disable for treble, which controls high frequencies tones
+ */
+typedef struct OMX_AUDIO_CONFIG_TREBLETYPE {
+    OMX_U32 nSize;             /**< size of the structure in bytes */
+    OMX_VERSIONTYPE nVersion;  /**< OMX specification version information */
+    OMX_U32 nPortIndex;        /**< port that this structure applies to */
+    OMX_BOOL bEnable;          /**< Enable/disable for treble control */
+    OMX_S32  nTreble;          /**< treble setting for the port, as a
+                                    continuous value from -100 to 100
+                                    (0 means no change in treble level) */
+} OMX_AUDIO_CONFIG_TREBLETYPE;
+
+
+/** An equalizer is typically used for two reasons: to compensate for an
+ *  sub-optimal frequency response of a system to make it sound more natural
+ *  or to create intentionally some unnatural coloring to the sound to create
+ *  an effect.
+ *  @ingroup effects
+ */
+typedef struct OMX_AUDIO_CONFIG_EQUALIZERTYPE {
+    OMX_U32 nSize;             /**< size of the structure in bytes */
+    OMX_VERSIONTYPE nVersion;  /**< OMX specification version information */
+    OMX_U32 nPortIndex;        /**< port that this structure applies to */
+    OMX_BOOL bEnable;          /**< Enable/disable for equalizer */
+    OMX_BU32 sBandIndex;       /**< Band number to be set.  Upper Limit is
+                                    N-1, where N is the number of bands, lower limit is 0 */
+    OMX_BU32 sCenterFreq;      /**< Center frequecies in Hz.  This is a
+                                    read only element and is used to determine
+                                    the lower, center and upper frequency of
+                                    this band.  */
+    OMX_BS32 sBandLevel;       /**< band level in millibels */
+} OMX_AUDIO_CONFIG_EQUALIZERTYPE;
+
+
+/** Stereo widening mode type
+ * @ingroup effects
+ */
+typedef enum OMX_AUDIO_STEREOWIDENINGTYPE {
+    OMX_AUDIO_StereoWideningHeadphones,    /**< Stereo widening for loudspeakers */
+    OMX_AUDIO_StereoWideningLoudspeakers,  /**< Stereo widening for closely spaced loudspeakers */
+    OMX_AUDIO_StereoWideningKhronosExtensions = 0x6F000000, /**< Reserved region for introducing Khronos Standard Extensions */
+    OMX_AUDIO_StereoWideningVendorStartUnused = 0x7F000000, /**< Reserved region for introducing Vendor Extensions */
+    OMX_AUDIO_StereoWideningMax = 0x7FFFFFFF
+} OMX_AUDIO_STEREOWIDENINGTYPE;
+
+
+/** Control for stereo widening, which is a special 2-channel
+ *  case of the audio virtualizer effect. For example, for 5.1-channel
+ *  output, it translates to virtual surround sound.
+ * @ingroup effects
+ */
+typedef struct OMX_AUDIO_CONFIG_STEREOWIDENINGTYPE {
+    OMX_U32 nSize;             /**< size of the structure in bytes */
+    OMX_VERSIONTYPE nVersion;  /**< OMX specification version information */
+    OMX_U32 nPortIndex;        /**< port that this structure applies to */
+    OMX_BOOL bEnable;          /**< Enable/disable for stereo widening control */
+    OMX_AUDIO_STEREOWIDENINGTYPE eWideningType; /**< Stereo widening algorithm type */
+    OMX_U32  nStereoWidening;  /**< stereo widening setting for the port,
+                                    as a continuous value from 0 to 100  */
+} OMX_AUDIO_CONFIG_STEREOWIDENINGTYPE;
+
+
+/** The chorus effect (or ``choralizer'') is any signal processor which makes
+ *  one sound source (such as a voice) sound like many such sources singing
+ *  (or playing) in unison. Since performance in unison is never exact, chorus
+ *  effects simulate this by making independently modified copies of the input
+ *  signal. Modifications may include (1) delay, (2) frequency shift, and
+ *  (3) amplitude modulation.
+ * @ingroup effects
+ */
+typedef struct OMX_AUDIO_CONFIG_CHORUSTYPE {
+    OMX_U32 nSize;             /**< size of the structure in bytes */
+    OMX_VERSIONTYPE nVersion;  /**< OMX specification version information */
+    OMX_U32 nPortIndex;        /**< port that this structure applies to */
+    OMX_BOOL bEnable;          /**< Enable/disable for chorus */
+    OMX_BU32 sDelay;           /**< average delay in milliseconds */
+    OMX_BU32 sModulationRate;  /**< rate of modulation in millihertz */
+    OMX_U32 nModulationDepth;  /**< depth of modulation as a percentage of
+                                    delay (i.e. 0 to 100) */
+    OMX_BU32 nFeedback;        /**< Feedback from chorus output to input in percentage */
+} OMX_AUDIO_CONFIG_CHORUSTYPE;
+
+
+/** Reverberation is part of the reflected sound that follows the early
+ *  reflections. In a typical room, this consists of a dense succession of
+ *  echoes whose energy decays exponentially. The reverberation effect structure
+ *  as defined here includes both (early) reflections as well as (late) reverberations.
+ * @ingroup effects
+ */
+typedef struct OMX_AUDIO_CONFIG_REVERBERATIONTYPE {
+    OMX_U32 nSize;                /**< size of the structure in bytes */
+    OMX_VERSIONTYPE nVersion;     /**< OMX specification version information */
+    OMX_U32 nPortIndex;           /**< port that this structure applies to */
+    OMX_BOOL bEnable;             /**< Enable/disable for reverberation control */
+    OMX_BS32 sRoomLevel;          /**< Intensity level for the whole room effect
+                                       (i.e. both early reflections and late
+                                       reverberation) in millibels */
+    OMX_BS32 sRoomHighFreqLevel;  /**< Attenuation at high frequencies
+                                       relative to the intensity at low
+                                       frequencies in millibels */
+    OMX_BS32 sReflectionsLevel;   /**< Intensity level of early reflections
+                                       (relative to room value), in millibels */
+    OMX_BU32 sReflectionsDelay;   /**< Delay time of the first reflection relative
+                                       to the direct path, in milliseconds */
+    OMX_BS32 sReverbLevel;        /**< Intensity level of late reverberation
+                                       relative to room level, in millibels */
+    OMX_BU32 sReverbDelay;        /**< Time delay from the first early reflection
+                                       to the beginning of the late reverberation
+                                       section, in milliseconds */
+    OMX_BU32 sDecayTime;          /**< Late reverberation decay time at low
+                                       frequencies, in milliseconds */
+    OMX_BU32 nDecayHighFreqRatio; /**< Ratio of high frequency decay time relative
+                                       to low frequency decay time in percent  */
+    OMX_U32 nDensity;             /**< Modal density in the late reverberation decay,
+                                       in percent (i.e. 0 - 100) */
+    OMX_U32 nDiffusion;           /**< Echo density in the late reverberation decay,
+                                       in percent (i.e. 0 - 100) */
+    OMX_BU32 sReferenceHighFreq;  /**< Reference high frequency in Hertz. This is
+                                       the frequency used as the reference for all
+                                       the high-frequency settings above */
+
+} OMX_AUDIO_CONFIG_REVERBERATIONTYPE;
+
+
+/** Possible settings for the Echo Cancelation structure to use
+ * @ingroup effects
+ */
+typedef enum OMX_AUDIO_ECHOCANTYPE {
+    OMX_AUDIO_EchoCanOff = 0,    /**< Echo Cancellation is disabled */
+    OMX_AUDIO_EchoCanNormal,     /**< Echo Cancellation normal operation -
+                                     echo from plastics and face */
+    OMX_AUDIO_EchoCanHFree,      /**< Echo Cancellation optimized for
+                                     Hands Free operation */
+    OMX_AUDIO_EchoCanCarKit,    /**< Echo Cancellation optimized for
+                                     Car Kit (longer echo) */
+    OMX_AUDIO_EchoCanKhronosExtensions = 0x6F000000, /**< Reserved region for introducing Khronos Standard Extensions */
+    OMX_AUDIO_EchoCanVendorStartUnused = 0x7F000000, /**< Reserved region for introducing Vendor Extensions */
+    OMX_AUDIO_EchoCanMax = 0x7FFFFFFF
+} OMX_AUDIO_ECHOCANTYPE;
+
+
+/** Enable / Disable for echo cancelation, which removes undesired echo's
+ *  from the audio
+ * @ingroup effects
+ */
+typedef struct OMX_AUDIO_CONFIG_ECHOCANCELATIONTYPE {
+    OMX_U32 nSize;             /**< size of the structure in bytes */
+    OMX_VERSIONTYPE nVersion;  /**< OMX specification version information */
+    OMX_U32 nPortIndex;        /**< port that this structure applies to */
+    OMX_AUDIO_ECHOCANTYPE eEchoCancelation; /**< Echo cancelation settings */
+} OMX_AUDIO_CONFIG_ECHOCANCELATIONTYPE;
+
+
+/** Enable / Disable for noise reduction, which undesired noise from
+ * the audio
+ * @ingroup effects
+ */
+typedef struct OMX_AUDIO_CONFIG_NOISEREDUCTIONTYPE {
+    OMX_U32 nSize;             /**< size of the structure in bytes */
+    OMX_VERSIONTYPE nVersion;  /**< OMX specification version information */
+    OMX_U32 nPortIndex;        /**< port that this structure applies to */
+    OMX_BOOL bNoiseReduction;  /**< Enable/disable for noise reduction */
+} OMX_AUDIO_CONFIG_NOISEREDUCTIONTYPE;
+
+/** @} */
+
+#ifdef __cplusplus
+}
+#endif /* __cplusplus */
+
+#endif
+/* File EOF */
+
diff --git a/sf-extra/omx-il/OMX_Component.h b/sf-extra/omx-il/OMX_Component.h
new file mode 100644
index 00000000..56fd37e9
--- /dev/null
+++ b/sf-extra/omx-il/OMX_Component.h
@@ -0,0 +1,569 @@
+/*
+ * Copyright (c) 2008 The Khronos Group Inc.
+ *
+ * Permission is hereby granted, free of charge, to any person obtaining
+ * a copy of this software and associated documentation files (the
+ * "Software"), to deal in the Software without restriction, including
+ * without limitation the rights to use, copy, modify, merge, publish,
+ * distribute, sublicense, and/or sell copies of the Software, and to
+ * permit persons to whom the Software is furnished to do so, subject
+ * to the following conditions:
+ * The above copyright notice and this permission notice shall be included
+ * in all copies or substantial portions of the Software.
+ *
+ * THE SOFTWARE IS PROVIDED "AS IS", WITHOUT WARRANTY OF ANY KIND, EXPRESS
+ * OR IMPLIED, INCLUDING BUT NOT LIMITED TO THE WARRANTIES OF
+ * MERCHANTABILITY, FITNESS FOR A PARTICULAR PURPOSE AND NONINFRINGEMENT.
+ * IN NO EVENT SHALL THE AUTHORS OR COPYRIGHT HOLDERS BE LIABLE FOR ANY
+ * CLAIM, DAMAGES OR OTHER LIABILITY, WHETHER IN AN ACTION OF CONTRACT,
+ * TORT OR OTHERWISE, ARISING FROM, OUT OF OR IN CONNECTION WITH THE
+ * SOFTWARE OR THE USE OR OTHER DEALINGS IN THE SOFTWARE.
+ *
+ */
+
+/** OMX_Component.h - OpenMax IL version 1.1.2
+ *  The OMX_Component header file contains the definitions used to define
+ *  the public interface of a component.  This header file is intended to
+ *  be used by both the application and the component.
+ */
+
+#ifndef OMX_Component_h
+#define OMX_Component_h
+
+#ifdef __cplusplus
+extern "C" {
+#endif /* __cplusplus */
+
+
+
+/* Each OMX header must include all required header files to allow the
+ *  header to compile without errors.  The includes below are required
+ *  for this header file to compile successfully
+ */
+
+#include <OMX_Audio.h>
+#include <OMX_Video.h>
+#include <OMX_Image.h>
+#include <OMX_Other.h>
+
+/** @ingroup comp */
+typedef enum OMX_PORTDOMAINTYPE {
+    OMX_PortDomainAudio,
+    OMX_PortDomainVideo,
+    OMX_PortDomainImage,
+    OMX_PortDomainOther,
+    OMX_PortDomainKhronosExtensions = 0x6F000000, /**< Reserved region for introducing Khronos Standard Extensions */
+    OMX_PortDomainVendorStartUnused = 0x7F000000, /**< Reserved region for introducing Vendor Extensions */
+    OMX_PortDomainMax = 0x7ffffff
+} OMX_PORTDOMAINTYPE;
+
+/** @ingroup comp */
+typedef struct OMX_PARAM_PORTDEFINITIONTYPE {
+    OMX_U32 nSize;                 /**< Size of the structure in bytes */
+    OMX_VERSIONTYPE nVersion;      /**< OMX specification version information */
+    OMX_U32 nPortIndex;            /**< Port number the structure applies to */
+    OMX_DIRTYPE eDir;              /**< Direction (input or output) of this port */
+    OMX_U32 nBufferCountActual;    /**< The actual number of buffers allocated on this port */
+    OMX_U32 nBufferCountMin;       /**< The minimum number of buffers this port requires */
+    OMX_U32 nBufferSize;           /**< Size, in bytes, for buffers to be used for this channel */
+    OMX_BOOL bEnabled;             /**< Ports default to enabled and are enabled/disabled by
+                                        OMX_CommandPortEnable/OMX_CommandPortDisable.
+                                        When disabled a port is unpopulated. A disabled port
+                                        is not populated with buffers on a transition to IDLE. */
+    OMX_BOOL bPopulated;           /**< Port is populated with all of its buffers as indicated by
+                                        nBufferCountActual. A disabled port is always unpopulated.
+                                        An enabled port is populated on a transition to OMX_StateIdle
+                                        and unpopulated on a transition to loaded. */
+    OMX_PORTDOMAINTYPE eDomain;    /**< Domain of the port. Determines the contents of metadata below. */
+    union {
+        OMX_AUDIO_PORTDEFINITIONTYPE audio;
+        OMX_VIDEO_PORTDEFINITIONTYPE video;
+        OMX_IMAGE_PORTDEFINITIONTYPE image;
+        OMX_OTHER_PORTDEFINITIONTYPE other;
+    } format;
+    OMX_BOOL bBuffersContiguous;
+    OMX_U32 nBufferAlignment;
+} OMX_PARAM_PORTDEFINITIONTYPE;
+
+/** @ingroup comp */
+typedef struct OMX_PARAM_U32TYPE {
+    OMX_U32 nSize;                    /**< Size of this structure, in Bytes */
+    OMX_VERSIONTYPE nVersion;         /**< OMX specification version information */
+    OMX_U32 nPortIndex;               /**< port that this structure applies to */
+    OMX_U32 nU32;                     /**< U32 value */
+} OMX_PARAM_U32TYPE;
+
+/** @ingroup rpm */
+typedef enum OMX_SUSPENSIONPOLICYTYPE {
+    OMX_SuspensionDisabled, /**< No suspension; v1.0 behavior */
+    OMX_SuspensionEnabled,  /**< Suspension allowed */
+    OMX_SuspensionPolicyKhronosExtensions = 0x6F000000, /**< Reserved region for introducing Khronos Standard Extensions */
+    OMX_SuspensionPolicyStartUnused = 0x7F000000, /**< Reserved region for introducing Vendor Extensions */
+    OMX_SuspensionPolicyMax = 0x7fffffff
+} OMX_SUSPENSIONPOLICYTYPE;
+
+/** @ingroup rpm */
+typedef struct OMX_PARAM_SUSPENSIONPOLICYTYPE {
+    OMX_U32 nSize;
+    OMX_VERSIONTYPE nVersion;
+    OMX_SUSPENSIONPOLICYTYPE ePolicy;
+} OMX_PARAM_SUSPENSIONPOLICYTYPE;
+
+/** @ingroup rpm */
+typedef enum OMX_SUSPENSIONTYPE {
+    OMX_NotSuspended, /**< component is not suspended */
+    OMX_Suspended,    /**< component is suspended */
+    OMX_SuspensionKhronosExtensions = 0x6F000000, /**< Reserved region for introducing Khronos Standard Extensions */
+    OMX_SuspensionVendorStartUnused = 0x7F000000, /**< Reserved region for introducing Vendor Extensions */
+    OMX_SuspendMax = 0x7FFFFFFF
+} OMX_SUSPENSIONTYPE;
+
+/** @ingroup rpm */
+typedef struct OMX_PARAM_SUSPENSIONTYPE {
+    OMX_U32 nSize;
+    OMX_VERSIONTYPE nVersion;
+    OMX_SUSPENSIONTYPE eType;
+} OMX_PARAM_SUSPENSIONTYPE ;
+
+typedef struct OMX_CONFIG_BOOLEANTYPE {
+    OMX_U32 nSize;
+    OMX_VERSIONTYPE nVersion;
+    OMX_BOOL bEnabled;
+} OMX_CONFIG_BOOLEANTYPE;
+
+/* Parameter specifying the content uri to use. */
+/** @ingroup cp */
+typedef struct OMX_PARAM_CONTENTURITYPE {
+    OMX_U32 nSize;                      /**< size of the structure in bytes, including
+                                             actual URI name */
+    OMX_VERSIONTYPE nVersion;           /**< OMX specification version information */
+    OMX_U8 contentURI[1];               /**< The URI name */
+} OMX_PARAM_CONTENTURITYPE;
+
+/* Parameter specifying the pipe to use. */
+/** @ingroup cp */
+typedef struct OMX_PARAM_CONTENTPIPETYPE {
+    OMX_U32 nSize;              /**< size of the structure in bytes */
+    OMX_VERSIONTYPE nVersion;   /**< OMX specification version information */
+    OMX_HANDLETYPE hPipe;       /**< The pipe handle*/
+} OMX_PARAM_CONTENTPIPETYPE;
+
+/** @ingroup rpm */
+typedef struct OMX_RESOURCECONCEALMENTTYPE {
+    OMX_U32 nSize;             /**< size of the structure in bytes */
+    OMX_VERSIONTYPE nVersion;  /**< OMX specification version information */
+    OMX_BOOL bResourceConcealmentForbidden; /**< disallow the use of resource concealment
+                                            methods (like degrading algorithm quality to
+                                            lower resource consumption or functional bypass)
+                                            on a component as a resolution to resource conflicts. */
+} OMX_RESOURCECONCEALMENTTYPE;
+
+
+/** @ingroup metadata */
+typedef enum OMX_METADATACHARSETTYPE {
+    OMX_MetadataCharsetUnknown = 0,
+    OMX_MetadataCharsetASCII,
+    OMX_MetadataCharsetBinary,
+    OMX_MetadataCharsetCodePage1252,
+    OMX_MetadataCharsetUTF8,
+    OMX_MetadataCharsetJavaConformantUTF8,
+    OMX_MetadataCharsetUTF7,
+    OMX_MetadataCharsetImapUTF7,
+    OMX_MetadataCharsetUTF16LE,
+    OMX_MetadataCharsetUTF16BE,
+    OMX_MetadataCharsetGB12345,
+    OMX_MetadataCharsetHZGB2312,
+    OMX_MetadataCharsetGB2312,
+    OMX_MetadataCharsetGB18030,
+    OMX_MetadataCharsetGBK,
+    OMX_MetadataCharsetBig5,
+    OMX_MetadataCharsetISO88591,
+    OMX_MetadataCharsetISO88592,
+    OMX_MetadataCharsetISO88593,
+    OMX_MetadataCharsetISO88594,
+    OMX_MetadataCharsetISO88595,
+    OMX_MetadataCharsetISO88596,
+    OMX_MetadataCharsetISO88597,
+    OMX_MetadataCharsetISO88598,
+    OMX_MetadataCharsetISO88599,
+    OMX_MetadataCharsetISO885910,
+    OMX_MetadataCharsetISO885913,
+    OMX_MetadataCharsetISO885914,
+    OMX_MetadataCharsetISO885915,
+    OMX_MetadataCharsetShiftJIS,
+    OMX_MetadataCharsetISO2022JP,
+    OMX_MetadataCharsetISO2022JP1,
+    OMX_MetadataCharsetISOEUCJP,
+    OMX_MetadataCharsetSMS7Bit,
+    OMX_MetadataCharsetKhronosExtensions = 0x6F000000, /**< Reserved region for introducing Khronos Standard Extensions */
+    OMX_MetadataCharsetVendorStartUnused = 0x7F000000, /**< Reserved region for introducing Vendor Extensions */
+    OMX_MetadataCharsetTypeMax = 0x7FFFFFFF
+} OMX_METADATACHARSETTYPE;
+
+/** @ingroup metadata */
+typedef enum OMX_METADATASCOPETYPE {
+    OMX_MetadataScopeAllLevels,
+    OMX_MetadataScopeTopLevel,
+    OMX_MetadataScopePortLevel,
+    OMX_MetadataScopeNodeLevel,
+    OMX_MetadataScopeKhronosExtensions = 0x6F000000, /**< Reserved region for introducing Khronos Standard Extensions */
+    OMX_MetadataScopeVendorStartUnused = 0x7F000000, /**< Reserved region for introducing Vendor Extensions */
+    OMX_MetadataScopeTypeMax = 0x7fffffff
+} OMX_METADATASCOPETYPE;
+
+/** @ingroup metadata */
+typedef enum OMX_METADATASEARCHMODETYPE {
+    OMX_MetadataSearchValueSizeByIndex,
+    OMX_MetadataSearchItemByIndex,
+    OMX_MetadataSearchNextItemByKey,
+    OMX_MetadataSearchKhronosExtensions = 0x6F000000, /**< Reserved region for introducing Khronos Standard Extensions */
+    OMX_MetadataSearchVendorStartUnused = 0x7F000000, /**< Reserved region for introducing Vendor Extensions */
+    OMX_MetadataSearchTypeMax = 0x7fffffff
+} OMX_METADATASEARCHMODETYPE;
+/** @ingroup metadata */
+typedef struct OMX_CONFIG_METADATAITEMCOUNTTYPE {
+    OMX_U32 nSize;
+    OMX_VERSIONTYPE nVersion;
+    OMX_METADATASCOPETYPE eScopeMode;
+    OMX_U32 nScopeSpecifier;
+    OMX_U32 nMetadataItemCount;
+} OMX_CONFIG_METADATAITEMCOUNTTYPE;
+
+/** @ingroup metadata */
+typedef struct OMX_CONFIG_METADATAITEMTYPE {
+    OMX_U32 nSize;
+    OMX_VERSIONTYPE nVersion;
+    OMX_METADATASCOPETYPE eScopeMode;
+    OMX_U32 nScopeSpecifier;
+    OMX_U32 nMetadataItemIndex;
+    OMX_METADATASEARCHMODETYPE eSearchMode;
+    OMX_METADATACHARSETTYPE eKeyCharset;
+    OMX_U8 nKeySizeUsed;
+    OMX_U8 nKey[128];
+    OMX_METADATACHARSETTYPE eValueCharset;
+    OMX_STRING sLanguageCountry;
+    OMX_U32 nValueMaxSize;
+    OMX_U32 nValueSizeUsed;
+    OMX_U8 nValue[1];
+} OMX_CONFIG_METADATAITEMTYPE;
+
+/* @ingroup metadata */
+typedef struct OMX_CONFIG_CONTAINERNODECOUNTTYPE {
+    OMX_U32 nSize;
+    OMX_VERSIONTYPE nVersion;
+    OMX_BOOL bAllKeys;
+    OMX_U32 nParentNodeID;
+    OMX_U32 nNumNodes;
+} OMX_CONFIG_CONTAINERNODECOUNTTYPE;
+
+/** @ingroup metadata */
+typedef struct OMX_CONFIG_CONTAINERNODEIDTYPE {
+    OMX_U32 nSize;
+    OMX_VERSIONTYPE nVersion;
+    OMX_BOOL bAllKeys;
+    OMX_U32 nParentNodeID;
+    OMX_U32 nNodeIndex;
+    OMX_U32 nNodeID;
+    OMX_STRING cNodeName;
+    OMX_BOOL bIsLeafType;
+} OMX_CONFIG_CONTAINERNODEIDTYPE;
+
+/** @ingroup metadata */
+typedef struct OMX_PARAM_METADATAFILTERTYPE {
+    OMX_U32 nSize;
+    OMX_VERSIONTYPE nVersion;
+    OMX_BOOL bAllKeys;  /* if true then this structure refers to all keys and
+                         * the three key fields below are ignored */
+    OMX_METADATACHARSETTYPE eKeyCharset;
+    OMX_U32 nKeySizeUsed;
+    OMX_U8   nKey [128];
+    OMX_U32 nLanguageCountrySizeUsed;
+    OMX_U8 nLanguageCountry[128];
+    OMX_BOOL bEnabled;  /* if true then key is part of filter (e.g.
+                         * retained for query later). If false then
+                         * key is not part of filter */
+} OMX_PARAM_METADATAFILTERTYPE;
+
+/** The OMX_HANDLETYPE structure defines the component handle.  The component
+ *  handle is used to access all of the component's public methods and also
+ *  contains pointers to the component's private data area.  The component
+ *  handle is initialized by the OMX core (with help from the component)
+ *  during the process of loading the component.  After the component is
+ *  successfully loaded, the application can safely access any of the
+ *  component's public functions (although some may return an error because
+ *  the state is inappropriate for the access).
+ *
+ *  @ingroup comp
+ */
+typedef struct OMX_COMPONENTTYPE {
+    /** The size of this structure, in bytes.  It is the responsibility
+        of the allocator of this structure to fill in this value.  Since
+        this structure is allocated by the GetHandle function, this
+        function will fill in this value. */
+    OMX_U32 nSize;
+
+    /** nVersion is the version of the OMX specification that the structure
+        is built against.  It is the responsibility of the creator of this
+        structure to initialize this value and every user of this structure
+        should verify that it knows how to use the exact version of
+        this structure found herein. */
+    OMX_VERSIONTYPE nVersion;
+
+    /** pComponentPrivate is a pointer to the component private data area.
+        This member is allocated and initialized by the component when the
+        component is first loaded.  The application should not access this
+        data area. */
+    OMX_PTR pComponentPrivate;
+
+    /** pApplicationPrivate is a pointer that is a parameter to the
+        OMX_GetHandle method, and contains an application private value
+        provided by the IL client.  This application private data is
+        returned to the IL Client by OMX in all callbacks */
+    OMX_PTR pApplicationPrivate;
+
+    /** refer to OMX_GetComponentVersion in OMX_core.h or the OMX IL
+        specification for details on the GetComponentVersion method.
+     */
+    OMX_ERRORTYPE (*GetComponentVersion)(
+        OMX_IN  OMX_HANDLETYPE hComponent,
+        OMX_OUT OMX_STRING pComponentName,
+        OMX_OUT OMX_VERSIONTYPE* pComponentVersion,
+        OMX_OUT OMX_VERSIONTYPE* pSpecVersion,
+        OMX_OUT OMX_UUIDTYPE* pComponentUUID);
+
+    /** refer to OMX_SendCommand in OMX_core.h or the OMX IL
+        specification for details on the SendCommand method.
+     */
+    OMX_ERRORTYPE (*SendCommand)(
+        OMX_IN  OMX_HANDLETYPE hComponent,
+        OMX_IN  OMX_COMMANDTYPE Cmd,
+        OMX_IN  OMX_U32 nParam1,
+        OMX_IN  OMX_PTR pCmdData);
+
+    /** refer to OMX_GetParameter in OMX_core.h or the OMX IL
+        specification for details on the GetParameter method.
+     */
+    OMX_ERRORTYPE (*GetParameter)(
+        OMX_IN  OMX_HANDLETYPE hComponent,
+        OMX_IN  OMX_INDEXTYPE nParamIndex,
+        OMX_INOUT OMX_PTR pComponentParameterStructure);
+
+
+    /** refer to OMX_SetParameter in OMX_core.h or the OMX IL
+        specification for details on the SetParameter method.
+     */
+    OMX_ERRORTYPE (*SetParameter)(
+        OMX_IN  OMX_HANDLETYPE hComponent,
+        OMX_IN  OMX_INDEXTYPE nIndex,
+        OMX_IN  OMX_PTR pComponentParameterStructure);
+
+
+    /** refer to OMX_GetConfig in OMX_core.h or the OMX IL
+        specification for details on the GetConfig method.
+     */
+    OMX_ERRORTYPE (*GetConfig)(
+        OMX_IN  OMX_HANDLETYPE hComponent,
+        OMX_IN  OMX_INDEXTYPE nIndex,
+        OMX_INOUT OMX_PTR pComponentConfigStructure);
+
+
+    /** refer to OMX_SetConfig in OMX_core.h or the OMX IL
+        specification for details on the SetConfig method.
+     */
+    OMX_ERRORTYPE (*SetConfig)(
+        OMX_IN  OMX_HANDLETYPE hComponent,
+        OMX_IN  OMX_INDEXTYPE nIndex,
+        OMX_IN  OMX_PTR pComponentConfigStructure);
+
+
+    /** refer to OMX_GetExtensionIndex in OMX_core.h or the OMX IL
+        specification for details on the GetExtensionIndex method.
+     */
+    OMX_ERRORTYPE (*GetExtensionIndex)(
+        OMX_IN  OMX_HANDLETYPE hComponent,
+        OMX_IN  OMX_STRING cParameterName,
+        OMX_OUT OMX_INDEXTYPE* pIndexType);
+
+
+    /** refer to OMX_GetState in OMX_core.h or the OMX IL
+        specification for details on the GetState method.
+     */
+    OMX_ERRORTYPE (*GetState)(
+        OMX_IN  OMX_HANDLETYPE hComponent,
+        OMX_OUT OMX_STATETYPE* pState);
+
+
+    /** The ComponentTunnelRequest method will interact with another OMX
+        component to determine if tunneling is possible and to setup the
+        tunneling.  The return codes for this method can be used to
+        determine if tunneling is not possible, or if tunneling is not
+        supported.
+
+        Base profile components (i.e. non-interop) do not support this
+        method and should return OMX_ErrorNotImplemented
+
+        The interop profile component MUST support tunneling to another
+        interop profile component with a compatible port parameters.
+        A component may also support proprietary communication.
+
+        If proprietary communication is supported the negotiation of
+        proprietary communication is done outside of OMX in a vendor
+        specific way. It is only required that the proper result be
+        returned and the details of how the setup is done is left
+        to the component implementation.
+
+        When this method is invoked when nPort in an output port, the
+        component will:
+        1.  Populate the pTunnelSetup structure with the output port's
+            requirements and constraints for the tunnel.
+
+        When this method is invoked when nPort in an input port, the
+        component will:
+        1.  Query the necessary parameters from the output port to
+            determine if the ports are compatible for tunneling
+        2.  If the ports are compatible, the component should store
+            the tunnel step provided by the output port
+        3.  Determine which port (either input or output) is the buffer
+            supplier, and call OMX_SetParameter on the output port to
+            indicate this selection.
+
+        The component will return from this call within 5 msec.
+
+        @param [in] hComp
+            Handle of the component to be accessed.  This is the component
+            handle returned by the call to the OMX_GetHandle method.
+        @param [in] nPort
+            nPort is used to select the port on the component to be used
+            for tunneling.
+        @param [in] hTunneledComp
+            Handle of the component to tunnel with.  This is the component
+            handle returned by the call to the OMX_GetHandle method.  When
+            this parameter is 0x0 the component should setup the port for
+            communication with the application / IL Client.
+        @param [in] nPortOutput
+            nPortOutput is used indicate the port the component should
+            tunnel with.
+        @param [in] pTunnelSetup
+            Pointer to the tunnel setup structure.  When nPort is an output port
+            the component should populate the fields of this structure.  When
+            When nPort is an input port the component should review the setup
+            provided by the component with the output port.
+        @return OMX_ERRORTYPE
+            If the command successfully executes, the return code will be
+            OMX_ErrorNone.  Otherwise the appropriate OMX error will be returned.
+        @ingroup tun
+    */
+
+    OMX_ERRORTYPE (*ComponentTunnelRequest)(
+        OMX_IN  OMX_HANDLETYPE hComp,
+        OMX_IN  OMX_U32 nPort,
+        OMX_IN  OMX_HANDLETYPE hTunneledComp,
+        OMX_IN  OMX_U32 nTunneledPort,
+        OMX_INOUT  OMX_TUNNELSETUPTYPE* pTunnelSetup);
+
+    /** refer to OMX_UseBuffer in OMX_core.h or the OMX IL
+        specification for details on the UseBuffer method.
+        @ingroup buf
+     */
+    OMX_ERRORTYPE (*UseBuffer)(
+        OMX_IN OMX_HANDLETYPE hComponent,
+        OMX_INOUT OMX_BUFFERHEADERTYPE** ppBufferHdr,
+        OMX_IN OMX_U32 nPortIndex,
+        OMX_IN OMX_PTR pAppPrivate,
+        OMX_IN OMX_U32 nSizeBytes,
+        OMX_IN OMX_U8* pBuffer);
+
+    /** refer to OMX_AllocateBuffer in OMX_core.h or the OMX IL
+        specification for details on the AllocateBuffer method.
+        @ingroup buf
+     */
+    OMX_ERRORTYPE (*AllocateBuffer)(
+        OMX_IN OMX_HANDLETYPE hComponent,
+        OMX_INOUT OMX_BUFFERHEADERTYPE** ppBuffer,
+        OMX_IN OMX_U32 nPortIndex,
+        OMX_IN OMX_PTR pAppPrivate,
+        OMX_IN OMX_U32 nSizeBytes);
+
+    /** refer to OMX_FreeBuffer in OMX_core.h or the OMX IL
+        specification for details on the FreeBuffer method.
+        @ingroup buf
+     */
+    OMX_ERRORTYPE (*FreeBuffer)(
+        OMX_IN  OMX_HANDLETYPE hComponent,
+        OMX_IN  OMX_U32 nPortIndex,
+        OMX_IN  OMX_BUFFERHEADERTYPE* pBuffer);
+
+    /** refer to OMX_EmptyThisBuffer in OMX_core.h or the OMX IL
+        specification for details on the EmptyThisBuffer method.
+        @ingroup buf
+     */
+    OMX_ERRORTYPE (*EmptyThisBuffer)(
+        OMX_IN  OMX_HANDLETYPE hComponent,
+        OMX_IN  OMX_BUFFERHEADERTYPE* pBuffer);
+
+    /** refer to OMX_FillThisBuffer in OMX_core.h or the OMX IL
+        specification for details on the FillThisBuffer method.
+        @ingroup buf
+     */
+    OMX_ERRORTYPE (*FillThisBuffer)(
+        OMX_IN  OMX_HANDLETYPE hComponent,
+        OMX_IN  OMX_BUFFERHEADERTYPE* pBuffer);
+
+    /** The SetCallbacks method is used by the core to specify the callback
+        structure from the application to the component.  This is a blocking
+        call.  The component will return from this call within 5 msec.
+        @param [in] hComponent
+            Handle of the component to be accessed.  This is the component
+            handle returned by the call to the GetHandle function.
+        @param [in] pCallbacks
+            pointer to an OMX_CALLBACKTYPE structure used to provide the
+            callback information to the component
+        @param [in] pAppData
+            pointer to an application defined value.  It is anticipated that
+            the application will pass a pointer to a data structure or a "this
+            pointer" in this area to allow the callback (in the application)
+            to determine the context of the call
+        @return OMX_ERRORTYPE
+            If the command successfully executes, the return code will be
+            OMX_ErrorNone.  Otherwise the appropriate OMX error will be returned.
+     */
+    OMX_ERRORTYPE (*SetCallbacks)(
+        OMX_IN  OMX_HANDLETYPE hComponent,
+        OMX_IN  OMX_CALLBACKTYPE* pCallbacks,
+        OMX_IN  OMX_PTR pAppData);
+
+    /** ComponentDeInit method is used to deinitialize the component
+        providing a means to free any resources allocated at component
+        initialization.  NOTE:  After this call the component handle is
+        not valid for further use.
+        @param [in] hComponent
+            Handle of the component to be accessed.  This is the component
+            handle returned by the call to the GetHandle function.
+        @return OMX_ERRORTYPE
+            If the command successfully executes, the return code will be
+            OMX_ErrorNone.  Otherwise the appropriate OMX error will be returned.
+     */
+    OMX_ERRORTYPE (*ComponentDeInit)(
+        OMX_IN  OMX_HANDLETYPE hComponent);
+
+    /** @ingroup buf */
+    OMX_ERRORTYPE (*UseEGLImage)(
+        OMX_IN OMX_HANDLETYPE hComponent,
+        OMX_INOUT OMX_BUFFERHEADERTYPE** ppBufferHdr,
+        OMX_IN OMX_U32 nPortIndex,
+        OMX_IN OMX_PTR pAppPrivate,
+        OMX_IN void* eglImage);
+
+    OMX_ERRORTYPE (*ComponentRoleEnum)(
+        OMX_IN OMX_HANDLETYPE hComponent,
+        OMX_OUT OMX_U8 *cRole,
+        OMX_IN OMX_U32 nIndex);
+
+} OMX_COMPONENTTYPE;
+
+#ifdef __cplusplus
+}
+#endif /* __cplusplus */
+
+#endif
+/* File EOF */
diff --git a/sf-extra/omx-il/OMX_ComponentExt.h b/sf-extra/omx-il/OMX_ComponentExt.h
new file mode 100644
index 00000000..24ec20c5
--- /dev/null
+++ b/sf-extra/omx-il/OMX_ComponentExt.h
@@ -0,0 +1,61 @@
+/*
+ * Copyright (c) 2016 The Khronos Group Inc.
+ *
+ * Permission is hereby granted, free of charge, to any person obtaining
+ * a copy of this software and associated documentation files (the
+ * "Software"), to deal in the Software without restriction, including
+ * without limitation the rights to use, copy, modify, merge, publish,
+ * distribute, sublicense, and/or sell copies of the Software, and to
+ * permit persons to whom the Software is furnished to do so, subject
+ * to the following conditions:
+ * The above copyright notice and this permission notice shall be included
+ * in all copies or substantial portions of the Software.
+ *
+ * THE SOFTWARE IS PROVIDED "AS IS", WITHOUT WARRANTY OF ANY KIND, EXPRESS
+ * OR IMPLIED, INCLUDING BUT NOT LIMITED TO THE WARRANTIES OF
+ * MERCHANTABILITY, FITNESS FOR A PARTICULAR PURPOSE AND NONINFRINGEMENT.
+ * IN NO EVENT SHALL THE AUTHORS OR COPYRIGHT HOLDERS BE LIABLE FOR ANY
+ * CLAIM, DAMAGES OR OTHER LIABILITY, WHETHER IN AN ACTION OF CONTRACT,
+ * TORT OR OTHERWISE, ARISING FROM, OUT OF OR IN CONNECTION WITH THE
+ * SOFTWARE OR THE USE OR OTHER DEALINGS IN THE SOFTWARE.
+ *
+ */
+
+/** OMX_ComponentExt.h - OpenMax IL version 1.1.2
+ * The OMX_ComponentExt header file contains extensions to the definitions used
+ * by both the application and the component to access common items.
+ */
+
+#ifndef OMX_ComponentExt_h
+#define OMX_ComponentExt_h
+
+#ifdef __cplusplus
+extern "C" {
+#endif /* __cplusplus */
+
+/* Each OMX header must include all required header files to allow the
+ * header to compile without errors.  The includes below are required
+ * for this header file to compile successfully 
+ */
+#include <OMX_Types.h>
+
+
+/** Set/query the commit mode */
+typedef struct OMX_CONFIG_COMMITMODETYPE {
+    OMX_U32 nSize;
+    OMX_VERSIONTYPE nVersion;
+    OMX_BOOL bDeferred;
+} OMX_CONFIG_COMMITMODETYPE;
+
+/** Explicit commit */
+typedef struct OMX_CONFIG_COMMITTYPE {
+    OMX_U32 nSize;
+    OMX_VERSIONTYPE nVersion;
+} OMX_CONFIG_COMMITTYPE;
+
+
+#ifdef __cplusplus
+}
+#endif /* __cplusplus */
+
+#endif /* OMX_ComponentExt_h */
diff --git a/sf-extra/omx-il/OMX_ContentPipe.h b/sf-extra/omx-il/OMX_ContentPipe.h
new file mode 100644
index 00000000..843cb7a4
--- /dev/null
+++ b/sf-extra/omx-il/OMX_ContentPipe.h
@@ -0,0 +1,193 @@
+/*
+ * Copyright (c) 2008 The Khronos Group Inc.
+ *
+ * Permission is hereby granted, free of charge, to any person obtaining
+ * a copy of this software and associated documentation files (the
+ * "Software"), to deal in the Software without restriction, including
+ * without limitation the rights to use, copy, modify, merge, publish,
+ * distribute, sublicense, and/or sell copies of the Software, and to
+ * permit persons to whom the Software is furnished to do so, subject
+ * to the following conditions:
+ * The above copyright notice and this permission notice shall be included
+ * in all copies or substantial portions of the Software.
+ *
+ * THE SOFTWARE IS PROVIDED "AS IS", WITHOUT WARRANTY OF ANY KIND, EXPRESS
+ * OR IMPLIED, INCLUDING BUT NOT LIMITED TO THE WARRANTIES OF
+ * MERCHANTABILITY, FITNESS FOR A PARTICULAR PURPOSE AND NONINFRINGEMENT.
+ * IN NO EVENT SHALL THE AUTHORS OR COPYRIGHT HOLDERS BE LIABLE FOR ANY
+ * CLAIM, DAMAGES OR OTHER LIABILITY, WHETHER IN AN ACTION OF CONTRACT,
+ * TORT OR OTHERWISE, ARISING FROM, OUT OF OR IN CONNECTION WITH THE
+ * SOFTWARE OR THE USE OR OTHER DEALINGS IN THE SOFTWARE.
+ *
+ */
+
+/** OMX_ContentPipe.h - OpenMax IL version 1.1.2
+ *  The OMX_ContentPipe header file contains the definitions used to define
+ *  the public interface for content piples.  This header file is intended to
+ *  be used by the component.
+ */
+
+#ifndef OMX_CONTENTPIPE_H
+#define OMX_CONTENTPIPE_H
+
+#ifndef KD_EACCES
+/* OpenKODE error codes. CPResult values may be zero (indicating success
+   or one of the following values) */
+#define KD_EACCES (1)
+#define KD_EADDRINUSE (2)
+#define KD_EAGAIN (5)
+#define KD_EBADF (7)
+#define KD_EBUSY (8)
+#define KD_ECONNREFUSED (9)
+#define KD_ECONNRESET (10)
+#define KD_EDEADLK (11)
+#define KD_EDESTADDRREQ (12)
+#define KD_ERANGE (35)
+#define KD_EEXIST (13)
+#define KD_EFBIG (14)
+#define KD_EHOSTUNREACH (15)
+#define KD_EINVAL (17)
+#define KD_EIO (18)
+#define KD_EISCONN (20)
+#define KD_EISDIR (21)
+#define KD_EMFILE (22)
+#define KD_ENAMETOOLONG (23)
+#define KD_ENOENT (24)
+#define KD_ENOMEM (25)
+#define KD_ENOSPC (26)
+#define KD_ENOSYS (27)
+#define KD_ENOTCONN (28)
+#define KD_EPERM (33)
+#define KD_ETIMEDOUT (36)
+#define KD_EILSEQ (19)
+#endif
+
+/** Map types from OMX standard types only here so interface is as generic as possible. */
+typedef OMX_U32    CPresult;
+typedef char *     CPstring;
+typedef void *     CPhandle;
+typedef OMX_U32    CPuint;
+typedef OMX_S32    CPint;
+typedef char       CPbyte;
+typedef OMX_BOOL   CPbool;
+
+/** enumeration of origin types used in the CP_PIPETYPE's Seek function
+ * @ingroup cp
+ */
+typedef enum CP_ORIGINTYPE {
+    CP_OriginBegin,
+    CP_OriginCur,
+    CP_OriginEnd,
+    CP_OriginKhronosExtensions = 0x6F000000, /**< Reserved region for introducing Khronos Standard Extensions */
+    CP_OriginVendorStartUnused = 0x7F000000, /**< Reserved region for introducing Vendor Extensions */
+    CP_OriginMax = 0X7FFFFFFF
+} CP_ORIGINTYPE;
+
+/** enumeration of contact access types used in the CP_PIPETYPE's Open function
+ * @ingroup cp
+ */
+typedef enum CP_ACCESSTYPE {
+    CP_AccessRead,
+    CP_AccessWrite,
+    CP_AccessReadWrite ,
+    CP_AccessKhronosExtensions = 0x6F000000, /**< Reserved region for introducing Khronos Standard Extensions */
+    CP_AccessVendorStartUnused = 0x7F000000, /**< Reserved region for introducing Vendor Extensions */
+    CP_AccessMax = 0X7FFFFFFF
+} CP_ACCESSTYPE;
+
+/** enumeration of results returned by the CP_PIPETYPE's CheckAvailableBytes function
+ * @ingroup cp
+ */
+typedef enum CP_CHECKBYTESRESULTTYPE {
+    CP_CheckBytesOk,                    /**< There are at least the request number
+                                              of bytes available */
+    CP_CheckBytesNotReady,              /**< The pipe is still retrieving bytes
+                                              and presently lacks sufficient bytes.
+                                              Client will be called when they are
+                                              sufficient bytes are available. */
+    CP_CheckBytesInsufficientBytes  ,     /**< The pipe has retrieved all bytes
+                                              but those available are less than those
+                                              requested */
+    CP_CheckBytesAtEndOfStream,         /**< The pipe has reached the end of stream
+                                              and no more bytes are available. */
+    CP_CheckBytesOutOfBuffers,          /**< All read/write buffers are currently in use. */
+    CP_CheckBytesKhronosExtensions = 0x6F000000, /**< Reserved region for introducing Khronos Standard Extensions */
+    CP_CheckBytesVendorStartUnused = 0x7F000000, /**< Reserved region for introducing Vendor Extensions */
+    CP_CheckBytesMax = 0X7FFFFFFF
+} CP_CHECKBYTESRESULTTYPE;
+
+/** enumeration of content pipe events sent to the client callback.
+ * @ingroup cp
+ */
+typedef enum CP_EVENTTYPE {
+    CP_BytesAvailable,              /** bytes requested in a CheckAvailableBytes call are now available*/
+    CP_Overflow,                   /** enumeration of content pipe events sent to the client callback*/
+    CP_PipeDisconnected  ,              /** enumeration of content pipe events sent to the client callback*/
+    CP_EventKhronosExtensions = 0x6F000000, /**< Reserved region for introducing Khronos Standard Extensions */
+    CP_EventVendorStartUnused = 0x7F000000, /**< Reserved region for introducing Vendor Extensions */
+    CP_EventMax = 0X7FFFFFFF
+} CP_EVENTTYPE;
+
+/** content pipe definition
+ * @ingroup cp
+ */
+typedef struct CP_PIPETYPE {
+    /** Open a content stream for reading or writing. */
+    CPresult (*Open)( CPhandle* hContent, CPstring szURI, CP_ACCESSTYPE eAccess );
+
+    /** Close a content stream. */
+    CPresult (*Close)( CPhandle hContent );
+
+    /** Create a content source and open it for writing. */
+    CPresult (*Create)( CPhandle *hContent, CPstring szURI );
+
+    /** Check the that specified number of bytes are available for reading or writing (depending on access type).*/
+    CPresult (*CheckAvailableBytes)( CPhandle hContent, CPuint nBytesRequested, CP_CHECKBYTESRESULTTYPE *eResult );
+
+    /** Seek to certain position in the content relative to the specified origin. */
+    CPresult (*SetPosition)( CPhandle  hContent, CPint nOffset, CP_ORIGINTYPE eOrigin);
+
+    /** Retrieve the current position relative to the start of the content. */
+    CPresult (*GetPosition)( CPhandle hContent, CPuint *pPosition);
+
+    /** Retrieve data of the specified size from the content stream (advance content pointer by size of data).
+       Note: pipe client provides pointer. This function is appropriate for small high frequency reads. */
+    CPresult (*Read)( CPhandle hContent, CPbyte *pData, CPuint nSize);
+
+    /** Retrieve a buffer allocated by the pipe that contains the requested number of bytes.
+       Buffer contains the next block of bytes, as specified by nSize, of the content. nSize also
+       returns the size of the block actually read. Content pointer advances the by the returned size.
+       Note: pipe provides pointer. This function is appropriate for large reads. The client must call
+       ReleaseReadBuffer when done with buffer.
+
+       In some cases the requested block may not reside in contiguous memory within the
+       pipe implementation. For instance if the pipe leverages a circular buffer then the requested
+       block may straddle the boundary of the circular buffer. By default a pipe implementation
+       performs a copy in this case to provide the block to the pipe client in one contiguous buffer.
+       If, however, the client sets bForbidCopy, then the pipe returns only those bytes preceding the memory
+       boundary. Here the client may retrieve the data in segments over successive calls. */
+    CPresult (*ReadBuffer)( CPhandle hContent, CPbyte **ppBuffer, CPuint *nSize, CPbool bForbidCopy);
+
+    /** Release a buffer obtained by ReadBuffer back to the pipe. */
+    CPresult (*ReleaseReadBuffer)(CPhandle hContent, CPbyte *pBuffer);
+
+    /** Write data of the specified size to the content (advance content pointer by size of data).
+       Note: pipe client provides pointer. This function is appropriate for small high frequency writes. */
+    CPresult (*Write)( CPhandle hContent, CPbyte *data, CPuint nSize);
+
+    /** Retrieve a buffer allocated by the pipe used to write data to the content.
+       Client will fill buffer with output data. Note: pipe provides pointer. This function is appropriate
+       for large writes. The client must call WriteBuffer when done it has filled the buffer with data.*/
+    CPresult (*GetWriteBuffer)( CPhandle hContent, CPbyte **ppBuffer, CPuint nSize);
+
+    /** Deliver a buffer obtained via GetWriteBuffer to the pipe. Pipe will write the
+       the contents of the buffer to content and advance content pointer by the size of the buffer */
+    CPresult (*WriteBuffer)( CPhandle hContent, CPbyte *pBuffer, CPuint nFilledSize);
+
+    /** Register a per-handle client callback with the content pipe. */
+    CPresult (*RegisterCallback)( CPhandle hContent, CPresult (*ClientCallback)(CP_EVENTTYPE eEvent, CPuint iParam));
+
+} CP_PIPETYPE;
+
+#endif
+
diff --git a/sf-extra/omx-il/OMX_Core.h b/sf-extra/omx-il/OMX_Core.h
new file mode 100644
index 00000000..c8f3c4b3
--- /dev/null
+++ b/sf-extra/omx-il/OMX_Core.h
@@ -0,0 +1,1422 @@
+/*
+ * Copyright (c) 2008 The Khronos Group Inc.
+ *
+ * Permission is hereby granted, free of charge, to any person obtaining
+ * a copy of this software and associated documentation files (the
+ * "Software"), to deal in the Software without restriction, including
+ * without limitation the rights to use, copy, modify, merge, publish,
+ * distribute, sublicense, and/or sell copies of the Software, and to
+ * permit persons to whom the Software is furnished to do so, subject
+ * to the following conditions:
+ * The above copyright notice and this permission notice shall be included
+ * in all copies or substantial portions of the Software.
+ *
+ * THE SOFTWARE IS PROVIDED "AS IS", WITHOUT WARRANTY OF ANY KIND, EXPRESS
+ * OR IMPLIED, INCLUDING BUT NOT LIMITED TO THE WARRANTIES OF
+ * MERCHANTABILITY, FITNESS FOR A PARTICULAR PURPOSE AND NONINFRINGEMENT.
+ * IN NO EVENT SHALL THE AUTHORS OR COPYRIGHT HOLDERS BE LIABLE FOR ANY
+ * CLAIM, DAMAGES OR OTHER LIABILITY, WHETHER IN AN ACTION OF CONTRACT,
+ * TORT OR OTHERWISE, ARISING FROM, OUT OF OR IN CONNECTION WITH THE
+ * SOFTWARE OR THE USE OR OTHER DEALINGS IN THE SOFTWARE.
+ *
+ */
+
+/** OMX_Core.h - OpenMax IL version 1.1.2
+ *  The OMX_Core header file contains the definitions used by both the
+ *  application and the component to access common items.
+ */
+
+#ifndef OMX_Core_h
+#define OMX_Core_h
+
+#ifdef __cplusplus
+extern "C" {
+#endif /* __cplusplus */
+
+
+/* Each OMX header shall include all required header files to allow the
+ *  header to compile without errors.  The includes below are required
+ *  for this header file to compile successfully
+ */
+
+#include <OMX_Index.h>
+
+
+/** The OMX_COMMANDTYPE enumeration is used to specify the action in the
+ *  OMX_SendCommand macro.
+ *  @ingroup core
+ */
+typedef enum OMX_COMMANDTYPE
+{
+    OMX_CommandStateSet,    /**< Change the component state */
+    OMX_CommandFlush,       /**< Flush the data queue(s) of a component */
+    OMX_CommandPortDisable, /**< Disable a port on a component. */
+    OMX_CommandPortEnable,  /**< Enable a port on a component. */
+    OMX_CommandMarkBuffer,  /**< Mark a component/buffer for observation */
+    OMX_CommandKhronosExtensions = 0x6F000000, /**< Reserved region for introducing Khronos Standard Extensions */
+    OMX_CommandVendorStartUnused = 0x7F000000, /**< Reserved region for introducing Vendor Extensions */
+    OMX_CommandMax = 0X7FFFFFFF
+} OMX_COMMANDTYPE;
+
+
+
+/** The OMX_STATETYPE enumeration is used to indicate or change the component
+ *  state.  This enumeration reflects the current state of the component when
+ *  used with the OMX_GetState macro or becomes the parameter in a state change
+ *  command when used with the OMX_SendCommand macro.
+ *
+ *  The component will be in the Loaded state after the component is initially
+ *  loaded into memory.  In the Loaded state, the component is not allowed to
+ *  allocate or hold resources other than to build it's internal parameter
+ *  and configuration tables.  The application will send one or more
+ *  SetParameters/GetParameters and SetConfig/GetConfig commands to the
+ *  component and the component will record each of these parameter and
+ *  configuration changes for use later.  When the application sends the
+ *  Idle command, the component will acquire the resources needed for the
+ *  specified configuration and will transition to the idle state if the
+ *  allocation is successful.  If the component cannot successfully
+ *  transition to the idle state for any reason, the state of the component
+ *  shall be fully rolled back to the Loaded state (e.g. all allocated
+ *  resources shall be released).  When the component receives the command
+ *  to go to the Executing state, it shall begin processing buffers by
+ *  sending all input buffers it holds to the application.  While
+ *  the component is in the Idle state, the application may also send the
+ *  Pause command.  If the component receives the pause command while in the
+ *  Idle state, the component shall send all input buffers it holds to the
+ *  application, but shall not begin processing buffers.  This will allow the
+ *  application to prefill buffers.
+ *
+ *  @ingroup comp
+ */
+
+typedef enum OMX_STATETYPE {
+    OMX_StateInvalid,      /**< component has detected that it's internal data
+                                structures are corrupted to the point that
+                                it cannot determine it's state properly */
+    OMX_StateLoaded,      /**< component has been loaded but has not completed
+                                initialization.  The OMX_SetParameter macro
+                                and the OMX_GetParameter macro are the only
+                                valid macros allowed to be sent to the
+                                component in this state. */
+    OMX_StateIdle,        /**< component initialization has been completed
+                                successfully and the component is ready to
+                                to start. */
+    OMX_StateExecuting,   /**< component has accepted the start command and
+                                is processing data (if data is available) */
+    OMX_StatePause,       /**< component has received pause command */
+    OMX_StateWaitForResources, /**< component is waiting for resources, either after
+                                preemption or before it gets the resources requested.
+                                See specification for complete details. */
+    OMX_StateKhronosExtensions = 0x6F000000, /**< Reserved region for introducing Khronos Standard Extensions */
+    OMX_StateVendorStartUnused = 0x7F000000, /**< Reserved region for introducing Vendor Extensions */
+    OMX_StateMax = 0X7FFFFFFF
+} OMX_STATETYPE;
+
+/** The OMX_ERRORTYPE enumeration defines the standard OMX Errors.  These
+ *  errors should cover most of the common failure cases.  However,
+ *  vendors are free to add additional error messages of their own as
+ *  long as they follow these rules:
+ *  1.  Vendor error messages shall be in the range of 0x90000000 to
+ *      0x9000FFFF.
+ *  2.  Vendor error messages shall be defined in a header file provided
+ *      with the component.  No error messages are allowed that are
+ *      not defined.
+ */
+typedef enum OMX_ERRORTYPE {
+    OMX_ErrorNone = 0,
+
+    /** There were insufficient resources to perform the requested operation */
+    OMX_ErrorInsufficientResources = (OMX_S32) 0x80001000,
+
+    /** There was an error, but the cause of the error could not be determined */
+    OMX_ErrorUndefined = (OMX_S32) 0x80001001,
+
+    /** The component name string was not valid */
+    OMX_ErrorInvalidComponentName = (OMX_S32) 0x80001002,
+
+    /** No component with the specified name string was found */
+    OMX_ErrorComponentNotFound = (OMX_S32) 0x80001003,
+
+    /** The component specified did not have a "OMX_ComponentInit" or
+        "OMX_ComponentDeInit entry point */
+    OMX_ErrorInvalidComponent = (OMX_S32) 0x80001004,
+
+    /** One or more parameters were not valid */
+    OMX_ErrorBadParameter = (OMX_S32) 0x80001005,
+
+    /** The requested function is not implemented */
+    OMX_ErrorNotImplemented = (OMX_S32) 0x80001006,
+
+    /** The buffer was emptied before the next buffer was ready */
+    OMX_ErrorUnderflow = (OMX_S32) 0x80001007,
+
+    /** The buffer was not available when it was needed */
+    OMX_ErrorOverflow = (OMX_S32) 0x80001008,
+
+    /** The hardware failed to respond as expected */
+    OMX_ErrorHardware = (OMX_S32) 0x80001009,
+
+    /** The component is in the state OMX_StateInvalid */
+    OMX_ErrorInvalidState = (OMX_S32) 0x8000100A,
+
+    /** Stream is found to be corrupt */
+    OMX_ErrorStreamCorrupt = (OMX_S32) 0x8000100B,
+
+    /** Ports being connected are not compatible */
+    OMX_ErrorPortsNotCompatible = (OMX_S32) 0x8000100C,
+
+    /** Resources allocated to an idle component have been
+        lost resulting in the component returning to the loaded state */
+    OMX_ErrorResourcesLost = (OMX_S32) 0x8000100D,
+
+    /** No more indicies can be enumerated */
+    OMX_ErrorNoMore = (OMX_S32) 0x8000100E,
+
+    /** The component detected a version mismatch */
+    OMX_ErrorVersionMismatch = (OMX_S32) 0x8000100F,
+
+    /** The component is not ready to return data at this time */
+    OMX_ErrorNotReady = (OMX_S32) 0x80001010,
+
+    /** There was a timeout that occurred */
+    OMX_ErrorTimeout = (OMX_S32) 0x80001011,
+
+    /** This error occurs when trying to transition into the state you are already in */
+    OMX_ErrorSameState = (OMX_S32) 0x80001012,
+
+    /** Resources allocated to an executing or paused component have been
+        preempted, causing the component to return to the idle state */
+    OMX_ErrorResourcesPreempted = (OMX_S32) 0x80001013,
+
+    /** A non-supplier port sends this error to the IL client (via the EventHandler callback)
+        during the allocation of buffers (on a transition from the LOADED to the IDLE state or
+        on a port restart) when it deems that it has waited an unusually long time for the supplier
+        to send it an allocated buffer via a UseBuffer call. */
+    OMX_ErrorPortUnresponsiveDuringAllocation = (OMX_S32) 0x80001014,
+
+    /** A non-supplier port sends this error to the IL client (via the EventHandler callback)
+        during the deallocation of buffers (on a transition from the IDLE to LOADED state or
+        on a port stop) when it deems that it has waited an unusually long time for the supplier
+        to request the deallocation of a buffer header via a FreeBuffer call. */
+    OMX_ErrorPortUnresponsiveDuringDeallocation = (OMX_S32) 0x80001015,
+
+    /** A supplier port sends this error to the IL client (via the EventHandler callback)
+        during the stopping of a port (either on a transition from the IDLE to LOADED
+        state or a port stop) when it deems that it has waited an unusually long time for
+        the non-supplier to return a buffer via an EmptyThisBuffer or FillThisBuffer call. */
+    OMX_ErrorPortUnresponsiveDuringStop = (OMX_S32) 0x80001016,
+
+    /** Attempting a state transtion that is not allowed */
+    OMX_ErrorIncorrectStateTransition = (OMX_S32) 0x80001017,
+
+    /* Attempting a command that is not allowed during the present state. */
+    OMX_ErrorIncorrectStateOperation = (OMX_S32) 0x80001018,
+
+    /** The values encapsulated in the parameter or config structure are not supported. */
+    OMX_ErrorUnsupportedSetting = (OMX_S32) 0x80001019,
+
+    /** The parameter or config indicated by the given index is not supported. */
+    OMX_ErrorUnsupportedIndex = (OMX_S32) 0x8000101A,
+
+    /** The port index supplied is incorrect. */
+    OMX_ErrorBadPortIndex = (OMX_S32) 0x8000101B,
+
+    /** The port has lost one or more of its buffers and it thus unpopulated. */
+    OMX_ErrorPortUnpopulated = (OMX_S32) 0x8000101C,
+
+    /** Component suspended due to temporary loss of resources */
+    OMX_ErrorComponentSuspended = (OMX_S32) 0x8000101D,
+
+    /** Component suspended due to an inability to acquire dynamic resources */
+    OMX_ErrorDynamicResourcesUnavailable = (OMX_S32) 0x8000101E,
+
+    /** When the macroblock error reporting is enabled the component returns new error
+    for every frame that has errors */
+    OMX_ErrorMbErrorsInFrame = (OMX_S32) 0x8000101F,
+
+    /** A component reports this error when it cannot parse or determine the format of an input stream. */
+    OMX_ErrorFormatNotDetected = (OMX_S32) 0x80001020,
+
+    /** The content open operation failed. */
+    OMX_ErrorContentPipeOpenFailed = (OMX_S32) 0x80001021,
+
+    /** The content creation operation failed. */
+    OMX_ErrorContentPipeCreationFailed = (OMX_S32) 0x80001022,
+
+    /** Separate table information is being used */
+    OMX_ErrorSeperateTablesUsed = (OMX_S32) 0x80001023,
+
+    /** Tunneling is unsupported by the component*/
+    OMX_ErrorTunnelingUnsupported = (OMX_S32) 0x80001024,
+
+    OMX_ErrorKhronosExtensions = (OMX_S32)0x8F000000, /**< Reserved region for introducing Khronos Standard Extensions */
+    OMX_ErrorVendorStartUnused = (OMX_S32)0x90000000, /**< Reserved region for introducing Vendor Extensions */
+    OMX_ErrorMax = 0x7FFFFFFF
+} OMX_ERRORTYPE;
+
+/** @ingroup core */
+typedef OMX_ERRORTYPE (* OMX_COMPONENTINITTYPE)(OMX_IN  OMX_HANDLETYPE hComponent);
+
+/** @ingroup core */
+typedef struct OMX_COMPONENTREGISTERTYPE {
+    const char          * pName;       /* Component name, 128 byte limit (including '\0') applies */
+    OMX_COMPONENTINITTYPE pInitialize; /* Component instance initialization function */
+} OMX_COMPONENTREGISTERTYPE;
+
+/** @ingroup core */
+extern OMX_COMPONENTREGISTERTYPE OMX_ComponentRegistered[];
+
+/** @ingroup rpm */
+typedef struct OMX_PRIORITYMGMTTYPE {
+    OMX_U32 nSize;             /**< size of the structure in bytes */
+    OMX_VERSIONTYPE nVersion;  /**< OMX specification version information */
+    OMX_U32 nGroupPriority;            /**< Priority of the component group */
+    OMX_U32 nGroupID;                  /**< ID of the component group */
+} OMX_PRIORITYMGMTTYPE;
+
+/* Component name and Role names are limited to 128 characters including the terminating '\0'. */
+#define OMX_MAX_STRINGNAME_SIZE 128
+
+/** @ingroup comp */
+typedef struct OMX_PARAM_COMPONENTROLETYPE {
+    OMX_U32 nSize;              /**< size of the structure in bytes */
+    OMX_VERSIONTYPE nVersion;   /**< OMX specification version information */
+    OMX_U8 cRole[OMX_MAX_STRINGNAME_SIZE];  /**< name of standard component which defines component role */
+} OMX_PARAM_COMPONENTROLETYPE;
+
+/** End of Stream Buffer Flag:
+  *
+  * A component sets EOS when it has no more data to emit on a particular
+  * output port. Thus an output port shall set EOS on the last buffer it
+  * emits. A component's determination of when an output port should
+  * cease sending data is implemenation specific.
+  * @ingroup buf
+  */
+
+#define OMX_BUFFERFLAG_EOS 0x00000001
+
+/** Start Time Buffer Flag:
+ *
+ * The source of a stream (e.g. a demux component) sets the STARTTIME
+ * flag on the buffer that contains the starting timestamp for the
+ * stream. The starting timestamp corresponds to the first data that
+ * should be displayed at startup or after a seek.
+ * The first timestamp of the stream is not necessarily the start time.
+ * For instance, in the case of a seek to a particular video frame,
+ * the target frame may be an interframe. Thus the first buffer of
+ * the stream will be the intra-frame preceding the target frame and
+ * the starttime will occur with the target frame (with any other
+ * required frames required to reconstruct the target intervening).
+ *
+ * The STARTTIME flag is directly associated with the buffer's
+ * timestamp ' thus its association to buffer data and its
+ * propagation is identical to the timestamp's.
+ *
+ * When a Sync Component client receives a buffer with the
+ * STARTTIME flag it shall perform a SetConfig on its sync port
+ * using OMX_ConfigTimeClientStartTime and passing the buffer's
+ * timestamp.
+ *
+ * @ingroup buf
+ */
+
+#define OMX_BUFFERFLAG_STARTTIME 0x00000002
+
+
+
+/** Decode Only Buffer Flag:
+ *
+ * The source of a stream (e.g. a demux component) sets the DECODEONLY
+ * flag on any buffer that should shall be decoded but should not be
+ * displayed. This flag is used, for instance, when a source seeks to
+ * a target interframe that requires the decode of frames preceding the
+ * target to facilitate the target's reconstruction. In this case the
+ * source would emit the frames preceding the target downstream
+ * but mark them as decode only.
+ *
+ * The DECODEONLY is associated with buffer data and propagated in a
+ * manner identical to the buffer timestamp.
+ *
+ * A component that renders data should ignore all buffers with
+ * the DECODEONLY flag set.
+ *
+ * @ingroup buf
+ */
+
+#define OMX_BUFFERFLAG_DECODEONLY 0x00000004
+
+
+/* Data Corrupt Flag: This flag is set when the IL client believes the data in the associated buffer is corrupt
+ * @ingroup buf
+ */
+
+#define OMX_BUFFERFLAG_DATACORRUPT 0x00000008
+
+/* End of Frame: The buffer contains exactly one end of frame and no data
+ *  occurs after the end of frame. This flag is an optional hint. The absence
+ *  of this flag does not imply the absence of an end of frame within the buffer.
+ * @ingroup buf
+*/
+#define OMX_BUFFERFLAG_ENDOFFRAME 0x00000010
+
+/* Sync Frame Flag: This flag is set when the buffer content contains a coded sync frame '
+ *  a frame that has no dependency on any other frame information
+ *  @ingroup buf
+ */
+#define OMX_BUFFERFLAG_SYNCFRAME 0x00000020
+
+/* Extra data present flag: there is extra data appended to the data stream
+ * residing in the buffer
+ * @ingroup buf
+ */
+#define OMX_BUFFERFLAG_EXTRADATA 0x00000040
+
+/** Codec Config Buffer Flag:
+* OMX_BUFFERFLAG_CODECCONFIG is an optional flag that is set by an
+* output port when all bytes in the buffer form part or all of a set of
+* codec specific configuration data.  Examples include SPS/PPS nal units
+* for OMX_VIDEO_CodingAVC or AudioSpecificConfig data for
+* OMX_AUDIO_CodingAAC.  Any component that for a given stream sets
+* OMX_BUFFERFLAG_CODECCONFIG shall not mix codec configuration bytes
+* with frame data in the same buffer, and shall send all buffers
+* containing codec configuration bytes before any buffers containing
+* frame data that those configurations bytes describe.
+* If the stream format for a particular codec has a frame specific
+* header at the start of each frame, for example OMX_AUDIO_CodingMP3 or
+* OMX_AUDIO_CodingAAC in ADTS mode, then these shall be presented as
+* normal without setting OMX_BUFFERFLAG_CODECCONFIG.
+ * @ingroup buf
+ */
+#define OMX_BUFFERFLAG_CODECCONFIG 0x00000080
+
+
+
+/** @ingroup buf */
+typedef struct OMX_BUFFERHEADERTYPE {
+    OMX_U32 nSize;              /**< size of the structure in bytes */
+    OMX_VERSIONTYPE nVersion;   /**< OMX specification version information */
+    OMX_U8* pBuffer;            /**< Pointer to actual block of memory
+                                     that is acting as the buffer */
+    OMX_U32 nAllocLen;          /**< size of the buffer allocated, in bytes */
+    OMX_U32 nFilledLen;         /**< number of bytes currently in the
+                                     buffer */
+    OMX_U32 nOffset;            /**< start offset of valid data in bytes from
+                                     the start of the buffer */
+    OMX_PTR pAppPrivate;        /**< pointer to any data the application
+                                     wants to associate with this buffer */
+    OMX_PTR pPlatformPrivate;   /**< pointer to any data the platform
+                                     wants to associate with this buffer */
+    OMX_PTR pInputPortPrivate;  /**< pointer to any data the input port
+                                     wants to associate with this buffer */
+    OMX_PTR pOutputPortPrivate; /**< pointer to any data the output port
+                                     wants to associate with this buffer */
+    OMX_HANDLETYPE hMarkTargetComponent; /**< The component that will generate a
+                                              mark event upon processing this buffer. */
+    OMX_PTR pMarkData;          /**< Application specific data associated with
+                                     the mark sent on a mark event to disambiguate
+                                     this mark from others. */
+    OMX_U32 nTickCount;         /**< Optional entry that the component and
+                                     application can update with a tick count
+                                     when they access the component.  This
+                                     value should be in microseconds.  Since
+                                     this is a value relative to an arbitrary
+                                     starting point, this value cannot be used
+                                     to determine absolute time.  This is an
+                                     optional entry and not all components
+                                     will update it.*/
+    OMX_TICKS nTimeStamp;          /**< Timestamp corresponding to the sample
+                                     starting at the first logical sample
+                                     boundary in the buffer. Timestamps of
+                                     successive samples within the buffer may
+                                     be inferred by adding the duration of the
+                                     of the preceding buffer to the timestamp
+                                     of the preceding buffer.*/
+    OMX_U32     nFlags;           /**< buffer specific flags */
+    OMX_U32 nOutputPortIndex;     /**< The index of the output port (if any) using
+                                     this buffer */
+    OMX_U32 nInputPortIndex;      /**< The index of the input port (if any) using
+                                     this buffer */
+} OMX_BUFFERHEADERTYPE;
+
+/** The OMX_EXTRADATATYPE enumeration is used to define the
+ * possible extra data payload types.
+ * NB: this enum is binary backwards compatible with the previous
+ * OMX_EXTRADATA_QUANT define.  This should be replaced with
+ * OMX_ExtraDataQuantization.
+ */
+typedef enum OMX_EXTRADATATYPE {
+    OMX_ExtraDataNone = 0,                       /**< Indicates that no more extra data sections follow */
+    OMX_ExtraDataQuantization,                   /**< The data payload contains quantization data */
+    OMX_ExtraDataKhronosExtensions = 0x6F000000, /**< Reserved region for introducing Khronos Standard Extensions */
+    OMX_ExtraDataVendorStartUnused = 0x7F000000, /**< Reserved region for introducing Vendor Extensions */
+    OMX_ExtraDataMax = 0x7FFFFFFF
+} OMX_EXTRADATATYPE;
+
+
+typedef struct OMX_OTHER_EXTRADATATYPE  {
+    OMX_U32 nSize;
+    OMX_VERSIONTYPE nVersion;
+    OMX_U32 nPortIndex;
+    OMX_EXTRADATATYPE eType;       /* Extra Data type */
+    OMX_U32 nDataSize;   /* Size of the supporting data to follow */
+    OMX_U8  data[1];     /* Supporting data hint  */
+} OMX_OTHER_EXTRADATATYPE;
+
+/** @ingroup comp */
+typedef struct OMX_PORT_PARAM_TYPE {
+    OMX_U32 nSize;              /**< size of the structure in bytes */
+    OMX_VERSIONTYPE nVersion;   /**< OMX specification version information */
+    OMX_U32 nPorts;             /**< The number of ports for this component */
+    OMX_U32 nStartPortNumber;   /** first port number for this type of port */
+} OMX_PORT_PARAM_TYPE;
+
+/** @ingroup comp */
+typedef enum OMX_EVENTTYPE {
+    OMX_EventCmdComplete,         /**< component has sucessfully completed a command */
+    OMX_EventError,               /**< component has detected an error condition */
+    OMX_EventMark,                /**< component has detected a buffer mark */
+    OMX_EventPortSettingsChanged, /**< component is reported a port settings change */
+    OMX_EventBufferFlag,          /**< component has detected an EOS */
+    OMX_EventResourcesAcquired,   /**< component has been granted resources and is
+                                       automatically starting the state change from
+                                       OMX_StateWaitForResources to OMX_StateIdle. */
+    OMX_EventComponentResumed,     /**< Component resumed due to reacquisition of resources */
+    OMX_EventDynamicResourcesAvailable, /**< Component has acquired previously unavailable dynamic resources */
+    OMX_EventPortFormatDetected,      /**< Component has detected a supported format. */
+    OMX_EventKhronosExtensions = 0x6F000000, /**< Reserved region for introducing Khronos Standard Extensions */
+    OMX_EventVendorStartUnused = 0x7F000000, /**< Reserved region for introducing Vendor Extensions */
+    OMX_EventMax = 0x7FFFFFFF
+} OMX_EVENTTYPE;
+
+typedef struct OMX_CALLBACKTYPE {
+    /** The EventHandler method is used to notify the application when an
+        event of interest occurs.  Events are defined in the OMX_EVENTTYPE
+        enumeration.  Please see that enumeration for details of what will
+        be returned for each type of event. Callbacks should not return
+        an error to the component, so if an error occurs, the application
+        shall handle it internally.  This is a blocking call.
+
+        The application should return from this call within 5 msec to avoid
+        blocking the component for an excessively long period of time.
+
+        @param hComponent
+            handle of the component to access.  This is the component
+            handle returned by the call to the GetHandle function.
+        @param pAppData
+            pointer to an application defined value that was provided in the
+            pAppData parameter to the OMX_GetHandle method for the component.
+            This application defined value is provided so that the application
+            can have a component specific context when receiving the callback.
+        @param eEvent
+            Event that the component wants to notify the application about.
+        @param nData1
+            nData will be the OMX_ERRORTYPE for an error event and will be
+            an OMX_COMMANDTYPE for a command complete event and OMX_INDEXTYPE for a OMX_PortSettingsChanged event.
+         @param nData2
+            nData2 will hold further information related to the event. Can be OMX_STATETYPE for
+            a OMX_CommandStateSet command or port index for a OMX_PortSettingsChanged event.
+            Default value is 0 if not used. )
+        @param pEventData
+            Pointer to additional event-specific data (see spec for meaning).
+      */
+
+    OMX_ERRORTYPE (*EventHandler)(
+        OMX_IN OMX_HANDLETYPE hComponent,
+        OMX_IN OMX_PTR pAppData,
+        OMX_IN OMX_EVENTTYPE eEvent,
+        OMX_IN OMX_U32 nData1,
+        OMX_IN OMX_U32 nData2,
+        OMX_IN OMX_PTR pEventData);
+
+    /** The EmptyBufferDone method is used to return emptied buffers from an
+        input port back to the application for reuse.  This is a blocking call
+        so the application should not attempt to refill the buffers during this
+        call, but should queue them and refill them in another thread.  There
+        is no error return, so the application shall handle any errors generated
+        internally.
+
+        The application should return from this call within 5 msec.
+
+        @param hComponent
+            handle of the component to access.  This is the component
+            handle returned by the call to the GetHandle function.
+        @param pAppData
+            pointer to an application defined value that was provided in the
+            pAppData parameter to the OMX_GetHandle method for the component.
+            This application defined value is provided so that the application
+            can have a component specific context when receiving the callback.
+        @param pBuffer
+            pointer to an OMX_BUFFERHEADERTYPE structure allocated with UseBuffer
+            or AllocateBuffer indicating the buffer that was emptied.
+        @ingroup buf
+     */
+    OMX_ERRORTYPE (*EmptyBufferDone)(
+        OMX_IN OMX_HANDLETYPE hComponent,
+        OMX_IN OMX_PTR pAppData,
+        OMX_IN OMX_BUFFERHEADERTYPE* pBuffer);
+
+    /** The FillBufferDone method is used to return filled buffers from an
+        output port back to the application for emptying and then reuse.
+        This is a blocking call so the application should not attempt to
+        empty the buffers during this call, but should queue the buffers
+        and empty them in another thread.  There is no error return, so
+        the application shall handle any errors generated internally.  The
+        application shall also update the buffer header to indicate the
+        number of bytes placed into the buffer.
+
+        The application should return from this call within 5 msec.
+
+        @param hComponent
+            handle of the component to access.  This is the component
+            handle returned by the call to the GetHandle function.
+        @param pAppData
+            pointer to an application defined value that was provided in the
+            pAppData parameter to the OMX_GetHandle method for the component.
+            This application defined value is provided so that the application
+            can have a component specific context when receiving the callback.
+        @param pBuffer
+            pointer to an OMX_BUFFERHEADERTYPE structure allocated with UseBuffer
+            or AllocateBuffer indicating the buffer that was filled.
+        @ingroup buf
+     */
+    OMX_ERRORTYPE (*FillBufferDone)(
+        OMX_OUT OMX_HANDLETYPE hComponent,
+        OMX_OUT OMX_PTR pAppData,
+        OMX_OUT OMX_BUFFERHEADERTYPE* pBuffer);
+
+} OMX_CALLBACKTYPE;
+
+/** The OMX_BUFFERSUPPLIERTYPE enumeration is used to dictate port supplier
+    preference when tunneling between two ports.
+    @ingroup tun buf
+*/
+typedef enum OMX_BUFFERSUPPLIERTYPE {
+    OMX_BufferSupplyUnspecified = 0x0, /**< port supplying the buffers is unspecified,
+                                              or don't care */
+    OMX_BufferSupplyInput,             /**< input port supplies the buffers */
+    OMX_BufferSupplyOutput,            /**< output port supplies the buffers */
+    OMX_BufferSupplyKhronosExtensions = 0x6F000000, /**< Reserved region for introducing Khronos Standard Extensions */
+    OMX_BufferSupplyVendorStartUnused = 0x7F000000, /**< Reserved region for introducing Vendor Extensions */
+    OMX_BufferSupplyMax = 0x7FFFFFFF
+} OMX_BUFFERSUPPLIERTYPE;
+
+
+/** buffer supplier parameter
+ * @ingroup tun
+ */
+typedef struct OMX_PARAM_BUFFERSUPPLIERTYPE {
+    OMX_U32 nSize; /**< size of the structure in bytes */
+    OMX_VERSIONTYPE nVersion; /**< OMX specification version information */
+    OMX_U32 nPortIndex; /**< port that this structure applies to */
+    OMX_BUFFERSUPPLIERTYPE eBufferSupplier; /**< buffer supplier */
+} OMX_PARAM_BUFFERSUPPLIERTYPE;
+
+
+/**< indicates that buffers received by an input port of a tunnel
+     may not modify the data in the buffers
+     @ingroup tun
+ */
+#define OMX_PORTTUNNELFLAG_READONLY 0x00000001
+
+
+/** The OMX_TUNNELSETUPTYPE structure is used to pass data from an output
+    port to an input port as part the two ComponentTunnelRequest calls
+    resulting from a OMX_SetupTunnel call from the IL Client.
+    @ingroup tun
+ */
+typedef struct OMX_TUNNELSETUPTYPE {
+    OMX_U32 nTunnelFlags;             /**< bit flags for tunneling */
+    OMX_BUFFERSUPPLIERTYPE eSupplier; /**< supplier preference */
+} OMX_TUNNELSETUPTYPE;
+
+/* OMX Component headers is included to enable the core to use
+   macros for functions into the component for OMX release 1.0.
+   Developers should not access any structures or data from within
+   the component header directly */
+/* TO BE REMOVED - #include <OMX_Component.h> */
+
+/** GetComponentVersion will return information about the component.
+    This is a blocking call.  This macro will go directly from the
+    application to the component (via a core macro).  The
+    component will return from this call within 5 msec.
+    @param [in] hComponent
+        handle of component to execute the command
+    @param [out] pComponentName
+        pointer to an empty string of length 128 bytes.  The component
+        will write its name into this string.  The name will be
+        terminated by a single zero byte.  The name of a component will
+        be 127 bytes or less to leave room for the trailing zero byte.
+        An example of a valid component name is "OMX.ABC.ChannelMixer\0".
+    @param [out] pComponentVersion
+        pointer to an OMX Version structure that the component will fill
+        in.  The component will fill in a value that indicates the
+        component version.  NOTE: the component version is NOT the same
+        as the OMX Specification version (found in all structures).  The
+        component version is defined by the vendor of the component and
+        its value is entirely up to the component vendor.
+    @param [out] pSpecVersion
+        pointer to an OMX Version structure that the component will fill
+        in.  The SpecVersion is the version of the specification that the
+        component was built against.  Please note that this value may or
+        may not match the structure's version.  For example, if the
+        component was built against the 2.0 specification, but the
+        application (which creates the structure is built against the
+        1.0 specification the versions would be different.
+    @param [out] pComponentUUID
+        pointer to the UUID of the component which will be filled in by
+        the component.  The UUID is a unique identifier that is set at
+        RUN time for the component and is unique to each instantion of
+        the component.
+    @return OMX_ERRORTYPE
+        If the command successfully executes, the return code will be
+        OMX_ErrorNone.  Otherwise the appropriate OMX error will be returned.
+    @ingroup comp
+ */
+#define OMX_GetComponentVersion(                            \
+        hComponent,                                         \
+        pComponentName,                                     \
+        pComponentVersion,                                  \
+        pSpecVersion,                                       \
+        pComponentUUID)                                     \
+    ((OMX_COMPONENTTYPE*)hComponent)->GetComponentVersion(  \
+        hComponent,                                         \
+        pComponentName,                                     \
+        pComponentVersion,                                  \
+        pSpecVersion,                                       \
+        pComponentUUID)                 /* Macro End */
+
+
+/** Send a command to the component.  This call is a non-blocking call.
+    The component should check the parameters and then queue the command
+    to the component thread to be executed.  The component thread shall
+    send the EventHandler() callback at the conclusion of the command.
+    This macro will go directly from the application to the component (via
+    a core macro).  The component will return from this call within 5 msec.
+
+    When the command is "OMX_CommandStateSet" the component will queue a
+    state transition to the new state idenfied in nParam.
+
+    When the command is "OMX_CommandFlush", to flush a port's buffer queues,
+    the command will force the component to return all buffers NOT CURRENTLY
+    BEING PROCESSED to the application, in the order in which the buffers
+    were received.
+
+    When the command is "OMX_CommandPortDisable" or
+    "OMX_CommandPortEnable", the component's port (given by the value of
+    nParam) will be stopped or restarted.
+
+    When the command "OMX_CommandMarkBuffer" is used to mark a buffer, the
+    pCmdData will point to a OMX_MARKTYPE structure containing the component
+    handle of the component to examine the buffer chain for the mark.  nParam1
+    contains the index of the port on which the buffer mark is applied.
+
+    Specification text for more details.
+
+    @param [in] hComponent
+        handle of component to execute the command
+    @param [in] Cmd
+        Command for the component to execute
+    @param [in] nParam
+        Parameter for the command to be executed.  When Cmd has the value
+        OMX_CommandStateSet, value is a member of OMX_STATETYPE.  When Cmd has
+        the value OMX_CommandFlush, value of nParam indicates which port(s)
+        to flush. -1 is used to flush all ports a single port index will
+        only flush that port.  When Cmd has the value "OMX_CommandPortDisable"
+        or "OMX_CommandPortEnable", the component's port is given by
+        the value of nParam.  When Cmd has the value "OMX_CommandMarkBuffer"
+        the components pot is given by the value of nParam.
+    @param [in] pCmdData
+        Parameter pointing to the OMX_MARKTYPE structure when Cmd has the value
+        "OMX_CommandMarkBuffer".
+    @return OMX_ERRORTYPE
+        If the command successfully executes, the return code will be
+        OMX_ErrorNone.  Otherwise the appropriate OMX error will be returned.
+    @ingroup comp
+ */
+#define OMX_SendCommand(                                    \
+         hComponent,                                        \
+         Cmd,                                               \
+         nParam,                                            \
+         pCmdData)                                          \
+     ((OMX_COMPONENTTYPE*)hComponent)->SendCommand(         \
+         hComponent,                                        \
+         Cmd,                                               \
+         nParam,                                            \
+         pCmdData)                          /* Macro End */
+
+
+/** The OMX_GetParameter macro will get one of the current parameter
+    settings from the component.  This macro cannot only be invoked when
+    the component is in the OMX_StateInvalid state.  The nParamIndex
+    parameter is used to indicate which structure is being requested from
+    the component.  The application shall allocate the correct structure
+    and shall fill in the structure size and version information before
+    invoking this macro.  When the parameter applies to a port, the
+    caller shall fill in the appropriate nPortIndex value indicating the
+    port on which the parameter applies. If the component has not had
+    any settings changed, then the component should return a set of
+    valid DEFAULT  parameters for the component.  This is a blocking
+    call.
+
+    The component should return from this call within 20 msec.
+
+    @param [in] hComponent
+        Handle of the component to be accessed.  This is the component
+        handle returned by the call to the OMX_GetHandle function.
+    @param [in] nParamIndex
+        Index of the structure to be filled.  This value is from the
+        OMX_INDEXTYPE enumeration.
+    @param [in,out] pComponentParameterStructure
+        Pointer to application allocated structure to be filled by the
+        component.
+    @return OMX_ERRORTYPE
+        If the command successfully executes, the return code will be
+        OMX_ErrorNone.  Otherwise the appropriate OMX error will be returned.
+    @ingroup comp
+ */
+#define OMX_GetParameter(                                   \
+        hComponent,                                         \
+        nParamIndex,                                        \
+        pComponentParameterStructure)                        \
+    ((OMX_COMPONENTTYPE*)hComponent)->GetParameter(         \
+        hComponent,                                         \
+        nParamIndex,                                        \
+        pComponentParameterStructure)    /* Macro End */
+
+
+/** The OMX_SetParameter macro will send an initialization parameter
+    structure to a component.  Each structure shall be sent one at a time,
+    in a separate invocation of the macro.  This macro can only be
+    invoked when the component is in the OMX_StateLoaded state, or the
+    port is disabled (when the parameter applies to a port). The
+    nParamIndex parameter is used to indicate which structure is being
+    passed to the component.  The application shall allocate the
+    correct structure and shall fill in the structure size and version
+    information (as well as the actual data) before invoking this macro.
+    The application is free to dispose of this structure after the call
+    as the component is required to copy any data it shall retain.  This
+    is a blocking call.
+
+    The component should return from this call within 20 msec.
+
+    @param [in] hComponent
+        Handle of the component to be accessed.  This is the component
+        handle returned by the call to the OMX_GetHandle function.
+    @param [in] nIndex
+        Index of the structure to be sent.  This value is from the
+        OMX_INDEXTYPE enumeration.
+    @param [in] pComponentParameterStructure
+        pointer to application allocated structure to be used for
+        initialization by the component.
+    @return OMX_ERRORTYPE
+        If the command successfully executes, the return code will be
+        OMX_ErrorNone.  Otherwise the appropriate OMX error will be returned.
+    @ingroup comp
+ */
+#define OMX_SetParameter(                                   \
+        hComponent,                                         \
+        nParamIndex,                                        \
+        pComponentParameterStructure)                        \
+    ((OMX_COMPONENTTYPE*)hComponent)->SetParameter(         \
+        hComponent,                                         \
+        nParamIndex,                                        \
+        pComponentParameterStructure)    /* Macro End */
+
+
+/** The OMX_GetConfig macro will get one of the configuration structures
+    from a component.  This macro can be invoked anytime after the
+    component has been loaded.  The nParamIndex call parameter is used to
+    indicate which structure is being requested from the component.  The
+    application shall allocate the correct structure and shall fill in the
+    structure size and version information before invoking this macro.
+    If the component has not had this configuration parameter sent before,
+    then the component should return a set of valid DEFAULT values for the
+    component.  This is a blocking call.
+
+    The component should return from this call within 5 msec.
+
+    @param [in] hComponent
+        Handle of the component to be accessed.  This is the component
+        handle returned by the call to the OMX_GetHandle function.
+    @param [in] nIndex
+        Index of the structure to be filled.  This value is from the
+        OMX_INDEXTYPE enumeration.
+    @param [in,out] pComponentConfigStructure
+        pointer to application allocated structure to be filled by the
+        component.
+    @return OMX_ERRORTYPE
+        If the command successfully executes, the return code will be
+        OMX_ErrorNone.  Otherwise the appropriate OMX error will be returned.
+    @ingroup comp
+*/
+#define OMX_GetConfig(                                      \
+        hComponent,                                         \
+        nConfigIndex,                                       \
+        pComponentConfigStructure)                           \
+    ((OMX_COMPONENTTYPE*)hComponent)->GetConfig(            \
+        hComponent,                                         \
+        nConfigIndex,                                       \
+        pComponentConfigStructure)       /* Macro End */
+
+
+/** The OMX_SetConfig macro will send one of the configuration
+    structures to a component.  Each structure shall be sent one at a time,
+    each in a separate invocation of the macro.  This macro can be invoked
+    anytime after the component has been loaded.  The application shall
+    allocate the correct structure and shall fill in the structure size
+    and version information (as well as the actual data) before invoking
+    this macro.  The application is free to dispose of this structure after
+    the call as the component is required to copy any data it shall retain.
+    This is a blocking call.
+
+    The component should return from this call within 5 msec.
+
+    @param [in] hComponent
+        Handle of the component to be accessed.  This is the component
+        handle returned by the call to the OMX_GetHandle function.
+    @param [in] nConfigIndex
+        Index of the structure to be sent.  This value is from the
+        OMX_INDEXTYPE enumeration above.
+    @param [in] pComponentConfigStructure
+        pointer to application allocated structure to be used for
+        initialization by the component.
+    @return OMX_ERRORTYPE
+        If the command successfully executes, the return code will be
+        OMX_ErrorNone.  Otherwise the appropriate OMX error will be returned.
+    @ingroup comp
+ */
+#define OMX_SetConfig(                                      \
+        hComponent,                                         \
+        nConfigIndex,                                       \
+        pComponentConfigStructure)                           \
+    ((OMX_COMPONENTTYPE*)hComponent)->SetConfig(            \
+        hComponent,                                         \
+        nConfigIndex,                                       \
+        pComponentConfigStructure)       /* Macro End */
+
+
+/** The OMX_GetExtensionIndex macro will invoke a component to translate
+    a vendor specific configuration or parameter string into an OMX
+    structure index.  There is no requirement for the vendor to support
+    this command for the indexes already found in the OMX_INDEXTYPE
+    enumeration (this is done to save space in small components).  The
+    component shall support all vendor supplied extension indexes not found
+    in the master OMX_INDEXTYPE enumeration.  This is a blocking call.
+
+    The component should return from this call within 5 msec.
+
+    @param [in] hComponent
+        Handle of the component to be accessed.  This is the component
+        handle returned by the call to the GetHandle function.
+    @param [in] cParameterName
+        OMX_STRING that shall be less than 128 characters long including
+        the trailing null byte.  This is the string that will get
+        translated by the component into a configuration index.
+    @param [out] pIndexType
+        a pointer to a OMX_INDEXTYPE to receive the index value.
+    @return OMX_ERRORTYPE
+        If the command successfully executes, the return code will be
+        OMX_ErrorNone.  Otherwise the appropriate OMX error will be returned.
+    @ingroup comp
+ */
+#define OMX_GetExtensionIndex(                              \
+        hComponent,                                         \
+        cParameterName,                                     \
+        pIndexType)                                         \
+    ((OMX_COMPONENTTYPE*)hComponent)->GetExtensionIndex(    \
+        hComponent,                                         \
+        cParameterName,                                     \
+        pIndexType)                     /* Macro End */
+
+
+/** The OMX_GetState macro will invoke the component to get the current
+    state of the component and place the state value into the location
+    pointed to by pState.
+
+    The component should return from this call within 5 msec.
+
+    @param [in] hComponent
+        Handle of the component to be accessed.  This is the component
+        handle returned by the call to the OMX_GetHandle function.
+    @param [out] pState
+        pointer to the location to receive the state.  The value returned
+        is one of the OMX_STATETYPE members
+    @return OMX_ERRORTYPE
+        If the command successfully executes, the return code will be
+        OMX_ErrorNone.  Otherwise the appropriate OMX error will be returned.
+    @ingroup comp
+ */
+#define OMX_GetState(                                       \
+        hComponent,                                         \
+        pState)                                             \
+    ((OMX_COMPONENTTYPE*)hComponent)->GetState(             \
+        hComponent,                                         \
+        pState)                         /* Macro End */
+
+
+/** The OMX_UseBuffer macro will request that the component use
+    a buffer (and allocate its own buffer header) already allocated
+    by another component, or by the IL Client. This is a blocking
+    call.
+
+    The component should return from this call within 20 msec.
+
+    @param [in] hComponent
+        Handle of the component to be accessed.  This is the component
+        handle returned by the call to the OMX_GetHandle function.
+    @param [out] ppBuffer
+        pointer to an OMX_BUFFERHEADERTYPE structure used to receive the
+        pointer to the buffer header
+    @return OMX_ERRORTYPE
+        If the command successfully executes, the return code will be
+        OMX_ErrorNone.  Otherwise the appropriate OMX error will be returned.
+    @ingroup comp buf
+ */
+
+#define OMX_UseBuffer(                                      \
+           hComponent,                                      \
+           ppBufferHdr,                                     \
+           nPortIndex,                                      \
+           pAppPrivate,                                     \
+           nSizeBytes,                                      \
+           pBuffer)                                         \
+    ((OMX_COMPONENTTYPE*)hComponent)->UseBuffer(            \
+           hComponent,                                      \
+           ppBufferHdr,                                     \
+           nPortIndex,                                      \
+           pAppPrivate,                                     \
+           nSizeBytes,                                      \
+           pBuffer)
+
+
+/** The OMX_AllocateBuffer macro will request that the component allocate
+    a new buffer and buffer header.  The component will allocate the
+    buffer and the buffer header and return a pointer to the buffer
+    header.  This is a blocking call.
+
+    The component should return from this call within 5 msec.
+
+    @param [in] hComponent
+        Handle of the component to be accessed.  This is the component
+        handle returned by the call to the OMX_GetHandle function.
+    @param [out] ppBuffer
+        pointer to an OMX_BUFFERHEADERTYPE structure used to receive
+        the pointer to the buffer header
+    @param [in] nPortIndex
+        nPortIndex is used to select the port on the component the buffer will
+        be used with.  The port can be found by using the nPortIndex
+        value as an index into the Port Definition array of the component.
+    @param [in] pAppPrivate
+        pAppPrivate is used to initialize the pAppPrivate member of the
+        buffer header structure.
+    @param [in] nSizeBytes
+        size of the buffer to allocate.  Used when bAllocateNew is true.
+    @return OMX_ERRORTYPE
+        If the command successfully executes, the return code will be
+        OMX_ErrorNone.  Otherwise the appropriate OMX error will be returned.
+    @ingroup comp buf
+ */
+#define OMX_AllocateBuffer(                                 \
+        hComponent,                                         \
+        ppBuffer,                                           \
+        nPortIndex,                                         \
+        pAppPrivate,                                        \
+        nSizeBytes)                                         \
+    ((OMX_COMPONENTTYPE*)hComponent)->AllocateBuffer(       \
+        hComponent,                                         \
+        ppBuffer,                                           \
+        nPortIndex,                                         \
+        pAppPrivate,                                        \
+        nSizeBytes)                     /* Macro End */
+
+
+/** The OMX_FreeBuffer macro will release a buffer header from the component
+    which was allocated using either OMX_AllocateBuffer or OMX_UseBuffer. If
+    the component allocated the buffer (see the OMX_UseBuffer macro) then
+    the component shall free the buffer and buffer header. This is a
+    blocking call.
+
+    The component should return from this call within 20 msec.
+
+    @param [in] hComponent
+        Handle of the component to be accessed.  This is the component
+        handle returned by the call to the OMX_GetHandle function.
+    @param [in] nPortIndex
+        nPortIndex is used to select the port on the component the buffer will
+        be used with.
+    @param [in] pBuffer
+        pointer to an OMX_BUFFERHEADERTYPE structure allocated with UseBuffer
+        or AllocateBuffer.
+    @return OMX_ERRORTYPE
+        If the command successfully executes, the return code will be
+        OMX_ErrorNone.  Otherwise the appropriate OMX error will be returned.
+    @ingroup comp buf
+ */
+#define OMX_FreeBuffer(                                     \
+        hComponent,                                         \
+        nPortIndex,                                         \
+        pBuffer)                                            \
+    ((OMX_COMPONENTTYPE*)hComponent)->FreeBuffer(           \
+        hComponent,                                         \
+        nPortIndex,                                         \
+        pBuffer)                        /* Macro End */
+
+
+/** The OMX_EmptyThisBuffer macro will send a buffer full of data to an
+    input port of a component.  The buffer will be emptied by the component
+    and returned to the application via the EmptyBufferDone call back.
+    This is a non-blocking call in that the component will record the buffer
+    and return immediately and then empty the buffer, later, at the proper
+    time.  As expected, this macro may be invoked only while the component
+    is in the OMX_StateExecuting.  If nPortIndex does not specify an input
+    port, the component shall return an error.
+
+    The component should return from this call within 5 msec.
+
+    @param [in] hComponent
+        Handle of the component to be accessed.  This is the component
+        handle returned by the call to the OMX_GetHandle function.
+    @param [in] pBuffer
+        pointer to an OMX_BUFFERHEADERTYPE structure allocated with UseBuffer
+        or AllocateBuffer.
+    @return OMX_ERRORTYPE
+        If the command successfully executes, the return code will be
+        OMX_ErrorNone.  Otherwise the appropriate OMX error will be returned.
+    @ingroup comp buf
+ */
+#define OMX_EmptyThisBuffer(                                \
+        hComponent,                                         \
+        pBuffer)                                            \
+    ((OMX_COMPONENTTYPE*)hComponent)->EmptyThisBuffer(      \
+        hComponent,                                         \
+        pBuffer)                        /* Macro End */
+
+
+/** The OMX_FillThisBuffer macro will send an empty buffer to an
+    output port of a component.  The buffer will be filled by the component
+    and returned to the application via the FillBufferDone call back.
+    This is a non-blocking call in that the component will record the buffer
+    and return immediately and then fill the buffer, later, at the proper
+    time.  As expected, this macro may be invoked only while the component
+    is in the OMX_ExecutingState.  If nPortIndex does not specify an output
+    port, the component shall return an error.
+
+    The component should return from this call within 5 msec.
+
+    @param [in] hComponent
+        Handle of the component to be accessed.  This is the component
+        handle returned by the call to the OMX_GetHandle function.
+    @param [in] pBuffer
+        pointer to an OMX_BUFFERHEADERTYPE structure allocated with UseBuffer
+        or AllocateBuffer.
+    @return OMX_ERRORTYPE
+        If the command successfully executes, the return code will be
+        OMX_ErrorNone.  Otherwise the appropriate OMX error will be returned.
+    @ingroup comp buf
+ */
+#define OMX_FillThisBuffer(                                 \
+        hComponent,                                         \
+        pBuffer)                                            \
+    ((OMX_COMPONENTTYPE*)hComponent)->FillThisBuffer(       \
+        hComponent,                                         \
+        pBuffer)                        /* Macro End */
+
+
+
+/** The OMX_UseEGLImage macro will request that the component use
+    a EGLImage provided by EGL (and allocate its own buffer header)
+    This is a blocking call.
+
+    The component should return from this call within 20 msec.
+
+    @param [in] hComponent
+        Handle of the component to be accessed.  This is the component
+        handle returned by the call to the OMX_GetHandle function.
+    @param [out] ppBuffer
+        pointer to an OMX_BUFFERHEADERTYPE structure used to receive the
+        pointer to the buffer header.  Note that the memory location used
+        for this buffer is NOT visible to the IL Client.
+    @param [in] nPortIndex
+        nPortIndex is used to select the port on the component the buffer will
+        be used with.  The port can be found by using the nPortIndex
+        value as an index into the Port Definition array of the component.
+    @param [in] pAppPrivate
+        pAppPrivate is used to initialize the pAppPrivate member of the
+        buffer header structure.
+    @param [in] eglImage
+        eglImage contains the handle of the EGLImage to use as a buffer on the
+        specified port.  The component is expected to validate properties of
+        the EGLImage against the configuration of the port to ensure the component
+        can use the EGLImage as a buffer.
+    @return OMX_ERRORTYPE
+        If the command successfully executes, the return code will be
+        OMX_ErrorNone.  Otherwise the appropriate OMX error will be returned.
+    @ingroup comp buf
+ */
+#define OMX_UseEGLImage(                                    \
+           hComponent,                                      \
+           ppBufferHdr,                                     \
+           nPortIndex,                                      \
+           pAppPrivate,                                     \
+           eglImage)                                        \
+    ((OMX_COMPONENTTYPE*)hComponent)->UseEGLImage(          \
+           hComponent,                                      \
+           ppBufferHdr,                                     \
+           nPortIndex,                                      \
+           pAppPrivate,                                     \
+           eglImage)
+
+/** The OMX_Init method is used to initialize the OMX core.  It shall be the
+    first call made into OMX and it should only be executed one time without
+    an interviening OMX_Deinit call.
+
+    The core should return from this call within 20 msec.
+
+    @return OMX_ERRORTYPE
+        If the command successfully executes, the return code will be
+        OMX_ErrorNone.  Otherwise the appropriate OMX error will be returned.
+    @ingroup core
+ */
+OMX_API OMX_ERRORTYPE OMX_APIENTRY OMX_Init(void);
+
+
+/** The OMX_Deinit method is used to deinitialize the OMX core.  It shall be
+    the last call made into OMX. In the event that the core determines that
+    thare are components loaded when this call is made, the core may return
+    with an error rather than try to unload the components.
+
+    The core should return from this call within 20 msec.
+
+    @return OMX_ERRORTYPE
+        If the command successfully executes, the return code will be
+        OMX_ErrorNone.  Otherwise the appropriate OMX error will be returned.
+    @ingroup core
+ */
+OMX_API OMX_ERRORTYPE OMX_APIENTRY OMX_Deinit(void);
+
+
+/** The OMX_ComponentNameEnum method will enumerate through all the names of
+    recognised valid components in the system. This function is provided
+    as a means to detect all the components in the system run-time. There is
+    no strict ordering to the enumeration order of component names, although
+    each name will only be enumerated once.  If the OMX core supports run-time
+    installation of new components, it is only requried to detect newly
+    installed components when the first call to enumerate component names
+    is made (i.e. when nIndex is 0x0).
+
+    The core should return from this call in 20 msec.
+
+    @param [out] cComponentName
+        pointer to a null terminated string with the component name.  The
+        names of the components are strings less than 127 bytes in length
+        plus the trailing null for a maximum size of 128 bytes.  An example
+        of a valid component name is "OMX.TI.AUDIO.DSP.MIXER\0".  Names are
+        assigned by the vendor, but shall start with "OMX." and then have
+        the Vendor designation next.
+    @param [in] nNameLength
+        number of characters in the cComponentName string.  With all
+        component name strings restricted to less than 128 characters
+        (including the trailing null) it is recomended that the caller
+        provide a input string for the cComponentName of 128 characters.
+    @param [in] nIndex
+        number containing the enumeration index for the component.
+        Multiple calls to OMX_ComponentNameEnum with increasing values
+        of nIndex will enumerate through the component names in the
+        system until OMX_ErrorNoMore is returned.  The value of nIndex
+        is 0 to (N-1), where N is the number of valid installed components
+        in the system.
+    @return OMX_ERRORTYPE
+        If the command successfully executes, the return code will be
+        OMX_ErrorNone.  When the value of nIndex exceeds the number of
+        components in the system minus 1, OMX_ErrorNoMore will be
+        returned. Otherwise the appropriate OMX error will be returned.
+    @ingroup core
+ */
+OMX_API OMX_ERRORTYPE OMX_APIENTRY OMX_ComponentNameEnum(
+    OMX_OUT OMX_STRING cComponentName,
+    OMX_IN  OMX_U32 nNameLength,
+    OMX_IN  OMX_U32 nIndex);
+
+
+/** The OMX_GetHandle method will locate the component specified by the
+    component name given, load that component into memory and then invoke
+    the component's methods to create an instance of the component.
+
+    The core should return from this call within 20 msec.
+
+    @param [out] pHandle
+        pointer to an OMX_HANDLETYPE pointer to be filled in by this method.
+    @param [in] cComponentName
+        pointer to a null terminated string with the component name.  The
+        names of the components are strings less than 127 bytes in length
+        plus the trailing null for a maximum size of 128 bytes.  An example
+        of a valid component name is "OMX.TI.AUDIO.DSP.MIXER\0".  Names are
+        assigned by the vendor, but shall start with "OMX." and then have
+        the Vendor designation next.
+    @param [in] pAppData
+        pointer to an application defined value that will be returned
+        during callbacks so that the application can identify the source
+        of the callback.
+    @param [in] pCallBacks
+        pointer to a OMX_CALLBACKTYPE structure that will be passed to the
+        component to initialize it with.
+    @return OMX_ERRORTYPE
+        If the command successfully executes, the return code will be
+        OMX_ErrorNone.  Otherwise the appropriate OMX error will be returned.
+    @ingroup core
+ */
+OMX_API OMX_ERRORTYPE OMX_APIENTRY OMX_GetHandle(
+    OMX_OUT OMX_HANDLETYPE* pHandle,
+    OMX_IN  OMX_STRING cComponentName,
+    OMX_IN  OMX_PTR pAppData,
+    OMX_IN  OMX_CALLBACKTYPE* pCallBacks);
+
+
+/** The OMX_FreeHandle method will free a handle allocated by the OMX_GetHandle
+    method.  If the component reference count goes to zero, the component will
+    be unloaded from memory.
+
+    The core should return from this call within 20 msec when the component is
+    in the OMX_StateLoaded state.
+
+    @param [in] hComponent
+        Handle of the component to be accessed.  This is the component
+        handle returned by the call to the GetHandle function.
+    @return OMX_ERRORTYPE
+        If the command successfully executes, the return code will be
+        OMX_ErrorNone.  Otherwise the appropriate OMX error will be returned.
+    @ingroup core
+ */
+OMX_API OMX_ERRORTYPE OMX_APIENTRY OMX_FreeHandle(
+    OMX_IN  OMX_HANDLETYPE hComponent);
+
+
+
+/** The OMX_SetupTunnel method will handle the necessary calls to the components
+    to setup the specified tunnel the two components.  NOTE: This is
+    an actual method (not a #define macro).  This method will make calls into
+    the component ComponentTunnelRequest method to do the actual tunnel
+    connection.
+
+    The ComponentTunnelRequest method on both components will be called.
+    This method shall not be called unless the component is in the
+    OMX_StateLoaded state except when the ports used for the tunnel are
+    disabled. In this case, the component may be in the OMX_StateExecuting,
+    OMX_StatePause, or OMX_StateIdle states.
+
+    The core should return from this call within 20 msec.
+
+    @param [in] hOutput
+        Handle of the component to be accessed.  Also this is the handle
+        of the component whose port, specified in the nPortOutput parameter
+        will be used the source for the tunnel. This is the component handle
+        returned by the call to the OMX_GetHandle function.  There is a
+        requirement that hOutput be the source for the data when
+        tunelling (i.e. nPortOutput is an output port).  If 0x0, the component
+        specified in hInput will have it's port specified in nPortInput
+        setup for communication with the application / IL client.
+    @param [in] nPortOutput
+        nPortOutput is used to select the source port on component to be
+        used in the tunnel.
+    @param [in] hInput
+        This is the component to setup the tunnel with. This is the handle
+        of the component whose port, specified in the nPortInput parameter
+        will be used the destination for the tunnel. This is the component handle
+        returned by the call to the OMX_GetHandle function.  There is a
+        requirement that hInput be the destination for the data when
+        tunelling (i.e. nPortInut is an input port).   If 0x0, the component
+        specified in hOutput will have it's port specified in nPortPOutput
+        setup for communication with the application / IL client.
+    @param [in] nPortInput
+        nPortInput is used to select the destination port on component to be
+        used in the tunnel.
+    @return OMX_ERRORTYPE
+        If the command successfully executes, the return code will be
+        OMX_ErrorNone.  Otherwise the appropriate OMX error will be returned.
+        When OMX_ErrorNotImplemented is returned, one or both components is
+        a non-interop component and does not support tunneling.
+
+        On failure, the ports of both components are setup for communication
+        with the application / IL Client.
+    @ingroup core tun
+ */
+OMX_API OMX_ERRORTYPE OMX_APIENTRY OMX_SetupTunnel(
+    OMX_IN  OMX_HANDLETYPE hOutput,
+    OMX_IN  OMX_U32 nPortOutput,
+    OMX_IN  OMX_HANDLETYPE hInput,
+    OMX_IN  OMX_U32 nPortInput);
+
+/** @ingroup cp */
+OMX_API OMX_ERRORTYPE   OMX_GetContentPipe(
+    OMX_OUT OMX_HANDLETYPE *hPipe,
+    OMX_IN OMX_STRING szURI);
+
+/** The OMX_GetComponentsOfRole method will return the number of components that support the given
+    role and (if the compNames field is non-NULL) the names of those components. The call will fail if
+    an insufficiently sized array of names is supplied. To ensure the array is sufficiently sized the
+    client should:
+        * first call this function with the compNames field NULL to determine the number of component names
+        * second call this function with the compNames field pointing to an array of names allocated
+          according to the number returned by the first call.
+
+    The core should return from this call within 5 msec.
+
+    @param [in] role
+        This is generic standard component name consisting only of component class
+        name and the type within that class (e.g. 'audio_decoder.aac').
+    @param [inout] pNumComps
+        This is used both as input and output.
+
+        If compNames is NULL, the input is ignored and the output specifies how many components support
+        the given role.
+
+        If compNames is not NULL, on input it bounds the size of the input structure and
+        on output, it specifies the number of components string names listed within the compNames parameter.
+    @param [inout] compNames
+        If NULL this field is ignored. If non-NULL this points to an array of 128-byte strings which accepts
+        a list of the names of all physical components that implement the specified standard component name.
+        Each name is NULL terminated. numComps indicates the number of names.
+    @ingroup core
+ */
+OMX_API OMX_ERRORTYPE OMX_GetComponentsOfRole (
+    OMX_IN      OMX_STRING role,
+    OMX_INOUT   OMX_U32 *pNumComps,
+    OMX_INOUT   OMX_U8  **compNames);
+
+/** The OMX_GetRolesOfComponent method will return the number of roles supported by the given
+    component and (if the roles field is non-NULL) the names of those roles. The call will fail if
+    an insufficiently sized array of names is supplied. To ensure the array is sufficiently sized the
+    client should:
+        * first call this function with the roles field NULL to determine the number of role names
+        * second call this function with the roles field pointing to an array of names allocated
+          according to the number returned by the first call.
+
+    The core should return from this call within 5 msec.
+
+    @param [in] compName
+        This is the name of the component being queried about.
+    @param [inout] pNumRoles
+        This is used both as input and output.
+
+        If roles is NULL, the input is ignored and the output specifies how many roles the component supports.
+
+        If compNames is not NULL, on input it bounds the size of the input structure and
+        on output, it specifies the number of roles string names listed within the roles parameter.
+    @param [out] roles
+        If NULL this field is ignored. If non-NULL this points to an array of 128-byte strings
+        which accepts a list of the names of all standard components roles implemented on the
+        specified component name. numComps indicates the number of names.
+    @ingroup core
+ */
+OMX_API OMX_ERRORTYPE OMX_GetRolesOfComponent (
+    OMX_IN      OMX_STRING compName,
+    OMX_INOUT   OMX_U32 *pNumRoles,
+    OMX_OUT     OMX_U8 **roles);
+
+#ifdef __cplusplus
+}
+#endif /* __cplusplus */
+
+#endif
+/* File EOF */
+
diff --git a/sf-extra/omx-il/OMX_CoreExt.h b/sf-extra/omx-il/OMX_CoreExt.h
new file mode 100644
index 00000000..e2e21cc0
--- /dev/null
+++ b/sf-extra/omx-il/OMX_CoreExt.h
@@ -0,0 +1,73 @@
+/*
+ * Copyright (c) 2016 The Khronos Group Inc.
+ *
+ * Permission is hereby granted, free of charge, to any person obtaining
+ * a copy of this software and associated documentation files (the
+ * "Software"), to deal in the Software without restriction, including
+ * without limitation the rights to use, copy, modify, merge, publish,
+ * distribute, sublicense, and/or sell copies of the Software, and to
+ * permit persons to whom the Software is furnished to do so, subject
+ * to the following conditions:
+ * The above copyright notice and this permission notice shall be included
+ * in all copies or substantial portions of the Software.
+ *
+ * THE SOFTWARE IS PROVIDED "AS IS", WITHOUT WARRANTY OF ANY KIND, EXPRESS
+ * OR IMPLIED, INCLUDING BUT NOT LIMITED TO THE WARRANTIES OF
+ * MERCHANTABILITY, FITNESS FOR A PARTICULAR PURPOSE AND NONINFRINGEMENT.
+ * IN NO EVENT SHALL THE AUTHORS OR COPYRIGHT HOLDERS BE LIABLE FOR ANY
+ * CLAIM, DAMAGES OR OTHER LIABILITY, WHETHER IN AN ACTION OF CONTRACT,
+ * TORT OR OTHERWISE, ARISING FROM, OUT OF OR IN CONNECTION WITH THE
+ * SOFTWARE OR THE USE OR OTHER DEALINGS IN THE SOFTWARE.
+ *
+ */
+
+/** OMX_CoreExt.h - OpenMax IL version 1.1.2
+ * The OMX_CoreExt header file contains extensions to the definitions used
+ * by both the application and the component to access common items.
+ */
+
+#ifndef OMX_CoreExt_h
+#define OMX_CoreExt_h
+
+#ifdef __cplusplus
+extern "C" {
+#endif /* __cplusplus */
+
+/* Each OMX header shall include all required header files to allow the
+ * header to compile without errors.  The includes below are required
+ * for this header file to compile successfully
+ */
+#include <OMX_Core.h>
+
+/** Extensions to the standard IL errors. */ 
+typedef enum OMX_ERROREXTTYPE 
+{
+    OMX_ErrorInvalidMode = (OMX_S32) (OMX_ErrorKhronosExtensions + 0x00000001),
+    OMX_ErrorExtMax = 0x7FFFFFFF
+} OMX_ERROREXTTYPE;
+
+
+/** Event type extensions. */
+typedef enum OMX_EVENTEXTTYPE
+{
+    OMX_EventIndexSettingChanged = OMX_EventKhronosExtensions, /**< component signals the IL client of a change
+                                                                    in a param, config, or extension */
+    OMX_EventExtMax = 0x7FFFFFFF
+} OMX_EVENTEXTTYPE;
+
+
+/** Enable or disable a callback event. */
+typedef struct OMX_CONFIG_CALLBACKREQUESTTYPE {
+    OMX_U32 nSize;              /**< size of the structure in bytes */
+    OMX_VERSIONTYPE nVersion;   /**< OMX specification version information */
+    OMX_U32 nPortIndex;         /**< port that this structure applies to */
+    OMX_INDEXTYPE nIndex;       /**< the index the callback is requested for */
+    OMX_BOOL bEnable;           /**< enable (OMX_TRUE) or disable (OMX_FALSE) the callback */
+} OMX_CONFIG_CALLBACKREQUESTTYPE;
+
+#ifdef __cplusplus
+}
+#endif /* __cplusplus */
+
+#endif /* OMX_CoreExt_h */
+/* File EOF */
diff --git a/sf-extra/omx-il/OMX_IVCommon.h b/sf-extra/omx-il/OMX_IVCommon.h
new file mode 100644
index 00000000..9aad7e96
--- /dev/null
+++ b/sf-extra/omx-il/OMX_IVCommon.h
@@ -0,0 +1,993 @@
+/**
+ * Copyright (c) 2008 The Khronos Group Inc.
+ *
+ * Permission is hereby granted, free of charge, to any person obtaining
+ * a copy of this software and associated documentation files (the
+ * "Software"), to deal in the Software without restriction, including
+ * without limitation the rights to use, copy, modify, merge, publish,
+ * distribute, sublicense, and/or sell copies of the Software, and to
+ * permit persons to whom the Software is furnished to do so, subject
+ * to the following conditions:
+ * The above copyright notice and this permission notice shall be included
+ * in all copies or substantial portions of the Software.
+ *
+ * THE SOFTWARE IS PROVIDED "AS IS", WITHOUT WARRANTY OF ANY KIND, EXPRESS
+ * OR IMPLIED, INCLUDING BUT NOT LIMITED TO THE WARRANTIES OF
+ * MERCHANTABILITY, FITNESS FOR A PARTICULAR PURPOSE AND NONINFRINGEMENT.
+ * IN NO EVENT SHALL THE AUTHORS OR COPYRIGHT HOLDERS BE LIABLE FOR ANY
+ * CLAIM, DAMAGES OR OTHER LIABILITY, WHETHER IN AN ACTION OF CONTRACT,
+ * TORT OR OTHERWISE, ARISING FROM, OUT OF OR IN CONNECTION WITH THE
+ * SOFTWARE OR THE USE OR OTHER DEALINGS IN THE SOFTWARE.
+ *
+ */
+
+/**
+ * @file OMX_IVCommon.h - OpenMax IL version 1.1.2
+ *  The structures needed by Video and Image components to exchange
+ *  parameters and configuration data with the components.
+ */
+#ifndef OMX_IVCommon_h
+#define OMX_IVCommon_h
+
+#ifdef __cplusplus
+extern "C" {
+#endif /* __cplusplus */
+
+/**
+ * Each OMX header must include all required header files to allow the header
+ * to compile without errors.  The includes below are required for this header
+ * file to compile successfully
+ */
+
+#include <OMX_Core.h>
+
+/** @defgroup iv OpenMAX IL Imaging and Video Domain
+ * Common structures for OpenMAX IL Imaging and Video domains
+ * @{
+ */
+
+
+/**
+ * Enumeration defining possible uncompressed image/video formats.
+ *
+ * ENUMS:
+ *  Unused                 : Placeholder value when format is N/A
+ *  Monochrome             : black and white
+ *  8bitRGB332             : Red 7:5, Green 4:2, Blue 1:0
+ *  12bitRGB444            : Red 11:8, Green 7:4, Blue 3:0
+ *  16bitARGB4444          : Alpha 15:12, Red 11:8, Green 7:4, Blue 3:0
+ *  16bitARGB1555          : Alpha 15, Red 14:10, Green 9:5, Blue 4:0
+ *  16bitRGB565            : Red 15:11, Green 10:5, Blue 4:0
+ *  16bitBGR565            : Blue 15:11, Green 10:5, Red 4:0
+ *  18bitRGB666            : Red 17:12, Green 11:6, Blue 5:0
+ *  18bitARGB1665          : Alpha 17, Red 16:11, Green 10:5, Blue 4:0
+ *  19bitARGB1666          : Alpha 18, Red 17:12, Green 11:6, Blue 5:0
+ *  24bitRGB888            : Red 24:16, Green 15:8, Blue 7:0
+ *  24bitBGR888            : Blue 24:16, Green 15:8, Red 7:0
+ *  24bitARGB1887          : Alpha 23, Red 22:15, Green 14:7, Blue 6:0
+ *  25bitARGB1888          : Alpha 24, Red 23:16, Green 15:8, Blue 7:0
+ *  32bitBGRA8888          : Blue 31:24, Green 23:16, Red 15:8, Alpha 7:0
+ *  32bitARGB8888          : Alpha 31:24, Red 23:16, Green 15:8, Blue 7:0
+ *  YUV411Planar           : U,Y are subsampled by a factor of 4 horizontally
+ *  YUV411PackedPlanar     : packed per payload in planar slices
+ *  YUV420Planar           : Three arrays Y,U,V.
+ *  YUV420PackedPlanar     : packed per payload in planar slices
+ *  YUV420SemiPlanar       : Two arrays, one is all Y, the other is U and V
+ *  YUV422Planar           : Three arrays Y,U,V.
+ *  YUV422PackedPlanar     : packed per payload in planar slices
+ *  YUV422SemiPlanar       : Two arrays, one is all Y, the other is U and V
+ *  YCbYCr                 : Organized as 16bit YUYV (i.e. YCbYCr)
+ *  YCrYCb                 : Organized as 16bit YVYU (i.e. YCrYCb)
+ *  CbYCrY                 : Organized as 16bit UYVY (i.e. CbYCrY)
+ *  CrYCbY                 : Organized as 16bit VYUY (i.e. CrYCbY)
+ *  YUV444Interleaved      : Each pixel contains equal parts YUV
+ *  RawBayer8bit           : SMIA camera output format
+ *  RawBayer10bit          : SMIA camera output format
+ *  RawBayer8bitcompressed : SMIA camera output format
+ */
+typedef enum OMX_COLOR_FORMATTYPE {
+    OMX_COLOR_FormatUnused,
+    OMX_COLOR_FormatMonochrome,
+    OMX_COLOR_Format8bitRGB332,
+    OMX_COLOR_Format12bitRGB444,
+    OMX_COLOR_Format16bitARGB4444,
+    OMX_COLOR_Format16bitARGB1555,
+    OMX_COLOR_Format16bitRGB565,
+    OMX_COLOR_Format16bitBGR565,
+    OMX_COLOR_Format18bitRGB666,
+    OMX_COLOR_Format18bitARGB1665,
+    OMX_COLOR_Format19bitARGB1666,
+    OMX_COLOR_Format24bitRGB888,
+    OMX_COLOR_Format24bitBGR888,
+    OMX_COLOR_Format24bitARGB1887,
+    OMX_COLOR_Format25bitARGB1888,
+    OMX_COLOR_Format32bitBGRA8888,
+    OMX_COLOR_Format32bitARGB8888,
+    OMX_COLOR_FormatYUV411Planar,
+    OMX_COLOR_FormatYUV411PackedPlanar,
+    OMX_COLOR_FormatYUV420Planar,
+    OMX_COLOR_FormatYUV420PackedPlanar,
+    OMX_COLOR_FormatYUV420SemiPlanar,
+    OMX_COLOR_FormatYUV422Planar,
+    OMX_COLOR_FormatYUV422PackedPlanar,
+    OMX_COLOR_FormatYUV422SemiPlanar,
+    OMX_COLOR_FormatYCbYCr,
+    OMX_COLOR_FormatYCrYCb,
+    OMX_COLOR_FormatCbYCrY,
+    OMX_COLOR_FormatCrYCbY,
+    OMX_COLOR_FormatYUV444Interleaved,
+    OMX_COLOR_FormatRawBayer8bit,
+    OMX_COLOR_FormatRawBayer10bit,
+    OMX_COLOR_FormatRawBayer8bitcompressed,
+    OMX_COLOR_FormatL2,
+    OMX_COLOR_FormatL4,
+    OMX_COLOR_FormatL8,
+    OMX_COLOR_FormatL16,
+    OMX_COLOR_FormatL24,
+    OMX_COLOR_FormatL32,
+    OMX_COLOR_FormatYUV420PackedSemiPlanar,
+    OMX_COLOR_FormatYUV422PackedSemiPlanar,
+    OMX_COLOR_Format18BitBGR666,
+    OMX_COLOR_Format24BitARGB6666,
+    OMX_COLOR_Format24BitABGR6666,
+    OMX_COLOR_FormatKhronosExtensions = 0x6F000000, /**< Reserved region for introducing Khronos Standard Extensions */
+    OMX_COLOR_FormatVendorStartUnused = 0x7F000000, /**< Reserved region for introducing Vendor Extensions */
+
+    /* Starfive extensions */
+    /* I420 */
+    OMX_COLOR_FormatYUV420Planar_P10_16BIT_MSB,
+    OMX_COLOR_FormatYUV420Planar_P10_16BIT_LSB,
+    OMX_COLOR_FormatYUV420Planar_P12_16BIT_MSB,
+    OMX_COLOR_FormatYUV420Planar_P12_16BIT_LSB,
+    /* NV12 */
+    OMX_COLOR_FormatYUV420SemiPlanar_P10_16BIT_MSB,
+    OMX_COLOR_FormatYUV420SemiPlanar_P10_16BIT_LSB,
+    OMX_COLOR_FormatYUV420SemiPlanar_P12_16BIT_MSB,
+    OMX_COLOR_FormatYUV420SemiPlanar_P12_16BIT_LSB,
+    /* NV21 */
+    OMX_COLOR_FormatYVU420SemiPlanar,
+    OMX_COLOR_FormatYVU420SemiPlanar_P10_16BIT_MSB,
+    OMX_COLOR_FormatYVU420SemiPlanar_P10_16BIT_LSB,
+    OMX_COLOR_FormatYVU420SemiPlanar_P12_16BIT_MSB,
+    OMX_COLOR_FormatYVU420SemiPlanar_P12_16BIT_LSB,
+    /* I422 */
+    OMX_COLOR_FormatYUV422Planar_P10_16BIT_MSB,
+    OMX_COLOR_FormatYUV422Planar_P10_16BIT_LSB,
+    OMX_COLOR_FormatYUV422Planar_P12_16BIT_MSB,
+    OMX_COLOR_FormatYUV422Planar_P12_16BIT_LSB,
+    /* NV16 */
+    OMX_COLOR_FormatYUV422SemiPlanar_P10_16BIT_MSB,
+    OMX_COLOR_FormatYUV422SemiPlanar_P10_16BIT_LSB,
+    OMX_COLOR_FormatYUV422SemiPlanar_P12_16BIT_MSB,
+    OMX_COLOR_FormatYUV422SemiPlanar_P12_16BIT_LSB,
+    /* NV61 */
+    OMX_COLOR_FormatYVU422SemiPlanar,
+    OMX_COLOR_FormatYVU422SemiPlanar_P10_16BIT_MSB,
+    OMX_COLOR_FormatYVU422SemiPlanar_P10_16BIT_LSB,
+    OMX_COLOR_FormatYVU422SemiPlanar_P12_16BIT_MSB,
+    OMX_COLOR_FormatYVU422SemiPlanar_P12_16BIT_LSB,
+    /* YUYV */
+    OMX_COLOR_FormatYCbYCr_P10_16BIT_MSB,
+    OMX_COLOR_FormatYCbYCr_P10_16BIT_LSB,
+    OMX_COLOR_FormatYCbYCr_P12_16BIT_MSB,
+    OMX_COLOR_FormatYCbYCr_P12_16BIT_LSB,
+    /* YVYU */
+    OMX_COLOR_FormatYCrYCb_P10_16BIT_MSB,
+    OMX_COLOR_FormatYCrYCb_P10_16BIT_LSB,
+    OMX_COLOR_FormatYCrYCb_P12_16BIT_MSB,
+    OMX_COLOR_FormatYCrYCb_P12_16BIT_LSB,
+    /* UYVY */
+    OMX_COLOR_FormatCbYCrY_P10_16BIT_MSB,
+    OMX_COLOR_FormatCbYCrY_P10_16BIT_LSB,
+    OMX_COLOR_FormatCbYCrY_P12_16BIT_MSB,
+    OMX_COLOR_FormatCbYCrY_P12_16BIT_LSB,
+    /* VYUY */
+    OMX_COLOR_FormatCrYCbY_P10_16BIT_MSB,
+    OMX_COLOR_FormatCrYCbY_P10_16BIT_LSB,
+    OMX_COLOR_FormatCrYCbY_P12_16BIT_MSB,
+    OMX_COLOR_FormatCrYCbY_P12_16BIT_LSB,
+    /* I444 */
+    OMX_COLOR_FormatYUV444Planar,
+    OMX_COLOR_FormatYUV444Planar_P10_16BIT_MSB,
+    OMX_COLOR_FormatYUV444Planar_P10_16BIT_LSB,
+    OMX_COLOR_FormatYUV444Planar_P12_16BIT_MSB,
+    OMX_COLOR_FormatYUV444Planar_P12_16BIT_LSB,
+    /* YUV444PACKED */
+    OMX_COLOR_FormatYUV444Interleaved_P10_16BIT_MSB,
+    OMX_COLOR_FormatYUV444Interleaved_P10_16BIT_LSB,
+    OMX_COLOR_FormatYUV444Interleaved_P12_16BIT_MSB,
+    OMX_COLOR_FormatYUV444Interleaved_P12_16BIT_LSB,
+    /* YUV400 */
+    OMX_COLOR_FormatYUV400,
+    OMX_COLOR_FormatYUV400_P10_16BIT_MSB,
+    OMX_COLOR_FormatYUV400_P10_16BIT_LSB,
+    OMX_COLOR_FormatYUV400_P12_16BIT_MSB,
+    OMX_COLOR_FormatYUV400_P12_16BIT_LSB,
+    /* Starfive extensions end */
+
+    OMX_COLOR_FormatMax = 0x7FFFFFFF
+} OMX_COLOR_FORMATTYPE;
+
+
+/**
+ * Defines the matrix for conversion from RGB to YUV or vice versa.
+ * iColorMatrix should be initialized with the fixed point values
+ * used in converting between formats.
+ */
+typedef struct OMX_CONFIG_COLORCONVERSIONTYPE {
+    OMX_U32 nSize;              /**< Size of the structure in bytes */
+    OMX_VERSIONTYPE nVersion;   /**< OMX specification version info */
+    OMX_U32 nPortIndex;         /**< Port that this struct applies to */
+    OMX_S32 xColorMatrix[3][3]; /**< Stored in signed Q16 format */
+    OMX_S32 xColorOffset[4];    /**< Stored in signed Q16 format */
+} OMX_CONFIG_COLORCONVERSIONTYPE;
+
+
+/**
+ * Structure defining percent to scale each frame dimension.  For example:
+ * To make the width 50% larger, use fWidth = 1.5 and to make the width
+ * 1/2 the original size, use fWidth = 0.5
+ */
+typedef struct OMX_CONFIG_SCALEFACTORTYPE {
+    OMX_U32 nSize;            /**< Size of the structure in bytes */
+    OMX_VERSIONTYPE nVersion; /**< OMX specification version info */
+    OMX_U32 nPortIndex;       /**< Port that this struct applies to */
+    OMX_S32 xWidth;           /**< Fixed point value stored as Q16 */
+    OMX_S32 xHeight;          /**< Fixed point value stored as Q16 */
+} OMX_CONFIG_SCALEFACTORTYPE;
+
+
+/**
+ * Enumeration of possible image filter types
+ */
+typedef enum OMX_IMAGEFILTERTYPE {
+    OMX_ImageFilterNone,
+    OMX_ImageFilterNoise,
+    OMX_ImageFilterEmboss,
+    OMX_ImageFilterNegative,
+    OMX_ImageFilterSketch,
+    OMX_ImageFilterOilPaint,
+    OMX_ImageFilterHatch,
+    OMX_ImageFilterGpen,
+    OMX_ImageFilterAntialias,
+    OMX_ImageFilterDeRing,
+    OMX_ImageFilterSolarize,
+    OMX_ImageFilterKhronosExtensions = 0x6F000000, /**< Reserved region for introducing Khronos Standard Extensions */
+    OMX_ImageFilterVendorStartUnused = 0x7F000000, /**< Reserved region for introducing Vendor Extensions */
+    OMX_ImageFilterMax = 0x7FFFFFFF
+} OMX_IMAGEFILTERTYPE;
+
+
+/**
+ * Image filter configuration
+ *
+ * STRUCT MEMBERS:
+ *  nSize        : Size of the structure in bytes
+ *  nVersion     : OMX specification version information
+ *  nPortIndex   : Port that this structure applies to
+ *  eImageFilter : Image filter type enumeration
+ */
+typedef struct OMX_CONFIG_IMAGEFILTERTYPE {
+    OMX_U32 nSize;
+    OMX_VERSIONTYPE nVersion;
+    OMX_U32 nPortIndex;
+    OMX_IMAGEFILTERTYPE eImageFilter;
+} OMX_CONFIG_IMAGEFILTERTYPE;
+
+
+/**
+ * Customized U and V for color enhancement
+ *
+ * STRUCT MEMBERS:
+ *  nSize             : Size of the structure in bytes
+ *  nVersion          : OMX specification version information
+ *  nPortIndex        : Port that this structure applies to
+ *  bColorEnhancement : Enable/disable color enhancement
+ *  nCustomizedU      : Practical values: 16-240, range: 0-255, value set for
+ *                      U component
+ *  nCustomizedV      : Practical values: 16-240, range: 0-255, value set for
+ *                      V component
+ */
+typedef struct OMX_CONFIG_COLORENHANCEMENTTYPE {
+    OMX_U32 nSize;
+    OMX_VERSIONTYPE nVersion;
+    OMX_U32 nPortIndex;
+    OMX_BOOL bColorEnhancement;
+    OMX_U8 nCustomizedU;
+    OMX_U8 nCustomizedV;
+} OMX_CONFIG_COLORENHANCEMENTTYPE;
+
+
+/**
+ * Define color key and color key mask
+ *
+ * STRUCT MEMBERS:
+ *  nSize      : Size of the structure in bytes
+ *  nVersion   : OMX specification version information
+ *  nPortIndex : Port that this structure applies to
+ *  nARGBColor : 32bit Alpha, Red, Green, Blue Color
+ *  nARGBMask  : 32bit Mask for Alpha, Red, Green, Blue channels
+ */
+typedef struct OMX_CONFIG_COLORKEYTYPE {
+    OMX_U32 nSize;
+    OMX_VERSIONTYPE nVersion;
+    OMX_U32 nPortIndex;
+    OMX_U32 nARGBColor;
+    OMX_U32 nARGBMask;
+} OMX_CONFIG_COLORKEYTYPE;
+
+
+/**
+ * List of color blend types for pre/post processing
+ *
+ * ENUMS:
+ *  None          : No color blending present
+ *  AlphaConstant : Function is (alpha_constant * src) +
+ *                  (1 - alpha_constant) * dst)
+ *  AlphaPerPixel : Function is (alpha * src) + (1 - alpha) * dst)
+ *  Alternate     : Function is alternating pixels from src and dst
+ *  And           : Function is (src & dst)
+ *  Or            : Function is (src | dst)
+ *  Invert        : Function is ~src
+ */
+typedef enum OMX_COLORBLENDTYPE {
+    OMX_ColorBlendNone,
+    OMX_ColorBlendAlphaConstant,
+    OMX_ColorBlendAlphaPerPixel,
+    OMX_ColorBlendAlternate,
+    OMX_ColorBlendAnd,
+    OMX_ColorBlendOr,
+    OMX_ColorBlendInvert,
+    OMX_ColorBlendKhronosExtensions = 0x6F000000, /**< Reserved region for introducing Khronos Standard Extensions */
+    OMX_ColorBlendVendorStartUnused = 0x7F000000, /**< Reserved region for introducing Vendor Extensions */
+    OMX_ColorBlendMax = 0x7FFFFFFF
+} OMX_COLORBLENDTYPE;
+
+
+/**
+ * Color blend configuration
+ *
+ * STRUCT MEMBERS:
+ *  nSize             : Size of the structure in bytes
+ *  nVersion          : OMX specification version information
+ *  nPortIndex        : Port that this structure applies to
+ *  nRGBAlphaConstant : Constant global alpha values when global alpha is used
+ *  eColorBlend       : Color blend type enumeration
+ */
+typedef struct OMX_CONFIG_COLORBLENDTYPE {
+    OMX_U32 nSize;
+    OMX_VERSIONTYPE nVersion;
+    OMX_U32 nPortIndex;
+    OMX_U32 nRGBAlphaConstant;
+    OMX_COLORBLENDTYPE  eColorBlend;
+} OMX_CONFIG_COLORBLENDTYPE;
+
+
+/**
+ * Hold frame dimension
+ *
+ * STRUCT MEMBERS:
+ *  nSize      : Size of the structure in bytes
+ *  nVersion   : OMX specification version information
+ *  nPortIndex : Port that this structure applies to
+ *  nWidth     : Frame width in pixels
+ *  nHeight    : Frame height in pixels
+ */
+typedef struct OMX_FRAMESIZETYPE {
+    OMX_U32 nSize;
+    OMX_VERSIONTYPE nVersion;
+    OMX_U32 nPortIndex;
+    OMX_U32 nWidth;
+    OMX_U32 nHeight;
+} OMX_FRAMESIZETYPE;
+
+
+/**
+ * Rotation configuration
+ *
+ * STRUCT MEMBERS:
+ *  nSize      : Size of the structure in bytes
+ *  nVersion   : OMX specification version information
+ *  nPortIndex : Port that this structure applies to
+ *  nRotation  : +/- integer rotation value
+ */
+typedef struct OMX_CONFIG_ROTATIONTYPE {
+    OMX_U32 nSize;
+    OMX_VERSIONTYPE nVersion;
+    OMX_U32 nPortIndex;
+    OMX_S32 nRotation;
+} OMX_CONFIG_ROTATIONTYPE;
+
+
+/**
+ * Possible mirroring directions for pre/post processing
+ *
+ * ENUMS:
+ *  None       : No mirroring
+ *  Vertical   : Vertical mirroring, flip on X axis
+ *  Horizontal : Horizontal mirroring, flip on Y axis
+ *  Both       : Both vertical and horizontal mirroring
+ */
+typedef enum OMX_MIRRORTYPE {
+    OMX_MirrorNone = 0,
+    OMX_MirrorVertical,
+    OMX_MirrorHorizontal,
+    OMX_MirrorBoth,
+    OMX_MirrorKhronosExtensions = 0x6F000000, /**< Reserved region for introducing Khronos Standard Extensions */
+    OMX_MirrorVendorStartUnused = 0x7F000000, /**< Reserved region for introducing Vendor Extensions */
+    OMX_MirrorMax = 0x7FFFFFFF
+} OMX_MIRRORTYPE;
+
+
+/**
+ * Mirroring configuration
+ *
+ * STRUCT MEMBERS:
+ *  nSize      : Size of the structure in bytes
+ *  nVersion   : OMX specification version information
+ *  nPortIndex : Port that this structure applies to
+ *  eMirror    : Mirror type enumeration
+ */
+typedef struct OMX_CONFIG_MIRRORTYPE {
+    OMX_U32 nSize;
+    OMX_VERSIONTYPE nVersion;
+    OMX_U32 nPortIndex;
+    OMX_MIRRORTYPE  eMirror;
+} OMX_CONFIG_MIRRORTYPE;
+
+
+/**
+ * Position information only
+ *
+ * STRUCT MEMBERS:
+ *  nSize      : Size of the structure in bytes
+ *  nVersion   : OMX specification version information
+ *  nPortIndex : Port that this structure applies to
+ *  nX         : X coordinate for the point
+ *  nY         : Y coordinate for the point
+ */
+typedef struct OMX_CONFIG_POINTTYPE {
+    OMX_U32 nSize;
+    OMX_VERSIONTYPE nVersion;
+    OMX_U32 nPortIndex;
+    OMX_S32 nX;
+    OMX_S32 nY;
+} OMX_CONFIG_POINTTYPE;
+
+
+/**
+ * Frame size plus position
+ *
+ * STRUCT MEMBERS:
+ *  nSize      : Size of the structure in bytes
+ *  nVersion   : OMX specification version information
+ *  nPortIndex : Port that this structure applies to
+ *  nLeft      : X Coordinate of the top left corner of the rectangle
+ *  nTop       : Y Coordinate of the top left corner of the rectangle
+ *  nWidth     : Width of the rectangle
+ *  nHeight    : Height of the rectangle
+ */
+typedef struct OMX_CONFIG_RECTTYPE {
+    OMX_U32 nSize;
+    OMX_VERSIONTYPE nVersion;
+    OMX_U32 nPortIndex;
+    OMX_S32 nLeft;
+    OMX_S32 nTop;
+    OMX_U32 nWidth;
+    OMX_U32 nHeight;
+} OMX_CONFIG_RECTTYPE;
+
+
+/**
+ * Deblocking state; it is required to be set up before starting the codec
+ *
+ * STRUCT MEMBERS:
+ *  nSize       : Size of the structure in bytes
+ *  nVersion    : OMX specification version information
+ *  nPortIndex  : Port that this structure applies to
+ *  bDeblocking : Enable/disable deblocking mode
+ */
+typedef struct OMX_PARAM_DEBLOCKINGTYPE {
+    OMX_U32 nSize;
+    OMX_VERSIONTYPE nVersion;
+    OMX_U32 nPortIndex;
+    OMX_BOOL bDeblocking;
+} OMX_PARAM_DEBLOCKINGTYPE;
+
+
+/**
+ * Stabilization state
+ *
+ * STRUCT MEMBERS:
+ *  nSize      : Size of the structure in bytes
+ *  nVersion   : OMX specification version information
+ *  nPortIndex : Port that this structure applies to
+ *  bStab      : Enable/disable frame stabilization state
+ */
+typedef struct OMX_CONFIG_FRAMESTABTYPE {
+    OMX_U32 nSize;
+    OMX_VERSIONTYPE nVersion;
+    OMX_U32 nPortIndex;
+    OMX_BOOL bStab;
+} OMX_CONFIG_FRAMESTABTYPE;
+
+
+/**
+ * White Balance control type
+ *
+ * STRUCT MEMBERS:
+ *  SunLight : Referenced in JSR-234
+ *  Flash    : Optimal for device's integrated flash
+ */
+typedef enum OMX_WHITEBALCONTROLTYPE {
+    OMX_WhiteBalControlOff = 0,
+    OMX_WhiteBalControlAuto,
+    OMX_WhiteBalControlSunLight,
+    OMX_WhiteBalControlCloudy,
+    OMX_WhiteBalControlShade,
+    OMX_WhiteBalControlTungsten,
+    OMX_WhiteBalControlFluorescent,
+    OMX_WhiteBalControlIncandescent,
+    OMX_WhiteBalControlFlash,
+    OMX_WhiteBalControlHorizon,
+    OMX_WhiteBalControlKhronosExtensions = 0x6F000000, /**< Reserved region for introducing Khronos Standard Extensions */
+    OMX_WhiteBalControlVendorStartUnused = 0x7F000000, /**< Reserved region for introducing Vendor Extensions */
+    OMX_WhiteBalControlMax = 0x7FFFFFFF
+} OMX_WHITEBALCONTROLTYPE;
+
+
+/**
+ * White Balance control configuration
+ *
+ * STRUCT MEMBERS:
+ *  nSize            : Size of the structure in bytes
+ *  nVersion         : OMX specification version information
+ *  nPortIndex       : Port that this structure applies to
+ *  eWhiteBalControl : White balance enumeration
+ */
+typedef struct OMX_CONFIG_WHITEBALCONTROLTYPE {
+    OMX_U32 nSize;
+    OMX_VERSIONTYPE nVersion;
+    OMX_U32 nPortIndex;
+    OMX_WHITEBALCONTROLTYPE eWhiteBalControl;
+} OMX_CONFIG_WHITEBALCONTROLTYPE;
+
+
+/**
+ * Exposure control type
+ */
+typedef enum OMX_EXPOSURECONTROLTYPE {
+    OMX_ExposureControlOff = 0,
+    OMX_ExposureControlAuto,
+    OMX_ExposureControlNight,
+    OMX_ExposureControlBackLight,
+    OMX_ExposureControlSpotLight,
+    OMX_ExposureControlSports,
+    OMX_ExposureControlSnow,
+    OMX_ExposureControlBeach,
+    OMX_ExposureControlLargeAperture,
+    OMX_ExposureControlSmallApperture,
+    OMX_ExposureControlKhronosExtensions = 0x6F000000, /**< Reserved region for introducing Khronos Standard Extensions */
+    OMX_ExposureControlVendorStartUnused = 0x7F000000, /**< Reserved region for introducing Vendor Extensions */
+    OMX_ExposureControlMax = 0x7FFFFFFF
+} OMX_EXPOSURECONTROLTYPE;
+
+
+/**
+ * White Balance control configuration
+ *
+ * STRUCT MEMBERS:
+ *  nSize            : Size of the structure in bytes
+ *  nVersion         : OMX specification version information
+ *  nPortIndex       : Port that this structure applies to
+ *  eExposureControl : Exposure control enumeration
+ */
+typedef struct OMX_CONFIG_EXPOSURECONTROLTYPE {
+    OMX_U32 nSize;
+    OMX_VERSIONTYPE nVersion;
+    OMX_U32 nPortIndex;
+    OMX_EXPOSURECONTROLTYPE eExposureControl;
+} OMX_CONFIG_EXPOSURECONTROLTYPE;
+
+
+/**
+ * Defines sensor supported mode.
+ *
+ * STRUCT MEMBERS:
+ *  nSize      : Size of the structure in bytes
+ *  nVersion   : OMX specification version information
+ *  nPortIndex : Port that this structure applies to
+ *  nFrameRate : Single shot mode is indicated by a 0
+ *  bOneShot   : Enable for single shot, disable for streaming
+ *  sFrameSize : Framesize
+ */
+typedef struct OMX_PARAM_SENSORMODETYPE {
+    OMX_U32 nSize;
+    OMX_VERSIONTYPE nVersion;
+    OMX_U32 nPortIndex;
+    OMX_U32 nFrameRate;
+    OMX_BOOL bOneShot;
+    OMX_FRAMESIZETYPE sFrameSize;
+} OMX_PARAM_SENSORMODETYPE;
+
+
+/**
+ * Defines contrast level
+ *
+ * STRUCT MEMBERS:
+ *  nSize      : Size of the structure in bytes
+ *  nVersion   : OMX specification version information
+ *  nPortIndex : Port that this structure applies to
+ *  nContrast  : Values allowed for contrast -100 to 100, zero means no change
+ */
+typedef struct OMX_CONFIG_CONTRASTTYPE {
+    OMX_U32 nSize;
+    OMX_VERSIONTYPE nVersion;
+    OMX_U32 nPortIndex;
+    OMX_S32 nContrast;
+} OMX_CONFIG_CONTRASTTYPE;
+
+
+/**
+ * Defines brightness level
+ *
+ * STRUCT MEMBERS:
+ *  nSize       : Size of the structure in bytes
+ *  nVersion    : OMX specification version information
+ *  nPortIndex  : Port that this structure applies to
+ *  nBrightness : 0-100%
+ */
+typedef struct OMX_CONFIG_BRIGHTNESSTYPE {
+    OMX_U32 nSize;
+    OMX_VERSIONTYPE nVersion;
+    OMX_U32 nPortIndex;
+    OMX_U32 nBrightness;
+} OMX_CONFIG_BRIGHTNESSTYPE;
+
+
+/**
+ * Defines backlight level configuration for a video sink, e.g. LCD panel
+ *
+ * STRUCT MEMBERS:
+ *  nSize      : Size of the structure in bytes
+ *  nVersion   : OMX specification version information
+ *  nPortIndex : Port that this structure applies to
+ *  nBacklight : Values allowed for backlight 0-100%
+ *  nTimeout   : Number of milliseconds before backlight automatically turns
+ *               off.  A value of 0x0 disables backight timeout
+ */
+typedef struct OMX_CONFIG_BACKLIGHTTYPE {
+    OMX_U32 nSize;
+    OMX_VERSIONTYPE nVersion;
+    OMX_U32 nPortIndex;
+    OMX_U32 nBacklight;
+    OMX_U32 nTimeout;
+} OMX_CONFIG_BACKLIGHTTYPE;
+
+
+/**
+ * Defines setting for Gamma
+ *
+ * STRUCT MEMBERS:
+ *  nSize      : Size of the structure in bytes
+ *  nVersion   : OMX specification version information
+ *  nPortIndex : Port that this structure applies to
+ *  nGamma     : Values allowed for gamma -100 to 100, zero means no change
+ */
+typedef struct OMX_CONFIG_GAMMATYPE {
+    OMX_U32 nSize;
+    OMX_VERSIONTYPE nVersion;
+    OMX_U32 nPortIndex;
+    OMX_S32 nGamma;
+} OMX_CONFIG_GAMMATYPE;
+
+
+/**
+ * Define for setting saturation
+ *
+ * STRUCT MEMBERS:
+ *  nSize       : Size of the structure in bytes
+ *  nVersion    : OMX specification version information
+ *  nPortIndex  : Port that this structure applies to
+ *  nSaturation : Values allowed for saturation -100 to 100, zero means
+ *                no change
+ */
+typedef struct OMX_CONFIG_SATURATIONTYPE {
+    OMX_U32 nSize;
+    OMX_VERSIONTYPE nVersion;
+    OMX_U32 nPortIndex;
+    OMX_S32 nSaturation;
+} OMX_CONFIG_SATURATIONTYPE;
+
+
+/**
+ * Define for setting Lightness
+ *
+ * STRUCT MEMBERS:
+ *  nSize      : Size of the structure in bytes
+ *  nVersion   : OMX specification version information
+ *  nPortIndex : Port that this structure applies to
+ *  nLightness : Values allowed for lightness -100 to 100, zero means no
+ *               change
+ */
+typedef struct OMX_CONFIG_LIGHTNESSTYPE {
+    OMX_U32 nSize;
+    OMX_VERSIONTYPE nVersion;
+    OMX_U32 nPortIndex;
+    OMX_S32 nLightness;
+} OMX_CONFIG_LIGHTNESSTYPE;
+
+
+/**
+ * Plane blend configuration
+ *
+ * STRUCT MEMBERS:
+ *  nSize      : Size of the structure in bytes
+ *  nVersion   : OMX specification version information
+ *  nPortIndex : Index of input port associated with the plane.
+ *  nDepth     : Depth of the plane in relation to the screen. Higher
+ *               numbered depths are "behind" lower number depths.
+ *               This number defaults to the Port Index number.
+ *  nAlpha     : Transparency blending component for the entire plane.
+ *               See blending modes for more detail.
+ */
+typedef struct OMX_CONFIG_PLANEBLENDTYPE {
+    OMX_U32 nSize;
+    OMX_VERSIONTYPE nVersion;
+    OMX_U32 nPortIndex;
+    OMX_U32 nDepth;
+    OMX_U32 nAlpha;
+} OMX_CONFIG_PLANEBLENDTYPE;
+
+
+/**
+ * Define interlace type
+ *
+ * STRUCT MEMBERS:
+ *  nSize                 : Size of the structure in bytes
+ *  nVersion              : OMX specification version information
+ *  nPortIndex            : Port that this structure applies to
+ *  bEnable               : Enable control variable for this functionality
+ *                          (see below)
+ *  nInterleavePortIndex  : Index of input or output port associated with
+ *                          the interleaved plane.
+ *  pPlanarPortIndexes[4] : Index of input or output planar ports.
+ */
+typedef struct OMX_PARAM_INTERLEAVETYPE {
+    OMX_U32 nSize;
+    OMX_VERSIONTYPE nVersion;
+    OMX_U32 nPortIndex;
+    OMX_BOOL bEnable;
+    OMX_U32 nInterleavePortIndex;
+} OMX_PARAM_INTERLEAVETYPE;
+
+
+/**
+ * Defines the picture effect used for an input picture
+ */
+typedef enum OMX_TRANSITIONEFFECTTYPE {
+    OMX_EffectNone,
+    OMX_EffectFadeFromBlack,
+    OMX_EffectFadeToBlack,
+    OMX_EffectUnspecifiedThroughConstantColor,
+    OMX_EffectDissolve,
+    OMX_EffectWipe,
+    OMX_EffectUnspecifiedMixOfTwoScenes,
+    OMX_EffectKhronosExtensions = 0x6F000000, /**< Reserved region for introducing Khronos Standard Extensions */
+    OMX_EffectVendorStartUnused = 0x7F000000, /**< Reserved region for introducing Vendor Extensions */
+    OMX_EffectMax = 0x7FFFFFFF
+} OMX_TRANSITIONEFFECTTYPE;
+
+
+/**
+ * Structure used to configure current transition effect
+ *
+ * STRUCT MEMBERS:
+ * nSize      : Size of the structure in bytes
+ * nVersion   : OMX specification version information
+ * nPortIndex : Port that this structure applies to
+ * eEffect    : Effect to enable
+ */
+typedef struct OMX_CONFIG_TRANSITIONEFFECTTYPE {
+    OMX_U32 nSize;
+    OMX_VERSIONTYPE nVersion;
+    OMX_U32 nPortIndex;
+    OMX_TRANSITIONEFFECTTYPE eEffect;
+} OMX_CONFIG_TRANSITIONEFFECTTYPE;
+
+
+/**
+ * Defines possible data unit types for encoded video data. The data unit
+ * types are used both for encoded video input for playback as well as
+ * encoded video output from recording.
+ */
+typedef enum OMX_DATAUNITTYPE {
+    OMX_DataUnitCodedPicture,
+    OMX_DataUnitVideoSegment,
+    OMX_DataUnitSeveralSegments,
+    OMX_DataUnitArbitraryStreamSection,
+    OMX_DataUnitKhronosExtensions = 0x6F000000, /**< Reserved region for introducing Khronos Standard Extensions */
+    OMX_DataUnitVendorStartUnused = 0x7F000000, /**< Reserved region for introducing Vendor Extensions */
+    OMX_DataUnitMax = 0x7FFFFFFF
+} OMX_DATAUNITTYPE;
+
+
+/**
+ * Defines possible encapsulation types for coded video data unit. The
+ * encapsulation information is used both for encoded video input for
+ * playback as well as encoded video output from recording.
+ */
+typedef enum OMX_DATAUNITENCAPSULATIONTYPE {
+    OMX_DataEncapsulationElementaryStream,
+    OMX_DataEncapsulationGenericPayload,
+    OMX_DataEncapsulationRtpPayload,
+    OMX_DataEncapsulationKhronosExtensions = 0x6F000000, /**< Reserved region for introducing Khronos Standard Extensions */
+    OMX_DataEncapsulationVendorStartUnused = 0x7F000000, /**< Reserved region for introducing Vendor Extensions */
+    OMX_DataEncapsulationMax = 0x7FFFFFFF
+} OMX_DATAUNITENCAPSULATIONTYPE;
+
+
+/**
+ * Structure used to configure the type of being decoded/encoded
+ */
+typedef struct OMX_PARAM_DATAUNITTYPE {
+    OMX_U32 nSize;            /**< Size of the structure in bytes */
+    OMX_VERSIONTYPE nVersion; /**< OMX specification version information */
+    OMX_U32 nPortIndex;       /**< Port that this structure applies to */
+    OMX_DATAUNITTYPE eUnitType;
+    OMX_DATAUNITENCAPSULATIONTYPE eEncapsulationType;
+} OMX_PARAM_DATAUNITTYPE;
+
+
+/**
+ * Defines dither types
+ */
+typedef enum OMX_DITHERTYPE {
+    OMX_DitherNone,
+    OMX_DitherOrdered,
+    OMX_DitherErrorDiffusion,
+    OMX_DitherOther,
+    OMX_DitherKhronosExtensions = 0x6F000000, /**< Reserved region for introducing Khronos Standard Extensions */
+    OMX_DitherVendorStartUnused = 0x7F000000, /**< Reserved region for introducing Vendor Extensions */
+    OMX_DitherMax = 0x7FFFFFFF
+} OMX_DITHERTYPE;
+
+
+/**
+ * Structure used to configure current type of dithering
+ */
+typedef struct OMX_CONFIG_DITHERTYPE {
+    OMX_U32 nSize;            /**< Size of the structure in bytes */
+    OMX_VERSIONTYPE nVersion; /**< OMX specification version information */
+    OMX_U32 nPortIndex;       /**< Port that this structure applies to */
+    OMX_DITHERTYPE eDither;   /**< Type of dithering to use */
+} OMX_CONFIG_DITHERTYPE;
+
+typedef struct OMX_CONFIG_CAPTUREMODETYPE {
+    OMX_U32 nSize;
+    OMX_VERSIONTYPE nVersion;
+    OMX_U32 nPortIndex;     /**< Port that this structure applies to */
+    OMX_BOOL bContinuous;   /**< If true then ignore frame rate and emit capture
+                             *   data as fast as possible (otherwise obey port's frame rate). */
+    OMX_BOOL bFrameLimited; /**< If true then terminate capture after the port emits the
+                             *   specified number of frames (otherwise the port does not
+                             *   terminate the capture until instructed to do so by the client).
+                             *   Even if set, the client may manually terminate the capture prior
+                             *   to reaching the limit. */
+    OMX_U32 nFrameLimit;      /**< Limit on number of frames emitted during a capture (only
+                               *   valid if bFrameLimited is set). */
+} OMX_CONFIG_CAPTUREMODETYPE;
+
+typedef enum OMX_METERINGTYPE {
+
+    OMX_MeteringModeAverage,     /**< Center-weighted average metering. */
+    OMX_MeteringModeSpot,         /**< Spot (partial) metering. */
+    OMX_MeteringModeMatrix,      /**< Matrix or evaluative metering. */
+
+    OMX_MeteringKhronosExtensions = 0x6F000000, /**< Reserved region for introducing Khronos Standard Extensions */
+    OMX_MeteringVendorStartUnused = 0x7F000000, /**< Reserved region for introducing Vendor Extensions */
+    OMX_EVModeMax = 0x7fffffff
+} OMX_METERINGTYPE;
+
+typedef struct OMX_CONFIG_EXPOSUREVALUETYPE {
+    OMX_U32 nSize;
+    OMX_VERSIONTYPE nVersion;
+    OMX_U32 nPortIndex;
+    OMX_METERINGTYPE eMetering;
+    OMX_S32 xEVCompensation;      /**< Fixed point value stored as Q16 */
+    OMX_U32 nApertureFNumber;     /**< e.g. nApertureFNumber = 2 implies "f/2" - Q16 format */
+    OMX_BOOL bAutoAperture;     /**< Whether aperture number is defined automatically */
+    OMX_U32 nShutterSpeedMsec;    /**< Shutterspeed in milliseconds */
+    OMX_BOOL bAutoShutterSpeed; /**< Whether shutter speed is defined automatically */
+    OMX_U32 nSensitivity;         /**< e.g. nSensitivity = 100 implies "ISO 100" */
+    OMX_BOOL bAutoSensitivity;  /**< Whether sensitivity is defined automatically */
+} OMX_CONFIG_EXPOSUREVALUETYPE;
+
+/**
+ * Focus region configuration
+ *
+ * STRUCT MEMBERS:
+ *  nSize           : Size of the structure in bytes
+ *  nVersion        : OMX specification version information
+ *  nPortIndex      : Port that this structure applies to
+ *  bCenter         : Use center region as focus region of interest
+ *  bLeft           : Use left region as focus region of interest
+ *  bRight          : Use right region as focus region of interest
+ *  bTop            : Use top region as focus region of interest
+ *  bBottom         : Use bottom region as focus region of interest
+ *  bTopLeft        : Use top left region as focus region of interest
+ *  bTopRight       : Use top right region as focus region of interest
+ *  bBottomLeft     : Use bottom left region as focus region of interest
+ *  bBottomRight    : Use bottom right region as focus region of interest
+ */
+typedef struct OMX_CONFIG_FOCUSREGIONTYPE {
+    OMX_U32 nSize;
+    OMX_VERSIONTYPE nVersion;
+    OMX_U32 nPortIndex;
+    OMX_BOOL bCenter;
+    OMX_BOOL bLeft;
+    OMX_BOOL bRight;
+    OMX_BOOL bTop;
+    OMX_BOOL bBottom;
+    OMX_BOOL bTopLeft;
+    OMX_BOOL bTopRight;
+    OMX_BOOL bBottomLeft;
+    OMX_BOOL bBottomRight;
+} OMX_CONFIG_FOCUSREGIONTYPE;
+
+/**
+ * Focus Status type
+ */
+typedef enum OMX_FOCUSSTATUSTYPE {
+    OMX_FocusStatusOff = 0,
+    OMX_FocusStatusRequest,
+    OMX_FocusStatusReached,
+    OMX_FocusStatusUnableToReach,
+    OMX_FocusStatusLost,
+    OMX_FocusStatusKhronosExtensions = 0x6F000000, /**< Reserved region for introducing Khronos Standard Extensions */
+    OMX_FocusStatusVendorStartUnused = 0x7F000000, /**< Reserved region for introducing Vendor Extensions */
+    OMX_FocusStatusMax = 0x7FFFFFFF
+} OMX_FOCUSSTATUSTYPE;
+
+/**
+ * Focus status configuration
+ *
+ * STRUCT MEMBERS:
+ *  nSize               : Size of the structure in bytes
+ *  nVersion            : OMX specification version information
+ *  nPortIndex          : Port that this structure applies to
+ *  eFocusStatus        : Specifies the focus status
+ *  bCenterStatus       : Use center region as focus region of interest
+ *  bLeftStatus         : Use left region as focus region of interest
+ *  bRightStatus        : Use right region as focus region of interest
+ *  bTopStatus          : Use top region as focus region of interest
+ *  bBottomStatus       : Use bottom region as focus region of interest
+ *  bTopLeftStatus      : Use top left region as focus region of interest
+ *  bTopRightStatus     : Use top right region as focus region of interest
+ *  bBottomLeftStatus   : Use bottom left region as focus region of interest
+ *  bBottomRightStatus  : Use bottom right region as focus region of interest
+ */
+typedef struct OMX_PARAM_FOCUSSTATUSTYPE {
+    OMX_U32 nSize;
+    OMX_VERSIONTYPE nVersion;
+    OMX_U32 nPortIndex;
+    OMX_FOCUSSTATUSTYPE eFocusStatus;
+    OMX_BOOL bCenterStatus;
+    OMX_BOOL bLeftStatus;
+    OMX_BOOL bRightStatus;
+    OMX_BOOL bTopStatus;
+    OMX_BOOL bBottomStatus;
+    OMX_BOOL bTopLeftStatus;
+    OMX_BOOL bTopRightStatus;
+    OMX_BOOL bBottomLeftStatus;
+    OMX_BOOL bBottomRightStatus;
+} OMX_PARAM_FOCUSSTATUSTYPE;
+
+/** @} */
+
+#ifdef __cplusplus
+}
+#endif /* __cplusplus */
+
+#endif
+/* File EOF */
diff --git a/sf-extra/omx-il/OMX_Image.h b/sf-extra/omx-il/OMX_Image.h
new file mode 100644
index 00000000..ca648825
--- /dev/null
+++ b/sf-extra/omx-il/OMX_Image.h
@@ -0,0 +1,328 @@
+/**
+ * Copyright (c) 2008 The Khronos Group Inc.
+ *
+ * Permission is hereby granted, free of charge, to any person obtaining
+ * a copy of this software and associated documentation files (the
+ * "Software"), to deal in the Software without restriction, including
+ * without limitation the rights to use, copy, modify, merge, publish,
+ * distribute, sublicense, and/or sell copies of the Software, and to
+ * permit persons to whom the Software is furnished to do so, subject
+ * to the following conditions:
+ * The above copyright notice and this permission notice shall be included
+ * in all copies or substantial portions of the Software.
+ *
+ * THE SOFTWARE IS PROVIDED "AS IS", WITHOUT WARRANTY OF ANY KIND, EXPRESS
+ * OR IMPLIED, INCLUDING BUT NOT LIMITED TO THE WARRANTIES OF
+ * MERCHANTABILITY, FITNESS FOR A PARTICULAR PURPOSE AND NONINFRINGEMENT.
+ * IN NO EVENT SHALL THE AUTHORS OR COPYRIGHT HOLDERS BE LIABLE FOR ANY
+ * CLAIM, DAMAGES OR OTHER LIABILITY, WHETHER IN AN ACTION OF CONTRACT,
+ * TORT OR OTHERWISE, ARISING FROM, OUT OF OR IN CONNECTION WITH THE
+ * SOFTWARE OR THE USE OR OTHER DEALINGS IN THE SOFTWARE.
+ */
+
+/**
+ * @file OMX_Image.h - OpenMax IL version 1.1.2
+ * The structures needed by Image components to exchange parameters and
+ * configuration data with the components.
+ */
+#ifndef OMX_Image_h
+#define OMX_Image_h
+
+#ifdef __cplusplus
+extern "C" {
+#endif /* __cplusplus */
+
+
+/**
+ * Each OMX header must include all required header files to allow the
+ * header to compile without errors.  The includes below are required
+ * for this header file to compile successfully
+ */
+
+#include <OMX_IVCommon.h>
+
+/** @defgroup imaging OpenMAX IL Imaging Domain
+ * @ingroup iv
+ * Structures for OpenMAX IL Imaging domain
+ * @{
+ */
+
+/**
+ * Enumeration used to define the possible image compression coding.
+ */
+typedef enum OMX_IMAGE_CODINGTYPE {
+    OMX_IMAGE_CodingUnused,      /**< Value when format is N/A */
+    OMX_IMAGE_CodingAutoDetect,  /**< Auto detection of image format */
+    OMX_IMAGE_CodingJPEG,        /**< JPEG/JFIF image format */
+    OMX_IMAGE_CodingJPEG2K,      /**< JPEG 2000 image format */
+    OMX_IMAGE_CodingEXIF,        /**< EXIF image format */
+    OMX_IMAGE_CodingTIFF,        /**< TIFF image format */
+    OMX_IMAGE_CodingGIF,         /**< Graphics image format */
+    OMX_IMAGE_CodingPNG,         /**< PNG image format */
+    OMX_IMAGE_CodingLZW,         /**< LZW image format */
+    OMX_IMAGE_CodingBMP,         /**< Windows Bitmap format */
+    OMX_IMAGE_CodingKhronosExtensions = 0x6F000000, /**< Reserved region for introducing Khronos Standard Extensions */
+    OMX_IMAGE_CodingVendorStartUnused = 0x7F000000, /**< Reserved region for introducing Vendor Extensions */
+    OMX_IMAGE_CodingMax = 0x7FFFFFFF
+} OMX_IMAGE_CODINGTYPE;
+
+
+/**
+ * Data structure used to define an image path. The number of image paths
+ * for input and output will vary by type of the image component.
+ *
+ *  Input (aka Source) : Zero Inputs, one Output,
+ *  Splitter           : One Input, 2 or more Outputs,
+ *  Processing Element : One Input, one output,
+ *  Mixer              : 2 or more inputs, one output,
+ *  Output (aka Sink)  : One Input, zero outputs.
+ *
+ * The PortDefinition structure is used to define all of the parameters
+ * necessary for the compliant component to setup an input or an output
+ * image path.  If additional vendor specific data is required, it should
+ * be transmitted to the component using the CustomCommand function.
+ * Compliant components will prepopulate this structure with optimal
+ * values during the OMX_GetParameter() command.
+ *
+ * STRUCT MEMBERS:
+ *  cMIMEType             : MIME type of data for the port
+ *  pNativeRender         : Platform specific reference for a display if a
+ *                          sync, otherwise this field is 0
+ *  nFrameWidth           : Width of frame to be used on port if
+ *                          uncompressed format is used.  Use 0 for
+ *                          unknown, don't care or variable
+ *  nFrameHeight          : Height of frame to be used on port if
+ *                          uncompressed format is used. Use 0 for
+ *                          unknown, don't care or variable
+ *  nStride               : Number of bytes per span of an image (i.e.
+ *                          indicates the number of bytes to get from
+ *                          span N to span N+1, where negative stride
+ *                          indicates the image is bottom up
+ *  nSliceHeight          : Height used when encoding in slices
+ *  bFlagErrorConcealment : Turns on error concealment if it is supported by
+ *                          the OMX component
+ *  eCompressionFormat    : Compression format used in this instance of
+ *                          the component. When OMX_IMAGE_CodingUnused is
+ *                          specified, eColorFormat is valid
+ *  eColorFormat          : Decompressed format used by this component
+ *  pNativeWindow         : Platform specific reference for a window object if a
+ *                          display sink , otherwise this field is 0x0.
+ */
+typedef struct OMX_IMAGE_PORTDEFINITIONTYPE {
+    OMX_STRING cMIMEType;
+    OMX_NATIVE_DEVICETYPE pNativeRender;
+    OMX_U32 nFrameWidth;
+    OMX_U32 nFrameHeight;
+    OMX_S32 nStride;
+    OMX_U32 nSliceHeight;
+    OMX_BOOL bFlagErrorConcealment;
+    OMX_IMAGE_CODINGTYPE eCompressionFormat;
+    OMX_COLOR_FORMATTYPE eColorFormat;
+    OMX_NATIVE_WINDOWTYPE pNativeWindow;
+} OMX_IMAGE_PORTDEFINITIONTYPE;
+
+
+/**
+ * Port format parameter.  This structure is used to enumerate the various
+ * data input/output format supported by the port.
+ *
+ * STRUCT MEMBERS:
+ *  nSize              : Size of the structure in bytes
+ *  nVersion           : OMX specification version information
+ *  nPortIndex         : Indicates which port to set
+ *  nIndex             : Indicates the enumeration index for the format from
+ *                       0x0 to N-1
+ *  eCompressionFormat : Compression format used in this instance of the
+ *                       component. When OMX_IMAGE_CodingUnused is specified,
+ *                       eColorFormat is valid
+ *  eColorFormat       : Decompressed format used by this component
+ */
+typedef struct OMX_IMAGE_PARAM_PORTFORMATTYPE {
+    OMX_U32 nSize;
+    OMX_VERSIONTYPE nVersion;
+    OMX_U32 nPortIndex;
+    OMX_U32 nIndex;
+    OMX_IMAGE_CODINGTYPE eCompressionFormat;
+    OMX_COLOR_FORMATTYPE eColorFormat;
+} OMX_IMAGE_PARAM_PORTFORMATTYPE;
+
+
+/**
+ * Flash control type
+ *
+ * ENUMS
+ *  Torch : Flash forced constantly on
+ */
+typedef enum OMX_IMAGE_FLASHCONTROLTYPE {
+    OMX_IMAGE_FlashControlOn = 0,
+    OMX_IMAGE_FlashControlOff,
+    OMX_IMAGE_FlashControlAuto,
+    OMX_IMAGE_FlashControlRedEyeReduction,
+    OMX_IMAGE_FlashControlFillin,
+    OMX_IMAGE_FlashControlTorch,
+    OMX_IMAGE_FlashControlKhronosExtensions = 0x6F000000, /**< Reserved region for introducing Khronos Standard Extensions */
+    OMX_IMAGE_FlashControlVendorStartUnused = 0x7F000000, /**< Reserved region for introducing Vendor Extensions */
+    OMX_IMAGE_FlashControlMax = 0x7FFFFFFF
+} OMX_IMAGE_FLASHCONTROLTYPE;
+
+
+/**
+ * Flash control configuration
+ *
+ * STRUCT MEMBERS:
+ *  nSize         : Size of the structure in bytes
+ *  nVersion      : OMX specification version information
+ *  nPortIndex    : Port that this structure applies to
+ *  eFlashControl : Flash control type
+ */
+typedef struct OMX_IMAGE_PARAM_FLASHCONTROLTYPE {
+    OMX_U32 nSize;
+    OMX_VERSIONTYPE nVersion;
+    OMX_U32 nPortIndex;
+    OMX_IMAGE_FLASHCONTROLTYPE eFlashControl;
+} OMX_IMAGE_PARAM_FLASHCONTROLTYPE;
+
+
+/**
+ * Focus control type
+ */
+typedef enum OMX_IMAGE_FOCUSCONTROLTYPE {
+    OMX_IMAGE_FocusControlOn = 0,
+    OMX_IMAGE_FocusControlOff,
+    OMX_IMAGE_FocusControlAuto,
+    OMX_IMAGE_FocusControlAutoLock,
+    OMX_IMAGE_FocusControlKhronosExtensions = 0x6F000000, /**< Reserved region for introducing Khronos Standard Extensions */
+    OMX_IMAGE_FocusControlVendorStartUnused = 0x7F000000, /**< Reserved region for introducing Vendor Extensions */
+    OMX_IMAGE_FocusControlMax = 0x7FFFFFFF
+} OMX_IMAGE_FOCUSCONTROLTYPE;
+
+
+/**
+ * Focus control configuration
+ *
+ * STRUCT MEMBERS:
+ *  nSize           : Size of the structure in bytes
+ *  nVersion        : OMX specification version information
+ *  nPortIndex      : Port that this structure applies to
+ *  eFocusControl   : Focus control
+ *  nFocusSteps     : Focus can take on values from 0 mm to infinity.
+ *                    Interest is only in number of steps over this range.
+ *  nFocusStepIndex : Current focus step index
+ */
+typedef struct OMX_IMAGE_CONFIG_FOCUSCONTROLTYPE {
+    OMX_U32 nSize;
+    OMX_VERSIONTYPE nVersion;
+    OMX_U32 nPortIndex;
+    OMX_IMAGE_FOCUSCONTROLTYPE eFocusControl;
+    OMX_U32 nFocusSteps;
+    OMX_U32 nFocusStepIndex;
+} OMX_IMAGE_CONFIG_FOCUSCONTROLTYPE;
+
+
+/**
+ * Q Factor for JPEG compression, which controls the tradeoff between image
+ * quality and size.  Q Factor provides a more simple means of controlling
+ * JPEG compression quality, without directly programming Quantization
+ * tables for chroma and luma
+ *
+ * STRUCT MEMBERS:
+ *  nSize      : Size of the structure in bytes
+ *  nVersion   : OMX specification version information
+ *  nPortIndex : Port that this structure applies to
+ *  nQFactor   : JPEG Q factor value in the range of 1-100. A factor of 1
+ *               produces the smallest, worst quality images, and a factor
+ *               of 100 produces the largest, best quality images.  A
+ *               typical default is 75 for small good quality images
+ */
+typedef struct OMX_IMAGE_PARAM_QFACTORTYPE {
+    OMX_U32 nSize;
+    OMX_VERSIONTYPE nVersion;
+    OMX_U32 nPortIndex;
+    OMX_U32 nQFactor;
+} OMX_IMAGE_PARAM_QFACTORTYPE;
+
+/**
+ * Quantization table type
+ */
+
+typedef enum OMX_IMAGE_QUANTIZATIONTABLETYPE {
+    OMX_IMAGE_QuantizationTableLuma = 0,
+    OMX_IMAGE_QuantizationTableChroma,
+    OMX_IMAGE_QuantizationTableChromaCb,
+    OMX_IMAGE_QuantizationTableChromaCr,
+    OMX_IMAGE_QuantizationTableKhronosExtensions = 0x6F000000, /**< Reserved region for introducing Khronos Standard Extensions */
+    OMX_IMAGE_QuantizationTableVendorStartUnused = 0x7F000000, /**< Reserved region for introducing Vendor Extensions */
+    OMX_IMAGE_QuantizationTableMax = 0x7FFFFFFF
+} OMX_IMAGE_QUANTIZATIONTABLETYPE;
+
+/**
+ * JPEG quantization tables are used to determine DCT compression for
+ * YUV data, as an alternative to specifying Q factor, providing exact
+ * control of compression
+ *
+ * STRUCT MEMBERS:
+ *  nSize                   : Size of the structure in bytes
+ *  nVersion                : OMX specification version information
+ *  nPortIndex              : Port that this structure applies to
+ *  eQuantizationTable      : Quantization table type
+ *  nQuantizationMatrix[64] : JPEG quantization table of coefficients stored
+ *                            in increasing columns then by rows of data (i.e.
+ *                            row 1, ... row 8). Quantization values are in
+ *                            the range 0-255 and stored in linear order
+ *                            (i.e. the component will zig-zag the
+ *                            quantization table data if required internally)
+ */
+typedef struct OMX_IMAGE_PARAM_QUANTIZATIONTABLETYPE {
+    OMX_U32 nSize;
+    OMX_VERSIONTYPE nVersion;
+    OMX_U32 nPortIndex;
+    OMX_IMAGE_QUANTIZATIONTABLETYPE eQuantizationTable;
+    OMX_U8 nQuantizationMatrix[64];
+} OMX_IMAGE_PARAM_QUANTIZATIONTABLETYPE;
+
+
+/**
+ * Huffman table type, the same Huffman table is applied for chroma and
+ * luma component
+ */
+typedef enum OMX_IMAGE_HUFFMANTABLETYPE {
+    OMX_IMAGE_HuffmanTableAC = 0,
+    OMX_IMAGE_HuffmanTableDC,
+    OMX_IMAGE_HuffmanTableACLuma,
+    OMX_IMAGE_HuffmanTableACChroma,
+    OMX_IMAGE_HuffmanTableDCLuma,
+    OMX_IMAGE_HuffmanTableDCChroma,
+    OMX_IMAGE_HuffmanTableKhronosExtensions = 0x6F000000, /**< Reserved region for introducing Khronos Standard Extensions */
+    OMX_IMAGE_HuffmanTableVendorStartUnused = 0x7F000000, /**< Reserved region for introducing Vendor Extensions */
+    OMX_IMAGE_HuffmanTableMax = 0x7FFFFFFF
+} OMX_IMAGE_HUFFMANTABLETYPE;
+
+/**
+ * JPEG Huffman table
+ *
+ * STRUCT MEMBERS:
+ *  nSize                            : Size of the structure in bytes
+ *  nVersion                         : OMX specification version information
+ *  nPortIndex                       : Port that this structure applies to
+ *  eHuffmanTable                    : Huffman table type
+ *  nNumberOfHuffmanCodeOfLength[16] : 0-16, number of Huffman codes of each
+ *                                     possible length
+ *  nHuffmanTable[256]               : 0-255, the size used for AC and DC
+ *                                     HuffmanTable are 16 and 162
+ */
+typedef struct OMX_IMAGE_PARAM_HUFFMANTTABLETYPE {
+    OMX_U32 nSize;
+    OMX_VERSIONTYPE nVersion;
+    OMX_U32 nPortIndex;
+    OMX_IMAGE_HUFFMANTABLETYPE eHuffmanTable;
+    OMX_U8 nNumberOfHuffmanCodeOfLength[16];
+    OMX_U8 nHuffmanTable[256];
+} OMX_IMAGE_PARAM_HUFFMANTTABLETYPE;
+
+/** @} */
+#ifdef __cplusplus
+}
+#endif /* __cplusplus */
+
+#endif
+/* File EOF */
diff --git a/sf-extra/omx-il/OMX_ImageExt.h b/sf-extra/omx-il/OMX_ImageExt.h
new file mode 100644
index 00000000..e7cae029
--- /dev/null
+++ b/sf-extra/omx-il/OMX_ImageExt.h
@@ -0,0 +1,55 @@
+/*
+ * Copyright (c) 2016 The Khronos Group Inc.
+ *
+ * Permission is hereby granted, free of charge, to any person obtaining
+ * a copy of this software and associated documentation files (the
+ * "Software"), to deal in the Software without restriction, including
+ * without limitation the rights to use, copy, modify, merge, publish,
+ * distribute, sublicense, and/or sell copies of the Software, and to
+ * permit persons to whom the Software is furnished to do so, subject
+ * to the following conditions:
+ * The above copyright notice and this permission notice shall be included
+ * in all copies or substantial portions of the Software.
+ *
+ * THE SOFTWARE IS PROVIDED "AS IS", WITHOUT WARRANTY OF ANY KIND, EXPRESS
+ * OR IMPLIED, INCLUDING BUT NOT LIMITED TO THE WARRANTIES OF
+ * MERCHANTABILITY, FITNESS FOR A PARTICULAR PURPOSE AND NONINFRINGEMENT.
+ * IN NO EVENT SHALL THE AUTHORS OR COPYRIGHT HOLDERS BE LIABLE FOR ANY
+ * CLAIM, DAMAGES OR OTHER LIABILITY, WHETHER IN AN ACTION OF CONTRACT,
+ * TORT OR OTHERWISE, ARISING FROM, OUT OF OR IN CONNECTION WITH THE
+ * SOFTWARE OR THE USE OR OTHER DEALINGS IN THE SOFTWARE.
+ *
+ */
+
+/** OMX_ImageExt.h - OpenMax IL version 1.1.2
+ * The OMX_ImageExt header file contains extensions to the
+ * definitions used by both the application and the component to
+ * access image items.
+ */
+
+#ifndef OMX_ImageExt_h
+#define OMX_ImageExt_h
+
+#ifdef __cplusplus
+extern "C" {
+#endif /* __cplusplus */
+
+/* Each OMX header shall include all required header files to allow the
+ * header to compile without errors.  The includes below are required
+ * for this header file to compile successfully
+ */
+#include <OMX_Core.h>
+
+/** Enum for standard image codingtype extensions */
+typedef enum OMX_IMAGE_CODINGEXTTYPE {
+    OMX_IMAGE_CodingExtUnused = OMX_IMAGE_CodingKhronosExtensions,
+    OMX_IMAGE_CodingWEBP,         /**< WebP image format */
+} OMX_IMAGE_CODINGEXTTYPE;
+
+
+#ifdef __cplusplus
+}
+#endif /* __cplusplus */
+
+#endif /* OMX_ImageExt_h */
+/* File EOF */
diff --git a/sf-extra/omx-il/OMX_Index.h b/sf-extra/omx-il/OMX_Index.h
new file mode 100644
index 00000000..20a109cf
--- /dev/null
+++ b/sf-extra/omx-il/OMX_Index.h
@@ -0,0 +1,260 @@
+/*
+ * Copyright (c) 2008 The Khronos Group Inc.
+ *
+ * Permission is hereby granted, free of charge, to any person obtaining
+ * a copy of this software and associated documentation files (the
+ * "Software"), to deal in the Software without restriction, including
+ * without limitation the rights to use, copy, modify, merge, publish,
+ * distribute, sublicense, and/or sell copies of the Software, and to
+ * permit persons to whom the Software is furnished to do so, subject
+ * to the following conditions:
+ * The above copyright notice and this permission notice shall be included
+ * in all copies or substantial portions of the Software.
+ *
+ * THE SOFTWARE IS PROVIDED "AS IS", WITHOUT WARRANTY OF ANY KIND, EXPRESS
+ * OR IMPLIED, INCLUDING BUT NOT LIMITED TO THE WARRANTIES OF
+ * MERCHANTABILITY, FITNESS FOR A PARTICULAR PURPOSE AND NONINFRINGEMENT.
+ * IN NO EVENT SHALL THE AUTHORS OR COPYRIGHT HOLDERS BE LIABLE FOR ANY
+ * CLAIM, DAMAGES OR OTHER LIABILITY, WHETHER IN AN ACTION OF CONTRACT,
+ * TORT OR OTHERWISE, ARISING FROM, OUT OF OR IN CONNECTION WITH THE
+ * SOFTWARE OR THE USE OR OTHER DEALINGS IN THE SOFTWARE.
+ *
+ */
+
+/** @file OMX_Index.h - OpenMax IL version 1.1.2
+ *  The OMX_Index header file contains the definitions for both applications
+ *  and components .
+ */
+
+
+#ifndef OMX_Index_h
+#define OMX_Index_h
+
+#ifdef __cplusplus
+extern "C" {
+#endif /* __cplusplus */
+
+
+/* Each OMX header must include all required header files to allow the
+ *  header to compile without errors.  The includes below are required
+ *  for this header file to compile successfully
+ */
+#include <OMX_Types.h>
+
+
+/** The OMX_INDEXTYPE enumeration is used to select a structure when either
+ *  getting or setting parameters and/or configuration data.  Each entry in
+ *  this enumeration maps to an OMX specified structure.  When the
+ *  OMX_GetParameter, OMX_SetParameter, OMX_GetConfig or OMX_SetConfig methods
+ *  are used, the second parameter will always be an entry from this enumeration
+ *  and the third entry will be the structure shown in the comments for the entry.
+ *  For example, if the application is initializing a cropping function, the
+ *  OMX_SetConfig command would have OMX_IndexConfigCommonInputCrop as the second parameter
+ *  and would send a pointer to an initialized OMX_RECTTYPE structure as the
+ *  third parameter.
+ *
+ *  The enumeration entries named with the OMX_Config prefix are sent using
+ *  the OMX_SetConfig command and the enumeration entries named with the
+ *  OMX_PARAM_ prefix are sent using the OMX_SetParameter command.
+ */
+typedef enum OMX_INDEXTYPE {
+
+    OMX_IndexComponentStartUnused = 0x01000000,
+    OMX_IndexParamPriorityMgmt,             /**< reference: OMX_PRIORITYMGMTTYPE */
+    OMX_IndexParamAudioInit,                /**< reference: OMX_PORT_PARAM_TYPE */
+    OMX_IndexParamImageInit,                /**< reference: OMX_PORT_PARAM_TYPE */
+    OMX_IndexParamVideoInit,                /**< reference: OMX_PORT_PARAM_TYPE */
+    OMX_IndexParamOtherInit,                /**< reference: OMX_PORT_PARAM_TYPE */
+    OMX_IndexParamNumAvailableStreams,      /**< reference: OMX_PARAM_U32TYPE */
+    OMX_IndexParamActiveStream,             /**< reference: OMX_PARAM_U32TYPE */
+    OMX_IndexParamSuspensionPolicy,         /**< reference: OMX_PARAM_SUSPENSIONPOLICYTYPE */
+    OMX_IndexParamComponentSuspended,       /**< reference: OMX_PARAM_SUSPENSIONTYPE */
+    OMX_IndexConfigCapturing,               /**< reference: OMX_CONFIG_BOOLEANTYPE */
+    OMX_IndexConfigCaptureMode,             /**< reference: OMX_CONFIG_CAPTUREMODETYPE */
+    OMX_IndexAutoPauseAfterCapture,         /**< reference: OMX_CONFIG_BOOLEANTYPE */
+    OMX_IndexParamContentURI,               /**< reference: OMX_PARAM_CONTENTURITYPE */
+    OMX_IndexParamCustomContentPipe,        /**< reference: OMX_PARAM_CONTENTPIPETYPE */
+    OMX_IndexParamDisableResourceConcealment, /**< reference: OMX_RESOURCECONCEALMENTTYPE */
+    OMX_IndexConfigMetadataItemCount,       /**< reference: OMX_CONFIG_METADATAITEMCOUNTTYPE */
+    OMX_IndexConfigContainerNodeCount,      /**< reference: OMX_CONFIG_CONTAINERNODECOUNTTYPE */
+    OMX_IndexConfigMetadataItem,            /**< reference: OMX_CONFIG_METADATAITEMTYPE */
+    OMX_IndexConfigCounterNodeID,           /**< reference: OMX_CONFIG_CONTAINERNODEIDTYPE */
+    OMX_IndexParamMetadataFilterType,       /**< reference: OMX_PARAM_METADATAFILTERTYPE */
+    OMX_IndexParamMetadataKeyFilter,        /**< reference: OMX_PARAM_METADATAFILTERTYPE */
+    OMX_IndexConfigPriorityMgmt,            /**< reference: OMX_PRIORITYMGMTTYPE */
+    OMX_IndexParamStandardComponentRole,    /**< reference: OMX_PARAM_COMPONENTROLETYPE */
+
+    OMX_IndexPortStartUnused = 0x02000000,
+    OMX_IndexParamPortDefinition,           /**< reference: OMX_PARAM_PORTDEFINITIONTYPE */
+    OMX_IndexParamCompBufferSupplier,       /**< reference: OMX_PARAM_BUFFERSUPPLIERTYPE */
+    OMX_IndexReservedStartUnused = 0x03000000,
+
+    /* Audio parameters and configurations */
+    OMX_IndexAudioStartUnused = 0x04000000,
+    OMX_IndexParamAudioPortFormat,          /**< reference: OMX_AUDIO_PARAM_PORTFORMATTYPE */
+    OMX_IndexParamAudioPcm,                 /**< reference: OMX_AUDIO_PARAM_PCMMODETYPE */
+    OMX_IndexParamAudioAac,                 /**< reference: OMX_AUDIO_PARAM_AACPROFILETYPE */
+    OMX_IndexParamAudioRa,                  /**< reference: OMX_AUDIO_PARAM_RATYPE */
+    OMX_IndexParamAudioMp3,                 /**< reference: OMX_AUDIO_PARAM_MP3TYPE */
+    OMX_IndexParamAudioAdpcm,               /**< reference: OMX_AUDIO_PARAM_ADPCMTYPE */
+    OMX_IndexParamAudioG723,                /**< reference: OMX_AUDIO_PARAM_G723TYPE */
+    OMX_IndexParamAudioG729,                /**< reference: OMX_AUDIO_PARAM_G729TYPE */
+    OMX_IndexParamAudioAmr,                 /**< reference: OMX_AUDIO_PARAM_AMRTYPE */
+    OMX_IndexParamAudioWma,                 /**< reference: OMX_AUDIO_PARAM_WMATYPE */
+    OMX_IndexParamAudioSbc,                 /**< reference: OMX_AUDIO_PARAM_SBCTYPE */
+    OMX_IndexParamAudioMidi,                /**< reference: OMX_AUDIO_PARAM_MIDITYPE */
+    OMX_IndexParamAudioGsm_FR,              /**< reference: OMX_AUDIO_PARAM_GSMFRTYPE */
+    OMX_IndexParamAudioMidiLoadUserSound,   /**< reference: OMX_AUDIO_PARAM_MIDILOADUSERSOUNDTYPE */
+    OMX_IndexParamAudioG726,                /**< reference: OMX_AUDIO_PARAM_G726TYPE */
+    OMX_IndexParamAudioGsm_EFR,             /**< reference: OMX_AUDIO_PARAM_GSMEFRTYPE */
+    OMX_IndexParamAudioGsm_HR,              /**< reference: OMX_AUDIO_PARAM_GSMHRTYPE */
+    OMX_IndexParamAudioPdc_FR,              /**< reference: OMX_AUDIO_PARAM_PDCFRTYPE */
+    OMX_IndexParamAudioPdc_EFR,             /**< reference: OMX_AUDIO_PARAM_PDCEFRTYPE */
+    OMX_IndexParamAudioPdc_HR,              /**< reference: OMX_AUDIO_PARAM_PDCHRTYPE */
+    OMX_IndexParamAudioTdma_FR,             /**< reference: OMX_AUDIO_PARAM_TDMAFRTYPE */
+    OMX_IndexParamAudioTdma_EFR,            /**< reference: OMX_AUDIO_PARAM_TDMAEFRTYPE */
+    OMX_IndexParamAudioQcelp8,              /**< reference: OMX_AUDIO_PARAM_QCELP8TYPE */
+    OMX_IndexParamAudioQcelp13,             /**< reference: OMX_AUDIO_PARAM_QCELP13TYPE */
+    OMX_IndexParamAudioEvrc,                /**< reference: OMX_AUDIO_PARAM_EVRCTYPE */
+    OMX_IndexParamAudioSmv,                 /**< reference: OMX_AUDIO_PARAM_SMVTYPE */
+    OMX_IndexParamAudioVorbis,              /**< reference: OMX_AUDIO_PARAM_VORBISTYPE */
+
+    OMX_IndexConfigAudioMidiImmediateEvent, /**< reference: OMX_AUDIO_CONFIG_MIDIIMMEDIATEEVENTTYPE */
+    OMX_IndexConfigAudioMidiControl,        /**< reference: OMX_AUDIO_CONFIG_MIDICONTROLTYPE */
+    OMX_IndexConfigAudioMidiSoundBankProgram, /**< reference: OMX_AUDIO_CONFIG_MIDISOUNDBANKPROGRAMTYPE */
+    OMX_IndexConfigAudioMidiStatus,         /**< reference: OMX_AUDIO_CONFIG_MIDISTATUSTYPE */
+    OMX_IndexConfigAudioMidiMetaEvent,      /**< reference: OMX_AUDIO_CONFIG_MIDIMETAEVENTTYPE */
+    OMX_IndexConfigAudioMidiMetaEventData,  /**< reference: OMX_AUDIO_CONFIG_MIDIMETAEVENTDATATYPE */
+    OMX_IndexConfigAudioVolume,             /**< reference: OMX_AUDIO_CONFIG_VOLUMETYPE */
+    OMX_IndexConfigAudioBalance,            /**< reference: OMX_AUDIO_CONFIG_BALANCETYPE */
+    OMX_IndexConfigAudioChannelMute,        /**< reference: OMX_AUDIO_CONFIG_CHANNELMUTETYPE */
+    OMX_IndexConfigAudioMute,               /**< reference: OMX_AUDIO_CONFIG_MUTETYPE */
+    OMX_IndexConfigAudioLoudness,           /**< reference: OMX_AUDIO_CONFIG_LOUDNESSTYPE */
+    OMX_IndexConfigAudioEchoCancelation,    /**< reference: OMX_AUDIO_CONFIG_ECHOCANCELATIONTYPE */
+    OMX_IndexConfigAudioNoiseReduction,     /**< reference: OMX_AUDIO_CONFIG_NOISEREDUCTIONTYPE */
+    OMX_IndexConfigAudioBass,               /**< reference: OMX_AUDIO_CONFIG_BASSTYPE */
+    OMX_IndexConfigAudioTreble,             /**< reference: OMX_AUDIO_CONFIG_TREBLETYPE */
+    OMX_IndexConfigAudioStereoWidening,     /**< reference: OMX_AUDIO_CONFIG_STEREOWIDENINGTYPE */
+    OMX_IndexConfigAudioChorus,             /**< reference: OMX_AUDIO_CONFIG_CHORUSTYPE */
+    OMX_IndexConfigAudioEqualizer,          /**< reference: OMX_AUDIO_CONFIG_EQUALIZERTYPE */
+    OMX_IndexConfigAudioReverberation,      /**< reference: OMX_AUDIO_CONFIG_REVERBERATIONTYPE */
+    OMX_IndexConfigAudioChannelVolume,      /**< reference: OMX_AUDIO_CONFIG_CHANNELVOLUMETYPE */
+
+    /* Image specific parameters and configurations */
+    OMX_IndexImageStartUnused = 0x05000000,
+    OMX_IndexParamImagePortFormat,          /**< reference: OMX_IMAGE_PARAM_PORTFORMATTYPE */
+    OMX_IndexParamFlashControl,             /**< reference: OMX_IMAGE_PARAM_FLASHCONTROLTYPE */
+    OMX_IndexConfigFocusControl,            /**< reference: OMX_IMAGE_CONFIG_FOCUSCONTROLTYPE */
+    OMX_IndexParamQFactor,                  /**< reference: OMX_IMAGE_PARAM_QFACTORTYPE */
+    OMX_IndexParamQuantizationTable,        /**< reference: OMX_IMAGE_PARAM_QUANTIZATIONTABLETYPE */
+    OMX_IndexParamHuffmanTable,             /**< reference: OMX_IMAGE_PARAM_HUFFMANTTABLETYPE */
+    OMX_IndexConfigFlashControl,            /**< reference: OMX_IMAGE_PARAM_FLASHCONTROLTYPE */
+
+    /* Video specific parameters and configurations */
+    OMX_IndexVideoStartUnused = 0x06000000,
+    OMX_IndexParamVideoPortFormat,          /**< reference: OMX_VIDEO_PARAM_PORTFORMATTYPE */
+    OMX_IndexParamVideoQuantization,        /**< reference: OMX_VIDEO_PARAM_QUANTIZATIONTYPE */
+    OMX_IndexParamVideoFastUpdate,          /**< reference: OMX_VIDEO_PARAM_VIDEOFASTUPDATETYPE */
+    OMX_IndexParamVideoBitrate,             /**< reference: OMX_VIDEO_PARAM_BITRATETYPE */
+    OMX_IndexParamVideoMotionVector,        /**< reference: OMX_VIDEO_PARAM_MOTIONVECTORTYPE */
+    OMX_IndexParamVideoIntraRefresh,        /**< reference: OMX_VIDEO_PARAM_INTRAREFRESHTYPE */
+    OMX_IndexParamVideoErrorCorrection,     /**< reference: OMX_VIDEO_PARAM_ERRORCORRECTIONTYPE */
+    OMX_IndexParamVideoVBSMC,               /**< reference: OMX_VIDEO_PARAM_VBSMCTYPE */
+    OMX_IndexParamVideoMpeg2,               /**< reference: OMX_VIDEO_PARAM_MPEG2TYPE */
+    OMX_IndexParamVideoMpeg4,               /**< reference: OMX_VIDEO_PARAM_MPEG4TYPE */
+    OMX_IndexParamVideoWmv,                 /**< reference: OMX_VIDEO_PARAM_WMVTYPE */
+    OMX_IndexParamVideoRv,                  /**< reference: OMX_VIDEO_PARAM_RVTYPE */
+    OMX_IndexParamVideoAvc,                 /**< reference: OMX_VIDEO_PARAM_AVCTYPE */
+    OMX_IndexParamVideoH263,                /**< reference: OMX_VIDEO_PARAM_H263TYPE */
+    OMX_IndexParamVideoProfileLevelQuerySupported, /**< reference: OMX_VIDEO_PARAM_PROFILELEVELTYPE */
+    OMX_IndexParamVideoProfileLevelCurrent, /**< reference: OMX_VIDEO_PARAM_PROFILELEVELTYPE */
+    OMX_IndexConfigVideoBitrate,            /**< reference: OMX_VIDEO_CONFIG_BITRATETYPE */
+    OMX_IndexConfigVideoFramerate,          /**< reference: OMX_CONFIG_FRAMERATETYPE */
+    OMX_IndexConfigVideoIntraVOPRefresh,    /**< reference: OMX_CONFIG_INTRAREFRESHVOPTYPE */
+    OMX_IndexConfigVideoIntraMBRefresh,     /**< reference: OMX_CONFIG_MACROBLOCKERRORMAPTYPE */
+    OMX_IndexConfigVideoMBErrorReporting,   /**< reference: OMX_CONFIG_MBERRORREPORTINGTYPE */
+    OMX_IndexParamVideoMacroblocksPerFrame, /**< reference: OMX_PARAM_MACROBLOCKSTYPE */
+    OMX_IndexConfigVideoMacroBlockErrorMap, /**< reference: OMX_CONFIG_MACROBLOCKERRORMAPTYPE */
+    OMX_IndexParamVideoSliceFMO,            /**< reference: OMX_VIDEO_PARAM_AVCSLICEFMO */
+    OMX_IndexConfigVideoAVCIntraPeriod,     /**< reference: OMX_VIDEO_CONFIG_AVCINTRAPERIOD */
+    OMX_IndexConfigVideoNalSize,            /**< reference: OMX_VIDEO_CONFIG_NALSIZE */
+
+    /* Image & Video common Configurations */
+    OMX_IndexCommonStartUnused = 0x07000000,
+    OMX_IndexParamCommonDeblocking,         /**< reference: OMX_PARAM_DEBLOCKINGTYPE */
+    OMX_IndexParamCommonSensorMode,         /**< reference: OMX_PARAM_SENSORMODETYPE */
+    OMX_IndexParamCommonInterleave,         /**< reference: OMX_PARAM_INTERLEAVETYPE */
+    OMX_IndexConfigCommonColorFormatConversion, /**< reference: OMX_CONFIG_COLORCONVERSIONTYPE */
+    OMX_IndexConfigCommonScale,             /**< reference: OMX_CONFIG_SCALEFACTORTYPE */
+    OMX_IndexConfigCommonImageFilter,       /**< reference: OMX_CONFIG_IMAGEFILTERTYPE */
+    OMX_IndexConfigCommonColorEnhancement,  /**< reference: OMX_CONFIG_COLORENHANCEMENTTYPE */
+    OMX_IndexConfigCommonColorKey,          /**< reference: OMX_CONFIG_COLORKEYTYPE */
+    OMX_IndexConfigCommonColorBlend,        /**< reference: OMX_CONFIG_COLORBLENDTYPE */
+    OMX_IndexConfigCommonFrameStabilisation,/**< reference: OMX_CONFIG_FRAMESTABTYPE */
+    OMX_IndexConfigCommonRotate,            /**< reference: OMX_CONFIG_ROTATIONTYPE */
+    OMX_IndexConfigCommonMirror,            /**< reference: OMX_CONFIG_MIRRORTYPE */
+    OMX_IndexConfigCommonOutputPosition,    /**< reference: OMX_CONFIG_POINTTYPE */
+    OMX_IndexConfigCommonInputCrop,         /**< reference: OMX_CONFIG_RECTTYPE */
+    OMX_IndexConfigCommonOutputCrop,        /**< reference: OMX_CONFIG_RECTTYPE */
+    OMX_IndexConfigCommonDigitalZoom,       /**< reference: OMX_CONFIG_SCALEFACTORTYPE */
+    OMX_IndexConfigCommonOpticalZoom,       /**< reference: OMX_CONFIG_SCALEFACTORTYPE*/
+    OMX_IndexConfigCommonWhiteBalance,      /**< reference: OMX_CONFIG_WHITEBALCONTROLTYPE */
+    OMX_IndexConfigCommonExposure,          /**< reference: OMX_CONFIG_EXPOSURECONTROLTYPE */
+    OMX_IndexConfigCommonContrast,          /**< reference: OMX_CONFIG_CONTRASTTYPE */
+    OMX_IndexConfigCommonBrightness,        /**< reference: OMX_CONFIG_BRIGHTNESSTYPE */
+    OMX_IndexConfigCommonBacklight,         /**< reference: OMX_CONFIG_BACKLIGHTTYPE */
+    OMX_IndexConfigCommonGamma,             /**< reference: OMX_CONFIG_GAMMATYPE */
+    OMX_IndexConfigCommonSaturation,        /**< reference: OMX_CONFIG_SATURATIONTYPE */
+    OMX_IndexConfigCommonLightness,         /**< reference: OMX_CONFIG_LIGHTNESSTYPE */
+    OMX_IndexConfigCommonExclusionRect,     /**< reference: OMX_CONFIG_RECTTYPE */
+    OMX_IndexConfigCommonDithering,         /**< reference: OMX_CONFIG_DITHERTYPE */
+    OMX_IndexConfigCommonPlaneBlend,        /**< reference: OMX_CONFIG_PLANEBLENDTYPE */
+    OMX_IndexConfigCommonExposureValue,     /**< reference: OMX_CONFIG_EXPOSUREVALUETYPE */
+    OMX_IndexConfigCommonOutputSize,        /**< reference: OMX_FRAMESIZETYPE */
+    OMX_IndexParamCommonExtraQuantData,     /**< reference: OMX_OTHER_EXTRADATATYPE */
+    OMX_IndexConfigCommonFocusRegion,       /**< reference: OMX_CONFIG_FOCUSREGIONTYPE */
+    OMX_IndexConfigCommonFocusStatus,       /**< reference: OMX_PARAM_FOCUSSTATUSTYPE */
+    OMX_IndexConfigCommonTransitionEffect,  /**< reference: OMX_CONFIG_TRANSITIONEFFECTTYPE */
+
+    /* Reserved Configuration range */
+    OMX_IndexOtherStartUnused = 0x08000000,
+    OMX_IndexParamOtherPortFormat,          /**< reference: OMX_OTHER_PARAM_PORTFORMATTYPE */
+    OMX_IndexConfigOtherPower,              /**< reference: OMX_OTHER_CONFIG_POWERTYPE */
+    OMX_IndexConfigOtherStats,              /**< reference: OMX_OTHER_CONFIG_STATSTYPE */
+
+
+    /* Reserved Time range */
+    OMX_IndexTimeStartUnused = 0x09000000,
+    OMX_IndexConfigTimeScale,               /**< reference: OMX_TIME_CONFIG_SCALETYPE */
+    OMX_IndexConfigTimeClockState,          /**< reference: OMX_TIME_CONFIG_CLOCKSTATETYPE */
+    OMX_IndexConfigTimeActiveRefClock,      /**< reference: OMX_TIME_CONFIG_ACTIVEREFCLOCKTYPE */
+    OMX_IndexConfigTimeCurrentMediaTime,    /**< reference: OMX_TIME_CONFIG_TIMESTAMPTYPE (read only) */
+    OMX_IndexConfigTimeCurrentWallTime,     /**< reference: OMX_TIME_CONFIG_TIMESTAMPTYPE (read only) */
+    OMX_IndexConfigTimeCurrentAudioReference, /**< reference: OMX_TIME_CONFIG_TIMESTAMPTYPE (write only) */
+    OMX_IndexConfigTimeCurrentVideoReference, /**< reference: OMX_TIME_CONFIG_TIMESTAMPTYPE (write only) */
+    OMX_IndexConfigTimeMediaTimeRequest,    /**< reference: OMX_TIME_CONFIG_MEDIATIMEREQUESTTYPE (write only) */
+    OMX_IndexConfigTimeClientStartTime,     /**<reference:  OMX_TIME_CONFIG_TIMESTAMPTYPE (write only) */
+    OMX_IndexConfigTimePosition,            /**< reference: OMX_TIME_CONFIG_TIMESTAMPTYPE */
+    OMX_IndexConfigTimeSeekMode,            /**< reference: OMX_TIME_CONFIG_SEEKMODETYPE */
+
+
+    OMX_IndexKhronosExtensions = 0x6F000000, /**< Reserved region for introducing Khronos Standard Extensions */
+    /* Vendor specific area */
+    OMX_IndexRockchipExtensions = 0x70000000, /**< Reserved region for introducing Rockchip Standard Extensions */
+    OMX_IndexParamVideoHDRRockchipExtensions,  /**< reference: OMX_EXTENSION_VIDEO_PARAM_HDR */
+    OMX_IndexVendorStartUnused = 0x7F000000,
+    /* Vendor specific structures should be in the range of 0x7F000000
+       to 0x7FFFFFFE.  This range is not broken out by vendor, so
+       private indexes are not guaranteed unique and therefore should
+       only be sent to the appropriate component. */
+
+    OMX_IndexMax = 0x7FFFFFFF
+
+} OMX_INDEXTYPE;
+
+#ifdef __cplusplus
+}
+#endif /* __cplusplus */
+
+#endif
+/* File EOF */
diff --git a/sf-extra/omx-il/OMX_IndexExt.h b/sf-extra/omx-il/OMX_IndexExt.h
new file mode 100644
index 00000000..b688d1d9
--- /dev/null
+++ b/sf-extra/omx-il/OMX_IndexExt.h
@@ -0,0 +1,105 @@
+/*
+ * Copyright (c) 2010 The Khronos Group Inc.
+ *
+ * Permission is hereby granted, free of charge, to any person obtaining
+ * a copy of this software and associated documentation files (the
+ * "Software"), to deal in the Software without restriction, including
+ * without limitation the rights to use, copy, modify, merge, publish,
+ * distribute, sublicense, and/or sell copies of the Software, and to
+ * permit persons to whom the Software is furnished to do so, subject
+ * to the following conditions:
+ * The above copyright notice and this permission notice shall be included
+ * in all copies or substantial portions of the Software.
+ *
+ * THE SOFTWARE IS PROVIDED "AS IS", WITHOUT WARRANTY OF ANY KIND, EXPRESS
+ * OR IMPLIED, INCLUDING BUT NOT LIMITED TO THE WARRANTIES OF
+ * MERCHANTABILITY, FITNESS FOR A PARTICULAR PURPOSE AND NONINFRINGEMENT.
+ * IN NO EVENT SHALL THE AUTHORS OR COPYRIGHT HOLDERS BE LIABLE FOR ANY
+ * CLAIM, DAMAGES OR OTHER LIABILITY, WHETHER IN AN ACTION OF CONTRACT,
+ * TORT OR OTHERWISE, ARISING FROM, OUT OF OR IN CONNECTION WITH THE
+ * SOFTWARE OR THE USE OR OTHER DEALINGS IN THE SOFTWARE.
+ *
+ */
+
+/** @file OMX_IndexExt.h - OpenMax IL version 1.1.2
+ * The OMX_IndexExt header file contains extensions to the definitions
+ * for both applications and components .
+ */
+
+#ifndef OMX_IndexExt_h
+#define OMX_IndexExt_h
+
+#ifdef __cplusplus
+extern "C" {
+#endif /* __cplusplus */
+
+/* Each OMX header shall include all required header files to allow the
+ * header to compile without errors.  The includes below are required
+ * for this header file to compile successfully
+ */
+#include <OMX_Index.h>
+
+
+/** Khronos standard extension indices.
+
+This enum lists the current Khronos extension indices to OpenMAX IL.
+*/
+typedef enum OMX_INDEXEXTTYPE {
+
+    /* Component parameters and configurations */
+    OMX_IndexExtComponentStartUnused = OMX_IndexKhronosExtensions + 0x00100000,
+    OMX_IndexConfigCallbackRequest,                 /**< reference: OMX_CONFIG_CALLBACKREQUESTTYPE */
+    OMX_IndexConfigCommitMode,                      /**< reference: OMX_CONFIG_COMMITMODETYPE */
+    OMX_IndexConfigCommit,                          /**< reference: OMX_CONFIG_COMMITTYPE */
+
+    /* Port parameters and configurations */
+    OMX_IndexExtPortStartUnused = OMX_IndexKhronosExtensions + 0x00200000,
+
+    /* Audio parameters and configurations */
+    OMX_IndexExtAudioStartUnused = OMX_IndexKhronosExtensions + 0x00400000,
+    OMX_IndexParamAudioAndroidAc3,                  /**< reference: OMX_AUDIO_PARAM_ANDROID_AC3TYPE */
+    OMX_IndexParamAudioAndroidOpus,                 /**< reference: OMX_AUDIO_PARAM_ANDROID_OPUSTYPE */
+    OMX_IndexParamAudioAndroidAacPresentation,      /**< reference: OMX_AUDIO_PARAM_ANDROID_AACPRESENTATIONTYPE */
+    OMX_IndexParamAudioAndroidEac3,                 /**< reference: OMX_AUDIO_PARAM_ANDROID_EAC3TYPE */
+    OMX_IndexParamAudioProfileQuerySupported,       /**< reference: OMX_AUDIO_PARAM_ANDROID_PROFILETYPE */
+
+    /* Image parameters and configurations */
+    OMX_IndexExtImageStartUnused = OMX_IndexKhronosExtensions + 0x00500000,
+
+    /* Video parameters and configurations */
+    OMX_IndexExtVideoStartUnused = OMX_IndexKhronosExtensions + 0x00600000,
+    OMX_IndexParamNalStreamFormatSupported,         /**< reference: OMX_NALSTREAMFORMATTYPE */
+    OMX_IndexParamNalStreamFormat,                  /**< reference: OMX_NALSTREAMFORMATTYPE */
+    OMX_IndexParamNalStreamFormatSelect,            /**< reference: OMX_NALSTREAMFORMATTYPE */
+    OMX_IndexParamVideoVp8,                         /**< reference: OMX_VIDEO_PARAM_VP8TYPE */
+    OMX_IndexConfigVideoVp8ReferenceFrame,          /**< reference: OMX_VIDEO_VP8REFERENCEFRAMETYPE */
+    OMX_IndexConfigVideoVp8ReferenceFrameType,      /**< reference: OMX_VIDEO_VP8REFERENCEFRAMEINFOTYPE */
+    OMX_IndexParamVideoAndroidVp8Encoder,           /**< reference: OMX_VIDEO_PARAM_ANDROID_VP8ENCODERTYPE */
+    OMX_IndexParamVideoHevc,                        /**< reference: OMX_VIDEO_PARAM_HEVCTYPE */
+    OMX_IndexParamSliceSegments,                    /**< reference: OMX_VIDEO_SLICESEGMENTSTYPE */
+    OMX_IndexConfigAndroidIntraRefresh,             /**< reference: OMX_VIDEO_CONFIG_ANDROID_INTRAREFRESHTYPE */
+    OMX_IndexParamAndroidVideoTemporalLayering,     /**< reference: OMX_VIDEO_PARAM_ANDROID_TEMPORALLAYERINGTYPE */
+    OMX_IndexConfigAndroidVideoTemporalLayering,    /**< reference: OMX_VIDEO_CONFIG_ANDROID_TEMPORALLAYERINGTYPE */
+
+    /* Image & Video common configurations */
+    OMX_IndexExtCommonStartUnused = OMX_IndexKhronosExtensions + 0x00700000,
+
+    /* Other configurations */
+    OMX_IndexExtOtherStartUnused = OMX_IndexKhronosExtensions + 0x00800000,
+    OMX_IndexConfigAutoFramerateConversion,         /**< reference: OMX_CONFIG_BOOLEANTYPE */
+    OMX_IndexConfigPriority,                        /**< reference: OMX_PARAM_U32TYPE */
+    OMX_IndexConfigOperatingRate,                   /**< reference: OMX_PARAM_U32TYPE in Q16 format for video and in Hz for audio */
+    OMX_IndexParamConsumerUsageBits,                /**< reference: OMX_PARAM_U32TYPE */
+
+    /* Time configurations */
+    OMX_IndexExtTimeStartUnused = OMX_IndexKhronosExtensions + 0x00900000,
+
+    OMX_IndexExtMax = 0x7FFFFFFF
+} OMX_INDEXEXTTYPE;
+
+#ifdef __cplusplus
+}
+#endif /* __cplusplus */
+
+#endif /* OMX_IndexExt_h */
+/* File EOF */
diff --git a/sf-extra/omx-il/OMX_Other.h b/sf-extra/omx-il/OMX_Other.h
new file mode 100644
index 00000000..8aa67b7e
--- /dev/null
+++ b/sf-extra/omx-il/OMX_Other.h
@@ -0,0 +1,366 @@
+/*
+ * Copyright (c) 2008 The Khronos Group Inc.
+ *
+ * Permission is hereby granted, free of charge, to any person obtaining
+ * a copy of this software and associated documentation files (the
+ * "Software"), to deal in the Software without restriction, including
+ * without limitation the rights to use, copy, modify, merge, publish,
+ * distribute, sublicense, and/or sell copies of the Software, and to
+ * permit persons to whom the Software is furnished to do so, subject
+ * to the following conditions:
+ * The above copyright notice and this permission notice shall be included
+ * in all copies or substantial portions of the Software.
+ *
+ * THE SOFTWARE IS PROVIDED "AS IS", WITHOUT WARRANTY OF ANY KIND, EXPRESS
+ * OR IMPLIED, INCLUDING BUT NOT LIMITED TO THE WARRANTIES OF
+ * MERCHANTABILITY, FITNESS FOR A PARTICULAR PURPOSE AND NONINFRINGEMENT.
+ * IN NO EVENT SHALL THE AUTHORS OR COPYRIGHT HOLDERS BE LIABLE FOR ANY
+ * CLAIM, DAMAGES OR OTHER LIABILITY, WHETHER IN AN ACTION OF CONTRACT,
+ * TORT OR OTHERWISE, ARISING FROM, OUT OF OR IN CONNECTION WITH THE
+ * SOFTWARE OR THE USE OR OTHER DEALINGS IN THE SOFTWARE.
+ *
+ */
+
+/** @file OMX_Other.h - OpenMax IL version 1.1.2
+ *  The structures needed by Other components to exchange
+ *  parameters and configuration data with the components.
+ */
+
+#ifndef OMX_Other_h
+#define OMX_Other_h
+
+#ifdef __cplusplus
+extern "C" {
+#endif /* __cplusplus */
+
+
+/* Each OMX header must include all required header files to allow the
+ *  header to compile without errors.  The includes below are required
+ *  for this header file to compile successfully
+ */
+
+#include <OMX_Core.h>
+
+
+/**
+ * Enumeration of possible data types which match to multiple domains or no
+ * domain at all.  For types which are vendor specific, a value above
+ * OMX_OTHER_VENDORTSTART should be used.
+ */
+typedef enum OMX_OTHER_FORMATTYPE {
+    OMX_OTHER_FormatTime = 0, /**< Transmission of various timestamps, elapsed time,
+                                   time deltas, etc */
+                           OMX_OTHER_FormatPower,    /**< Perhaps used for enabling/disabling power
+                                   management, setting clocks? */
+                           OMX_OTHER_FormatStats,    /**< Could be things such as frame rate, frames
+                                   dropped, etc */
+                           OMX_OTHER_FormatBinary,   /**< Arbitrary binary data */
+                           OMX_OTHER_FormatVendorReserved = 1000, /**< Starting value for vendor specific
+                                                formats */
+
+                                                            OMX_OTHER_FormatKhronosExtensions = 0x6F000000, /**< Reserved region for introducing Khronos Standard Extensions */
+                                                            OMX_OTHER_FormatVendorStartUnused = 0x7F000000, /**< Reserved region for introducing Vendor Extensions */
+                                                            OMX_OTHER_FormatMax = 0x7FFFFFFF
+} OMX_OTHER_FORMATTYPE;
+
+/**
+ * Enumeration of seek modes.
+ */
+typedef enum OMX_TIME_SEEKMODETYPE {
+    OMX_TIME_SeekModeFast = 0, /**< Prefer seeking to an approximation
+                                * of the requested seek position over
+                                * the actual seek position if it
+                                * results in a faster seek. */
+    OMX_TIME_SeekModeAccurate, /**< Prefer seeking to the actual seek
+                                * position over an approximation
+                                * of the requested seek position even
+                                * if it results in a slower seek. */
+    OMX_TIME_SeekModeKhronosExtensions = 0x6F000000, /**< Reserved region for introducing Khronos Standard Extensions */
+    OMX_TIME_SeekModeVendorStartUnused = 0x7F000000, /**< Reserved region for introducing Vendor Extensions */
+    OMX_TIME_SeekModeMax = 0x7FFFFFFF
+} OMX_TIME_SEEKMODETYPE;
+
+/* Structure representing the seekmode of the component */
+typedef struct OMX_TIME_CONFIG_SEEKMODETYPE {
+    OMX_U32 nSize;                  /**< size of the structure in bytes */
+    OMX_VERSIONTYPE nVersion;       /**< OMX specification version information */
+    OMX_TIME_SEEKMODETYPE eType;    /**< The seek mode */
+} OMX_TIME_CONFIG_SEEKMODETYPE;
+
+/**
+ * colorspace 
+ */
+typedef enum OMX_ROCKCHIP_EXT_COLORSPACE {
+    OMX_RK_EXT_ColorspaceBT709 = 1,
+    OMX_RK_EXT_ColorspaceBT2020,
+    OMX_RK_EXT_ColorspaceMax = 0x7FFFFFFF
+} OMX_RK_EXT_COLORSPACE;
+
+/**
+ * dynamic range
+ */
+typedef enum OMX_ROCKCHIP_EXT_DYNCRANGE {
+    OMX_RK_EXT_DyncrangeSDR = 0,
+    OMX_RK_EXT_DyncrangeHDR10,
+    OMX_RK_EXT_DyncrangeHDRHLG,
+    OMX_RK_EXT_DyncrangeHDRDOLBY,
+    OMX_RK_EXT_DyncrangeMax = 0x7FFFFFFF
+} OMX_RK_EXT_DYNCRANGE;
+
+
+/* Structure Rockchip extension HDR param of the component */
+ typedef struct OMX_EXTENSION_VIDEO_PARAM_HDR {
+    OMX_U32 nSize;                  /**< size of the structure in bytes */
+    OMX_VERSIONTYPE nVersion;       /**< OMX specification version information */
+    OMX_RK_EXT_COLORSPACE eColorSpace;    /**< Color space */
+    OMX_RK_EXT_DYNCRANGE eDyncRange;    /**< dynamic range */
+} OMX_EXTENSION_VIDEO_PARAM_HDR;
+
+/** Structure representing a time stamp used with the following configs
+ * on the Clock Component (CC):
+ *
+ * OMX_IndexConfigTimeCurrentWallTime: query of the CC’s current wall
+ *     time
+ * OMX_IndexConfigTimeCurrentMediaTime: query of the CC’s current media
+ *     time
+ * OMX_IndexConfigTimeCurrentAudioReference and
+ * OMX_IndexConfigTimeCurrentVideoReference: audio/video reference
+ *     clock sending SC its reference time
+ * OMX_IndexConfigTimeClientStartTime: a Clock Component client sends
+ *     this structure to the Clock Component via a SetConfig on its
+ *     client port when it receives a buffer with
+ *     OMX_BUFFERFLAG_STARTTIME set. It must use the timestamp
+ *     specified by that buffer for nStartTimestamp.
+ *
+ * It’s also used with the following config on components in general:
+ *
+ * OMX_IndexConfigTimePosition: IL client querying component position
+ * (GetConfig) or commanding a component to seek to the given location
+ * (SetConfig)
+ */
+typedef struct OMX_TIME_CONFIG_TIMESTAMPTYPE {
+    OMX_U32 nSize;               /**< size of the structure in bytes */
+    OMX_VERSIONTYPE nVersion;    /**< OMX specification version
+                                  *   information */
+    OMX_U32 nPortIndex;     /**< port that this structure applies to */
+    OMX_TICKS nTimestamp;        /**< timestamp .*/
+} OMX_TIME_CONFIG_TIMESTAMPTYPE;
+
+/** Enumeration of possible reference clocks to the media time. */
+typedef enum OMX_TIME_UPDATETYPE {
+    OMX_TIME_UpdateRequestFulfillment,    /**< Update is the fulfillment of a media time request. */
+    OMX_TIME_UpdateScaleChanged,          /**< Update was generated because the scale chagned. */
+    OMX_TIME_UpdateClockStateChanged,     /**< Update was generated because the clock state changed. */
+    OMX_TIME_UpdateKhronosExtensions = 0x6F000000, /**< Reserved region for introducing Khronos Standard Extensions */
+    OMX_TIME_UpdateVendorStartUnused = 0x7F000000, /**< Reserved region for introducing Vendor Extensions */
+    OMX_TIME_UpdateMax = 0x7FFFFFFF
+} OMX_TIME_UPDATETYPE;
+
+/** Enumeration of possible reference clocks to the media time. */
+typedef enum OMX_TIME_REFCLOCKTYPE {
+    OMX_TIME_RefClockNone,    /**< Use no references. */
+    OMX_TIME_RefClockAudio,   /**< Use references sent through OMX_IndexConfigTimeCurrentAudioReference */
+    OMX_TIME_RefClockVideo,   /**< Use references sent through OMX_IndexConfigTimeCurrentVideoReference */
+    OMX_TIME_RefClockKhronosExtensions = 0x6F000000, /**< Reserved region for introducing Khronos Standard Extensions */
+    OMX_TIME_RefClockVendorStartUnused = 0x7F000000, /**< Reserved region for introducing Vendor Extensions */
+    OMX_TIME_RefClockMax = 0x7FFFFFFF
+} OMX_TIME_REFCLOCKTYPE;
+
+/** Enumeration of clock states. */
+typedef enum OMX_TIME_CLOCKSTATE {
+    OMX_TIME_ClockStateRunning,             /**< Clock running. */
+    OMX_TIME_ClockStateWaitingForStartTime, /**< Clock waiting until the
+                                               *   prescribed clients emit their
+                                               *   start time. */
+    OMX_TIME_ClockStateStopped,             /**< Clock stopped. */
+    OMX_TIME_ClockStateKhronosExtensions = 0x6F000000, /**< Reserved region for introducing Khronos Standard Extensions */
+    OMX_TIME_ClockStateVendorStartUnused = 0x7F000000, /**< Reserved region for introducing Vendor Extensions */
+    OMX_TIME_ClockStateMax = 0x7FFFFFFF
+} OMX_TIME_CLOCKSTATE;
+
+/** Structure representing a media time request to the clock component.
+ *
+ *  A client component sends this structure to the Clock Component via a SetConfig
+ *  on its client port to specify a media timestamp the Clock Component
+ *  should emit.  The Clock Component should fulfill the request by sending a
+ *  OMX_TIME_MEDIATIMETYPE when its media clock matches the requested
+ *  timestamp.
+ *
+ *  The client may require a media time request be fulfilled slightly
+ *  earlier than the media time specified. In this case the client specifies
+ *  an offset which is equal to the difference between wall time corresponding
+ *  to the requested media time and the wall time when it will be
+ *  fulfilled.
+ *
+ *  A client component may uses these requests and the OMX_TIME_MEDIATIMETYPE to
+ *  time events according to timestamps. If a client must perform an operation O at
+ *  a time T (e.g. deliver a video frame at its corresponding timestamp), it makes a
+ *  media time request at T (perhaps specifying an offset to ensure the request fulfillment
+ *  is a little early). When the clock component passes the resulting OMX_TIME_MEDIATIMETYPE
+ *  structure back to the client component, the client may perform operation O (perhaps having
+ *  to wait a slight amount more time itself as specified by the return values).
+ */
+
+typedef struct OMX_TIME_CONFIG_MEDIATIMEREQUESTTYPE {
+    OMX_U32 nSize;              /**< size of the structure in bytes */
+    OMX_VERSIONTYPE nVersion;   /**< OMX specification version information */
+    OMX_U32 nPortIndex;         /**< port that this structure applies to */
+    OMX_PTR pClientPrivate;     /**< Client private data to disabiguate this media time
+                                 *   from others (e.g. the number of the frame to deliver).
+                                 *   Duplicated in the media time structure that fulfills
+                                 *   this request. A value of zero is reserved for time scale
+                                 *   updates. */
+    OMX_TICKS nMediaTimestamp;  /**< Media timestamp requested.*/
+    OMX_TICKS nOffset;          /**< Amount of wall clock time by which this
+                                 *   request should be fulfilled early */
+} OMX_TIME_CONFIG_MEDIATIMEREQUESTTYPE;
+
+/**< Structure sent from the clock component client either when fulfilling
+ *   a media time request or when the time scale has changed.
+ *
+ *   In the former case the Clock Component fills this structure and times its emission
+ *   to a client component (via the client port) according to the corresponding media
+ *   time request sent by the client. The Clock Component should time the emission to occur
+ *   when the requested timestamp matches the Clock Component's media time but also the
+ *   prescribed offset early.
+ *
+ *   Upon scale changes the clock component clears the nClientPrivate data, sends the current
+ *   media time and sets the nScale to the new scale via the client port. It emits a
+ *   OMX_TIME_MEDIATIMETYPE to all clients independent of any requests. This allows clients to
+ *   alter processing to accomodate scaling. For instance a video component might skip inter-frames
+ *   in the case of extreme fastforward. Likewise an audio component might add or remove samples
+ *   from an audio frame to scale audio data.
+ *
+ *   It is expected that some clock components may not be able to fulfill requests
+ *   at exactly the prescribed time. This is acceptable so long as the request is
+ *   fulfilled at least as early as described and not later. This structure provides
+ *   fields the client may use to wait for the remaining time.
+ *
+ *   The client may use either the nOffset or nWallTimeAtMedia fields to determine the
+ *   wall time until the nMediaTimestamp actually occurs. In the latter case the
+ *   client can get a more accurate value for offset by getting the current wall
+ *   from the cloc component and subtracting it from nWallTimeAtMedia.
+ */
+
+typedef struct OMX_TIME_MEDIATIMETYPE {
+    OMX_U32 nSize;                  /**< size of the structure in bytes */
+    OMX_VERSIONTYPE nVersion;       /**< OMX specification version information */
+    OMX_U32 nClientPrivate;         /**< Client private data to disabiguate this media time
+                                     *   from others. Copied from the media time request.
+                                     *   A value of zero is reserved for time scale updates. */
+    OMX_TIME_UPDATETYPE eUpdateType; /**< Reason for the update */
+    OMX_TICKS nMediaTimestamp;      /**< Media time requested. If no media time was
+                                     *   requested then this is the current media time. */
+    OMX_TICKS nOffset;              /**< Amount of wall clock time by which this
+                                     *   request was actually fulfilled early */
+
+    OMX_TICKS nWallTimeAtMediaTime; /**< Wall time corresponding to nMediaTimeStamp.
+                                     *   A client may compare this value to current
+                                     *   media time obtained from the Clock Component to determine
+                                     *   the wall time until the media timestamp is really
+                                     *   current. */
+    OMX_S32 xScale;                 /**< Current media time scale in Q16 format. */
+    OMX_TIME_CLOCKSTATE eState;     /* Seeking Change. Added 7/12.*/
+    /**< State of the media time. */
+} OMX_TIME_MEDIATIMETYPE;
+
+/** Structure representing the current media time scale factor. Applicable only to clock
+ *  component, other components see scale changes via OMX_TIME_MEDIATIMETYPE buffers sent via
+ *  the clock component client ports. Upon recieving this config the clock component changes
+ *  the rate by which the media time increases or decreases effectively implementing trick modes.
+ */
+typedef struct OMX_TIME_CONFIG_SCALETYPE {
+    OMX_U32 nSize;                  /**< size of the structure in bytes */
+    OMX_VERSIONTYPE nVersion;       /**< OMX specification version information */
+    OMX_S32 xScale;                 /**< This is a value in Q16 format which is used for
+                                     * scaling the media time */
+} OMX_TIME_CONFIG_SCALETYPE;
+
+/** Bits used to identify a clock port. Used in OMX_TIME_CONFIG_CLOCKSTATETYPE’s nWaitMask field */
+#define OMX_CLOCKPORT0 0x00000001
+#define OMX_CLOCKPORT1 0x00000002
+#define OMX_CLOCKPORT2 0x00000004
+#define OMX_CLOCKPORT3 0x00000008
+#define OMX_CLOCKPORT4 0x00000010
+#define OMX_CLOCKPORT5 0x00000020
+#define OMX_CLOCKPORT6 0x00000040
+#define OMX_CLOCKPORT7 0x00000080
+
+/** Structure representing the current mode of the media clock.
+ *  IL Client uses this config to change or query the mode of the
+ *  media clock of the clock component. Applicable only to clock
+ *  component.
+ *
+ *  On a SetConfig if eState is OMX_TIME_ClockStateRunning media time
+ *  starts immediately at the prescribed start time. If
+ *  OMX_TIME_ClockStateWaitingForStartTime the Clock Component ignores
+ *  the given nStartTime and waits for all clients specified in the
+ *  nWaitMask to send starttimes (via
+ *  OMX_IndexConfigTimeClientStartTime). The Clock Component then starts
+ *  the media clock using the earliest start time supplied. */
+typedef struct OMX_TIME_CONFIG_CLOCKSTATETYPE {
+    OMX_U32 nSize;              /**< size of the structure in bytes */
+    OMX_VERSIONTYPE nVersion;   /**< OMX specification version
+                                 *   information */
+    OMX_TIME_CLOCKSTATE eState; /**< State of the media time. */
+    OMX_TICKS nStartTime;       /**< Start time of the media time. */
+    OMX_TICKS nOffset;          /**< Time to offset the media time by
+                                 * (e.g. preroll). Media time will be
+                                 * reported to be nOffset ticks earlier.
+                                 */
+    OMX_U32 nWaitMask;          /**< Mask of OMX_CLOCKPORT values. */
+} OMX_TIME_CONFIG_CLOCKSTATETYPE;
+
+/** Structure representing the reference clock currently being used to
+ *  compute media time. IL client uses this config to change or query the
+ *  clock component's active reference clock */
+typedef struct OMX_TIME_CONFIG_ACTIVEREFCLOCKTYPE {
+    OMX_U32 nSize;                  /**< size of the structure in bytes */
+    OMX_VERSIONTYPE nVersion;       /**< OMX specification version information */
+    OMX_TIME_REFCLOCKTYPE eClock;   /**< Reference clock used to compute media time */
+} OMX_TIME_CONFIG_ACTIVEREFCLOCKTYPE;
+
+/** Descriptor for setting specifics of power type.
+ *  Note: this structure is listed for backwards compatibility. */
+typedef struct OMX_OTHER_CONFIG_POWERTYPE {
+    OMX_U32 nSize;            /**< size of the structure in bytes */
+    OMX_VERSIONTYPE nVersion; /**< OMX specification version information */
+    OMX_BOOL bEnablePM;       /**< Flag to enable Power Management */
+} OMX_OTHER_CONFIG_POWERTYPE;
+
+
+/** Descriptor for setting specifics of stats type.
+ *  Note: this structure is listed for backwards compatibility. */
+typedef struct OMX_OTHER_CONFIG_STATSTYPE {
+    OMX_U32 nSize;            /**< size of the structure in bytes */
+    OMX_VERSIONTYPE nVersion; /**< OMX specification version information */
+    /* what goes here */
+} OMX_OTHER_CONFIG_STATSTYPE;
+
+
+/**
+ * The PortDefinition structure is used to define all of the parameters
+ * necessary for the compliant component to setup an input or an output other
+ * path.
+ */
+typedef struct OMX_OTHER_PORTDEFINITIONTYPE {
+    OMX_OTHER_FORMATTYPE eFormat;  /**< Type of data expected for this channel */
+} OMX_OTHER_PORTDEFINITIONTYPE;
+
+/**  Port format parameter.  This structure is used to enumerate
+  *  the various data input/output format supported by the port.
+  */
+typedef struct OMX_OTHER_PARAM_PORTFORMATTYPE {
+    OMX_U32 nSize; /**< size of the structure in bytes */
+    OMX_VERSIONTYPE nVersion; /**< OMX specification version information */
+    OMX_U32 nPortIndex; /**< Indicates which port to set */
+    OMX_U32 nIndex; /**< Indicates the enumeration index for the format from 0x0 to N-1 */
+    OMX_OTHER_FORMATTYPE eFormat; /**< Type of data expected for this channel */
+} OMX_OTHER_PARAM_PORTFORMATTYPE;
+
+#ifdef __cplusplus
+}
+#endif /* __cplusplus */
+
+#endif
+/* File EOF */
diff --git a/sf-extra/omx-il/OMX_Types.h b/sf-extra/omx-il/OMX_Types.h
new file mode 100644
index 00000000..527ba235
--- /dev/null
+++ b/sf-extra/omx-il/OMX_Types.h
@@ -0,0 +1,361 @@
+/*
+ * Copyright (c) 2016 The Khronos Group Inc.
+ *
+ * Permission is hereby granted, free of charge, to any person obtaining
+ * a copy of this software and associated documentation files (the
+ * "Software"), to deal in the Software without restriction, including
+ * without limitation the rights to use, copy, modify, merge, publish,
+ * distribute, sublicense, and/or sell copies of the Software, and to
+ * permit persons to whom the Software is furnished to do so, subject
+ * to the following conditions:
+ * The above copyright notice and this permission notice shall be included
+ * in all copies or substantial portions of the Software.
+ *
+ * THE SOFTWARE IS PROVIDED "AS IS", WITHOUT WARRANTY OF ANY KIND, EXPRESS
+ * OR IMPLIED, INCLUDING BUT NOT LIMITED TO THE WARRANTIES OF
+ * MERCHANTABILITY, FITNESS FOR A PARTICULAR PURPOSE AND NONINFRINGEMENT.
+ * IN NO EVENT SHALL THE AUTHORS OR COPYRIGHT HOLDERS BE LIABLE FOR ANY
+ * CLAIM, DAMAGES OR OTHER LIABILITY, WHETHER IN AN ACTION OF CONTRACT,
+ * TORT OR OTHERWISE, ARISING FROM, OUT OF OR IN CONNECTION WITH THE
+ * SOFTWARE OR THE USE OR OTHER DEALINGS IN THE SOFTWARE.
+ *
+ */
+
+/** OMX_Types.h - OpenMax IL version 1.1.2
+ *  The OMX_Types header file contains the primitive type definitions used by
+ *  the core, the application and the component.  This file may need to be
+ *  modified to be used on systems that do not have "char" set to 8 bits,
+ *  "short" set to 16 bits and "long" set to 32 bits.
+ */
+
+#ifndef OMX_Types_h
+#define OMX_Types_h
+
+#include <stdint.h>
+
+#ifdef __cplusplus
+extern "C" {
+#endif /* __cplusplus */
+
+/** The OMX_API and OMX_APIENTRY are platform specific definitions used
+ *  to declare OMX function prototypes.  They are modified to meet the
+ *  requirements for a particular platform */
+#ifdef __SYMBIAN32__
+#   ifdef __OMX_EXPORTS
+#       define OMX_API __declspec(dllexport)
+#   else
+#       ifdef _WIN32
+#           define OMX_API __declspec(dllexport)
+#       else
+#           define OMX_API __declspec(dllimport)
+#       endif
+#   endif
+#else
+#   ifdef _WIN32
+#      ifdef __OMX_EXPORTS
+#          define OMX_API __declspec(dllexport)
+#      else
+#          define OMX_API __declspec(dllimport)
+#      endif
+#   else
+#      ifdef __OMX_EXPORTS
+#          define OMX_API
+#      else
+#          define OMX_API extern
+#      endif
+#   endif
+#endif
+
+#ifndef OMX_APIENTRY
+#define OMX_APIENTRY
+#endif
+
+/** OMX_IN is used to identify inputs to an OMX function.  This designation
+    will also be used in the case of a pointer that points to a parameter
+    that is used as an output. */
+#ifndef OMX_IN
+#define OMX_IN
+#endif
+
+/** OMX_OUT is used to identify outputs from an OMX function.  This
+    designation will also be used in the case of a pointer that points
+    to a parameter that is used as an input. */
+#ifndef OMX_OUT
+#define OMX_OUT
+#endif
+
+
+/** OMX_INOUT is used to identify parameters that may be either inputs or
+    outputs from an OMX function at the same time.  This designation will
+    also be used in the case of a pointer that  points to a parameter that
+    is used both as an input and an output. */
+#ifndef OMX_INOUT
+#define OMX_INOUT
+#endif
+
+/** OMX_ALL is used to as a wildcard to select all entities of the same type
+ *  when specifying the index, or referring to a object by an index.  (i.e.
+ *  use OMX_ALL to indicate all N channels). When used as a port index
+ *  for a config or parameter this OMX_ALL denotes that the config or
+ *  parameter applies to the entire component not just one port. */
+#define OMX_ALL 0xFFFFFFFF
+
+/** In the following we define groups that help building doxygen documentation */
+
+/** @defgroup core OpenMAX IL core
+ * Functions and structure related to the OMX IL core
+ */
+
+ /** @defgroup comp OpenMAX IL component
+ * Functions and structure related to the OMX IL component
+ */
+
+/** @defgroup rpm Resource and Policy Management
+ * Structures for resource and policy management of components
+ */
+
+/** @defgroup buf Buffer Management
+ * Buffer handling functions and structures
+ */
+
+/** @defgroup tun Tunneling
+ * @ingroup core comp
+ * Structures and functions to manage tunnels among component ports
+ */
+
+/** @defgroup cp Content Pipes
+ *  @ingroup core
+ */
+
+ /** @defgroup metadata Metadata handling
+  *
+  */
+
+/** OMX_U8 is an 8 bit unsigned quantity that is byte aligned */
+typedef uint8_t OMX_U8;
+
+/** OMX_S8 is an 8 bit signed quantity that is byte aligned */
+typedef int8_t OMX_S8;
+
+/** OMX_U16 is a 16 bit unsigned quantity that is 16 bit word aligned */
+typedef uint16_t OMX_U16;
+
+/** OMX_S16 is a 16 bit signed quantity that is 16 bit word aligned */
+typedef int16_t OMX_S16;
+
+/** OMX_U32 is a 32 bit unsigned quantity that is 32 bit word aligned */
+typedef uint32_t OMX_U32;
+
+/** OMX_S32 is a 32 bit signed quantity that is 32 bit word aligned */
+typedef int32_t OMX_S32;
+
+
+/* Users with compilers that cannot accept the "long long" designation should
+   define the OMX_SKIP64BIT macro.  It should be noted that this may cause
+   some components to fail to compile if the component was written to require
+   64 bit integral types.  However, these components would NOT compile anyway
+   since the compiler does not support the way the component was written.
+*/
+#ifndef OMX_SKIP64BIT
+#ifdef __SYMBIAN32__
+/** OMX_U64 is a 64 bit unsigned quantity that is 64 bit word aligned */
+typedef unsigned long long OMX_U64;
+
+/** OMX_S64 is a 64 bit signed quantity that is 64 bit word aligned */
+typedef signed long long OMX_S64;
+
+#elif defined(WIN32)
+
+/** OMX_U64 is a 64 bit unsigned quantity that is 64 bit word aligned */
+typedef unsigned __int64  OMX_U64;
+
+/** OMX_S64 is a 64 bit signed quantity that is 64 bit word aligned */
+typedef signed   __int64  OMX_S64;
+
+#else /* WIN32 */
+
+/** OMX_U64 is a 64 bit unsigned quantity that is 64 bit word aligned */
+typedef uint64_t OMX_U64;
+
+/** OMX_S64 is a 64 bit signed quantity that is 64 bit word aligned */
+typedef int64_t OMX_S64;
+
+#endif /* WIN32 */
+#endif
+
+
+/** The OMX_BOOL type is intended to be used to represent a true or a false
+    value when passing parameters to and from the OMX core and components.  The
+    OMX_BOOL is a 32 bit quantity and is aligned on a 32 bit word boundary.
+ */
+typedef enum OMX_BOOL {
+    OMX_FALSE = 0,
+    OMX_TRUE = !OMX_FALSE,
+    OMX_BOOL_MAX = 0x7FFFFFFF
+} OMX_BOOL;
+
+/** The OMX_PTR type is intended to be used to pass pointers between the OMX
+    applications and the OMX Core and components.  This is a 32 bit pointer and
+    is aligned on a 32 bit boundary.
+ */
+typedef void* OMX_PTR;
+
+/** The OMX_STRING type is intended to be used to pass "C" type strings between
+    the application and the core and component.  The OMX_STRING type is a 32
+    bit pointer to a zero terminated string.  The  pointer is word aligned and
+    the string is byte aligned.
+ */
+typedef char* OMX_STRING;
+
+/** The OMX_BYTE type is intended to be used to pass arrays of bytes such as
+    buffers between the application and the component and core.  The OMX_BYTE
+    type is a 32 bit pointer to a zero terminated string.  The  pointer is word
+    aligned and the string is byte aligned.
+ */
+typedef unsigned char* OMX_BYTE;
+
+/** OMX_UUIDTYPE is a very long unique identifier to uniquely identify
+    at runtime.  This identifier should be generated by a component in a way
+    that guarantees that every instance of the identifier running on the system
+    is unique. */
+typedef unsigned char OMX_UUIDTYPE[128];
+
+/** The OMX_DIRTYPE enumeration is used to indicate if a port is an input or
+    an output port.  This enumeration is common across all component types.
+ */
+typedef enum OMX_DIRTYPE
+{
+    OMX_DirInput,              /**< Port is an input port */
+    OMX_DirOutput,             /**< Port is an output port */
+    OMX_DirMax = 0x7FFFFFFF
+} OMX_DIRTYPE;
+
+/** The OMX_ENDIANTYPE enumeration is used to indicate the bit ordering
+    for numerical data (i.e. big endian, or little endian).
+ */
+typedef enum OMX_ENDIANTYPE
+{
+    OMX_EndianBig, /**< big endian */
+    OMX_EndianLittle, /**< little endian */
+    OMX_EndianMax = 0x7FFFFFFF
+} OMX_ENDIANTYPE;
+
+
+/** The OMX_NUMERICALDATATYPE enumeration is used to indicate if data
+    is signed or unsigned
+ */
+typedef enum OMX_NUMERICALDATATYPE
+{
+    OMX_NumericalDataSigned, /**< signed data */
+    OMX_NumericalDataUnsigned, /**< unsigned data */
+    OMX_NumercialDataMax = 0x7FFFFFFF
+} OMX_NUMERICALDATATYPE;
+
+
+/** Unsigned bounded value type */
+typedef struct OMX_BU32 {
+    OMX_U32 nValue; /**< actual value */
+    OMX_U32 nMin;   /**< minimum for value (i.e. nValue >= nMin) */
+    OMX_U32 nMax;   /**< maximum for value (i.e. nValue <= nMax) */
+} OMX_BU32;
+
+
+/** Signed bounded value type */
+typedef struct OMX_BS32 {
+    OMX_S32 nValue; /**< actual value */
+    OMX_S32 nMin;   /**< minimum for value (i.e. nValue >= nMin) */
+    OMX_S32 nMax;   /**< maximum for value (i.e. nValue <= nMax) */
+} OMX_BS32;
+
+
+/** Structure representing some time or duration in microseconds. This structure
+  *  must be interpreted as a signed 64 bit value. The quantity is signed to accommodate
+  *  negative deltas and preroll scenarios. The quantity is represented in microseconds
+  *  to accomodate high resolution timestamps (e.g. DVD presentation timestamps based
+  *  on a 90kHz clock) and to allow more accurate and synchronized delivery (e.g.
+  *  individual audio samples delivered at 192 kHz). The quantity is 64 bit to
+  *  accommodate a large dynamic range (signed 32 bit values would allow only for plus
+  *  or minus 35 minutes).
+  *
+  *  Implementations with limited precision may convert the signed 64 bit value to
+  *  a signed 32 bit value internally but risk loss of precision.
+  */
+#ifndef OMX_SKIP64BIT
+typedef OMX_S64 OMX_TICKS;
+#else
+typedef struct OMX_TICKS
+{
+    OMX_U32 nLowPart;    /** low bits of the signed 64 bit tick value */
+    OMX_U32 nHighPart;   /** high bits of the signed 64 bit tick value */
+} OMX_TICKS;
+#endif
+#define OMX_TICKS_PER_SECOND 1000000
+
+/** Define the public interface for the OMX Handle.  The core will not use
+    this value internally, but the application should only use this value.
+ */
+typedef void* OMX_HANDLETYPE;
+
+typedef struct OMX_MARKTYPE
+{
+    OMX_HANDLETYPE hMarkTargetComponent;   /**< The component that will
+                                                generate a mark event upon
+                                                processing the mark. */
+    OMX_PTR pMarkData;   /**< Application specific data associated with
+                              the mark sent on a mark event to disambiguate
+                              this mark from others. */
+} OMX_MARKTYPE;
+
+
+/** OMX_NATIVE_DEVICETYPE is used to map a OMX video port to the
+ *  platform & operating specific object used to reference the display
+ *  or can be used by a audio port for native audio rendering */
+typedef void* OMX_NATIVE_DEVICETYPE;
+
+/** OMX_NATIVE_WINDOWTYPE is used to map a OMX video port to the
+ *  platform & operating specific object used to reference the window */
+typedef void* OMX_NATIVE_WINDOWTYPE;
+
+
+/** Define the OMX IL version that corresponds to this set of header files.
+ *  We also define a combined version that can be used to write or compare
+ *  values of the 32bit nVersion field, assuming a little endian architecture */
+#define OMX_VERSION_MAJOR 1
+#define OMX_VERSION_MINOR 1
+#define OMX_VERSION_REVISION 2
+#define OMX_VERSION_STEP 0
+
+#define OMX_VERSION ((OMX_VERSION_STEP<<24) | (OMX_VERSION_REVISION<<16) | (OMX_VERSION_MINOR<<8) | OMX_VERSION_MAJOR)
+
+
+/** The OMX_VERSIONTYPE union is used to specify the version for
+    a structure or component.  For a component, the version is entirely
+    specified by the component vendor.  Components doing the same function
+    from different vendors may or may not have the same version.  For
+    structures, the version shall be set by the entity that allocates the
+    structure.  For structures specified in the OMX 1.1 specification, the
+    value of the version shall be set to 1.1.0.0 in all cases.  Access to the
+    OMX_VERSIONTYPE can be by a single 32 bit access (e.g. by nVersion) or
+    by accessing one of the structure elements to, for example, check only
+    the Major revision.
+ */
+typedef union OMX_VERSIONTYPE
+{
+    struct
+    {
+        OMX_U8 nVersionMajor;   /**< Major version accessor element */
+        OMX_U8 nVersionMinor;   /**< Minor version accessor element */
+        OMX_U8 nRevision;       /**< Revision version accessor element */
+        OMX_U8 nStep;           /**< Step version accessor element */
+    } s;
+    OMX_U32 nVersion;           /**< 32 bit value to make accessing the
+                                    version easily done in a single word
+                                    size copy/compare operation */
+} OMX_VERSIONTYPE;
+
+#ifdef __cplusplus
+}
+#endif /* __cplusplus */
+
+#endif
+/* File EOF */
diff --git a/sf-extra/omx-il/OMX_Video.h b/sf-extra/omx-il/OMX_Video.h
new file mode 100644
index 00000000..6fa26266
--- /dev/null
+++ b/sf-extra/omx-il/OMX_Video.h
@@ -0,0 +1,1141 @@
+/**
+ * Copyright (c) 2008 The Khronos Group Inc.
+ *
+ * Permission is hereby granted, free of charge, to any person obtaining
+ * a copy of this software and associated documentation files (the
+ * "Software"), to deal in the Software without restriction, including
+ * without limitation the rights to use, copy, modify, merge, publish,
+ * distribute, sublicense, and/or sell copies of the Software, and to
+ * permit persons to whom the Software is furnished to do so, subject
+ * to the following conditions:
+ * The above copyright notice and this permission notice shall be included
+ * in all copies or substantial portions of the Software.
+ *
+ * THE SOFTWARE IS PROVIDED "AS IS", WITHOUT WARRANTY OF ANY KIND, EXPRESS
+ * OR IMPLIED, INCLUDING BUT NOT LIMITED TO THE WARRANTIES OF
+ * MERCHANTABILITY, FITNESS FOR A PARTICULAR PURPOSE AND NONINFRINGEMENT.
+ * IN NO EVENT SHALL THE AUTHORS OR COPYRIGHT HOLDERS BE LIABLE FOR ANY
+ * CLAIM, DAMAGES OR OTHER LIABILITY, WHETHER IN AN ACTION OF CONTRACT,
+ * TORT OR OTHERWISE, ARISING FROM, OUT OF OR IN CONNECTION WITH THE
+ * SOFTWARE OR THE USE OR OTHER DEALINGS IN THE SOFTWARE.
+ *
+ */
+
+/**
+ *  @file OMX_Video.h - OpenMax IL version 1.1.2
+ *  The structures is needed by Video components to exchange parameters
+ *  and configuration data with OMX components.
+ */
+#ifndef OMX_Video_h
+#define OMX_Video_h
+
+/** @defgroup video OpenMAX IL Video Domain
+ * @ingroup iv
+ * Structures for OpenMAX IL Video domain
+ * @{
+ */
+
+#ifdef __cplusplus
+extern "C" {
+#endif /* __cplusplus */
+
+
+/**
+ * Each OMX header must include all required header files to allow the
+ * header to compile without errors.  The includes below are required
+ * for this header file to compile successfully
+ */
+
+#include <OMX_IVCommon.h>
+
+
+/**
+ * Enumeration used to define the possible video compression codings.
+ * NOTE:  This essentially refers to file extensions. If the coding is
+ *        being used to specify the ENCODE type, then additional work
+ *        must be done to configure the exact flavor of the compression
+ *        to be used.  For decode cases where the user application can
+ *        not differentiate between MPEG-4 and H.264 bit streams, it is
+ *        up to the codec to handle this.
+ */
+typedef enum OMX_VIDEO_CODINGTYPE {
+    OMX_VIDEO_CodingUnused,     /**< Value when coding is N/A */
+    OMX_VIDEO_CodingAutoDetect, /**< Autodetection of coding type */
+    OMX_VIDEO_CodingMPEG2,      /**< AKA: H.262 */
+    OMX_VIDEO_CodingH263,       /**< H.263 */
+    OMX_VIDEO_CodingMPEG4,      /**< MPEG-4 */
+    OMX_VIDEO_CodingWMV,        /**< all versions of Windows Media Video */
+    OMX_VIDEO_CodingRV,         /**< all versions of Real Video */
+    OMX_VIDEO_CodingAVC,        /**< H.264/AVC */
+    OMX_VIDEO_CodingMJPEG,      /**< Motion JPEG */
+    OMX_VIDEO_CodingVP8,        /**< Google VP8, formerly known as On2 VP8 */
+    OMX_VIDEO_CodingVP9,        /**< Google VP9 */
+    OMX_VIDEO_CodingHEVC,       /**< ITU H.265/HEVC */
+    OMX_VIDEO_CodingKhronosExtensions = 0x6F000000, /**< Reserved region for introducing Khronos Standard Extensions */
+    OMX_VIDEO_CodingVendorStartUnused = 0x7F000000, /**< Reserved region for introducing Vendor Extensions */
+    OMX_VIDEO_CodingMax = 0x7FFFFFFF
+} OMX_VIDEO_CODINGTYPE;
+
+
+/**
+ * Data structure used to define a video path.  The number of Video paths for
+ * input and output will vary by type of the Video component.
+ *
+ *    Input (aka Source) : zero Inputs, one Output,
+ *    Splitter           : one Input, 2 or more Outputs,
+ *    Processing Element : one Input, one output,
+ *    Mixer              : 2 or more inputs, one output,
+ *    Output (aka Sink)  : one Input, zero outputs.
+ *
+ * The PortDefinition structure is used to define all of the parameters
+ * necessary for the compliant component to setup an input or an output video
+ * path.  If additional vendor specific data is required, it should be
+ * transmitted to the component using the CustomCommand function.  Compliant
+ * components will prepopulate this structure with optimal values during the
+ * GetDefaultInitParams command.
+ *
+ * STRUCT MEMBERS:
+ *  cMIMEType             : MIME type of data for the port
+ *  pNativeRender         : Platform specific reference for a display if a
+ *                          sync, otherwise this field is 0
+ *  nFrameWidth           : Width of frame to be used on channel if
+ *                          uncompressed format is used.  Use 0 for unknown,
+ *                          don't care or variable
+ *  nFrameHeight          : Height of frame to be used on channel if
+ *                          uncompressed format is used. Use 0 for unknown,
+ *                          don't care or variable
+ *  nStride               : Number of bytes per span of an image
+ *                          (i.e. indicates the number of bytes to get
+ *                          from span N to span N+1, where negative stride
+ *                          indicates the image is bottom up
+ *  nSliceHeight          : Height used when encoding in slices
+ *  nBitrate              : Bit rate of frame to be used on channel if
+ *                          compressed format is used. Use 0 for unknown,
+ *                          don't care or variable
+ *  xFramerate            : Frame rate to be used on channel if uncompressed
+ *                          format is used. Use 0 for unknown, don't care or
+ *                          variable.  Units are Q16 frames per second.
+ *  bFlagErrorConcealment : Turns on error concealment if it is supported by
+ *                          the OMX component
+ *  eCompressionFormat    : Compression format used in this instance of the
+ *                          component. When OMX_VIDEO_CodingUnused is
+ *                          specified, eColorFormat is used
+ *  eColorFormat : Decompressed format used by this component
+ *  pNativeWindow : Platform specific reference for a window object if a
+ *                          display sink , otherwise this field is 0x0.
+ */
+typedef struct OMX_VIDEO_PORTDEFINITIONTYPE {
+    OMX_STRING cMIMEType;
+    OMX_NATIVE_DEVICETYPE pNativeRender;
+    OMX_U32 nFrameWidth;
+    OMX_U32 nFrameHeight;
+    OMX_S32 nStride;
+    OMX_U32 nSliceHeight;
+    OMX_U32 nBitrate;
+    OMX_U32 xFramerate;
+    OMX_BOOL bFlagErrorConcealment;
+    OMX_VIDEO_CODINGTYPE eCompressionFormat;
+    OMX_COLOR_FORMATTYPE eColorFormat;
+    OMX_NATIVE_WINDOWTYPE pNativeWindow;
+} OMX_VIDEO_PORTDEFINITIONTYPE;
+
+/**
+ * Port format parameter.  This structure is used to enumerate the various
+ * data input/output format supported by the port.
+ *
+ * STRUCT MEMBERS:
+ *  nSize              : Size of the structure in bytes
+ *  nVersion           : OMX specification version information
+ *  nPortIndex         : Indicates which port to set
+ *  nIndex             : Indicates the enumeration index for the format from
+ *                       0x0 to N-1
+ *  eCompressionFormat : Compression format used in this instance of the
+ *                       component. When OMX_VIDEO_CodingUnused is specified,
+ *                       eColorFormat is used
+ *  eColorFormat       : Decompressed format used by this component
+ *  xFrameRate         : Indicates the video frame rate in Q16 format
+ */
+typedef struct OMX_VIDEO_PARAM_PORTFORMATTYPE {
+    OMX_U32 nSize;
+    OMX_VERSIONTYPE nVersion;
+    OMX_U32 nPortIndex;
+    OMX_U32 nIndex;
+    OMX_VIDEO_CODINGTYPE eCompressionFormat;
+    OMX_COLOR_FORMATTYPE eColorFormat;
+    OMX_U32 xFramerate;
+} OMX_VIDEO_PARAM_PORTFORMATTYPE;
+
+
+/**
+ * This is a structure for configuring video compression quantization
+ * parameter values.  Codecs may support different QP values for different
+ * frame types.
+ *
+ * STRUCT MEMBERS:
+ *  nSize      : Size of the structure in bytes
+ *  nVersion   : OMX specification version info
+ *  nPortIndex : Port that this structure applies to
+ *  nQpI       : QP value to use for index frames
+ *  nQpP       : QP value to use for P frames
+ *  nQpB       : QP values to use for bidirectional frames
+ */
+typedef struct OMX_VIDEO_PARAM_QUANTIZATIONTYPE {
+    OMX_U32 nSize;
+    OMX_VERSIONTYPE nVersion;
+    OMX_U32 nPortIndex;
+    OMX_U32 nQpI;
+    OMX_U32 nQpP;
+    OMX_U32 nQpB;
+} OMX_VIDEO_PARAM_QUANTIZATIONTYPE;
+
+
+/**
+ * Structure for configuration of video fast update parameters.
+ *
+ * STRUCT MEMBERS:
+ *  nSize      : Size of the structure in bytes
+ *  nVersion   : OMX specification version info
+ *  nPortIndex : Port that this structure applies to
+ *  bEnableVFU : Enable/Disable video fast update
+ *  nFirstGOB  : Specifies the number of the first macroblock row
+ *  nFirstMB   : specifies the first MB relative to the specified first GOB
+ *  nNumMBs    : Specifies the number of MBs to be refreshed from nFirstGOB
+ *               and nFirstMB
+ */
+typedef struct OMX_VIDEO_PARAM_VIDEOFASTUPDATETYPE {
+    OMX_U32 nSize;
+    OMX_VERSIONTYPE nVersion;
+    OMX_U32 nPortIndex;
+    OMX_BOOL bEnableVFU;
+    OMX_U32 nFirstGOB;
+    OMX_U32 nFirstMB;
+    OMX_U32 nNumMBs;
+} OMX_VIDEO_PARAM_VIDEOFASTUPDATETYPE;
+
+
+/**
+ * Enumeration of possible bitrate control types
+ */
+typedef enum OMX_VIDEO_CONTROLRATETYPE {
+    OMX_Video_ControlRateDisable,
+    OMX_Video_ControlRateVariable,
+    OMX_Video_ControlRateConstant,
+    OMX_Video_ControlRateVariableSkipFrames,
+    OMX_Video_ControlRateConstantSkipFrames,
+    OMX_Video_ControlRateKhronosExtensions = 0x6F000000, /**< Reserved region for introducing Khronos Standard Extensions */
+    OMX_Video_ControlRateVendorStartUnused = 0x7F000000, /**< Reserved region for introducing Vendor Extensions */
+    OMX_Video_ControlRateMax = 0x7FFFFFFF
+} OMX_VIDEO_CONTROLRATETYPE;
+
+
+/**
+ * Structure for configuring bitrate mode of a codec.
+ *
+ * STRUCT MEMBERS:
+ *  nSize          : Size of the struct in bytes
+ *  nVersion       : OMX spec version info
+ *  nPortIndex     : Port that this struct applies to
+ *  eControlRate   : Control rate type enum
+ *  nTargetBitrate : Target bitrate to encode with
+ */
+typedef struct OMX_VIDEO_PARAM_BITRATETYPE {
+    OMX_U32 nSize;
+    OMX_VERSIONTYPE nVersion;
+    OMX_U32 nPortIndex;
+    OMX_VIDEO_CONTROLRATETYPE eControlRate;
+    OMX_U32 nTargetBitrate;
+} OMX_VIDEO_PARAM_BITRATETYPE;
+
+
+/**
+ * Enumeration of possible motion vector (MV) types
+ */
+typedef enum OMX_VIDEO_MOTIONVECTORTYPE {
+    OMX_Video_MotionVectorPixel,
+    OMX_Video_MotionVectorHalfPel,
+    OMX_Video_MotionVectorQuarterPel,
+    OMX_Video_MotionVectorEighthPel,
+    OMX_Video_MotionVectorKhronosExtensions = 0x6F000000, /**< Reserved region for introducing Khronos Standard Extensions */
+    OMX_Video_MotionVectorVendorStartUnused = 0x7F000000, /**< Reserved region for introducing Vendor Extensions */
+    OMX_Video_MotionVectorMax = 0x7FFFFFFF
+} OMX_VIDEO_MOTIONVECTORTYPE;
+
+
+/**
+ * Structure for configuring the number of motion vectors used as well
+ * as their accuracy.
+ *
+ * STRUCT MEMBERS:
+ *  nSize            : Size of the struct in bytes
+ *  nVersion         : OMX spec version info
+ *  nPortIndex       : port that this structure applies to
+ *  eAccuracy        : Enumerated MV accuracy
+ *  bUnrestrictedMVs : Allow unrestricted MVs
+ *  bFourMV          : Allow use of 4 MVs
+ *  sXSearchRange    : Search range in horizontal direction for MVs
+ *  sYSearchRange    : Search range in vertical direction for MVs
+ */
+typedef struct OMX_VIDEO_PARAM_MOTIONVECTORTYPE {
+    OMX_U32 nSize;
+    OMX_VERSIONTYPE nVersion;
+    OMX_U32 nPortIndex;
+    OMX_VIDEO_MOTIONVECTORTYPE eAccuracy;
+    OMX_BOOL bUnrestrictedMVs;
+    OMX_BOOL bFourMV;
+    OMX_S32 sXSearchRange;
+    OMX_S32 sYSearchRange;
+} OMX_VIDEO_PARAM_MOTIONVECTORTYPE;
+
+
+/**
+ * Enumeration of possible methods to use for Intra Refresh
+ */
+typedef enum OMX_VIDEO_INTRAREFRESHTYPE {
+    OMX_VIDEO_IntraRefreshCyclic,
+    OMX_VIDEO_IntraRefreshAdaptive,
+    OMX_VIDEO_IntraRefreshBoth,
+    OMX_VIDEO_IntraRefreshKhronosExtensions = 0x6F000000, /**< Reserved region for introducing Khronos Standard Extensions */
+    OMX_VIDEO_IntraRefreshVendorStartUnused = 0x7F000000, /**< Reserved region for introducing Vendor Extensions */
+    OMX_VIDEO_IntraRefreshMax = 0x7FFFFFFF
+} OMX_VIDEO_INTRAREFRESHTYPE;
+
+
+/**
+ * Structure for configuring intra refresh mode
+ *
+ * STRUCT MEMBERS:
+ *  nSize        : Size of the structure in bytes
+ *  nVersion     : OMX specification version information
+ *  nPortIndex   : Port that this structure applies to
+ *  eRefreshMode : Cyclic, Adaptive, or Both
+ *  nAirMBs      : Number of intra macroblocks to refresh in a frame when
+ *                 AIR is enabled
+ *  nAirRef      : Number of times a motion marked macroblock has to be
+ *                 intra coded
+ *  nCirMBs      : Number of consecutive macroblocks to be coded as "intra"
+ *                 when CIR is enabled
+ */
+typedef struct OMX_VIDEO_PARAM_INTRAREFRESHTYPE {
+    OMX_U32 nSize;
+    OMX_VERSIONTYPE nVersion;
+    OMX_U32 nPortIndex;
+    OMX_VIDEO_INTRAREFRESHTYPE eRefreshMode;
+    OMX_U32 nAirMBs;
+    OMX_U32 nAirRef;
+    OMX_U32 nCirMBs;
+} OMX_VIDEO_PARAM_INTRAREFRESHTYPE;
+
+
+/**
+ * Structure for enabling various error correction methods for video
+ * compression.
+ *
+ * STRUCT MEMBERS:
+ *  nSize                   : Size of the structure in bytes
+ *  nVersion                : OMX specification version information
+ *  nPortIndex              : Port that this structure applies to
+ *  bEnableHEC              : Enable/disable header extension codes (HEC)
+ *  bEnableResync           : Enable/disable resynchronization markers
+ *  nResynchMarkerSpacing   : Resynch markers interval (in bits) to be
+ *                            applied in the stream
+ *  bEnableDataPartitioning : Enable/disable data partitioning
+ *  bEnableRVLC             : Enable/disable reversible variable length
+ *                            coding
+ */
+typedef struct OMX_VIDEO_PARAM_ERRORCORRECTIONTYPE {
+    OMX_U32 nSize;
+    OMX_VERSIONTYPE nVersion;
+    OMX_U32 nPortIndex;
+    OMX_BOOL bEnableHEC;
+    OMX_BOOL bEnableResync;
+    OMX_U32  nResynchMarkerSpacing;
+    OMX_BOOL bEnableDataPartitioning;
+    OMX_BOOL bEnableRVLC;
+} OMX_VIDEO_PARAM_ERRORCORRECTIONTYPE;
+
+
+/**
+ * Configuration of variable block-size motion compensation (VBSMC)
+ *
+ * STRUCT MEMBERS:
+ *  nSize      : Size of the structure in bytes
+ *  nVersion   : OMX specification version information
+ *  nPortIndex : Port that this structure applies to
+ *  b16x16     : Enable inter block search 16x16
+ *  b16x8      : Enable inter block search 16x8
+ *  b8x16      : Enable inter block search 8x16
+ *  b8x8       : Enable inter block search 8x8
+ *  b8x4       : Enable inter block search 8x4
+ *  b4x8       : Enable inter block search 4x8
+ *  b4x4       : Enable inter block search 4x4
+ */
+typedef struct OMX_VIDEO_PARAM_VBSMCTYPE {
+    OMX_U32 nSize;
+    OMX_VERSIONTYPE nVersion;
+    OMX_U32 nPortIndex;
+    OMX_BOOL b16x16;
+    OMX_BOOL b16x8;
+    OMX_BOOL b8x16;
+    OMX_BOOL b8x8;
+    OMX_BOOL b8x4;
+    OMX_BOOL b4x8;
+    OMX_BOOL b4x4;
+} OMX_VIDEO_PARAM_VBSMCTYPE;
+
+
+/**
+ * H.263 profile types, each profile indicates support for various
+ * performance bounds and different annexes.
+ *
+ * ENUMS:
+ *  Baseline           : Baseline Profile: H.263 (V1), no optional modes
+ *  H320 Coding        : H.320 Coding Efficiency Backward Compatibility
+ *                       Profile: H.263+ (V2), includes annexes I, J, L.4
+ *                       and T
+ *  BackwardCompatible : Backward Compatibility Profile: H.263 (V1),
+ *                       includes annex F
+ *  ISWV2              : Interactive Streaming Wireless Profile: H.263+
+ *                       (V2), includes annexes I, J, K and T
+ *  ISWV3              : Interactive Streaming Wireless Profile: H.263++
+ *                       (V3), includes profile 3 and annexes V and W.6.3.8
+ *  HighCompression    : Conversational High Compression Profile: H.263++
+ *                       (V3), includes profiles 1 & 2 and annexes D and U
+ *  Internet           : Conversational Internet Profile: H.263++ (V3),
+ *                       includes profile 5 and annex K
+ *  Interlace          : Conversational Interlace Profile: H.263++ (V3),
+ *                       includes profile 5 and annex W.6.3.11
+ *  HighLatency        : High Latency Profile: H.263++ (V3), includes
+ *                       profile 6 and annexes O.1 and P.5
+ */
+typedef enum OMX_VIDEO_H263PROFILETYPE {
+    OMX_VIDEO_H263ProfileBaseline            = 0x01,
+    OMX_VIDEO_H263ProfileH320Coding          = 0x02,
+    OMX_VIDEO_H263ProfileBackwardCompatible  = 0x04,
+    OMX_VIDEO_H263ProfileISWV2               = 0x08,
+    OMX_VIDEO_H263ProfileISWV3               = 0x10,
+    OMX_VIDEO_H263ProfileHighCompression     = 0x20,
+    OMX_VIDEO_H263ProfileInternet            = 0x40,
+    OMX_VIDEO_H263ProfileInterlace           = 0x80,
+    OMX_VIDEO_H263ProfileHighLatency         = 0x100,
+    OMX_VIDEO_H263ProfileKhronosExtensions = 0x6F000000, /**< Reserved region for introducing Khronos Standard Extensions */
+    OMX_VIDEO_H263ProfileVendorStartUnused = 0x7F000000, /**< Reserved region for introducing Vendor Extensions */
+    OMX_VIDEO_H263ProfileMax                 = 0x7FFFFFFF
+} OMX_VIDEO_H263PROFILETYPE;
+
+
+/**
+ * H.263 level types, each level indicates support for various frame sizes,
+ * bit rates, decoder frame rates.
+ */
+typedef enum OMX_VIDEO_H263LEVELTYPE {
+    OMX_VIDEO_H263Level10  = 0x01,
+    OMX_VIDEO_H263Level20  = 0x02,
+    OMX_VIDEO_H263Level30  = 0x04,
+    OMX_VIDEO_H263Level40  = 0x08,
+    OMX_VIDEO_H263Level45  = 0x10,
+    OMX_VIDEO_H263Level50  = 0x20,
+    OMX_VIDEO_H263Level60  = 0x40,
+    OMX_VIDEO_H263Level70  = 0x80,
+    OMX_VIDEO_H263LevelKhronosExtensions = 0x6F000000, /**< Reserved region for introducing Khronos Standard Extensions */
+    OMX_VIDEO_H263LevelVendorStartUnused = 0x7F000000, /**< Reserved region for introducing Vendor Extensions */
+    OMX_VIDEO_H263LevelMax = 0x7FFFFFFF
+} OMX_VIDEO_H263LEVELTYPE;
+
+
+/**
+ * Specifies the picture type. These values should be OR'd to signal all
+ * pictures types which are allowed.
+ *
+ * ENUMS:
+ *  Generic Picture Types:          I, P and B
+ *  H.263 Specific Picture Types:   SI and SP
+ *  H.264 Specific Picture Types:   EI and EP
+ *  MPEG-4 Specific Picture Types:  S
+ */
+typedef enum OMX_VIDEO_PICTURETYPE {
+    OMX_VIDEO_PictureTypeI   = 0x01,
+    OMX_VIDEO_PictureTypeP   = 0x02,
+    OMX_VIDEO_PictureTypeB   = 0x04,
+    OMX_VIDEO_PictureTypeSI  = 0x08,
+    OMX_VIDEO_PictureTypeSP  = 0x10,
+    OMX_VIDEO_PictureTypeEI  = 0x11,
+    OMX_VIDEO_PictureTypeEP  = 0x12,
+    OMX_VIDEO_PictureTypeS   = 0x14,
+    OMX_VIDEO_PictureTypeKhronosExtensions = 0x6F000000, /**< Reserved region for introducing Khronos Standard Extensions */
+    OMX_VIDEO_PictureTypeVendorStartUnused = 0x7F000000, /**< Reserved region for introducing Vendor Extensions */
+    OMX_VIDEO_PictureTypeMax = 0x7FFFFFFF
+} OMX_VIDEO_PICTURETYPE;
+
+
+/**
+ * H.263 Params
+ *
+ * STRUCT MEMBERS:
+ *  nSize                    : Size of the structure in bytes
+ *  nVersion                 : OMX specification version information
+ *  nPortIndex               : Port that this structure applies to
+ *  nPFrames                 : Number of P frames between each I frame
+ *  nBFrames                 : Number of B frames between each I frame
+ *  eProfile                 : H.263 profile(s) to use
+ *  eLevel                   : H.263 level(s) to use
+ *  bPLUSPTYPEAllowed        : Indicating that it is allowed to use PLUSPTYPE
+ *                             (specified in the 1998 version of H.263) to
+ *                             indicate custom picture sizes or clock
+ *                             frequencies
+ *  nAllowedPictureTypes     : Specifies the picture types allowed in the
+ *                             bitstream
+ *  bForceRoundingTypeToZero : value of the RTYPE bit (bit 6 of MPPTYPE) is
+ *                             not constrained. It is recommended to change
+ *                             the value of the RTYPE bit for each reference
+ *                             picture in error-free communication
+ *  nPictureHeaderRepetition : Specifies the frequency of picture header
+ *                             repetition
+ *  nGOBHeaderInterval       : Specifies the interval of non-empty GOB
+ *                             headers in units of GOBs
+ */
+typedef struct OMX_VIDEO_PARAM_H263TYPE {
+    OMX_U32 nSize;
+    OMX_VERSIONTYPE nVersion;
+    OMX_U32 nPortIndex;
+    OMX_U32 nPFrames;
+    OMX_U32 nBFrames;
+    OMX_VIDEO_H263PROFILETYPE eProfile;
+    OMX_VIDEO_H263LEVELTYPE eLevel;
+    OMX_BOOL bPLUSPTYPEAllowed;
+    OMX_U32 nAllowedPictureTypes;
+    OMX_BOOL bForceRoundingTypeToZero;
+    OMX_U32 nPictureHeaderRepetition;
+    OMX_U32 nGOBHeaderInterval;
+} OMX_VIDEO_PARAM_H263TYPE;
+
+
+/**
+ * MPEG-2 profile types, each profile indicates support for various
+ * performance bounds and different annexes.
+ */
+typedef enum OMX_VIDEO_MPEG2PROFILETYPE {
+    OMX_VIDEO_MPEG2ProfileSimple = 0,  /**< Simple Profile */
+    OMX_VIDEO_MPEG2ProfileMain,        /**< Main Profile */
+    OMX_VIDEO_MPEG2Profile422,         /**< 4:2:2 Profile */
+    OMX_VIDEO_MPEG2ProfileSNR,         /**< SNR Profile */
+    OMX_VIDEO_MPEG2ProfileSpatial,     /**< Spatial Profile */
+    OMX_VIDEO_MPEG2ProfileHigh,        /**< High Profile */
+    OMX_VIDEO_MPEG2ProfileKhronosExtensions = 0x6F000000, /**< Reserved region for introducing Khronos Standard Extensions */
+    OMX_VIDEO_MPEG2ProfileVendorStartUnused = 0x7F000000, /**< Reserved region for introducing Vendor Extensions */
+    OMX_VIDEO_MPEG2ProfileMax = 0x7FFFFFFF
+} OMX_VIDEO_MPEG2PROFILETYPE;
+
+
+/**
+ * MPEG-2 level types, each level indicates support for various frame
+ * sizes, bit rates, decoder frame rates.  No need
+ */
+typedef enum OMX_VIDEO_MPEG2LEVELTYPE {
+    OMX_VIDEO_MPEG2LevelLL = 0,  /**< Low Level */
+    OMX_VIDEO_MPEG2LevelML,      /**< Main Level */
+    OMX_VIDEO_MPEG2LevelH14,     /**< High 1440 */
+    OMX_VIDEO_MPEG2LevelHL,      /**< High Level */
+    OMX_VIDEO_MPEG2LevelKhronosExtensions = 0x6F000000, /**< Reserved region for introducing Khronos Standard Extensions */
+    OMX_VIDEO_MPEG2LevelVendorStartUnused = 0x7F000000, /**< Reserved region for introducing Vendor Extensions */
+    OMX_VIDEO_MPEG2LevelMax = 0x7FFFFFFF
+} OMX_VIDEO_MPEG2LEVELTYPE;
+
+
+/**
+ * MPEG-2 params
+ *
+ * STRUCT MEMBERS:
+ *  nSize      : Size of the structure in bytes
+ *  nVersion   : OMX specification version information
+ *  nPortIndex : Port that this structure applies to
+ *  nPFrames   : Number of P frames between each I frame
+ *  nBFrames   : Number of B frames between each I frame
+ *  eProfile   : MPEG-2 profile(s) to use
+ *  eLevel     : MPEG-2 levels(s) to use
+ */
+typedef struct OMX_VIDEO_PARAM_MPEG2TYPE {
+    OMX_U32 nSize;
+    OMX_VERSIONTYPE nVersion;
+    OMX_U32 nPortIndex;
+    OMX_U32 nPFrames;
+    OMX_U32 nBFrames;
+    OMX_VIDEO_MPEG2PROFILETYPE eProfile;
+    OMX_VIDEO_MPEG2LEVELTYPE eLevel;
+} OMX_VIDEO_PARAM_MPEG2TYPE;
+
+
+/**
+ * MPEG-4 profile types, each profile indicates support for various
+ * performance bounds and different annexes.
+ *
+ * ENUMS:
+ *  - Simple Profile, Levels 1-3
+ *  - Simple Scalable Profile, Levels 1-2
+ *  - Core Profile, Levels 1-2
+ *  - Main Profile, Levels 2-4
+ *  - N-bit Profile, Level 2
+ *  - Scalable Texture Profile, Level 1
+ *  - Simple Face Animation Profile, Levels 1-2
+ *  - Simple Face and Body Animation (FBA) Profile, Levels 1-2
+ *  - Basic Animated Texture Profile, Levels 1-2
+ *  - Hybrid Profile, Levels 1-2
+ *  - Advanced Real Time Simple Profiles, Levels 1-4
+ *  - Core Scalable Profile, Levels 1-3
+ *  - Advanced Coding Efficiency Profile, Levels 1-4
+ *  - Advanced Core Profile, Levels 1-2
+ *  - Advanced Scalable Texture, Levels 2-3
+ */
+typedef enum OMX_VIDEO_MPEG4PROFILETYPE {
+    OMX_VIDEO_MPEG4ProfileSimple           = 0x01,
+    OMX_VIDEO_MPEG4ProfileSimpleScalable   = 0x02,
+    OMX_VIDEO_MPEG4ProfileCore             = 0x04,
+    OMX_VIDEO_MPEG4ProfileMain             = 0x08,
+    OMX_VIDEO_MPEG4ProfileNbit             = 0x10,
+    OMX_VIDEO_MPEG4ProfileScalableTexture  = 0x20,
+    OMX_VIDEO_MPEG4ProfileSimpleFace       = 0x40,
+    OMX_VIDEO_MPEG4ProfileSimpleFBA        = 0x80,
+    OMX_VIDEO_MPEG4ProfileBasicAnimated    = 0x100,
+    OMX_VIDEO_MPEG4ProfileHybrid           = 0x200,
+    OMX_VIDEO_MPEG4ProfileAdvancedRealTime = 0x400,
+    OMX_VIDEO_MPEG4ProfileCoreScalable     = 0x800,
+    OMX_VIDEO_MPEG4ProfileAdvancedCoding   = 0x1000,
+    OMX_VIDEO_MPEG4ProfileAdvancedCore     = 0x2000,
+    OMX_VIDEO_MPEG4ProfileAdvancedScalable = 0x4000,
+    OMX_VIDEO_MPEG4ProfileAdvancedSimple   = 0x8000,
+    OMX_VIDEO_MPEG4ProfileKhronosExtensions = 0x6F000000, /**< Reserved region for introducing Khronos Standard Extensions */
+    OMX_VIDEO_MPEG4ProfileVendorStartUnused = 0x7F000000, /**< Reserved region for introducing Vendor Extensions */
+    OMX_VIDEO_MPEG4ProfileMax              = 0x7FFFFFFF
+} OMX_VIDEO_MPEG4PROFILETYPE;
+
+
+/**
+ * MPEG-4 level types, each level indicates support for various frame
+ * sizes, bit rates, decoder frame rates.  No need
+ */
+typedef enum OMX_VIDEO_MPEG4LEVELTYPE {
+    OMX_VIDEO_MPEG4Level0  = 0x01,   /**< Level 0 */
+    OMX_VIDEO_MPEG4Level0b = 0x02,   /**< Level 0b */
+    OMX_VIDEO_MPEG4Level1  = 0x04,   /**< Level 1 */
+    OMX_VIDEO_MPEG4Level2  = 0x08,   /**< Level 2 */
+    OMX_VIDEO_MPEG4Level3  = 0x10,   /**< Level 3 */
+    OMX_VIDEO_MPEG4Level4  = 0x20,   /**< Level 4 */
+    OMX_VIDEO_MPEG4Level4a = 0x40,   /**< Level 4a */
+    OMX_VIDEO_MPEG4Level5  = 0x80,   /**< Level 5 */
+    OMX_VIDEO_MPEG4LevelKhronosExtensions = 0x6F000000, /**< Reserved region for introducing Khronos Standard Extensions */
+    OMX_VIDEO_MPEG4LevelVendorStartUnused = 0x7F000000, /**< Reserved region for introducing Vendor Extensions */
+    OMX_VIDEO_MPEG4LevelMax = 0x7FFFFFFF
+} OMX_VIDEO_MPEG4LEVELTYPE;
+
+
+/**
+ * MPEG-4 configuration.  This structure handles configuration options
+ * which are specific to MPEG4 algorithms
+ *
+ * STRUCT MEMBERS:
+ *  nSize                : Size of the structure in bytes
+ *  nVersion             : OMX specification version information
+ *  nPortIndex           : Port that this structure applies to
+ *  nSliceHeaderSpacing  : Number of macroblocks between slice header (H263+
+ *                         Annex K). Put zero if not used
+ *  bSVH                 : Enable Short Video Header mode
+ *  bGov                 : Flag to enable GOV
+ *  nPFrames             : Number of P frames between each I frame (also called
+ *                         GOV period)
+ *  nBFrames             : Number of B frames between each I frame
+ *  nIDCVLCThreshold     : Value of intra DC VLC threshold
+ *  bACPred              : Flag to use ac prediction
+ *  nMaxPacketSize       : Maximum size of packet in bytes.
+ *  nTimeIncRes          : Used to pass VOP time increment resolution for MPEG4.
+ *                         Interpreted as described in MPEG4 standard.
+ *  eProfile             : MPEG-4 profile(s) to use.
+ *  eLevel               : MPEG-4 level(s) to use.
+ *  nAllowedPictureTypes : Specifies the picture types allowed in the bitstream
+ *  nHeaderExtension     : Specifies the number of consecutive video packet
+ *                         headers within a VOP
+ *  bReversibleVLC       : Specifies whether reversible variable length coding
+ *                         is in use
+ */
+typedef struct OMX_VIDEO_PARAM_MPEG4TYPE {
+    OMX_U32 nSize;
+    OMX_VERSIONTYPE nVersion;
+    OMX_U32 nPortIndex;
+    OMX_U32 nSliceHeaderSpacing;
+    OMX_BOOL bSVH;
+    OMX_BOOL bGov;
+    OMX_U32 nPFrames;
+    OMX_U32 nBFrames;
+    OMX_U32 nIDCVLCThreshold;
+    OMX_BOOL bACPred;
+    OMX_U32 nMaxPacketSize;
+    OMX_U32 nTimeIncRes;
+    OMX_VIDEO_MPEG4PROFILETYPE eProfile;
+    OMX_VIDEO_MPEG4LEVELTYPE eLevel;
+    OMX_U32 nAllowedPictureTypes;
+    OMX_U32 nHeaderExtension;
+    OMX_BOOL bReversibleVLC;
+} OMX_VIDEO_PARAM_MPEG4TYPE;
+
+
+/**
+ * WMV Versions
+ */
+typedef enum OMX_VIDEO_WMVFORMATTYPE {
+    OMX_VIDEO_WMVFormatUnused = 0x01,   /**< Format unused or unknown */
+    OMX_VIDEO_WMVFormat7      = 0x02,   /**< Windows Media Video format 7 */
+    OMX_VIDEO_WMVFormat8      = 0x04,   /**< Windows Media Video format 8 */
+    OMX_VIDEO_WMVFormat9      = 0x08,   /**< Windows Media Video format 9 */
+    OMX_VIDEO_WMFFormatKhronosExtensions = 0x6F000000, /**< Reserved region for introducing Khronos Standard Extensions */
+    OMX_VIDEO_WMFFormatVendorStartUnused = 0x7F000000, /**< Reserved region for introducing Vendor Extensions */
+    OMX_VIDEO_WMVFormatMax    = 0x7FFFFFFF
+} OMX_VIDEO_WMVFORMATTYPE;
+
+
+/**
+ * WMV Params
+ *
+ * STRUCT MEMBERS:
+ *  nSize      : Size of the structure in bytes
+ *  nVersion   : OMX specification version information
+ *  nPortIndex : Port that this structure applies to
+ *  eFormat    : Version of WMV stream / data
+ */
+typedef struct OMX_VIDEO_PARAM_WMVTYPE {
+    OMX_U32 nSize;
+    OMX_VERSIONTYPE nVersion;
+    OMX_U32 nPortIndex;
+    OMX_VIDEO_WMVFORMATTYPE eFormat;
+} OMX_VIDEO_PARAM_WMVTYPE;
+
+
+/**
+ * Real Video Version
+ */
+typedef enum OMX_VIDEO_RVFORMATTYPE {
+    OMX_VIDEO_RVFormatUnused = 0, /**< Format unused or unknown */
+    OMX_VIDEO_RVFormat8,          /**< Real Video format 8 */
+    OMX_VIDEO_RVFormat9,          /**< Real Video format 9 */
+    OMX_VIDEO_RVFormatG2,         /**< Real Video Format G2 */
+    OMX_VIDEO_RVFormatKhronosExtensions = 0x6F000000, /**< Reserved region for introducing Khronos Standard Extensions */
+    OMX_VIDEO_RVFormatVendorStartUnused = 0x7F000000, /**< Reserved region for introducing Vendor Extensions */
+    OMX_VIDEO_RVFormatMax = 0x7FFFFFFF
+} OMX_VIDEO_RVFORMATTYPE;
+
+
+/**
+ * Real Video Params
+ *
+ * STUCT MEMBERS:
+ *  nSize              : Size of the structure in bytes
+ *  nVersion           : OMX specification version information
+ *  nPortIndex         : Port that this structure applies to
+ *  eFormat            : Version of RV stream / data
+ *  nBitsPerPixel      : Bits per pixel coded in the frame
+ *  nPaddedWidth       : Padded width in pixel of a video frame
+ *  nPaddedHeight      : Padded Height in pixels of a video frame
+ *  nFrameRate         : Rate of video in frames per second
+ *  nBitstreamFlags    : Flags which internal information about the bitstream
+ *  nBitstreamVersion  : Bitstream version
+ *  nMaxEncodeFrameSize: Max encoded frame size
+ *  bEnablePostFilter  : Turn on/off post filter
+ *  bEnableTemporalInterpolation : Turn on/off temporal interpolation
+ *  bEnableLatencyMode : When enabled, the decoder does not display a decoded
+ *                       frame until it has detected that no enhancement layer
+ *                       frames or dependent B frames will be coming. This
+ *                       detection usually occurs when a subsequent non-B
+ *                       frame is encountered
+ */
+typedef struct OMX_VIDEO_PARAM_RVTYPE {
+    OMX_U32 nSize;
+    OMX_VERSIONTYPE nVersion;
+    OMX_U32 nPortIndex;
+    OMX_VIDEO_RVFORMATTYPE eFormat;
+    OMX_U16 nBitsPerPixel;
+    OMX_U16 nPaddedWidth;
+    OMX_U16 nPaddedHeight;
+    OMX_U32 nFrameRate;
+    OMX_U32 nBitstreamFlags;
+    OMX_U32 nBitstreamVersion;
+    OMX_U32 nMaxEncodeFrameSize;
+    OMX_BOOL bEnablePostFilter;
+    OMX_BOOL bEnableTemporalInterpolation;
+    OMX_BOOL bEnableLatencyMode;
+} OMX_VIDEO_PARAM_RVTYPE;
+
+
+/**
+ * AVC profile types, each profile indicates support for various
+ * performance bounds and different annexes.
+ */
+typedef enum OMX_VIDEO_AVCPROFILETYPE {
+    OMX_VIDEO_AVCProfileBaseline = 0x01,   /**< Baseline profile */
+    OMX_VIDEO_AVCProfileMain     = 0x02,   /**< Main profile */
+    OMX_VIDEO_AVCProfileExtended = 0x04,   /**< Extended profile */
+    OMX_VIDEO_AVCProfileHigh     = 0x08,   /**< High profile */
+    OMX_VIDEO_AVCProfileHigh10   = 0x10,   /**< High 10 profile */
+    OMX_VIDEO_AVCProfileHigh422  = 0x20,   /**< High 4:2:2 profile */
+    OMX_VIDEO_AVCProfileHigh444  = 0x40,   /**< High 4:4:4 profile */
+    OMX_VIDEO_AVCProfileKhronosExtensions = 0x6F000000, /**< Reserved region for introducing Khronos Standard Extensions */
+    OMX_VIDEO_AVCProfileVendorStartUnused = 0x7F000000, /**< Reserved region for introducing Vendor Extensions */
+    OMX_VIDEO_AVCProfileMax      = 0x7FFFFFFF
+} OMX_VIDEO_AVCPROFILETYPE;
+
+
+/**
+ * AVC level types, each level indicates support for various frame sizes,
+ * bit rates, decoder frame rates.  No need
+ */
+typedef enum OMX_VIDEO_AVCLEVELTYPE {
+    OMX_VIDEO_AVCLevel1   = 0x01,     /**< Level 1 */
+    OMX_VIDEO_AVCLevel1b  = 0x02,     /**< Level 1b */
+    OMX_VIDEO_AVCLevel11  = 0x04,     /**< Level 1.1 */
+    OMX_VIDEO_AVCLevel12  = 0x08,     /**< Level 1.2 */
+    OMX_VIDEO_AVCLevel13  = 0x10,     /**< Level 1.3 */
+    OMX_VIDEO_AVCLevel2   = 0x20,     /**< Level 2 */
+    OMX_VIDEO_AVCLevel21  = 0x40,     /**< Level 2.1 */
+    OMX_VIDEO_AVCLevel22  = 0x80,     /**< Level 2.2 */
+    OMX_VIDEO_AVCLevel3   = 0x100,    /**< Level 3 */
+    OMX_VIDEO_AVCLevel31  = 0x200,    /**< Level 3.1 */
+    OMX_VIDEO_AVCLevel32  = 0x400,    /**< Level 3.2 */
+    OMX_VIDEO_AVCLevel4   = 0x800,    /**< Level 4 */
+    OMX_VIDEO_AVCLevel41  = 0x1000,   /**< Level 4.1 */
+    OMX_VIDEO_AVCLevel42  = 0x2000,   /**< Level 4.2 */
+    OMX_VIDEO_AVCLevel5   = 0x4000,   /**< Level 5 */
+    OMX_VIDEO_AVCLevel51  = 0x8000,   /**< Level 5.1 */
+    OMX_VIDEO_AVCLevel52  = 0x10000,  /**< Level 5.2 */
+    OMX_VIDEO_AVCLevelKhronosExtensions = 0x6F000000, /**< Reserved region for introducing Khronos Standard Extensions */
+    OMX_VIDEO_AVCLevelVendorStartUnused = 0x7F000000, /**< Reserved region for introducing Vendor Extensions */
+    OMX_VIDEO_AVCLevelMax = 0x7FFFFFFF
+} OMX_VIDEO_AVCLEVELTYPE;
+
+
+/**
+ * AVC loop filter modes
+ *
+ * OMX_VIDEO_AVCLoopFilterEnable               : Enable
+ * OMX_VIDEO_AVCLoopFilterDisable              : Disable
+ * OMX_VIDEO_AVCLoopFilterDisableSliceBoundary : Disabled on slice boundaries
+ */
+typedef enum OMX_VIDEO_AVCLOOPFILTERTYPE {
+    OMX_VIDEO_AVCLoopFilterEnable = 0,
+    OMX_VIDEO_AVCLoopFilterDisable,
+    OMX_VIDEO_AVCLoopFilterDisableSliceBoundary,
+    OMX_VIDEO_AVCLoopFilterKhronosExtensions = 0x6F000000, /**< Reserved region for introducing Khronos Standard Extensions */
+    OMX_VIDEO_AVCLoopFilterVendorStartUnused = 0x7F000000, /**< Reserved region for introducing Vendor Extensions */
+    OMX_VIDEO_AVCLoopFilterMax = 0x7FFFFFFF
+} OMX_VIDEO_AVCLOOPFILTERTYPE;
+
+
+/**
+ * AVC params
+ *
+ * STRUCT MEMBERS:
+ *  nSize                     : Size of the structure in bytes
+ *  nVersion                  : OMX specification version information
+ *  nPortIndex                : Port that this structure applies to
+ *  nSliceHeaderSpacing       : Number of macroblocks between slice header, put
+ *                              zero if not used
+ *  nPFrames                  : Number of P frames between each I frame
+ *  nBFrames                  : Number of B frames between each I frame
+ *  bUseHadamard              : Enable/disable Hadamard transform
+ *  nRefFrames                : Max number of reference frames to use for inter
+ *                              motion search (1-16)
+ *  nRefIdxTrailing           : Pic param set ref frame index (index into ref
+ *                              frame buffer of trailing frames list), B frame
+ *                              support
+ *  nRefIdxForward            : Pic param set ref frame index (index into ref
+ *                              frame buffer of forward frames list), B frame
+ *                              support
+ *  bEnableUEP                : Enable/disable unequal error protection. This
+ *                              is only valid of data partitioning is enabled.
+ *  bEnableFMO                : Enable/disable flexible macroblock ordering
+ *  bEnableASO                : Enable/disable arbitrary slice ordering
+ *  bEnableRS                 : Enable/disable sending of redundant slices
+ *  eProfile                  : AVC profile(s) to use
+ *  eLevel                    : AVC level(s) to use
+ *  nAllowedPictureTypes      : Specifies the picture types allowed in the
+ *                              bitstream
+ *  bFrameMBsOnly             : specifies that every coded picture of the
+ *                              coded video sequence is a coded frame
+ *                              containing only frame macroblocks
+ *  bMBAFF                    : Enable/disable switching between frame and
+ *                              field macroblocks within a picture
+ *  bEntropyCodingCABAC       : Entropy decoding method to be applied for the
+ *                              syntax elements for which two descriptors appear
+ *                              in the syntax tables
+ *  bWeightedPPrediction      : Enable/disable weighted prediction shall not
+ *                              be applied to P and SP slices
+ *  nWeightedBipredicitonMode : Default weighted prediction is applied to B
+ *                              slices
+ *  bconstIpred               : Enable/disable intra prediction
+ *  bDirect8x8Inference       : Specifies the method used in the derivation
+ *                              process for luma motion vectors for B_Skip,
+ *                              B_Direct_16x16 and B_Direct_8x8 as specified
+ *                              in subclause 8.4.1.2 of the AVC spec
+ *  bDirectSpatialTemporal    : Flag indicating spatial or temporal direct
+ *                              mode used in B slice coding (related to
+ *                              bDirect8x8Inference) . Spatial direct mode is
+ *                              more common and should be the default.
+ *  nCabacInitIdx             : Index used to init CABAC contexts
+ *  eLoopFilterMode           : Enable/disable loop filter
+ */
+typedef struct OMX_VIDEO_PARAM_AVCTYPE {
+    OMX_U32 nSize;
+    OMX_VERSIONTYPE nVersion;
+    OMX_U32 nPortIndex;
+    OMX_U32 nSliceHeaderSpacing;
+    OMX_U32 nPFrames;
+    OMX_U32 nBFrames;
+    OMX_BOOL bUseHadamard;
+    OMX_U32 nRefFrames;
+    OMX_U32 nRefIdx10ActiveMinus1;
+    OMX_U32 nRefIdx11ActiveMinus1;
+    OMX_BOOL bEnableUEP;
+    OMX_BOOL bEnableFMO;
+    OMX_BOOL bEnableASO;
+    OMX_BOOL bEnableRS;
+    OMX_VIDEO_AVCPROFILETYPE eProfile;
+    OMX_VIDEO_AVCLEVELTYPE eLevel;
+    OMX_U32 nAllowedPictureTypes;
+    OMX_BOOL bFrameMBsOnly;
+    OMX_BOOL bMBAFF;
+    OMX_BOOL bEntropyCodingCABAC;
+    OMX_BOOL bWeightedPPrediction;
+    OMX_U32 nWeightedBipredicitonMode;
+    OMX_BOOL bconstIpred ;
+    OMX_BOOL bDirect8x8Inference;
+    OMX_BOOL bDirectSpatialTemporal;
+    OMX_U32 nCabacInitIdc;
+    OMX_VIDEO_AVCLOOPFILTERTYPE eLoopFilterMode;
+} OMX_VIDEO_PARAM_AVCTYPE;
+
+typedef struct OMX_VIDEO_PARAM_PROFILELEVELTYPE {
+    OMX_U32 nSize;
+    OMX_VERSIONTYPE nVersion;
+    OMX_U32 nPortIndex;
+    OMX_U32 eProfile;      /**< type is OMX_VIDEO_AVCPROFILETYPE, OMX_VIDEO_H263PROFILETYPE,
+                                 or OMX_VIDEO_MPEG4PROFILETYPE depending on context */
+    OMX_U32 eLevel;        /**< type is OMX_VIDEO_AVCLEVELTYPE, OMX_VIDEO_H263LEVELTYPE,
+                                 or OMX_VIDEO_MPEG4PROFILETYPE depending on context */
+    OMX_U32 nProfileIndex; /**< Used to query for individual profile support information,
+                               This parameter is valid only for
+                               OMX_IndexParamVideoProfileLevelQuerySupported index,
+                               For all other indices this parameter is to be ignored. */
+} OMX_VIDEO_PARAM_PROFILELEVELTYPE;
+
+/**
+ * Structure for dynamically configuring bitrate mode of a codec.
+ *
+ * STRUCT MEMBERS:
+ *  nSize          : Size of the struct in bytes
+ *  nVersion       : OMX spec version info
+ *  nPortIndex     : Port that this struct applies to
+ *  nEncodeBitrate : Target average bitrate to be generated in bps
+ */
+typedef struct OMX_VIDEO_CONFIG_BITRATETYPE {
+    OMX_U32 nSize;
+    OMX_VERSIONTYPE nVersion;
+    OMX_U32 nPortIndex;
+    OMX_U32 nEncodeBitrate;
+} OMX_VIDEO_CONFIG_BITRATETYPE;
+
+/**
+ * Defines Encoder Frame Rate setting
+ *
+ * STRUCT MEMBERS:
+ *  nSize            : Size of the structure in bytes
+ *  nVersion         : OMX specification version information
+ *  nPortIndex       : Port that this structure applies to
+ *  xEncodeFramerate : Encoding framerate represented in Q16 format
+ */
+typedef struct OMX_CONFIG_FRAMERATETYPE {
+    OMX_U32 nSize;
+    OMX_VERSIONTYPE nVersion;
+    OMX_U32 nPortIndex;
+    OMX_U32 xEncodeFramerate; /* Q16 format */
+} OMX_CONFIG_FRAMERATETYPE;
+
+typedef struct OMX_CONFIG_INTRAREFRESHVOPTYPE {
+    OMX_U32 nSize;
+    OMX_VERSIONTYPE nVersion;
+    OMX_U32 nPortIndex;
+    OMX_BOOL IntraRefreshVOP;
+} OMX_CONFIG_INTRAREFRESHVOPTYPE;
+
+typedef struct OMX_CONFIG_MACROBLOCKERRORMAPTYPE {
+    OMX_U32 nSize;
+    OMX_VERSIONTYPE nVersion;
+    OMX_U32 nPortIndex;
+    OMX_U32 nErrMapSize;           /* Size of the Error Map in bytes */
+    OMX_U8  ErrMap[1];             /* Error map hint */
+} OMX_CONFIG_MACROBLOCKERRORMAPTYPE;
+
+typedef struct OMX_CONFIG_MBERRORREPORTINGTYPE {
+    OMX_U32 nSize;
+    OMX_VERSIONTYPE nVersion;
+    OMX_U32 nPortIndex;
+    OMX_BOOL bEnabled;
+} OMX_CONFIG_MBERRORREPORTINGTYPE;
+
+typedef struct OMX_PARAM_MACROBLOCKSTYPE {
+    OMX_U32 nSize;
+    OMX_VERSIONTYPE nVersion;
+    OMX_U32 nPortIndex;
+    OMX_U32 nMacroblocks;
+} OMX_PARAM_MACROBLOCKSTYPE;
+
+
+#ifdef AVS80
+/**
+ * Aspects of color.
+ */
+
+// NOTE: this structure is expected to grow in the future if new color aspects are
+// added to codec bitstreams. OMX component should not require a specific nSize
+// though could verify that nSize is at least the size of the structure at the
+// time of implementation. All new fields will be added at the end of the structure
+// ensuring backward compatibility.
+
+typedef enum OMX_RANGE {
+    RangeUnspecified,
+    RangeFull,
+    RangeLimited,
+    RangeOther = 0xff,
+} OMX_RANGE;
+
+typedef enum OMX_PRIMARIES {
+    PrimariesUnspecified,
+    PrimariesBT709_5,		// Rec.ITU-R BT.709-5 or equivalent
+    PrimariesBT470_6M,		// Rec.ITU-R BT.470-6 System M or equivalent
+    PrimariesBT601_6_625,	// Rec.ITU-R BT.601-6 625 or equivalent
+    PrimariesBT601_6_525,	// Rec.ITU-R BT.601-6 525 or equivalent
+    PrimariesGenericFilm,	// Generic Film
+    PrimariesBT2020,		// Rec.ITU-R BT.2020 or equivalent
+    PrimariesOther = 0xff,
+} OMX_PRIMARIES;
+
+typedef enum OMX_TRANSFER {
+    TransferUnspecified,
+    TransferLinear, 		// Linear transfer characteristics
+    TransferSRGB,			// sRGB or equivalent
+    TransferSMPTE170M,		// SMPTE 170M or equivalent (e.g. BT.601/709/2020)
+    TransferGamma22,		// Assumed display gamma 2.2
+    TransferGamma28,		// Assumed display gamma 2.8
+    TransferST2084, 		// SMPTE ST 2084 for 10/12/14/16 bit systems
+    TransferHLG,			// ARIB STD-B67 hybrid-log-gamma
+    // transfers unlikely to be required by Android
+    TransferSMPTE240M = 0x40, // SMPTE 240M
+    TransferXvYCC,			// IEC 61966-2-4
+    TransferBT1361, 		// Rec.ITU-R BT.1361 extended gamut
+    TransferST428,			// SMPTE ST 428-1
+    TransferOther = 0xff,
+} OMX_TRANSFER;
+
+typedef enum OMX_MATRIXCOEFFS {
+    MatrixUnspecified,
+    MatrixBT709_5,			// Rec.ITU-R BT.709-5 or equivalent
+    MatrixBT470_6M, 		// KR=0.30, KB=0.11 or equivalent
+    MatrixBT601_6,			// Rec.ITU-R BT.601-6 625 or equivalent
+    MatrixSMPTE240M,		// SMPTE 240M or equivalent
+    MatrixBT2020,			// Rec.ITU-R BT.2020 non-constant luminance
+    MatrixBT2020Constant,	// Rec.ITU-R BT.2020 constant luminance
+    MatrixOther = 0xff,
+} OMX_MATRIXCOEFFS;
+
+typedef struct OMX_COLORASPECTS {
+    OMX_RANGE mRange;                // IN/OUT
+    OMX_PRIMARIES mPrimaries;        // IN/OUT
+    OMX_TRANSFER mTransfer;          // IN/OUT
+    OMX_MATRIXCOEFFS mMatrixCoeffs;  // IN/OUT
+} OMX_COLORASPECTS;
+
+typedef struct OMX_CONFIG_DESCRIBECOLORASPECTSPARAMS {
+    OMX_U32  nSize;                // IN
+    OMX_VERSIONTYPE nVersion;      // IN
+    OMX_U32  nPortIndex;           // IN
+    OMX_BOOL bRequestingDataSpace; // IN
+    OMX_BOOL bDataSpaceChanged;    // IN
+    OMX_U32  nPixelFormat;         // IN
+    OMX_U32  nDataSpace;           // OUT
+    OMX_COLORASPECTS sAspects;  // IN/OUT
+} OMX_CONFIG_DESCRIBECOLORASPECTSPARAMS;
+#endif
+
+/**
+ * AVC Slice Mode modes
+ *
+ * OMX_VIDEO_SLICEMODE_AVCDefault   : Normal frame encoding, one slice per frame
+ * OMX_VIDEO_SLICEMODE_AVCMBSlice   : NAL mode, number of MBs per frame
+ * OMX_VIDEO_SLICEMODE_AVCByteSlice : NAL mode, number of bytes per frame
+ */
+typedef enum OMX_VIDEO_AVCSLICEMODETYPE {
+    OMX_VIDEO_SLICEMODE_AVCDefault = 0,
+    OMX_VIDEO_SLICEMODE_AVCMBSlice,
+    OMX_VIDEO_SLICEMODE_AVCByteSlice,
+    OMX_VIDEO_SLICEMODE_AVCKhronosExtensions = 0x6F000000, /**< Reserved region for introducing Khronos Standard Extensions */
+    OMX_VIDEO_SLICEMODE_AVCVendorStartUnused = 0x7F000000, /**< Reserved region for introducing Vendor Extensions */
+    OMX_VIDEO_SLICEMODE_AVCLevelMax = 0x7FFFFFFF
+} OMX_VIDEO_AVCSLICEMODETYPE;
+
+/**
+ * AVC FMO Slice Mode Params
+ *
+ * STRUCT MEMBERS:
+ *  nSize      : Size of the structure in bytes
+ *  nVersion   : OMX specification version information
+ *  nPortIndex : Port that this structure applies to
+ *  nNumSliceGroups : Specifies the number of slice groups
+ *  nSliceGroupMapType : Specifies the type of slice groups
+ *  eSliceMode : Specifies the type of slice
+ */
+typedef struct OMX_VIDEO_PARAM_AVCSLICEFMO {
+    OMX_U32 nSize;
+    OMX_VERSIONTYPE nVersion;
+    OMX_U32 nPortIndex;
+    OMX_U8 nNumSliceGroups;
+    OMX_U8 nSliceGroupMapType;
+    OMX_VIDEO_AVCSLICEMODETYPE eSliceMode;
+} OMX_VIDEO_PARAM_AVCSLICEFMO;
+
+/**
+ * AVC IDR Period Configs
+ *
+ * STRUCT MEMBERS:
+ *  nSize      : Size of the structure in bytes
+ *  nVersion   : OMX specification version information
+ *  nPortIndex : Port that this structure applies to
+ *  nIDRPeriod : Specifies periodicity of IDR frames
+ *  nPFrames : Specifies internal of coding Intra frames
+ */
+typedef struct OMX_VIDEO_CONFIG_AVCINTRAPERIOD {
+    OMX_U32 nSize;
+    OMX_VERSIONTYPE nVersion;
+    OMX_U32 nPortIndex;
+    OMX_U32 nIDRPeriod;
+    OMX_U32 nPFrames;
+} OMX_VIDEO_CONFIG_AVCINTRAPERIOD;
+
+/**
+ * AVC NAL Size Configs
+ *
+ * STRUCT MEMBERS:
+ *  nSize      : Size of the structure in bytes
+ *  nVersion   : OMX specification version information
+ *  nPortIndex : Port that this structure applies to
+ *  nNaluBytes : Specifies the NAL unit size
+ */
+typedef struct OMX_VIDEO_CONFIG_NALSIZE {
+    OMX_U32 nSize;
+    OMX_VERSIONTYPE nVersion;
+    OMX_U32 nPortIndex;
+    OMX_U32 nNaluBytes;
+} OMX_VIDEO_CONFIG_NALSIZE;
+
+/** @} */
+
+#ifdef __cplusplus
+}
+#endif /* __cplusplus */
+
+#endif
+/* File EOF */
+
diff --git a/sf-extra/omx-il/OMX_VideoExt.h b/sf-extra/omx-il/OMX_VideoExt.h
new file mode 100644
index 00000000..2c024317
--- /dev/null
+++ b/sf-extra/omx-il/OMX_VideoExt.h
@@ -0,0 +1,401 @@
+/*
+ * Copyright (c) 2010 The Khronos Group Inc.
+ *
+ * Permission is hereby granted, free of charge, to any person obtaining
+ * a copy of this software and associated documentation files (the
+ * "Software"), to deal in the Software without restriction, including
+ * without limitation the rights to use, copy, modify, merge, publish,
+ * distribute, sublicense, and/or sell copies of the Software, and to
+ * permit persons to whom the Software is furnished to do so, subject
+ * to the following conditions:
+ * The above copyright notice and this permission notice shall be included
+ * in all copies or substantial portions of the Software.
+ *
+ * THE SOFTWARE IS PROVIDED "AS IS", WITHOUT WARRANTY OF ANY KIND, EXPRESS
+ * OR IMPLIED, INCLUDING BUT NOT LIMITED TO THE WARRANTIES OF
+ * MERCHANTABILITY, FITNESS FOR A PARTICULAR PURPOSE AND NONINFRINGEMENT.
+ * IN NO EVENT SHALL THE AUTHORS OR COPYRIGHT HOLDERS BE LIABLE FOR ANY
+ * CLAIM, DAMAGES OR OTHER LIABILITY, WHETHER IN AN ACTION OF CONTRACT,
+ * TORT OR OTHERWISE, ARISING FROM, OUT OF OR IN CONNECTION WITH THE
+ * SOFTWARE OR THE USE OR OTHER DEALINGS IN THE SOFTWARE.
+ *
+ */
+
+/** OMX_VideoExt.h - OpenMax IL version 1.1.2
+ * The OMX_VideoExt header file contains extensions to the
+ * definitions used by both the application and the component to
+ * access video items.
+ */
+
+#ifndef OMX_VideoExt_h
+#define OMX_VideoExt_h
+
+#ifdef __cplusplus
+extern "C" {
+#endif /* __cplusplus */
+
+/* Each OMX header shall include all required header files to allow the
+ * header to compile without errors.  The includes below are required
+ * for this header file to compile successfully
+ */
+#include <OMX_Core.h>
+
+/** NALU Formats */
+typedef enum OMX_NALUFORMATSTYPE {
+    OMX_NaluFormatStartCodes = 1,
+    OMX_NaluFormatOneNaluPerBuffer = 2,
+    OMX_NaluFormatOneByteInterleaveLength = 4,
+    OMX_NaluFormatTwoByteInterleaveLength = 8,
+    OMX_NaluFormatFourByteInterleaveLength = 16,
+    OMX_NaluFormatCodingMax = 0x7FFFFFFF
+} OMX_NALUFORMATSTYPE;
+
+/** NAL Stream Format */
+typedef struct OMX_NALSTREAMFORMATTYPE{
+    OMX_U32 nSize;
+    OMX_VERSIONTYPE nVersion;
+    OMX_U32 nPortIndex;
+    OMX_NALUFORMATSTYPE eNaluFormat;
+} OMX_NALSTREAMFORMATTYPE;
+
+/** VP8 profiles */
+typedef enum OMX_VIDEO_VP8PROFILETYPE {
+    OMX_VIDEO_VP8ProfileMain = 0x01,
+    OMX_VIDEO_VP8ProfileUnknown = 0x6EFFFFFF,
+    OMX_VIDEO_VP8ProfileMax = 0x7FFFFFFF
+} OMX_VIDEO_VP8PROFILETYPE;
+
+/** VP8 levels */
+typedef enum OMX_VIDEO_VP8LEVELTYPE {
+    OMX_VIDEO_VP8Level_Version0 = 0x01,
+    OMX_VIDEO_VP8Level_Version1 = 0x02,
+    OMX_VIDEO_VP8Level_Version2 = 0x04,
+    OMX_VIDEO_VP8Level_Version3 = 0x08,
+    OMX_VIDEO_VP8LevelUnknown = 0x6EFFFFFF,
+    OMX_VIDEO_VP8LevelMax = 0x7FFFFFFF
+} OMX_VIDEO_VP8LEVELTYPE;
+
+/** VP9 profiles */
+typedef enum OMX_VIDEO_VP9PROFILETYPE {
+    OMX_VIDEO_VP9Profile0       = 0x1,
+    OMX_VIDEO_VP9Profile1       = 0x2,
+    OMX_VIDEO_VP9Profile2       = 0x4,
+    OMX_VIDEO_VP9Profile3       = 0x8,
+    // HDR profiles also support passing HDR metadata
+    OMX_VIDEO_VP9Profile2HDR    = 0x1000,
+    OMX_VIDEO_VP9Profile3HDR    = 0x2000,
+    OMX_VIDEO_VP9ProfileUnknown = 0x6EFFFFFF,
+    OMX_VIDEO_VP9ProfileMax     = 0x7FFFFFFF
+} OMX_VIDEO_VP9PROFILETYPE;
+
+/** VP9 levels */
+typedef enum OMX_VIDEO_VP9LEVELTYPE {
+    OMX_VIDEO_VP9Level1       = 0x1,
+    OMX_VIDEO_VP9Level11      = 0x2,
+    OMX_VIDEO_VP9Level2       = 0x4,
+    OMX_VIDEO_VP9Level21      = 0x8,
+    OMX_VIDEO_VP9Level3       = 0x10,
+    OMX_VIDEO_VP9Level31      = 0x20,
+    OMX_VIDEO_VP9Level4       = 0x40,
+    OMX_VIDEO_VP9Level41      = 0x80,
+    OMX_VIDEO_VP9Level5       = 0x100,
+    OMX_VIDEO_VP9Level51      = 0x200,
+    OMX_VIDEO_VP9Level52      = 0x400,
+    OMX_VIDEO_VP9Level6       = 0x800,
+    OMX_VIDEO_VP9Level61      = 0x1000,
+    OMX_VIDEO_VP9Level62      = 0x2000,
+    OMX_VIDEO_VP9LevelUnknown = 0x6EFFFFFF,
+    OMX_VIDEO_VP9LevelMax     = 0x7FFFFFFF
+} OMX_VIDEO_VP9LEVELTYPE;
+
+/** VP8 Param */
+typedef struct OMX_VIDEO_PARAM_VP8TYPE {
+    OMX_U32 nSize;
+    OMX_VERSIONTYPE nVersion;
+    OMX_U32 nPortIndex;
+    OMX_VIDEO_VP8PROFILETYPE eProfile;
+    OMX_VIDEO_VP8LEVELTYPE eLevel;
+    OMX_U32 nDCTPartitions;
+    OMX_BOOL bErrorResilientMode;
+} OMX_VIDEO_PARAM_VP8TYPE;
+
+/** Structure for configuring VP8 reference frames */
+typedef struct OMX_VIDEO_VP8REFERENCEFRAMETYPE {
+    OMX_U32 nSize;
+    OMX_VERSIONTYPE nVersion;
+    OMX_U32 nPortIndex;
+    OMX_BOOL bPreviousFrameRefresh;
+    OMX_BOOL bGoldenFrameRefresh;
+    OMX_BOOL bAlternateFrameRefresh;
+    OMX_BOOL bUsePreviousFrame;
+    OMX_BOOL bUseGoldenFrame;
+    OMX_BOOL bUseAlternateFrame;
+} OMX_VIDEO_VP8REFERENCEFRAMETYPE;
+
+/** Structure for querying VP8 reference frame type */
+typedef struct OMX_VIDEO_VP8REFERENCEFRAMEINFOTYPE {
+    OMX_U32 nSize;
+    OMX_VERSIONTYPE nVersion;
+    OMX_U32 nPortIndex;
+    OMX_BOOL bIsIntraFrame;
+    OMX_BOOL bIsGoldenOrAlternateFrame;
+} OMX_VIDEO_VP8REFERENCEFRAMEINFOTYPE;
+
+/** Maximum number of VP8 temporal layers */
+#define OMX_VIDEO_ANDROID_MAXVP8TEMPORALLAYERS 3
+
+/** VP8 temporal layer patterns */
+typedef enum OMX_VIDEO_ANDROID_VPXTEMPORALLAYERPATTERNTYPE {
+    OMX_VIDEO_VPXTemporalLayerPatternNone = 0,
+    OMX_VIDEO_VPXTemporalLayerPatternWebRTC = 1,
+    OMX_VIDEO_VPXTemporalLayerPatternMax = 0x7FFFFFFF
+} OMX_VIDEO_ANDROID_VPXTEMPORALLAYERPATTERNTYPE;
+
+/**
+ * Android specific VP8 encoder params
+ *
+ * STRUCT MEMBERS:
+ *  nSize                      : Size of the structure in bytes
+ *  nVersion                   : OMX specification version information
+ *  nPortIndex                 : Port that this structure applies to
+ *  nKeyFrameInterval          : Key frame interval in frames
+ *  eTemporalPattern           : Type of temporal layer pattern
+ *  nTemporalLayerCount        : Number of temporal coding layers
+ *  nTemporalLayerBitrateRatio : Bitrate ratio allocation between temporal
+ *                               streams in percentage
+ *  nMinQuantizer              : Minimum (best quality) quantizer
+ *  nMaxQuantizer              : Maximum (worst quality) quantizer
+ */
+typedef struct OMX_VIDEO_PARAM_ANDROID_VP8ENCODERTYPE {
+    OMX_U32 nSize;
+    OMX_VERSIONTYPE nVersion;
+    OMX_U32 nPortIndex;
+    OMX_U32 nKeyFrameInterval;        // distance between consecutive key_frames (including one
+                                      // of the key_frames). 0 means interval is unspecified and
+                                      // can be freely chosen by the codec. 1 means a stream of
+                                      // only key_frames.
+
+    OMX_VIDEO_ANDROID_VPXTEMPORALLAYERPATTERNTYPE eTemporalPattern;
+    OMX_U32 nTemporalLayerCount;
+    OMX_U32 nTemporalLayerBitrateRatio[OMX_VIDEO_ANDROID_MAXVP8TEMPORALLAYERS];
+    OMX_U32 nMinQuantizer;
+    OMX_U32 nMaxQuantizer;
+} OMX_VIDEO_PARAM_ANDROID_VP8ENCODERTYPE;
+
+/** HEVC Profile enum type */
+typedef enum OMX_VIDEO_HEVCPROFILETYPE {
+    OMX_VIDEO_HEVCProfileUnknown      = 0x0,
+    OMX_VIDEO_HEVCProfileMain         = 0x1,
+    OMX_VIDEO_HEVCProfileMain10       = 0x2,
+    // Main10 profile with HDR SEI support.
+    OMX_VIDEO_HEVCProfileMain10HDR10  = 0x1000,
+    OMX_VIDEO_HEVCProfileMax          = 0x7FFFFFFF
+} OMX_VIDEO_HEVCPROFILETYPE;
+
+/** HEVC Level enum type */
+typedef enum OMX_VIDEO_HEVCLEVELTYPE {
+    OMX_VIDEO_HEVCLevelUnknown    = 0x0,
+    OMX_VIDEO_HEVCMainTierLevel1  = 0x1,
+    OMX_VIDEO_HEVCHighTierLevel1  = 0x2,
+    OMX_VIDEO_HEVCMainTierLevel2  = 0x4,
+    OMX_VIDEO_HEVCHighTierLevel2  = 0x8,
+    OMX_VIDEO_HEVCMainTierLevel21 = 0x10,
+    OMX_VIDEO_HEVCHighTierLevel21 = 0x20,
+    OMX_VIDEO_HEVCMainTierLevel3  = 0x40,
+    OMX_VIDEO_HEVCHighTierLevel3  = 0x80,
+    OMX_VIDEO_HEVCMainTierLevel31 = 0x100,
+    OMX_VIDEO_HEVCHighTierLevel31 = 0x200,
+    OMX_VIDEO_HEVCMainTierLevel4  = 0x400,
+    OMX_VIDEO_HEVCHighTierLevel4  = 0x800,
+    OMX_VIDEO_HEVCMainTierLevel41 = 0x1000,
+    OMX_VIDEO_HEVCHighTierLevel41 = 0x2000,
+    OMX_VIDEO_HEVCMainTierLevel5  = 0x4000,
+    OMX_VIDEO_HEVCHighTierLevel5  = 0x8000,
+    OMX_VIDEO_HEVCMainTierLevel51 = 0x10000,
+    OMX_VIDEO_HEVCHighTierLevel51 = 0x20000,
+    OMX_VIDEO_HEVCMainTierLevel52 = 0x40000,
+    OMX_VIDEO_HEVCHighTierLevel52 = 0x80000,
+    OMX_VIDEO_HEVCMainTierLevel6  = 0x100000,
+    OMX_VIDEO_HEVCHighTierLevel6  = 0x200000,
+    OMX_VIDEO_HEVCMainTierLevel61 = 0x400000,
+    OMX_VIDEO_HEVCHighTierLevel61 = 0x800000,
+    OMX_VIDEO_HEVCMainTierLevel62 = 0x1000000,
+    OMX_VIDEO_HEVCHighTierLevel62 = 0x2000000,
+    OMX_VIDEO_HEVCHighTiermax     = 0x7FFFFFFF
+} OMX_VIDEO_HEVCLEVELTYPE;
+
+/** Structure for controlling HEVC video encoding */
+typedef struct OMX_VIDEO_PARAM_HEVCTYPE {
+    OMX_U32 nSize;
+    OMX_VERSIONTYPE nVersion;
+    OMX_U32 nPortIndex;
+    OMX_VIDEO_HEVCPROFILETYPE eProfile;
+    OMX_VIDEO_HEVCLEVELTYPE eLevel;
+    OMX_U32 nKeyFrameInterval;        // distance between consecutive I-frames (including one
+                                      // of the I frames). 0 means interval is unspecified and
+                                      // can be freely chosen by the codec. 1 means a stream of
+                                      // only I frames.
+} OMX_VIDEO_PARAM_HEVCTYPE;
+
+/** Structure to define if dependent slice segments should be used */
+typedef struct OMX_VIDEO_SLICESEGMENTSTYPE {
+    OMX_U32 nSize;
+    OMX_VERSIONTYPE nVersion;
+    OMX_U32 nPortIndex;
+    OMX_BOOL bDepedentSegments;
+    OMX_BOOL bEnableLoopFilterAcrossSlices;
+} OMX_VIDEO_SLICESEGMENTSTYPE;
+
+/** Structure to return timestamps of rendered output frames as well as EOS
+ *  for tunneled components.
+ */
+typedef struct OMX_VIDEO_RENDEREVENTTYPE {
+    OMX_S64 nMediaTimeUs;  // timestamp of rendered video frame
+    OMX_S64 nSystemTimeNs; // system monotonic time at the time frame was rendered
+                           // Use INT64_MAX for nMediaTimeUs to signal that the EOS
+                           // has been reached. In this case, nSystemTimeNs MUST be
+                           // the system time when the last frame was rendered.
+                           // This MUST be done in addition to returning (and
+                           // following) the render information for the last frame.
+} OMX_VIDEO_RENDEREVENTTYPE;
+
+/** Dolby Vision Profile enum type */
+typedef enum OMX_VIDEO_DOLBYVISIONPROFILETYPE {
+    OMX_VIDEO_DolbyVisionProfileUnknown = 0x0,
+    OMX_VIDEO_DolbyVisionProfileDvavPer = 0x1,
+    OMX_VIDEO_DolbyVisionProfileDvavPen = 0x2,
+    OMX_VIDEO_DolbyVisionProfileDvheDer = 0x4,
+    OMX_VIDEO_DolbyVisionProfileDvheDen = 0x8,
+    OMX_VIDEO_DolbyVisionProfileDvheDtr = 0x10,
+    OMX_VIDEO_DolbyVisionProfileDvheStn = 0x20,
+    OMX_VIDEO_DolbyVisionProfileDvheDth = 0x40,
+    OMX_VIDEO_DolbyVisionProfileDvheDtb = 0x80,
+    OMX_VIDEO_DolbyVisionProfileMax     = 0x7FFFFFFF
+} OMX_VIDEO_DOLBYVISIONPROFILETYPE;
+
+/** Dolby Vision Level enum type */
+typedef enum OMX_VIDEO_DOLBYVISIONLEVELTYPE {
+    OMX_VIDEO_DolbyVisionLevelUnknown = 0x0,
+    OMX_VIDEO_DolbyVisionLevelHd24    = 0x1,
+    OMX_VIDEO_DolbyVisionLevelHd30    = 0x2,
+    OMX_VIDEO_DolbyVisionLevelFhd24   = 0x4,
+    OMX_VIDEO_DolbyVisionLevelFhd30   = 0x8,
+    OMX_VIDEO_DolbyVisionLevelFhd60   = 0x10,
+    OMX_VIDEO_DolbyVisionLevelUhd24   = 0x20,
+    OMX_VIDEO_DolbyVisionLevelUhd30   = 0x40,
+    OMX_VIDEO_DolbyVisionLevelUhd48   = 0x80,
+    OMX_VIDEO_DolbyVisionLevelUhd60   = 0x100,
+    OMX_VIDEO_DolbyVisionLevelmax     = 0x7FFFFFFF
+} OMX_VIDEO_DOLBYVISIONLEVELTYPE;
+
+/**
+ * Structure for configuring video compression intra refresh period
+ *
+ * STRUCT MEMBERS:
+ *  nSize               : Size of the structure in bytes
+ *  nVersion            : OMX specification version information
+ *  nPortIndex          : Port that this structure applies to
+ *  nRefreshPeriod      : Intra refreh period in frames. Value 0 means disable intra refresh
+ */
+typedef struct OMX_VIDEO_CONFIG_ANDROID_INTRAREFRESHTYPE {
+    OMX_U32 nSize;
+    OMX_VERSIONTYPE nVersion;
+    OMX_U32 nPortIndex;
+    OMX_U32 nRefreshPeriod;
+} OMX_VIDEO_CONFIG_ANDROID_INTRAREFRESHTYPE;
+
+/** Maximum number of temporal layers supported by AVC/HEVC */
+#define OMX_VIDEO_ANDROID_MAXTEMPORALLAYERS 8
+
+/** temporal layer patterns */
+typedef enum OMX_VIDEO_ANDROID_TEMPORALLAYERINGPATTERNTYPE {
+    OMX_VIDEO_AndroidTemporalLayeringPatternNone = 0,
+    // pattern as defined by WebRTC
+    OMX_VIDEO_AndroidTemporalLayeringPatternWebRTC = 1 << 0,
+    // pattern where frames in any layer other than the base layer only depend on at most the very
+    // last frame from each preceding layer (other than the base layer.)
+    OMX_VIDEO_AndroidTemporalLayeringPatternAndroid = 1 << 1,
+} OMX_VIDEO_ANDROID_TEMPORALLAYERINGPATTERNTYPE;
+
+/**
+ * Android specific param for configuration of temporal layering.
+ * Android only supports temporal layering where successive layers each double the
+ * previous layer's framerate.
+ * NOTE: Reading this parameter at run-time SHALL return actual run-time values.
+ *
+ *  nSize                      : Size of the structure in bytes
+ *  nVersion                   : OMX specification version information
+ *  nPortIndex                 : Port that this structure applies to (output port for encoders)
+ *  eSupportedPatterns         : A bitmask of supported layering patterns
+ *  nLayerCountMax             : Max number of temporal coding layers supported
+ *                               by the encoder (must be at least 1, 1 meaning temporal layering
+ *                               is NOT supported)
+ *  nBLayerCountMax            : Max number of layers that can contain B frames
+ *                               (0) to (nLayerCountMax - 1)
+ *  ePattern                   : Layering pattern.
+ *  nPLayerCountActual         : Number of temporal layers to be coded with non-B frames,
+ *                               starting from and including the base-layer.
+ *                               (1 to nLayerCountMax - nBLayerCountActual)
+ *                               If nPLayerCountActual is 1 and nBLayerCountActual is 0, temporal
+ *                               layering is disabled. Otherwise, it is enabled.
+ *  nBLayerCountActual         : Number of temporal layers to be coded with B frames,
+ *                               starting after non-B layers.
+ *                               (0 to nBLayerCountMax)
+ *  bBitrateRatiosSpecified    : Flag to indicate if layer-wise bitrate
+ *                               distribution is specified.
+ *  nBitrateRatios             : Bitrate ratio (100 based) per layer (index 0 is base layer).
+ *                               Honored if bBitrateRatiosSpecified is set.
+ *                               i.e for 4 layers with desired distribution (25% 25% 25% 25%),
+ *                               nBitrateRatio = {25, 50, 75, 100, ... }
+ *                               Values in indices not less than 'the actual number of layers
+ *                               minus 1' MAY be ignored and assumed to be 100.
+ */
+typedef struct OMX_VIDEO_PARAM_ANDROID_TEMPORALLAYERINGTYPE {
+    OMX_U32 nSize;
+    OMX_VERSIONTYPE nVersion;
+    OMX_U32 nPortIndex;
+    OMX_VIDEO_ANDROID_TEMPORALLAYERINGPATTERNTYPE eSupportedPatterns;
+    OMX_U32 nLayerCountMax;
+    OMX_U32 nBLayerCountMax;
+    OMX_VIDEO_ANDROID_TEMPORALLAYERINGPATTERNTYPE ePattern;
+    OMX_U32 nPLayerCountActual;
+    OMX_U32 nBLayerCountActual;
+    OMX_BOOL bBitrateRatiosSpecified;
+    OMX_U32 nBitrateRatios[OMX_VIDEO_ANDROID_MAXTEMPORALLAYERS];
+} OMX_VIDEO_PARAM_ANDROID_TEMPORALLAYERINGTYPE;
+
+/**
+ * Android specific config for changing the temporal-layer count or
+ * bitrate-distribution at run-time.
+ *
+ *  nSize                      : Size of the structure in bytes
+ *  nVersion                   : OMX specification version information
+ *  nPortIndex                 : Port that this structure applies to (output port for encoders)
+ *  ePattern                   : Layering pattern.
+ *  nPLayerCountActual         : Number of temporal layers to be coded with non-B frames.
+ *                               (same OMX_VIDEO_PARAM_ANDROID_TEMPORALLAYERINGTYPE limits apply.)
+ *  nBLayerCountActual         : Number of temporal layers to be coded with B frames.
+ *                               (same OMX_VIDEO_PARAM_ANDROID_TEMPORALLAYERINGTYPE limits apply.)
+ *  bBitrateRatiosSpecified    : Flag to indicate if layer-wise bitrate
+ *                               distribution is specified.
+ *  nBitrateRatios             : Bitrate ratio (100 based, Q16 values) per layer (0 is base layer).
+ *                               Honored if bBitrateRatiosSpecified is set.
+ *                               (same OMX_VIDEO_PARAM_ANDROID_TEMPORALLAYERINGTYPE limits apply.)
+ */
+typedef struct OMX_VIDEO_CONFIG_ANDROID_TEMPORALLAYERINGTYPE {
+    OMX_U32 nSize;
+    OMX_VERSIONTYPE nVersion;
+    OMX_U32 nPortIndex;
+    OMX_VIDEO_ANDROID_TEMPORALLAYERINGPATTERNTYPE ePattern;
+    OMX_U32 nPLayerCountActual;
+    OMX_U32 nBLayerCountActual;
+    OMX_BOOL bBitrateRatiosSpecified;
+    OMX_U32 nBitrateRatios[OMX_VIDEO_ANDROID_MAXTEMPORALLAYERS];
+} OMX_VIDEO_CONFIG_ANDROID_TEMPORALLAYERINGTYPE;
+
+#ifdef __cplusplus
+}
+#endif /* __cplusplus */
+
+#endif /* OMX_VideoExt_h */
+/* File EOF */
-- 
2.30.2

