From: =?utf-8?b?IlNaIExpbiAo5p6X5LiK5pm6KSI=?= <szlin@debian.org>
Date: Thu, 27 Sep 2018 14:51:32 +0800
Subject: Fix typo

---
 doc/modbus_mapping_new_start_address.txt | 4 ++--
 doc/modbus_reply.txt                     | 2 +-
 doc/modbus_reply_exception.txt           | 2 +-
 3 files changed, 4 insertions(+), 4 deletions(-)

diff --git a/doc/modbus_mapping_new_start_address.txt b/doc/modbus_mapping_new_start_address.txt
index 4fa196a..94a81fb 100644
--- a/doc/modbus_mapping_new_start_address.txt
+++ b/doc/modbus_mapping_new_start_address.txt
@@ -21,9 +21,9 @@ The _modbus_mapping_new_start_address()_ function shall allocate four arrays to
 store bits, input bits, registers and inputs registers. The pointers are stored
 in modbus_mapping_t structure. All values of the arrays are initialized to zero.
 
-The different starting adresses make it possible to place the mapping at any
+The different starting addresses make it possible to place the mapping at any
 address in each address space. This way, you can give access to values stored
-at high adresses without allocating memory from the address zero, for eg. to
+at high addresses without allocating memory from the address zero, for eg. to
 make available registers from 10000 to 10009, you can use:
 
 [source,c]
diff --git a/doc/modbus_reply.txt b/doc/modbus_reply.txt
index 0b29d6f..6b71d11 100644
--- a/doc/modbus_reply.txt
+++ b/doc/modbus_reply.txt
@@ -3,7 +3,7 @@ modbus_reply(3)
 
 NAME
 ----
-modbus_reply - send a reponse to the received request
+modbus_reply - send a response to the received request
 
 
 SYNOPSIS
diff --git a/doc/modbus_reply_exception.txt b/doc/modbus_reply_exception.txt
index 7e6324f..b2170be 100644
--- a/doc/modbus_reply_exception.txt
+++ b/doc/modbus_reply_exception.txt
@@ -3,7 +3,7 @@ modbus_reply_exception(3)
 
 NAME
 ----
-modbus_reply_exception - send an exception reponse
+modbus_reply_exception - send an exception response
 
 
 SYNOPSIS
