From 375bc56fd3d66f40a9650224e5bfea4002494ade Mon Sep 17 00:00:00 2001
From: Tanu Kaskinen <tanuk@iki.fi>
Date: Fri, 23 Oct 2015 13:50:35 +0300
Subject: [PATCH 4/5] card: remove pa_card_new_data.active_profile

It's not being used any more.

Upstream-Status: Accepted [expected in 10.0]

Signed-off-by: Tanu Kaskinen <tanuk@iki.fi>
---
 src/pulsecore/card.c | 8 --------
 src/pulsecore/card.h | 5 -----
 2 files changed, 13 deletions(-)

diff --git a/src/pulsecore/card.c b/src/pulsecore/card.c
index a0c3d93..bc5b75b 100644
--- a/src/pulsecore/card.c
+++ b/src/pulsecore/card.c
@@ -96,13 +96,6 @@ void pa_card_new_data_set_name(pa_card_new_data *data, const char *name) {
     data->name = pa_xstrdup(name);
 }
 
-void pa_card_new_data_set_profile(pa_card_new_data *data, const char *profile) {
-    pa_assert(data);
-
-    pa_xfree(data->active_profile);
-    data->active_profile = pa_xstrdup(profile);
-}
-
 void pa_card_new_data_set_preferred_port(pa_card_new_data *data, pa_direction_t direction, pa_device_port *port) {
     pa_assert(data);
 
@@ -125,7 +118,6 @@ void pa_card_new_data_done(pa_card_new_data *data) {
         pa_hashmap_free(data->ports);
 
     pa_xfree(data->name);
-    pa_xfree(data->active_profile);
 }
 
 pa_card *pa_card_new(pa_core *core, pa_card_new_data *data) {
diff --git a/src/pulsecore/card.h b/src/pulsecore/card.h
index fd1fe0a..5699475 100644
--- a/src/pulsecore/card.h
+++ b/src/pulsecore/card.h
@@ -101,15 +101,11 @@ typedef struct pa_card_new_data {
     pa_module *module;
 
     pa_hashmap *profiles;
-    char *active_profile;
-
     pa_hashmap *ports;
     pa_device_port *preferred_input_port;
     pa_device_port *preferred_output_port;
 
     bool namereg_fail:1;
-
-    bool save_profile:1;
 } pa_card_new_data;
 
 typedef struct {
@@ -125,7 +121,6 @@ void pa_card_profile_set_available(pa_card_profile *c, pa_available_t available)
 
 pa_card_new_data *pa_card_new_data_init(pa_card_new_data *data);
 void pa_card_new_data_set_name(pa_card_new_data *data, const char *name);
-void pa_card_new_data_set_profile(pa_card_new_data *data, const char *profile);
 void pa_card_new_data_set_preferred_port(pa_card_new_data *data, pa_direction_t direction, pa_device_port *port);
 void pa_card_new_data_done(pa_card_new_data *data);
 
-- 
2.8.1

