From baf7c861e1cc523425029dcf81467f16c734fbd5 Mon Sep 17 00:00:00 2001
From: segher <segher@138bc75d-0d04-0410-961f-82ee72b054a4>
Date: Fri, 30 Aug 2019 14:13:51 +0000
Subject: [PATCH 1/3] 	Backport from trunk 	2019-08-22  Segher Boessenkool
  <segher@kernel.crashing.org>

	* config/rs6000/altivec.md (unspec): Delete UNSPEC_DARN, UNSPEC_DARN_32,
	UNSPEC_DARN_RAW, UNSPEC_CMPRB, UNSPEC_CMPRB2, UNSPEC_CMPEQB; move to...
	* config/rs6000/rs6000.md (unspec): ... here.
	* config/rs6000/altivec.md (darn_32, darn_raw, darn, cmprb,
	*cmprb_internal, setb_signed, setb_unsigned, cmprb2, *cmprb2_internal,
	cmpeqb, *cmpeqb_internal): Delete, move to...
	* config/rs6000/rs6000.md (darn_32, darn_raw, darn, cmprb,
	*cmprb_internal, setb_signed, setb_unsigned, cmprb2, *cmprb2_internal,
	cmpeqb, *cmpeqb_internal): ... here.


git-svn-id: svn+ssh://gcc.gnu.org/svn/gcc/branches/gcc-8-branch@275180 138bc75d-0d04-0410-961f-82ee72b054a4

Upstream-Status: Backport
CVE: CVE-2019-14847 p1
Affects <= 9.2.0
Dropped Changelog changes
Signed-off-by: Armin Kuster <akuster@mvista.com>

---
 gcc/config/rs6000/altivec.md | 223 ------------------------------------------
 gcc/config/rs6000/rs6000.md  | 224 +++++++++++++++++++++++++++++++++++++++++++
 3 files changed, 239 insertions(+), 223 deletions(-)

Index: gcc-8.3.0/gcc/config/rs6000/altivec.md
===================================================================
--- gcc-8.3.0.orig/gcc/config/rs6000/altivec.md
+++ gcc-8.3.0/gcc/config/rs6000/altivec.md
@@ -80,9 +80,6 @@
    UNSPEC_VUPKHPX
    UNSPEC_VUPKLPX
    UNSPEC_CONVERT_4F32_8I16
-   UNSPEC_DARN
-   UNSPEC_DARN_32
-   UNSPEC_DARN_RAW
    UNSPEC_DST
    UNSPEC_DSTT
    UNSPEC_DSTST
@@ -161,9 +158,6 @@
    UNSPEC_BCDADD
    UNSPEC_BCDSUB
    UNSPEC_BCD_OVERFLOW
-   UNSPEC_CMPRB
-   UNSPEC_CMPRB2
-   UNSPEC_CMPEQB
    UNSPEC_VRLMI
    UNSPEC_VRLNM
 ])
@@ -4317,223 +4311,6 @@
   [(set_attr "length" "4")
    (set_attr "type" "vecsimple")])
 
-(define_insn "darn_32"
-  [(set (match_operand:SI 0 "register_operand" "=r")
-        (unspec:SI [(const_int 0)] UNSPEC_DARN_32))]
-  "TARGET_P9_MISC"
-  "darn %0,0"
-  [(set_attr "type" "integer")])
-
-(define_insn "darn_raw"
-  [(set (match_operand:DI 0 "register_operand" "=r")
-        (unspec:DI [(const_int 0)] UNSPEC_DARN_RAW))]
-  "TARGET_P9_MISC && TARGET_64BIT"
-  "darn %0,2"
-  [(set_attr "type" "integer")])
-
-(define_insn "darn"
-  [(set (match_operand:DI 0 "register_operand" "=r")
-        (unspec:DI [(const_int 0)] UNSPEC_DARN))]
-  "TARGET_P9_MISC && TARGET_64BIT"
-  "darn %0,1"
-  [(set_attr "type" "integer")])
-
-;; Test byte within range.
-;;
-;; The bytes of operand 1 are organized as xx:xx:xx:vv, where xx
-;; represents a byte whose value is ignored in this context and
-;; vv, the least significant byte, holds the byte value that is to
-;; be tested for membership within the range specified by operand 2.
-;; The bytes of operand 2 are organized as xx:xx:hi:lo.
-;;
-;; Return in target register operand 0 a value of 1 if lo <= vv and
-;; vv <= hi.  Otherwise, set register operand 0 to 0.
-;;
-;; Though the instructions to which this expansion maps operate on
-;; 64-bit registers, the current implementation only operates on
-;; SI-mode operands as the high-order bits provide no information
-;; that is not already available in the low-order bits.  To avoid the
-;; costs of data widening operations, future enhancements might allow
-;; DI mode for operand 0 and/or might allow operand 1 to be QI mode.
-(define_expand "cmprb"
-  [(set (match_dup 3)
-	(unspec:CC [(match_operand:SI 1 "gpc_reg_operand" "r")
-		    (match_operand:SI 2 "gpc_reg_operand" "r")]
-	 UNSPEC_CMPRB))
-   (set (match_operand:SI 0 "gpc_reg_operand" "=r")
-	(if_then_else:SI (lt (match_dup 3)
-			     (const_int 0))
-			 (const_int -1)
-			 (if_then_else (gt (match_dup 3)
-					   (const_int 0))
-				       (const_int 1)
-				       (const_int 0))))]
-  "TARGET_P9_MISC"
-{
-  operands[3] = gen_reg_rtx (CCmode);
-})
-
-;; The bytes of operand 1 are organized as xx:xx:xx:vv, where xx
-;; represents a byte whose value is ignored in this context and
-;; vv, the least significant byte, holds the byte value that is to
-;; be tested for membership within the range specified by operand 2.
-;; The bytes of operand 2 are organized as xx:xx:hi:lo.
-;;
-;; Set bit 1 (the GT bit, 0x4) of CR register operand 0 to 1 if
-;; lo <= vv and vv <= hi.  Otherwise, set the GT bit to 0.  The other
-;; 3 bits of the target CR register are all set to 0.
-(define_insn "*cmprb_internal"
-  [(set (match_operand:CC 0 "cc_reg_operand" "=y")
-	(unspec:CC [(match_operand:SI 1 "gpc_reg_operand" "r")
-		    (match_operand:SI 2 "gpc_reg_operand" "r")]
-	 UNSPEC_CMPRB))]
-  "TARGET_P9_MISC"
-  "cmprb %0,0,%1,%2"
-  [(set_attr "type" "logical")])
-
-;; Set operand 0 register to -1 if the LT bit (0x8) of condition
-;; register operand 1 is on.  Otherwise, set operand 0 register to 1
-;; if the GT bit (0x4) of condition register operand 1 is on.
-;; Otherwise, set operand 0 to 0.  Note that the result stored into
-;; register operand 0 is non-zero iff either the LT or GT bits are on
-;; within condition register operand 1.
-(define_insn "setb_signed"
-   [(set (match_operand:SI 0 "gpc_reg_operand" "=r")
-	 (if_then_else:SI (lt (match_operand:CC 1 "cc_reg_operand" "y")
-			      (const_int 0))
-			  (const_int -1)
-			  (if_then_else (gt (match_dup 1)
-					    (const_int 0))
-					(const_int 1)
-					(const_int 0))))]
-  "TARGET_P9_MISC"
-  "setb %0,%1"
-  [(set_attr "type" "logical")])
-
-(define_insn "setb_unsigned"
-   [(set (match_operand:SI 0 "gpc_reg_operand" "=r")
-	 (if_then_else:SI (ltu (match_operand:CCUNS 1 "cc_reg_operand" "y")
-			      (const_int 0))
-			  (const_int -1)
-			  (if_then_else (gtu (match_dup 1)
-					    (const_int 0))
-					(const_int 1)
-					(const_int 0))))]
-  "TARGET_P9_MISC"
-  "setb %0,%1"
-  [(set_attr "type" "logical")])
-
-;; Test byte within two ranges.
-;;
-;; The bytes of operand 1 are organized as xx:xx:xx:vv, where xx
-;; represents a byte whose value is ignored in this context and
-;; vv, the least significant byte, holds the byte value that is to
-;; be tested for membership within the range specified by operand 2.
-;; The bytes of operand 2 are organized as hi_1:lo_1:hi_2:lo_2.
-;;
-;; Return in target register operand 0 a value of 1 if (lo_1 <= vv and
-;; vv <= hi_1) or if (lo_2 <= vv and vv <= hi_2).  Otherwise, set register
-;; operand 0 to 0.
-;;
-;; Though the instructions to which this expansion maps operate on
-;; 64-bit registers, the current implementation only operates on
-;; SI-mode operands as the high-order bits provide no information
-;; that is not already available in the low-order bits.  To avoid the
-;; costs of data widening operations, future enhancements might allow
-;; DI mode for operand 0 and/or might allow operand 1 to be QI mode.
-(define_expand "cmprb2"
-  [(set (match_dup 3)
-	(unspec:CC [(match_operand:SI 1 "gpc_reg_operand" "r")
-		    (match_operand:SI 2 "gpc_reg_operand" "r")]
-	 UNSPEC_CMPRB2))
-   (set (match_operand:SI 0 "gpc_reg_operand" "=r")
-	(if_then_else:SI (lt (match_dup 3)
-			     (const_int 0))
-			 (const_int -1)
-			 (if_then_else (gt (match_dup 3)
-					   (const_int 0))
-				       (const_int 1)
-				       (const_int 0))))]
-  "TARGET_P9_MISC"
-{
-  operands[3] = gen_reg_rtx (CCmode);
-})
-
-;; The bytes of operand 1 are organized as xx:xx:xx:vv, where xx
-;; represents a byte whose value is ignored in this context and
-;; vv, the least significant byte, holds the byte value that is to
-;; be tested for membership within the ranges specified by operand 2.
-;; The bytes of operand 2 are organized as hi_1:lo_1:hi_2:lo_2.
-;;
-;; Set bit 1 (the GT bit, 0x4) of CR register operand 0 to 1 if
-;; (lo_1 <= vv and vv <= hi_1) or if (lo_2 <= vv and vv <= hi_2).
-;; Otherwise, set the GT bit to 0.  The other 3 bits of the target
-;; CR register are all set to 0.
-(define_insn "*cmprb2_internal"
-  [(set (match_operand:CC 0 "cc_reg_operand" "=y")
-	(unspec:CC [(match_operand:SI 1 "gpc_reg_operand" "r")
-		    (match_operand:SI 2 "gpc_reg_operand" "r")]
-	 UNSPEC_CMPRB2))]
-  "TARGET_P9_MISC"
-  "cmprb %0,1,%1,%2"
-  [(set_attr "type" "logical")])
-
-;; Test byte membership within set of 8 bytes.
-;;
-;; The bytes of operand 1 are organized as xx:xx:xx:vv, where xx
-;; represents a byte whose value is ignored in this context and
-;; vv, the least significant byte, holds the byte value that is to
-;; be tested for membership within the set specified by operand 2.
-;; The bytes of operand 2 are organized as e0:e1:e2:e3:e4:e5:e6:e7.
-;;
-;; Return in target register operand 0 a value of 1 if vv equals one
-;; of the values e0, e1, e2, e3, e4, e5, e6, or e7.  Otherwise, set
-;; register operand 0 to 0.  Note that the 8 byte values held within
-;; operand 2 need not be unique.
-;;
-;; Though the instructions to which this expansion maps operate on
-;; 64-bit registers, the current implementation requires that operands
-;; 0 and 1 have mode SI as the high-order bits provide no information
-;; that is not already available in the low-order bits.  To avoid the
-;; costs of data widening operations, future enhancements might allow
-;; DI mode for operand 0 and/or might allow operand 1 to be QI mode.
-(define_expand "cmpeqb"
-  [(set (match_dup 3)
-	(unspec:CC [(match_operand:SI 1 "gpc_reg_operand" "r")
-		    (match_operand:DI 2 "gpc_reg_operand" "r")]
-	 UNSPEC_CMPEQB))
-   (set (match_operand:SI 0 "gpc_reg_operand" "=r")
-	(if_then_else:SI (lt (match_dup 3)
-			     (const_int 0))
-			 (const_int -1)
-			 (if_then_else (gt (match_dup 3)
-					   (const_int 0))
-				       (const_int 1)
-				       (const_int 0))))]
-  "TARGET_P9_MISC && TARGET_64BIT"
-{
-  operands[3] = gen_reg_rtx (CCmode);
-})
-
-;; The bytes of operand 1 are organized as xx:xx:xx:vv, where xx
-;; represents a byte whose value is ignored in this context and
-;; vv, the least significant byte, holds the byte value that is to
-;; be tested for membership within the set specified by operand 2.
-;; The bytes of operand 2 are organized as e0:e1:e2:e3:e4:e5:e6:e7.
-;;
-;; Set bit 1 (the GT bit, 0x4) of CR register operand 0 to 1 if vv
-;; equals one of the values e0, e1, e2, e3, e4, e5, e6, or e7.  Otherwise,
-;; set the GT bit to zero.  The other 3 bits of the target CR register
-;; are all set to 0.
-(define_insn "*cmpeqb_internal"
-  [(set (match_operand:CC 0 "cc_reg_operand" "=y")
-	 (unspec:CC [(match_operand:SI 1 "gpc_reg_operand" "r")
-		     (match_operand:DI 2 "gpc_reg_operand" "r")]
-	  UNSPEC_CMPEQB))]
-  "TARGET_P9_MISC && TARGET_64BIT"
-  "cmpeqb %0,%1,%2"
-  [(set_attr "type" "logical")])
-
 (define_expand "bcd<bcd_add_sub>_<code>"
   [(parallel [(set (reg:CCFP CR6_REGNO)
 		   (compare:CCFP
Index: gcc-8.3.0/gcc/config/rs6000/rs6000.md
===================================================================
--- gcc-8.3.0.orig/gcc/config/rs6000/rs6000.md
+++ gcc-8.3.0/gcc/config/rs6000/rs6000.md
@@ -136,6 +136,12 @@
    UNSPEC_LSQ
    UNSPEC_FUSION_GPR
    UNSPEC_STACK_CHECK
+   UNSPEC_DARN
+   UNSPEC_DARN_32
+   UNSPEC_DARN_RAW
+   UNSPEC_CMPRB
+   UNSPEC_CMPRB2
+   UNSPEC_CMPEQB
    UNSPEC_FUSION_P9
    UNSPEC_FUSION_ADDIS
    UNSPEC_ADD_ROUND_TO_ODD
@@ -14597,7 +14603,225 @@
    "xscmpuqp %0,%1,%2"
   [(set_attr "type" "veccmp")
    (set_attr "size" "128")])
+
+;; Miscellaneous ISA 3.0 (power9) instructions
+
+(define_insn "darn_32"
+  [(set (match_operand:SI 0 "register_operand" "=r")
+        (unspec:SI [(const_int 0)] UNSPEC_DARN_32))]
+  "TARGET_P9_MISC"
+  "darn %0,0"
+  [(set_attr "type" "integer")])
+
+(define_insn "darn_raw"
+  [(set (match_operand:DI 0 "register_operand" "=r")
+        (unspec:DI [(const_int 0)] UNSPEC_DARN_RAW))]
+  "TARGET_P9_MISC && TARGET_64BIT"
+  "darn %0,2"
+  [(set_attr "type" "integer")])
+
+(define_insn "darn"
+  [(set (match_operand:DI 0 "register_operand" "=r")
+        (unspec:DI [(const_int 0)] UNSPEC_DARN))]
+  "TARGET_P9_MISC && TARGET_64BIT"
+  "darn %0,1"
+  [(set_attr "type" "integer")])
 
+;; Test byte within range.
+;;
+;; The bytes of operand 1 are organized as xx:xx:xx:vv, where xx
+;; represents a byte whose value is ignored in this context and
+;; vv, the least significant byte, holds the byte value that is to
+;; be tested for membership within the range specified by operand 2.
+;; The bytes of operand 2 are organized as xx:xx:hi:lo.
+;;
+;; Return in target register operand 0 a value of 1 if lo <= vv and
+;; vv <= hi.  Otherwise, set register operand 0 to 0.
+;;
+;; Though the instructions to which this expansion maps operate on
+;; 64-bit registers, the current implementation only operates on
+;; SI-mode operands as the high-order bits provide no information
+;; that is not already available in the low-order bits.  To avoid the
+;; costs of data widening operations, future enhancements might allow
+;; DI mode for operand 0 and/or might allow operand 1 to be QI mode.
+(define_expand "cmprb"
+  [(set (match_dup 3)
+	(unspec:CC [(match_operand:SI 1 "gpc_reg_operand" "r")
+		    (match_operand:SI 2 "gpc_reg_operand" "r")]
+	 UNSPEC_CMPRB))
+   (set (match_operand:SI 0 "gpc_reg_operand" "=r")
+	(if_then_else:SI (lt (match_dup 3)
+			     (const_int 0))
+			 (const_int -1)
+			 (if_then_else (gt (match_dup 3)
+					   (const_int 0))
+				       (const_int 1)
+				       (const_int 0))))]
+  "TARGET_P9_MISC"
+{
+  operands[3] = gen_reg_rtx (CCmode);
+})
+
+;; The bytes of operand 1 are organized as xx:xx:xx:vv, where xx
+;; represents a byte whose value is ignored in this context and
+;; vv, the least significant byte, holds the byte value that is to
+;; be tested for membership within the range specified by operand 2.
+;; The bytes of operand 2 are organized as xx:xx:hi:lo.
+;;
+;; Set bit 1 (the GT bit, 0x4) of CR register operand 0 to 1 if
+;; lo <= vv and vv <= hi.  Otherwise, set the GT bit to 0.  The other
+;; 3 bits of the target CR register are all set to 0.
+(define_insn "*cmprb_internal"
+  [(set (match_operand:CC 0 "cc_reg_operand" "=y")
+	(unspec:CC [(match_operand:SI 1 "gpc_reg_operand" "r")
+		    (match_operand:SI 2 "gpc_reg_operand" "r")]
+	 UNSPEC_CMPRB))]
+  "TARGET_P9_MISC"
+  "cmprb %0,0,%1,%2"
+  [(set_attr "type" "logical")])
+
+;; Set operand 0 register to -1 if the LT bit (0x8) of condition
+;; register operand 1 is on.  Otherwise, set operand 0 register to 1
+;; if the GT bit (0x4) of condition register operand 1 is on.
+;; Otherwise, set operand 0 to 0.  Note that the result stored into
+;; register operand 0 is non-zero iff either the LT or GT bits are on
+;; within condition register operand 1.
+(define_insn "setb_signed"
+   [(set (match_operand:SI 0 "gpc_reg_operand" "=r")
+	 (if_then_else:SI (lt (match_operand:CC 1 "cc_reg_operand" "y")
+			      (const_int 0))
+			  (const_int -1)
+			  (if_then_else (gt (match_dup 1)
+					    (const_int 0))
+					(const_int 1)
+					(const_int 0))))]
+  "TARGET_P9_MISC"
+  "setb %0,%1"
+  [(set_attr "type" "logical")])
+
+(define_insn "setb_unsigned"
+   [(set (match_operand:SI 0 "gpc_reg_operand" "=r")
+	 (if_then_else:SI (ltu (match_operand:CCUNS 1 "cc_reg_operand" "y")
+			      (const_int 0))
+			  (const_int -1)
+			  (if_then_else (gtu (match_dup 1)
+					    (const_int 0))
+					(const_int 1)
+					(const_int 0))))]
+  "TARGET_P9_MISC"
+  "setb %0,%1"
+  [(set_attr "type" "logical")])
+
+;; Test byte within two ranges.
+;;
+;; The bytes of operand 1 are organized as xx:xx:xx:vv, where xx
+;; represents a byte whose value is ignored in this context and
+;; vv, the least significant byte, holds the byte value that is to
+;; be tested for membership within the range specified by operand 2.
+;; The bytes of operand 2 are organized as hi_1:lo_1:hi_2:lo_2.
+;;
+;; Return in target register operand 0 a value of 1 if (lo_1 <= vv and
+;; vv <= hi_1) or if (lo_2 <= vv and vv <= hi_2).  Otherwise, set register
+;; operand 0 to 0.
+;;
+;; Though the instructions to which this expansion maps operate on
+;; 64-bit registers, the current implementation only operates on
+;; SI-mode operands as the high-order bits provide no information
+;; that is not already available in the low-order bits.  To avoid the
+;; costs of data widening operations, future enhancements might allow
+;; DI mode for operand 0 and/or might allow operand 1 to be QI mode.
+(define_expand "cmprb2"
+  [(set (match_dup 3)
+	(unspec:CC [(match_operand:SI 1 "gpc_reg_operand" "r")
+		    (match_operand:SI 2 "gpc_reg_operand" "r")]
+	 UNSPEC_CMPRB2))
+   (set (match_operand:SI 0 "gpc_reg_operand" "=r")
+	(if_then_else:SI (lt (match_dup 3)
+			     (const_int 0))
+			 (const_int -1)
+			 (if_then_else (gt (match_dup 3)
+					   (const_int 0))
+				       (const_int 1)
+				       (const_int 0))))]
+  "TARGET_P9_MISC"
+{
+  operands[3] = gen_reg_rtx (CCmode);
+})
+
+;; The bytes of operand 1 are organized as xx:xx:xx:vv, where xx
+;; represents a byte whose value is ignored in this context and
+;; vv, the least significant byte, holds the byte value that is to
+;; be tested for membership within the ranges specified by operand 2.
+;; The bytes of operand 2 are organized as hi_1:lo_1:hi_2:lo_2.
+;;
+;; Set bit 1 (the GT bit, 0x4) of CR register operand 0 to 1 if
+;; (lo_1 <= vv and vv <= hi_1) or if (lo_2 <= vv and vv <= hi_2).
+;; Otherwise, set the GT bit to 0.  The other 3 bits of the target
+;; CR register are all set to 0.
+(define_insn "*cmprb2_internal"
+  [(set (match_operand:CC 0 "cc_reg_operand" "=y")
+	(unspec:CC [(match_operand:SI 1 "gpc_reg_operand" "r")
+		    (match_operand:SI 2 "gpc_reg_operand" "r")]
+	 UNSPEC_CMPRB2))]
+  "TARGET_P9_MISC"
+  "cmprb %0,1,%1,%2"
+  [(set_attr "type" "logical")])
+
+;; Test byte membership within set of 8 bytes.
+;;
+;; The bytes of operand 1 are organized as xx:xx:xx:vv, where xx
+;; represents a byte whose value is ignored in this context and
+;; vv, the least significant byte, holds the byte value that is to
+;; be tested for membership within the set specified by operand 2.
+;; The bytes of operand 2 are organized as e0:e1:e2:e3:e4:e5:e6:e7.
+;;
+;; Return in target register operand 0 a value of 1 if vv equals one
+;; of the values e0, e1, e2, e3, e4, e5, e6, or e7.  Otherwise, set
+;; register operand 0 to 0.  Note that the 8 byte values held within
+;; operand 2 need not be unique.
+;;
+;; Though the instructions to which this expansion maps operate on
+;; 64-bit registers, the current implementation requires that operands
+;; 0 and 1 have mode SI as the high-order bits provide no information
+;; that is not already available in the low-order bits.  To avoid the
+;; costs of data widening operations, future enhancements might allow
+;; DI mode for operand 0 and/or might allow operand 1 to be QI mode.
+(define_expand "cmpeqb"
+  [(set (match_dup 3)
+	(unspec:CC [(match_operand:SI 1 "gpc_reg_operand" "r")
+		    (match_operand:DI 2 "gpc_reg_operand" "r")]
+	 UNSPEC_CMPEQB))
+   (set (match_operand:SI 0 "gpc_reg_operand" "=r")
+	(if_then_else:SI (lt (match_dup 3)
+			     (const_int 0))
+			 (const_int -1)
+			 (if_then_else (gt (match_dup 3)
+					   (const_int 0))
+				       (const_int 1)
+				       (const_int 0))))]
+  "TARGET_P9_MISC && TARGET_64BIT"
+{
+  operands[3] = gen_reg_rtx (CCmode);
+})
+
+;; The bytes of operand 1 are organized as xx:xx:xx:vv, where xx
+;; represents a byte whose value is ignored in this context and
+;; vv, the least significant byte, holds the byte value that is to
+;; be tested for membership within the set specified by operand 2.
+;; The bytes of operand 2 are organized as e0:e1:e2:e3:e4:e5:e6:e7.
+;;
+;; Set bit 1 (the GT bit, 0x4) of CR register operand 0 to 1 if vv
+;; equals one of the values e0, e1, e2, e3, e4, e5, e6, or e7.  Otherwise,
+;; set the GT bit to zero.  The other 3 bits of the target CR register
+;; are all set to 0.
+(define_insn "*cmpeqb_internal"
+  [(set (match_operand:CC 0 "cc_reg_operand" "=y")
+	 (unspec:CC [(match_operand:SI 1 "gpc_reg_operand" "r")
+		     (match_operand:DI 2 "gpc_reg_operand" "r")]
+	  UNSPEC_CMPEQB))]
+  "TARGET_P9_MISC && TARGET_64BIT"
+  "cmpeqb %0,%1,%2"
+  [(set_attr "type" "logical")])
 
 
 (include "sync.md")
