From c7722d10c7bcf6be0adcf54abb1d406599dd7914 Mon Sep 17 00:00:00 2001
From: Patrick Ohly <patrick.ohly@intel.com>
Date: Fri, 24 Feb 2017 01:40:02 +0100
Subject: [PATCH] VfrCompile: increase path length limit

The VfrCompile tool has a hard-coded maximum length for path names
which turned out to be too small by around 20 characters in the Yocto
autobuilder setup. Increasing the maximum by a factor of 4 is
relatively easy and makes the problem less likely.

Upstream-Status: Inappropriate [configuration]

Signed-off-by: Patrick Ohly <patrick.ohly@intel.com>
---
 BaseTools/Source/C/VfrCompile/EfiVfr.h | 2 +-
 1 file changed, 1 insertion(+), 1 deletion(-)

diff --git a/BaseTools/Source/C/VfrCompile/EfiVfr.h b/BaseTools/Source/C/VfrCompile/EfiVfr.h
index d187902..9ad4a7b 100644
--- a/BaseTools/Source/C/VfrCompile/EfiVfr.h
+++ b/BaseTools/Source/C/VfrCompile/EfiVfr.h
@@ -19,7 +19,7 @@ WITHOUT WARRANTIES OR REPRESENTATIONS OF ANY KIND, EITHER EXPRESS OR IMPLIED.
 #include "Common/UefiInternalFormRepresentation.h"
 #include "Common/MdeModuleHii.h"
 
-#define MAX_PATH                 255
+#define MAX_PATH                 1023
 #define MAX_VFR_LINE_LEN         4096
 
 #define EFI_IFR_MAX_LENGTH       0xFF
-- 
2.1.4

