# Architecture
BR2_aarch64=y

# Linux headers same as kernel, a 4.1 series
BR2_PACKAGE_HOST_LINUX_HEADERS_CUSTOM_4_1=y

# System settings
BR2_TARGET_GENERIC_HOSTNAME="ucls1012a"
BR2_TARGET_GENERIC_ISSUE="Welcome to uCLS1012A-SOM"
BR2_SYSTEM_DHCP="eth0"
BR2_ROOTFS_OVERLAY="board/arcturus/aarch64-ucls1012a/rootfs_overlay"
BR2_ROOTFS_POST_IMAGE_SCRIPT="board/arcturus/aarch64-ucls1012a/post-image.sh"

# Kernel
BR2_LINUX_KERNEL=y
BR2_LINUX_KERNEL_CUSTOM_TARBALL=y
BR2_LINUX_KERNEL_CUSTOM_TARBALL_LOCATION="$(call github,ArcturusNetworks,uCLS1012A-kernel,v0.2.1811)/linux-v0.2.1811.tar.gz"
BR2_LINUX_KERNEL_DEFCONFIG="ucls1012a"
BR2_LINUX_KERNEL_DTS_SUPPORT=y
BR2_LINUX_KERNEL_INTREE_DTS_NAME="arcturus/arc-ucls1012a"

# Filesystem
BR2_TARGET_ROOTFS_CPIO=y
BR2_TARGET_ROOTFS_CPIO_GZIP=y

# U-boot
BR2_TARGET_UBOOT=y
BR2_TARGET_UBOOT_BUILD_SYSTEM_KCONFIG=y
BR2_TARGET_UBOOT_CUSTOM_GIT=y
BR2_TARGET_UBOOT_CUSTOM_REPO_URL="https://github.com/ArcturusNetworks/uCLS1012A-uboot.git"
BR2_TARGET_UBOOT_CUSTOM_REPO_VERSION="v0.2.1823"
BR2_TARGET_UBOOT_BOARD_DEFCONFIG="UCLS1012A_QSPI128"

# Tools
BR2_PACKAGE_HOST_UBOOT_TOOLS=y
BR2_PACKAGE_HOST_UBOOT_TOOLS_FIT_SUPPORT=y
