Cmp-Mod V01 Genere par PcbNew le Thu 06 Jan 2011 06:56:15 PM CET

BeginCmp
TimeStamp = 4BEDD157
Path = /4B6E16F2/4B6E1740
Reference = U101;
ValeurCmp = 74ALVC164245;
IdModule  = TSSOP48;
EndCmp

BeginCmp
TimeStamp = 4BEDD1A3
Path = /4B6E16F2/4B6E1748
Reference = U103;
ValeurCmp = 74ALVC164245;
IdModule  = TSSOP48;
EndCmp

BeginCmp
TimeStamp = 4BEDD19A
Path = /4B6E16F2/4B6E1744
Reference = U102;
ValeurCmp = 74ALVC164245;
IdModule  = TSSOP48;
EndCmp

BeginCmp
TimeStamp = 4B6ED33B
Path = /4B6EC9C3/4B6ED134
Reference = U321;
ValeurCmp = MCP1824-2.5;
IdModule  = SOT23-5;
EndCmp

BeginCmp
TimeStamp = 4B6ED33D
Path = /4B6EC9C3/4B6ED144
Reference = U311;
ValeurCmp = MCP1824-1.8;
IdModule  = SOT23-5;
EndCmp

BeginCmp
TimeStamp = 4BF3E245
Path = /4B6ED75B/4B6F321A
Reference = U401;
ValeurCmp = LPC1754;
IdModule  = LQFP80-.5;
EndCmp

BeginCmp
TimeStamp = 4B6E26C2
Path = /4B6E18FC/4B6E1931
Reference = U201;
ValeurCmp = XC3S400-PQ208;
IdModule  = PQFP208;
EndCmp

BeginCmp
TimeStamp = 4BEE66BC
Path = /4BAA6ABD/4BF19DCA
Reference = D511;
ValeurCmp = BAT54C;
IdModule  = SOT23EBC;
EndCmp

BeginCmp
TimeStamp = 4C13969B
Path = /4B6ED75B/4BC243CB
Reference = X402;
ValeurCmp = 32.768kHz;
IdModule  = XTAL_SMD_05019;
EndCmp

BeginCmp
TimeStamp = 4BEFC8C5
Path = /4B6ED75B/4BEFBC73
Reference = P402;
ValeurCmp = CONN_2;
IdModule  = PIN_ARRAY_2X1;
EndCmp

BeginCmp
TimeStamp = 4BEFB152
Path = /4B6ED75B/4BF00175
Reference = J421;
ValeurCmp = USB_MINIB;
IdModule  = USB-MINIB-THT;
EndCmp

BeginCmp
TimeStamp = 4BF2FF04
Path = /4BAA6ABD/4BF2FD9F
Reference = Q511;
ValeurCmp = 2N2222A;
IdModule  = SOT23EBC;
EndCmp

BeginCmp
TimeStamp = 4BF3D1C4
Path = /4B6ED75B/4C4A0B6F
Reference = P403;
ValeurCmp = CONN_2;
IdModule  = PIN_ARRAY_2X1;
EndCmp

BeginCmp
TimeStamp = 4BEE7B7D
Path = /4B6EC9C3/4BAF2EAF
Reference = BT351;
ValeurCmp = Keystone_1059_/_KZH20PCB;
IdModule  = BT_KEYSTONE_1059_20MM;
EndCmp

BeginCmp
TimeStamp = 4BF2734A
Path = /4BAA6ABD/4B868602
Reference = U501;
ValeurCmp = MT45W8MW16;
IdModule  = VFBGA54;
EndCmp

BeginCmp
TimeStamp = 4BAA892D
Path = /4BAA6ABD/4B86E25C
Reference = U511;
ValeurCmp = CY62148EV30-BVXI;
IdModule  = VFBGA36;
EndCmp

BeginCmp
TimeStamp = 4BAA93D8
Path = /4B6EC9C3/4BAA9331
Reference = U341;
ValeurCmp = CS4344;
IdModule  = TSSOP10;
EndCmp

BeginCmp
TimeStamp = 4C09447D
Path = /4B6ED75B/4C0943CA
Reference = P401;
ValeurCmp = CONN_7X2;
IdModule  = pin_array_7x2;
EndCmp

BeginCmp
TimeStamp = 4C8642EF
Path = /4B6EC9C3/4C42D578
Reference = R331;
ValeurCmp = 680;
IdModule  = SM0805_FIXEDMASK;
EndCmp

BeginCmp
TimeStamp = 4C1A7291
Path = /4B6EC9C3/4C17DE31
Reference = C342;
ValeurCmp = 1u;
IdModule  = SM0805_FIXEDMASK;
EndCmp

BeginCmp
TimeStamp = 4C12872B
Path = /4B6ED75B/4C1286D5
Reference = C412;
ValeurCmp = 100n;
IdModule  = SM0805_FIXEDMASK;
EndCmp

BeginCmp
TimeStamp = 4C0DA806
Path = /4B6ED75B/4C0DA785
Reference = R403;
ValeurCmp = 680;
IdModule  = SM0805_FIXEDMASK;
EndCmp

BeginCmp
TimeStamp = 4C063CEB
Path = /4B6ED75B/4C063C47
Reference = C405;
ValeurCmp = 100n;
IdModule  = SM0805_FIXEDMASK;
EndCmp

BeginCmp
TimeStamp = 4C063CE9
Path = /4B6ED75B/4C063C2F
Reference = R404;
ValeurCmp = 10k;
IdModule  = SM0805_FIXEDMASK;
EndCmp

BeginCmp
TimeStamp = 4C05B204
Path = /4B6EC9C3/4C05ACA2
Reference = C301;
ValeurCmp = 4.7u;
IdModule  = SM0805_FIXEDMASK;
EndCmp

BeginCmp
TimeStamp = 4C05B202
Path = /4B6EC9C3/4C05ACA4
Reference = C303;
ValeurCmp = 4.7u;
IdModule  = SM0805_FIXEDMASK;
EndCmp

BeginCmp
TimeStamp = 4C05B200
Path = /4B6EC9C3/4C05AC9D
Reference = C302;
ValeurCmp = 10n;
IdModule  = SM0805_FIXEDMASK;
EndCmp

BeginCmp
TimeStamp = 4C05B1FE
Path = /4B6EC9C3/4C05AC9A
Reference = C304;
ValeurCmp = 4.7u;
IdModule  = SM0805_FIXEDMASK;
EndCmp

BeginCmp
TimeStamp = 4C017B5E
Path = /4B6ED75B/4C01596A
Reference = R423;
ValeurCmp = 1.5k;
IdModule  = SM0805_FIXEDMASK;
EndCmp

BeginCmp
TimeStamp = 4BABDA69
Path = /4B6EC9C3/4BABCAD2
Reference = C322;
ValeurCmp = 4.7u;
IdModule  = SM0805_FIXEDMASK;
EndCmp

BeginCmp
TimeStamp = 4BABDA6B
Path = /4B6EC9C3/4BABCB68
Reference = C312;
ValeurCmp = 4.7u;
IdModule  = SM0805_FIXEDMASK;
EndCmp

BeginCmp
TimeStamp = 4BABDA6D
Path = /4B6EC9C3/4BABCA9C
Reference = C321;
ValeurCmp = 4.7u;
IdModule  = SM0805_FIXEDMASK;
EndCmp

BeginCmp
TimeStamp = 4BABDA6F
Path = /4B6EC9C3/4BABCB5C
Reference = C311;
ValeurCmp = 4.7u;
IdModule  = SM0805_FIXEDMASK;
EndCmp

BeginCmp
TimeStamp = 4BAD47FF
Path = /4BAA6ABD/4BAD3D55
Reference = C502;
ValeurCmp = 100n;
IdModule  = SM0805_FIXEDMASK;
EndCmp

BeginCmp
TimeStamp = 4BEDCF0C
Path = /4BAA6ABD/4BAD3D53
Reference = C511;
ValeurCmp = 100n;
IdModule  = SM0805_FIXEDMASK;
EndCmp

BeginCmp
TimeStamp = 4D2528F3
Path = /4BAA6ABD/4BAD3D47
Reference = C501;
ValeurCmp = 100n;
IdModule  = SM0805_FIXEDMASK;
EndCmp

BeginCmp
TimeStamp = 4BAD4805
Path = /4B6E16F2/4BAD42E2
Reference = C116;
ValeurCmp = 100n;
IdModule  = SM0805_FIXEDMASK;
EndCmp

BeginCmp
TimeStamp = 4BAD4807
Path = /4B6E16F2/4BAD42E0
Reference = C115;
ValeurCmp = 100n;
IdModule  = SM0805_FIXEDMASK;
EndCmp

BeginCmp
TimeStamp = 4BAD4809
Path = /4B6E16F2/4BAD42DF
Reference = C114;
ValeurCmp = 100n;
IdModule  = SM0805_FIXEDMASK;
EndCmp

BeginCmp
TimeStamp = 4BEDD15D
Path = /4B6E16F2/4BAD42DA
Reference = C103;
ValeurCmp = 100n;
IdModule  = SM0805_FIXEDMASK;
EndCmp

BeginCmp
TimeStamp = 4BEDD15A
Path = /4B6E16F2/4BAD42D8
Reference = C102;
ValeurCmp = 100n;
IdModule  = SM0805_FIXEDMASK;
EndCmp

BeginCmp
TimeStamp = 4BAD480F
Path = /4B6E16F2/4BAD42D5
Reference = C101;
ValeurCmp = 100n;
IdModule  = SM0805_FIXEDMASK;
EndCmp

BeginCmp
TimeStamp = 4BAE3C6B
Path = /4B6EC9C3/4BADC720
Reference = C341;
ValeurCmp = 100n;
IdModule  = SM0805_FIXEDMASK;
EndCmp

BeginCmp
TimeStamp = 4C8642E9
Path = /4B6EC9C3/4BADC719
Reference = C331;
ValeurCmp = 100n;
IdModule  = SM0805_FIXEDMASK;
EndCmp

BeginCmp
TimeStamp = 4BAE3C6F
Path = /4B6E18FC/4BADCE85
Reference = C222;
ValeurCmp = 100n;
IdModule  = SM0805_FIXEDMASK;
EndCmp

BeginCmp
TimeStamp = 4C06E5AC
Path = /4B6E18FC/4BADCE7D
Reference = C221;
ValeurCmp = 100n;
IdModule  = SM0805_FIXEDMASK;
EndCmp

BeginCmp
TimeStamp = 4BAE3C73
Path = /4B6E18FC/4BADCE7B
Reference = C213;
ValeurCmp = 100n;
IdModule  = SM0805_FIXEDMASK;
EndCmp

BeginCmp
TimeStamp = 4BAE3C75
Path = /4B6E18FC/4BADCE7A
Reference = C212;
ValeurCmp = 100n;
IdModule  = SM0805_FIXEDMASK;
EndCmp

BeginCmp
TimeStamp = 4BAE3C77
Path = /4B6E18FC/4BADCE78
Reference = C211;
ValeurCmp = 100n;
IdModule  = SM0805_FIXEDMASK;
EndCmp

BeginCmp
TimeStamp = 4BAE3C79
Path = /4B6E18FC/4BADCE74
Reference = C210;
ValeurCmp = 100n;
IdModule  = SM0805_FIXEDMASK;
EndCmp

BeginCmp
TimeStamp = 4BAE3C7B
Path = /4B6E18FC/4BADCE6D
Reference = C208;
ValeurCmp = 100n;
IdModule  = SM0805_FIXEDMASK;
EndCmp

BeginCmp
TimeStamp = 4BAE3C7D
Path = /4B6E18FC/4BADCE6B
Reference = C207;
ValeurCmp = 100n;
IdModule  = SM0805_FIXEDMASK;
EndCmp

BeginCmp
TimeStamp = 4BAE3C7F
Path = /4B6E18FC/4BADCE6A
Reference = C206;
ValeurCmp = 100n;
IdModule  = SM0805_FIXEDMASK;
EndCmp

BeginCmp
TimeStamp = 4BAE3C81
Path = /4B6E18FC/4BADCE67
Reference = C205;
ValeurCmp = 100n;
IdModule  = SM0805_FIXEDMASK;
EndCmp

BeginCmp
TimeStamp = 4BAE3C83
Path = /4B6E18FC/4BADCE65
Reference = C204;
ValeurCmp = 100n;
IdModule  = SM0805_FIXEDMASK;
EndCmp

BeginCmp
TimeStamp = 4BAE3C85
Path = /4B6E18FC/4BADCE64
Reference = C203;
ValeurCmp = 100n;
IdModule  = SM0805_FIXEDMASK;
EndCmp

BeginCmp
TimeStamp = 4BF5AE0A
Path = /4B6E18FC/4BADCE62
Reference = C202;
ValeurCmp = 100n;
IdModule  = SM0805_FIXEDMASK;
EndCmp

BeginCmp
TimeStamp = 4BAE3C89
Path = /4B6E18FC/4BADCE47
Reference = C201;
ValeurCmp = 100n;
IdModule  = SM0805_FIXEDMASK;
EndCmp

BeginCmp
TimeStamp = 4BAE5213
Path = /4B6E16F2/4BAE51CA
Reference = R101;
ValeurCmp = 270;
IdModule  = SM0805_FIXEDMASK;
EndCmp

BeginCmp
TimeStamp = 4C1396A7
Path = /4B6ED75B/4BEECBCD
Reference = C408;
ValeurCmp = 22p;
IdModule  = SM0805_FIXEDMASK;
EndCmp

BeginCmp
TimeStamp = 4BEEE8BE
Path = /4B6ED75B/4BEECBCA
Reference = C407;
ValeurCmp = 33p;
IdModule  = SM0805_FIXEDMASK;
EndCmp

BeginCmp
TimeStamp = 4BEEE8C0
Path = /4B6ED75B/4BEECBC1
Reference = C406;
ValeurCmp = 33p;
IdModule  = SM0805_FIXEDMASK;
EndCmp

BeginCmp
TimeStamp = 4BF2FEFF
Path = /4BAA6ABD/4BF2FDA9
Reference = R512;
ValeurCmp = 4k7;
IdModule  = SM0805_FIXEDMASK;
EndCmp

BeginCmp
TimeStamp = 4BF2FF01
Path = /4BAA6ABD/4BF2FDAC
Reference = R513;
ValeurCmp = 1k;
IdModule  = SM0805_FIXEDMASK;
EndCmp

BeginCmp
TimeStamp = 4BF2FF03
Path = /4BAA6ABD/4BF2FDAF
Reference = R511;
ValeurCmp = 20k;
IdModule  = SM0805_FIXEDMASK;
EndCmp

BeginCmp
TimeStamp = 4BF5A49C
Path = /4B6E18FC/4BF5A43F
Reference = C223;
ValeurCmp = 100n;
IdModule  = SM0805_FIXEDMASK;
EndCmp

BeginCmp
TimeStamp = 4BF5A49E
Path = /4B6E18FC/4BF5A441
Reference = C224;
ValeurCmp = 100n;
IdModule  = SM0805_FIXEDMASK;
EndCmp

BeginCmp
TimeStamp = 4BF6C25D
Path = /4B6ED75B/4BF6BFBB
Reference = C411;
ValeurCmp = 10u;
IdModule  = SM0805_FIXEDMASK;
EndCmp

BeginCmp
TimeStamp = 4C139698
Path = /4B6ED75B/4BF6BFE1
Reference = C401;
ValeurCmp = 100n;
IdModule  = SM0805_FIXEDMASK;
EndCmp

BeginCmp
TimeStamp = 4BF6C261
Path = /4B6ED75B/4BF6BFE2
Reference = C402;
ValeurCmp = 100n;
IdModule  = SM0805_FIXEDMASK;
EndCmp

BeginCmp
TimeStamp = 4BF6C263
Path = /4B6ED75B/4BF6BFE5
Reference = C403;
ValeurCmp = 100n;
IdModule  = SM0805_FIXEDMASK;
EndCmp

BeginCmp
TimeStamp = 4BF6C265
Path = /4B6ED75B/4BF6BFE6
Reference = C404;
ValeurCmp = 100n;
IdModule  = SM0805_FIXEDMASK;
EndCmp

BeginCmp
TimeStamp = 4C59442F
Path = /4B6ED75B/4BF847A7
Reference = R401;
ValeurCmp = 680;
IdModule  = SM0805_FIXEDMASK;
EndCmp

BeginCmp
TimeStamp = 4BF851B9
Path = /4B6ED75B/4BF847B1
Reference = R402;
ValeurCmp = 680;
IdModule  = SM0805_FIXEDMASK;
EndCmp

BeginCmp
TimeStamp = 4BF851BB
Path = /4B6ED75B/4BF850A9
Reference = R406;
ValeurCmp = 100;
IdModule  = SM0805_FIXEDMASK;
EndCmp

BeginCmp
TimeStamp = 4BF851BD
Path = /4B6ED75B/4BF850D1
Reference = R405;
ValeurCmp = 100;
IdModule  = SM0805_FIXEDMASK;
EndCmp

BeginCmp
TimeStamp = 4BF99039
Path = /4B6EC9C3/4BF98AA2
Reference = C343;
ValeurCmp = 100n;
IdModule  = SM0805_FIXEDMASK;
EndCmp

BeginCmp
TimeStamp = 4BF9903B
Path = /4B6EC9C3/4BF98AA5
Reference = C344;
ValeurCmp = 10u;
IdModule  = SM0805_FIXEDMASK;
EndCmp

BeginCmp
TimeStamp = 4BF9903D
Path = /4B6EC9C3/4BF98AAB
Reference = C345;
ValeurCmp = 10u;
IdModule  = SM0805_FIXEDMASK;
EndCmp

BeginCmp
TimeStamp = 4BF9903F
Path = /4B6EC9C3/4BF98E9E
Reference = C347;
ValeurCmp = 10n;
IdModule  = SM0805_FIXEDMASK;
EndCmp

BeginCmp
TimeStamp = 4BF99041
Path = /4B6EC9C3/4BF98EB4
Reference = R343;
ValeurCmp = 470;
IdModule  = SM0805_FIXEDMASK;
EndCmp

BeginCmp
TimeStamp = 4BF99043
Path = /4B6EC9C3/4BF98EB9
Reference = R344;
ValeurCmp = 10k;
IdModule  = SM0805_FIXEDMASK;
EndCmp

BeginCmp
TimeStamp = 4BF99045
Path = /4B6EC9C3/4BF98EBB
Reference = C348;
ValeurCmp = 3.3u;
IdModule  = SM0805_FIXEDMASK;
EndCmp

BeginCmp
TimeStamp = 4BF99047
Path = /4B6EC9C3/4BF98EBE
Reference = C346;
ValeurCmp = 3.3u;
IdModule  = SM0805_FIXEDMASK;
EndCmp

BeginCmp
TimeStamp = 4BF99049
Path = /4B6EC9C3/4BF98EBF
Reference = C349;
ValeurCmp = 3,3n;
IdModule  = SM0805_FIXEDMASK;
EndCmp

BeginCmp
TimeStamp = 4BF9904B
Path = /4B6EC9C3/4BF98EC4
Reference = R342;
ValeurCmp = 10k;
IdModule  = SM0805_FIXEDMASK;
EndCmp

BeginCmp
TimeStamp = 4BF9904D
Path = /4B6EC9C3/4BF98EC6
Reference = R341;
ValeurCmp = 470;
IdModule  = SM0805_FIXEDMASK;
EndCmp

BeginCmp
TimeStamp = 4BFB12D0
Path = /4B6E16F2/4BFB1190
Reference = C104;
ValeurCmp = 100n;
IdModule  = SM0805_FIXEDMASK;
EndCmp

BeginCmp
TimeStamp = 4BFB12D2
Path = /4B6E16F2/4BFB1192
Reference = C105;
ValeurCmp = 100n;
IdModule  = SM0805_FIXEDMASK;
EndCmp

BeginCmp
TimeStamp = 4BFB12D4
Path = /4B6E16F2/4BFB1194
Reference = C106;
ValeurCmp = 100n;
IdModule  = SM0805_FIXEDMASK;
EndCmp

BeginCmp
TimeStamp = 4BFF8E85
Path = /4B6E16F2/4BFB1197
Reference = C113;
ValeurCmp = 100n;
IdModule  = SM0805_FIXEDMASK;
EndCmp

BeginCmp
TimeStamp = 4BFB12D8
Path = /4B6E16F2/4BFB1199
Reference = C112;
ValeurCmp = 100n;
IdModule  = SM0805_FIXEDMASK;
EndCmp

BeginCmp
TimeStamp = 4BFB12DA
Path = /4B6E16F2/4BFB119A
Reference = C111;
ValeurCmp = 100n;
IdModule  = SM0805_FIXEDMASK;
EndCmp

BeginCmp
TimeStamp = 4C1396A1
Path = /4B6ED75B/4BEECBD1
Reference = C409;
ValeurCmp = 22p;
IdModule  = SM0805_FIXEDMASK;
EndCmp

BeginCmp
TimeStamp = 4BFDB494
Path = /4B6ED75B/4BAA6A9C
Reference = J411;
ValeurCmp = SD_CARD;
IdModule  = HRS-DM1AA;
EndCmp

BeginCmp
TimeStamp = 4C05889D
Path = /4B6EC9C3/4C05879D
Reference = U301;
ValeurCmp = MIC23250-S4YMT;
IdModule  = QFN10-2x2;
EndCmp

BeginCmp
TimeStamp = 4C5608E7
Path = /4B6ED75B/4C5608C6
Reference = R421;
ValeurCmp = 33;
IdModule  = SM0805_FIXEDMASK;
EndCmp

BeginCmp
TimeStamp = 4C5608E9
Path = /4B6ED75B/4C5608C9
Reference = R422;
ValeurCmp = 33;
IdModule  = SM0805_FIXEDMASK;
EndCmp

BeginCmp
TimeStamp = 4C7EAD87
Path = /4B6E16F2/4C7EAD01
Reference = Q101;
ValeurCmp = 2N2222A;
IdModule  = SOT23EBC;
EndCmp

BeginCmp
TimeStamp = 4C7EAF70
Path = /4B6E16F2/4C7EAEBF
Reference = R102;
ValeurCmp = 1k;
IdModule  = SM0805_FIXEDMASK;
EndCmp

BeginCmp
TimeStamp = 4C7EAF72
Path = /4B6E16F2/4C7EAF13
Reference = R103;
ValeurCmp = 4k7;
IdModule  = SM0805_FIXEDMASK;
EndCmp

BeginCmp
TimeStamp = 4C7FF8C4
Path = /4B6E18FC/4C7FF87E
Reference = P113;
ValeurCmp = CONN_1;
IdModule  = PAD_1x1mm;
EndCmp

BeginCmp
TimeStamp = 4C829461
Path = /4B6ED75B/4C814430
Reference = R407;
ValeurCmp = 10k;
IdModule  = SM0805_FIXEDMASK;
EndCmp

BeginCmp
TimeStamp = 4C863298
Path = /4B6ED75B/4C86265B
Reference = JP401;
ValeurCmp = JUMPER;
IdModule  = GS2;
EndCmp

BeginCmp
TimeStamp = 4BAA9371
Path = /4B6EC9C3/4BAA92DB
Reference = U331;
ValeurCmp = PIC12F629;
IdModule  = DIP-8__300;
EndCmp

BeginCmp
TimeStamp = 4D0BC965
Path = /4B6EC9C3/4CA6556E
Reference = R332;
ValeurCmp = 680;
IdModule  = SM0805_FIXEDMASK;
EndCmp

BeginCmp
TimeStamp = 4D0BC967
Path = /4B6EC9C3/4CA65577
Reference = R333;
ValeurCmp = 680;
IdModule  = SM0805_FIXEDMASK;
EndCmp

BeginCmp
TimeStamp = 4D0BC969
Path = /4B6EC9C3/4CA65597
Reference = C333;
ValeurCmp = 100p;
IdModule  = SM0805_FIXEDMASK;
EndCmp

BeginCmp
TimeStamp = 4D0BC96B
Path = /4B6EC9C3/4CA655D4
Reference = C332;
ValeurCmp = 100p;
IdModule  = SM0805_FIXEDMASK;
EndCmp

BeginCmp
TimeStamp = 4D1787BE
Path = /4B6E16F2/4D1151E8
Reference = R128;
ValeurCmp = 220;
IdModule  = SM0805_FIXEDMASK;
EndCmp

BeginCmp
TimeStamp = 4D1787C0
Path = /4B6E16F2/4D1151EA
Reference = R127;
ValeurCmp = 220;
IdModule  = SM0805_FIXEDMASK;
EndCmp

BeginCmp
TimeStamp = 4D1787C2
Path = /4B6E16F2/4D1151ED
Reference = R126;
ValeurCmp = 220;
IdModule  = SM0805_FIXEDMASK;
EndCmp

BeginCmp
TimeStamp = 4D1787C4
Path = /4B6E16F2/4D113BED
Reference = R125;
ValeurCmp = 220;
IdModule  = SM0805_FIXEDMASK;
EndCmp

BeginCmp
TimeStamp = 4D1787C6
Path = /4B6E16F2/4D113BF1
Reference = R124;
ValeurCmp = 220;
IdModule  = SM0805_FIXEDMASK;
EndCmp

BeginCmp
TimeStamp = 4D1787C8
Path = /4B6E16F2/4D113BF4
Reference = R123;
ValeurCmp = 220;
IdModule  = SM0805_FIXEDMASK;
EndCmp

BeginCmp
TimeStamp = 4D1787CA
Path = /4B6E16F2/4D113BF7
Reference = R122;
ValeurCmp = 220;
IdModule  = SM0805_FIXEDMASK;
EndCmp

BeginCmp
TimeStamp = 4D1FFB60
Path = /4B6E16F2/4C82A889
Reference = R121;
ValeurCmp = 220;
IdModule  = SM0805_FIXEDMASK;
EndCmp

BeginCmp
TimeStamp = 4D1787CE
Path = /4B6E16F2/4D115250
Reference = C128;
ValeurCmp = 10p;
IdModule  = SM0805_FIXEDMASK;
EndCmp

BeginCmp
TimeStamp = 4D1787D0
Path = /4B6E16F2/4D11524F
Reference = C127;
ValeurCmp = 10p;
IdModule  = SM0805_FIXEDMASK;
EndCmp

BeginCmp
TimeStamp = 4D1787D2
Path = /4B6E16F2/4D11524E
Reference = C126;
ValeurCmp = 10p;
IdModule  = SM0805_FIXEDMASK;
EndCmp

BeginCmp
TimeStamp = 4D1787D4
Path = /4B6E16F2/4D113CAF
Reference = C125;
ValeurCmp = 10p;
IdModule  = SM0805_FIXEDMASK;
EndCmp

BeginCmp
TimeStamp = 4D1787D6
Path = /4B6E16F2/4D113CAC
Reference = C124;
ValeurCmp = 10p;
IdModule  = SM0805_FIXEDMASK;
EndCmp

BeginCmp
TimeStamp = 4D1787D8
Path = /4B6E16F2/4D113CAA
Reference = C123;
ValeurCmp = 10p;
IdModule  = SM0805_FIXEDMASK;
EndCmp

BeginCmp
TimeStamp = 4D1787DA
Path = /4B6E16F2/4D113C9C
Reference = C122;
ValeurCmp = 10p;
IdModule  = SM0805_FIXEDMASK;
EndCmp

BeginCmp
TimeStamp = 4D1787DC
Path = /4B6E16F2/4D113C55
Reference = C121;
ValeurCmp = 10p;
IdModule  = SM0805_FIXEDMASK;
EndCmp

BeginCmp
TimeStamp = 4B6D9041
Path = /4B6E16F2/4B6E1766
Reference = J101;
ValeurCmp = SNESCART_EXT;
IdModule  = SNESCART_EXT;
EndCmp

BeginCmp
TimeStamp = 4C05B20B
Path = /4B6EC9C3/4C05A983
Reference = L302;
ValeurCmp = 1uH;
IdModule  = SM1210L_NEW;
EndCmp

BeginCmp
TimeStamp = 4C05B209
Path = /4B6EC9C3/4C05A97C
Reference = L301;
ValeurCmp = 1uH;
IdModule  = SM1210L_NEW;
EndCmp

BeginCmp
TimeStamp = 4BF851B4
Path = /4B6ED75B/4BF8324A
Reference = D402;
ValeurCmp = LED_2mA_1.8V,_yellow;
IdModule  = LED-3MM-FIXED;
EndCmp

BeginCmp
TimeStamp = 4BF851B6
Path = /4B6ED75B/4BF8328D
Reference = D401;
ValeurCmp = LED_2mA_1.9V,_green;
IdModule  = LED-3MM-FIXED;
EndCmp

BeginCmp
TimeStamp = 4C0DA805
Path = /4B6ED75B/4C0DA78D
Reference = D403;
ValeurCmp = LED_2mA_1.7V,_red;
IdModule  = LED-3MM-FIXED;
EndCmp

BeginCmp
TimeStamp = 4D252B91
Path = /4B6E18FC/4D252B5C
Reference = C214;
ValeurCmp = 100n;
IdModule  = SM0805_FIXEDMASK;
EndCmp

BeginCmp
TimeStamp = 4C13968F
Path = /4B6ED75B/4BC243C8
Reference = X401;
ValeurCmp = 12MHz;
IdModule  = HC49US;
EndCmp

EndListe
