Cmp-Mod V01 Created by CvPCB (20100409 SVN-R2518)-unstable date = Thu 05 Aug 2010 10:55:28 AM CEST

BeginCmp
TimeStamp = /4B6EC9C3/4BAF2EAF;
Reference = BT351;
ValeurCmp = Keystone_1059_/_KZH20PCB;
IdModule  = BT_KEYSTONE_1059_20MM;
EndCmp

BeginCmp
TimeStamp = /4B6E16F2/4BAD42D5;
Reference = C101;
ValeurCmp = 100n;
IdModule  = SM0805_FIXEDMASK;
EndCmp

BeginCmp
TimeStamp = /4B6E16F2/4BAD42D8;
Reference = C102;
ValeurCmp = 100n;
IdModule  = SM0805_FIXEDMASK;
EndCmp

BeginCmp
TimeStamp = /4B6E16F2/4BAD42DA;
Reference = C103;
ValeurCmp = 100n;
IdModule  = SM0805_FIXEDMASK;
EndCmp

BeginCmp
TimeStamp = /4B6E16F2/4BFB1190;
Reference = C104;
ValeurCmp = 100n;
IdModule  = SM0805_FIXEDMASK;
EndCmp

BeginCmp
TimeStamp = /4B6E16F2/4BFB1192;
Reference = C105;
ValeurCmp = 100n;
IdModule  = SM0805_FIXEDMASK;
EndCmp

BeginCmp
TimeStamp = /4B6E16F2/4BFB1194;
Reference = C106;
ValeurCmp = 100n;
IdModule  = SM0805_FIXEDMASK;
EndCmp

BeginCmp
TimeStamp = /4B6E16F2/4BFB119A;
Reference = C111;
ValeurCmp = 100n;
IdModule  = SM0805_FIXEDMASK;
EndCmp

BeginCmp
TimeStamp = /4B6E16F2/4BFB1199;
Reference = C112;
ValeurCmp = 100n;
IdModule  = SM0805_FIXEDMASK;
EndCmp

BeginCmp
TimeStamp = /4B6E16F2/4BFB1197;
Reference = C113;
ValeurCmp = 100n;
IdModule  = SM0805_FIXEDMASK;
EndCmp

BeginCmp
TimeStamp = /4B6E16F2/4BAD42DF;
Reference = C114;
ValeurCmp = 100n;
IdModule  = SM0805_FIXEDMASK;
EndCmp

BeginCmp
TimeStamp = /4B6E16F2/4BAD42E0;
Reference = C115;
ValeurCmp = 100n;
IdModule  = SM0805_FIXEDMASK;
EndCmp

BeginCmp
TimeStamp = /4B6E16F2/4BAD42E2;
Reference = C116;
ValeurCmp = 100n;
IdModule  = SM0805_FIXEDMASK;
EndCmp

BeginCmp
TimeStamp = /4B6E18FC/4BADCE47;
Reference = C201;
ValeurCmp = 100n;
IdModule  = SM0805_FIXEDMASK;
EndCmp

BeginCmp
TimeStamp = /4B6E18FC/4BADCE62;
Reference = C202;
ValeurCmp = 100n;
IdModule  = SM0805_FIXEDMASK;
EndCmp

BeginCmp
TimeStamp = /4B6E18FC/4BADCE64;
Reference = C203;
ValeurCmp = 100n;
IdModule  = SM0805_FIXEDMASK;
EndCmp

BeginCmp
TimeStamp = /4B6E18FC/4BADCE65;
Reference = C204;
ValeurCmp = 100n;
IdModule  = SM0805_FIXEDMASK;
EndCmp

BeginCmp
TimeStamp = /4B6E18FC/4BADCE67;
Reference = C205;
ValeurCmp = 100n;
IdModule  = SM0805_FIXEDMASK;
EndCmp

BeginCmp
TimeStamp = /4B6E18FC/4BADCE6A;
Reference = C206;
ValeurCmp = 100n;
IdModule  = SM0805_FIXEDMASK;
EndCmp

BeginCmp
TimeStamp = /4B6E18FC/4BADCE6B;
Reference = C207;
ValeurCmp = 100n;
IdModule  = SM0805_FIXEDMASK;
EndCmp

BeginCmp
TimeStamp = /4B6E18FC/4BADCE6D;
Reference = C208;
ValeurCmp = 100n;
IdModule  = SM0805_FIXEDMASK;
EndCmp

BeginCmp
TimeStamp = /4B6E18FC/4BADCE74;
Reference = C210;
ValeurCmp = 100n;
IdModule  = SM0805_FIXEDMASK;
EndCmp

BeginCmp
TimeStamp = /4B6E18FC/4BADCE78;
Reference = C211;
ValeurCmp = 100n;
IdModule  = SM0805_FIXEDMASK;
EndCmp

BeginCmp
TimeStamp = /4B6E18FC/4BADCE7A;
Reference = C212;
ValeurCmp = 100n;
IdModule  = SM0805_FIXEDMASK;
EndCmp

BeginCmp
TimeStamp = /4B6E18FC/4BADCE7B;
Reference = C213;
ValeurCmp = 100n;
IdModule  = SM0805_FIXEDMASK;
EndCmp

BeginCmp
TimeStamp = /4B6E18FC/4BADCE7D;
Reference = C221;
ValeurCmp = 100n;
IdModule  = SM0805_FIXEDMASK;
EndCmp

BeginCmp
TimeStamp = /4B6E18FC/4BADCE85;
Reference = C222;
ValeurCmp = 100n;
IdModule  = SM0805_FIXEDMASK;
EndCmp

BeginCmp
TimeStamp = /4B6E18FC/4BF5A43F;
Reference = C223;
ValeurCmp = 100n;
IdModule  = SM0805_FIXEDMASK;
EndCmp

BeginCmp
TimeStamp = /4B6E18FC/4BF5A441;
Reference = C224;
ValeurCmp = 100n;
IdModule  = SM0805_FIXEDMASK;
EndCmp

BeginCmp
TimeStamp = /4B6EC9C3/4C05ACA2;
Reference = C301;
ValeurCmp = 4.7u;
IdModule  = SM0805_FIXEDMASK;
EndCmp

BeginCmp
TimeStamp = /4B6EC9C3/4C05AC9D;
Reference = C302;
ValeurCmp = 10n;
IdModule  = SM0805_FIXEDMASK;
EndCmp

BeginCmp
TimeStamp = /4B6EC9C3/4C05ACA4;
Reference = C303;
ValeurCmp = 4.7u;
IdModule  = SM0805_FIXEDMASK;
EndCmp

BeginCmp
TimeStamp = /4B6EC9C3/4C05AC9A;
Reference = C304;
ValeurCmp = 4.7u;
IdModule  = SM0805_FIXEDMASK;
EndCmp

BeginCmp
TimeStamp = /4B6EC9C3/4BABCB5C;
Reference = C311;
ValeurCmp = 4.7u;
IdModule  = SM0805_FIXEDMASK;
EndCmp

BeginCmp
TimeStamp = /4B6EC9C3/4BABCB68;
Reference = C312;
ValeurCmp = 4.7u;
IdModule  = SM0805_FIXEDMASK;
EndCmp

BeginCmp
TimeStamp = /4B6EC9C3/4BABCA9C;
Reference = C321;
ValeurCmp = 4.7u;
IdModule  = SM0805_FIXEDMASK;
EndCmp

BeginCmp
TimeStamp = /4B6EC9C3/4BABCAD2;
Reference = C322;
ValeurCmp = 4.7u;
IdModule  = SM0805_FIXEDMASK;
EndCmp

BeginCmp
TimeStamp = /4B6EC9C3/4BADC719;
Reference = C331;
ValeurCmp = 100n;
IdModule  = SM0805_FIXEDMASK;
EndCmp

BeginCmp
TimeStamp = /4B6EC9C3/4BADC720;
Reference = C341;
ValeurCmp = 100n;
IdModule  = SM0805_FIXEDMASK;
EndCmp

BeginCmp
TimeStamp = /4B6EC9C3/4C17DE31;
Reference = C342;
ValeurCmp = 1u;
IdModule  = SM0805_FIXEDMASK;
EndCmp

BeginCmp
TimeStamp = /4B6EC9C3/4BF98AA2;
Reference = C343;
ValeurCmp = 100n;
IdModule  = SM0805_FIXEDMASK;
EndCmp

BeginCmp
TimeStamp = /4B6EC9C3/4BF98AA5;
Reference = C344;
ValeurCmp = 10u;
IdModule  = SM0805_FIXEDMASK;
EndCmp

BeginCmp
TimeStamp = /4B6EC9C3/4BF98AAB;
Reference = C345;
ValeurCmp = 10u;
IdModule  = SM0805_FIXEDMASK;
EndCmp

BeginCmp
TimeStamp = /4B6EC9C3/4BF98EBE;
Reference = C346;
ValeurCmp = 3.3u;
IdModule  = SM0805_FIXEDMASK;
EndCmp

BeginCmp
TimeStamp = /4B6EC9C3/4BF98E9E;
Reference = C347;
ValeurCmp = 3,3n;
IdModule  = SM0805_FIXEDMASK;
EndCmp

BeginCmp
TimeStamp = /4B6EC9C3/4BF98EBB;
Reference = C348;
ValeurCmp = 3.3u;
IdModule  = SM0805_FIXEDMASK;
EndCmp

BeginCmp
TimeStamp = /4B6EC9C3/4BF98EBF;
Reference = C349;
ValeurCmp = 3,3n;
IdModule  = SM0805_FIXEDMASK;
EndCmp

BeginCmp
TimeStamp = /4B6ED75B/4BF6BFE1;
Reference = C401;
ValeurCmp = 100n;
IdModule  = SM0805_FIXEDMASK;
EndCmp

BeginCmp
TimeStamp = /4B6ED75B/4BF6BFE2;
Reference = C402;
ValeurCmp = 100n;
IdModule  = SM0805_FIXEDMASK;
EndCmp

BeginCmp
TimeStamp = /4B6ED75B/4BF6BFE5;
Reference = C403;
ValeurCmp = 100n;
IdModule  = SM0805_FIXEDMASK;
EndCmp

BeginCmp
TimeStamp = /4B6ED75B/4BF6BFE6;
Reference = C404;
ValeurCmp = 100n;
IdModule  = SM0805_FIXEDMASK;
EndCmp

BeginCmp
TimeStamp = /4B6ED75B/4C063C47;
Reference = C405;
ValeurCmp = 100n;
IdModule  = SM0805_FIXEDMASK;
EndCmp

BeginCmp
TimeStamp = /4B6ED75B/4BEECBC1;
Reference = C406;
ValeurCmp = 22p;
IdModule  = SM0805_FIXEDMASK;
EndCmp

BeginCmp
TimeStamp = /4B6ED75B/4BEECBCA;
Reference = C407;
ValeurCmp = 22p;
IdModule  = SM0805_FIXEDMASK;
EndCmp

BeginCmp
TimeStamp = /4B6ED75B/4BEECBCD;
Reference = C408;
ValeurCmp = 22p;
IdModule  = SM0805_FIXEDMASK;
EndCmp

BeginCmp
TimeStamp = /4B6ED75B/4BEECBD1;
Reference = C409;
ValeurCmp = 22p;
IdModule  = SM0805_FIXEDMASK;
EndCmp

BeginCmp
TimeStamp = /4B6ED75B/4BF6BFBB;
Reference = C411;
ValeurCmp = 10u;
IdModule  = SM0805_FIXEDMASK;
EndCmp

BeginCmp
TimeStamp = /4B6ED75B/4C1286D5;
Reference = C412;
ValeurCmp = 100n;
IdModule  = SM0805_FIXEDMASK;
EndCmp

BeginCmp
TimeStamp = /4BAA6ABD/4BAD3D47;
Reference = C501;
ValeurCmp = 100n;
IdModule  = SM0805_FIXEDMASK;
EndCmp

BeginCmp
TimeStamp = /4BAA6ABD/4BAD3D55;
Reference = C502;
ValeurCmp = 100n;
IdModule  = SM0805_FIXEDMASK;
EndCmp

BeginCmp
TimeStamp = /4BAA6ABD/4BAD3D53;
Reference = C511;
ValeurCmp = 100n;
IdModule  = SM0805_FIXEDMASK;
EndCmp

BeginCmp
TimeStamp = /4B6ED75B/4BF8328D;
Reference = D401;
ValeurCmp = LED_2mA_1.9V,_green;
IdModule  = LED-3MM-FIXED;
EndCmp

BeginCmp
TimeStamp = /4B6ED75B/4BF8324A;
Reference = D402;
ValeurCmp = LED_2mA_1.8V,_yellow;
IdModule  = LED-3MM-FIXED;
EndCmp

BeginCmp
TimeStamp = /4B6ED75B/4C0DA78D;
Reference = D403;
ValeurCmp = LED_2mA_1.7V,_red;
IdModule  = LED-3MM-FIXED;
EndCmp

BeginCmp
TimeStamp = /4BAA6ABD/4BF19DCA;
Reference = D511;
ValeurCmp = BAT54C;
IdModule  = SOT23EBC;
EndCmp

BeginCmp
TimeStamp = /4B6E16F2/4B6E1766;
Reference = J101;
ValeurCmp = SNESCART_EXT;
IdModule  = SNESCART_EXT;
EndCmp

BeginCmp
TimeStamp = /4B6ED75B/4BAA6A9C;
Reference = J411;
ValeurCmp = SD_CARD;
IdModule  = HRS-DM1AA;
EndCmp

BeginCmp
TimeStamp = /4B6ED75B/4BF00175;
Reference = J421;
ValeurCmp = USB_MINIB;
IdModule  = USB-MINIB-THT;
EndCmp

BeginCmp
TimeStamp = /4B6EC9C3/4C05A97C;
Reference = L301;
ValeurCmp = 1uH;
IdModule  = SM1210L_NEW;
EndCmp

BeginCmp
TimeStamp = /4B6EC9C3/4C05A983;
Reference = L302;
ValeurCmp = 1uH;
IdModule  = SM1210L_NEW;
EndCmp

BeginCmp
TimeStamp = /4B6ED75B/4C0943CA;
Reference = P401;
ValeurCmp = CONN_7X2;
IdModule  = pin_array_7x2;
EndCmp

BeginCmp
TimeStamp = /4B6ED75B/4BEFBC73;
Reference = P402;
ValeurCmp = CONN_2;
IdModule  = PIN_ARRAY_2X1;
EndCmp

BeginCmp
TimeStamp = /4B6ED75B/4C4A0B6F;
Reference = P403;
ValeurCmp = CONN_2;
IdModule  = PIN_ARRAY_2X1;
EndCmp

BeginCmp
TimeStamp = /4BAA6ABD/4BF2FD9F;
Reference = Q511;
ValeurCmp = 2N2222A;
IdModule  = SOT23EBC;
EndCmp

BeginCmp
TimeStamp = /4B6E16F2/4BAE51CA;
Reference = R101;
ValeurCmp = 220;
IdModule  = SM0805_FIXEDMASK;
EndCmp

BeginCmp
TimeStamp = /4B6E18FC/4C501B82;
Reference = R201;
ValeurCmp = 100;
IdModule  = SM0805_FIXEDMASK;
EndCmp

BeginCmp
TimeStamp = /4B6E18FC/4C501B89;
Reference = R202;
ValeurCmp = 100;
IdModule  = SM0805_FIXEDMASK;
EndCmp

BeginCmp
TimeStamp = /4B6E18FC/4C501B8C;
Reference = R203;
ValeurCmp = 100;
IdModule  = SM0805_FIXEDMASK;
EndCmp

BeginCmp
TimeStamp = /4B6EC9C3/4C42D578;
Reference = R331;
ValeurCmp = 680;
IdModule  = SM0805_FIXEDMASK;
EndCmp

BeginCmp
TimeStamp = /4B6EC9C3/4BF98EC6;
Reference = R341;
ValeurCmp = 470;
IdModule  = SM0805_FIXEDMASK;
EndCmp

BeginCmp
TimeStamp = /4B6EC9C3/4BF98EC4;
Reference = R342;
ValeurCmp = 10k;
IdModule  = SM0805_FIXEDMASK;
EndCmp

BeginCmp
TimeStamp = /4B6EC9C3/4BF98EB4;
Reference = R343;
ValeurCmp = 470;
IdModule  = SM0805_FIXEDMASK;
EndCmp

BeginCmp
TimeStamp = /4B6EC9C3/4BF98EB9;
Reference = R344;
ValeurCmp = 10k;
IdModule  = SM0805_FIXEDMASK;
EndCmp

BeginCmp
TimeStamp = /4B6ED75B/4BF847A7;
Reference = R401;
ValeurCmp = 680;
IdModule  = SM0805_FIXEDMASK;
EndCmp

BeginCmp
TimeStamp = /4B6ED75B/4BF847B1;
Reference = R402;
ValeurCmp = 680;
IdModule  = SM0805_FIXEDMASK;
EndCmp

BeginCmp
TimeStamp = /4B6ED75B/4C0DA785;
Reference = R403;
ValeurCmp = 680;
IdModule  = SM0805_FIXEDMASK;
EndCmp

BeginCmp
TimeStamp = /4B6ED75B/4C063C2F;
Reference = R404;
ValeurCmp = 10k;
IdModule  = SM0805_FIXEDMASK;
EndCmp

BeginCmp
TimeStamp = /4B6ED75B/4BF850D1;
Reference = R405;
ValeurCmp = 100;
IdModule  = SM0805_FIXEDMASK;
EndCmp

BeginCmp
TimeStamp = /4B6ED75B/4BF850A9;
Reference = R406;
ValeurCmp = 100;
IdModule  = SM0805_FIXEDMASK;
EndCmp

BeginCmp
TimeStamp = /4B6ED75B/4C5608C6;
Reference = R421;
ValeurCmp = 33;
IdModule  = SM0805_FIXEDMASK;
EndCmp

BeginCmp
TimeStamp = /4B6ED75B/4C5608C9;
Reference = R422;
ValeurCmp = 33;
IdModule  = SM0805_FIXEDMASK;
EndCmp

BeginCmp
TimeStamp = /4B6ED75B/4C01596A;
Reference = R423;
ValeurCmp = 1.5k;
IdModule  = SM0805_FIXEDMASK;
EndCmp

BeginCmp
TimeStamp = /4BAA6ABD/4BF2FDAF;
Reference = R511;
ValeurCmp = 20k;
IdModule  = SM0805_FIXEDMASK;
EndCmp

BeginCmp
TimeStamp = /4BAA6ABD/4BF2FDA9;
Reference = R512;
ValeurCmp = 4k7;
IdModule  = SM0805_FIXEDMASK;
EndCmp

BeginCmp
TimeStamp = /4BAA6ABD/4BF2FDAC;
Reference = R513;
ValeurCmp = 1k;
IdModule  = SM0805_FIXEDMASK;
EndCmp

BeginCmp
TimeStamp = /4B6E16F2/4B6E1740;
Reference = U101;
ValeurCmp = 74ALVC164245;
IdModule  = TSSOP48;
EndCmp

BeginCmp
TimeStamp = /4B6E16F2/4B6E1744;
Reference = U102;
ValeurCmp = 74ALVC164245;
IdModule  = TSSOP48;
EndCmp

BeginCmp
TimeStamp = /4B6E16F2/4B6E1748;
Reference = U103;
ValeurCmp = 74ALVC164245;
IdModule  = TSSOP48;
EndCmp

BeginCmp
TimeStamp = /4B6E16F2/4B6EB593;
Reference = U104;
ValeurCmp = 74LVC1T45;
IdModule  = SOT563;
EndCmp

BeginCmp
TimeStamp = /4B6E18FC/4B6E1931;
Reference = U201;
ValeurCmp = XC3S400-PQ208;
IdModule  = PQFP208;
EndCmp

BeginCmp
TimeStamp = /4B6EC9C3/4C05879D;
Reference = U301;
ValeurCmp = MIC23250-S4YMT;
IdModule  = QFN10-2x2;
EndCmp

BeginCmp
TimeStamp = /4B6EC9C3/4B6ED144;
Reference = U311;
ValeurCmp = MCP1824-1.8;
IdModule  = SOT23-5;
EndCmp

BeginCmp
TimeStamp = /4B6EC9C3/4B6ED134;
Reference = U321;
ValeurCmp = MCP1824-2.5;
IdModule  = SOT23-5;
EndCmp

BeginCmp
TimeStamp = /4B6EC9C3/4BAA92DB;
Reference = U331;
ValeurCmp = PIC12F629;
IdModule  = SO8N;
EndCmp

BeginCmp
TimeStamp = /4B6EC9C3/4BAA9331;
Reference = U341;
ValeurCmp = CS4344;
IdModule  = TSSOP10;
EndCmp

BeginCmp
TimeStamp = /4B6ED75B/4B6F321A;
Reference = U401;
ValeurCmp = LPC1754;
IdModule  = LQFP80-.5;
EndCmp

BeginCmp
TimeStamp = /4BAA6ABD/4B868602;
Reference = U501;
ValeurCmp = MT45W8MW16;
IdModule  = VFBGA54;
EndCmp

BeginCmp
TimeStamp = /4BAA6ABD/4B86E25C;
Reference = U511;
ValeurCmp = CY62148EV30-BVXI;
IdModule  = VFBGA36;
EndCmp

BeginCmp
TimeStamp = /4B6ED75B/4BC243C8;
Reference = X401;
ValeurCmp = 12MHz;
IdModule  = XTAL_SMD_05032;
EndCmp

BeginCmp
TimeStamp = /4B6ED75B/4BC243CB;
Reference = X402;
ValeurCmp = 32.768kHz;
IdModule  = XTAL_SMD_05019;
EndCmp

EndListe
