#
#  Copyright (c) 2015 - 2016, AMD Incorporated. All rights reserved.
#
#  SPDX-License-Identifier: BSD-2-Clause-Patent
#

################################################################################
#
# Defines Section - statements that will be processed to create a Makefile.
#
################################################################################
[Defines]

DEFINE NUM_CORES    = 4

  PLATFORM_NAME                  = Cello
  PLATFORM_GUID                  = 77861b3e-74b0-4ff3-8d18-c5ba5803e1bf
  PLATFORM_VERSION               = 0.1
  DSC_SPECIFICATION              = 0x00010005
  OUTPUT_DIRECTORY               = Build/Cello
  SUPPORTED_ARCHITECTURES        = AARCH64
  BUILD_TARGETS                  = DEBUG|RELEASE
  SKUID_IDENTIFIER               = DEFAULT
  FLASH_DEFINITION               = Platform/LeMaker/CelloBoard/CelloBoard.fdf

  #
  # Network definition
  #
  DEFINE NETWORK_IP6_ENABLE             = FALSE
  DEFINE NETWORK_TLS_ENABLE             = FALSE
  DEFINE NETWORK_HTTP_BOOT_ENABLE       = FALSE

################################################################################
#
# Library Class section - list of all Library Classes needed by this Platform.
#
################################################################################
[LibraryClasses.common]
!if $(TARGET) == RELEASE
  DebugLib|MdePkg/Library/BaseDebugLibNull/BaseDebugLibNull.inf
!else
  DebugLib|MdePkg/Library/BaseDebugLibSerialPort/BaseDebugLibSerialPort.inf
!endif
  DebugPrintErrorLevelLib|MdePkg/Library/BaseDebugPrintErrorLevelLib/BaseDebugPrintErrorLevelLib.inf

  BaseLib|MdePkg/Library/BaseLib/BaseLib.inf
  SynchronizationLib|MdePkg/Library/BaseSynchronizationLib/BaseSynchronizationLib.inf
  PerformanceLib|MdePkg/Library/BasePerformanceLibNull/BasePerformanceLibNull.inf
  ReportStatusCodeLib|MdePkg/Library/BaseReportStatusCodeLibNull/BaseReportStatusCodeLibNull.inf
  PrintLib|MdePkg/Library/BasePrintLib/BasePrintLib.inf
  PeCoffGetEntryPointLib|MdePkg/Library/BasePeCoffGetEntryPointLib/BasePeCoffGetEntryPointLib.inf
  PeCoffLib|MdePkg/Library/BasePeCoffLib/BasePeCoffLib.inf
  IoLib|MdePkg/Library/BaseIoLibIntrinsic/BaseIoLibIntrinsic.inf
  PciExpressLib|MdePkg/Library/BasePciExpressLib/BasePciExpressLib.inf
  UefiDecompressLib|MdePkg/Library/BaseUefiDecompressLib/BaseUefiDecompressLib.inf
  CpuLib|MdePkg/Library/BaseCpuLib/BaseCpuLib.inf

  UefiLib|MdePkg/Library/UefiLib/UefiLib.inf
  UefiUsbLib|MdePkg/Library/UefiUsbLib/UefiUsbLib.inf
  HobLib|MdePkg/Library/DxeHobLib/DxeHobLib.inf
  UefiRuntimeServicesTableLib|MdePkg/Library/UefiRuntimeServicesTableLib/UefiRuntimeServicesTableLib.inf
  DevicePathLib|MdePkg/Library/UefiDevicePathLibDevicePathProtocol/UefiDevicePathLibDevicePathProtocol.inf
  UefiBootServicesTableLib|MdePkg/Library/UefiBootServicesTableLib/UefiBootServicesTableLib.inf
  DxeServicesTableLib|MdePkg/Library/DxeServicesTableLib/DxeServicesTableLib.inf
  UefiDriverEntryPoint|MdePkg/Library/UefiDriverEntryPoint/UefiDriverEntryPoint.inf
  UefiApplicationEntryPoint|MdePkg/Library/UefiApplicationEntryPoint/UefiApplicationEntryPoint.inf
  HiiLib|MdeModulePkg/Library/UefiHiiLib/UefiHiiLib.inf
  UefiHiiServicesLib|MdeModulePkg/Library/UefiHiiServicesLib/UefiHiiServicesLib.inf

  UefiRuntimeLib|MdePkg/Library/UefiRuntimeLib/UefiRuntimeLib.inf

  #
  # Allow dynamic PCDs
  #
  PcdLib|MdePkg/Library/DxePcdLib/DxePcdLib.inf
  PeiServicesLib|MdePkg/Library/PeiServicesLib/PeiServicesLib.inf

  BaseMemoryLib|MdePkg/Library/BaseMemoryLibOptDxe/BaseMemoryLibOptDxe.inf

  # ARM Architectural Libraries
  CacheMaintenanceLib|ArmPkg/Library/ArmCacheMaintenanceLib/ArmCacheMaintenanceLib.inf
  DefaultExceptionHandlerLib|ArmPkg/Library/DefaultExceptionHandlerLib/DefaultExceptionHandlerLib.inf
  CpuExceptionHandlerLib|ArmPkg/Library/ArmExceptionLib/ArmExceptionLib.inf
  ArmDisassemblerLib|ArmPkg/Library/ArmDisassemblerLib/ArmDisassemblerLib.inf
  ArmGicLib|ArmPkg/Drivers/ArmGic/ArmGicLib.inf
  ArmGicArchLib|ArmPkg/Library/ArmGicArchLib/ArmGicArchLib.inf
  ArmPlatformStackLib|ArmPlatformPkg/Library/ArmPlatformStackLib/ArmPlatformStackLib.inf
  ArmSmcLib|ArmPkg/Library/ArmSmcLib/ArmSmcLib.inf
  ArmGenericTimerCounterLib|ArmPkg/Library/ArmGenericTimerPhyCounterLib/ArmGenericTimerPhyCounterLib.inf
  PlatformPeiLib|ArmPlatformPkg/PlatformPei/PlatformPeiLib.inf

  ArmLib|ArmPkg/Library/ArmLib/ArmBaseLib.inf
  ArmMmuLib|ArmPkg/Library/ArmMmuLib/ArmMmuBaseLib.inf
  ArmPlatformLib|Silicon/AMD/Styx/Library/AmdStyxLib/AmdStyxLib.inf
  TimerLib|ArmPkg/Library/ArmArchTimerLib/ArmArchTimerLib.inf
  UefiScsiLib|MdePkg/Library/UefiScsiLib/UefiScsiLib.inf

  # ARM PL011 UART Driver
  PL011UartClockLib|ArmPlatformPkg/Library/PL011UartClockLib/PL011UartClockLib.inf
  PL011UartLib|ArmPlatformPkg/Library/PL011UartLib/PL011UartLib.inf
  SerialPortLib|ArmPlatformPkg/Library/PL011SerialPortLib/PL011SerialPortLib.inf

  #
  # PCI support
  #
  PciSegmentLib|MdePkg/Library/BasePciSegmentLibPci/BasePciSegmentLibPci.inf
  PciLib|MdePkg/Library/BasePciLibPciExpress/BasePciLibPciExpress.inf
  PciHostBridgeLib|Silicon/AMD/Styx/Library/AmdStyxPciHostBridgeLib/AmdStyxPciHostBridgeLib.inf

  #
  # Styx specific libraries
  #
  AmdSataInit|Silicon/AMD/Styx/AmdModulePkg/Library/AmdSataInitLib/AmdSataInitLib.inf
  ResetSystemLib|ArmPkg/Library/ArmSmcPsciResetSystemLib/ArmSmcPsciResetSystemLib.inf
  RealTimeClockLib|Silicon/AMD/Styx/Library/RealTimeClockLib/RealTimeClockLib.inf

  CapsuleLib|MdeModulePkg/Library/DxeCapsuleLibNull/DxeCapsuleLibNull.inf
  UefiBootManagerLib|MdeModulePkg/Library/UefiBootManagerLib/UefiBootManagerLib.inf
  BootLogoLib|MdeModulePkg/Library/BootLogoLib/BootLogoLib.inf
  PlatformBootManagerLib|ArmPkg/Library/PlatformBootManagerLib/PlatformBootManagerLib.inf
  CustomizedDisplayLib|MdeModulePkg/Library/CustomizedDisplayLib/CustomizedDisplayLib.inf

  #
  # Uncomment (and comment out the next line) For RealView Debugger. The Standard IO window
  # in the debugger will show load and unload commands for symbols. You can cut and paste this
  # into the command window to load symbols. We should be able to use a script to do this, but
  # the version of RVD I have does not support scripts accessing system memory.
  #
  #PeCoffExtraActionLib|ArmPkg/Library/RvdPeCoffExtraActionLib/RvdPeCoffExtraActionLib.inf
  PeCoffExtraActionLib|ArmPkg/Library/DebugPeCoffExtraActionLib/DebugPeCoffExtraActionLib.inf
  #PeCoffExtraActionLib|MdePkg/Library/BasePeCoffExtraActionLibNull/BasePeCoffExtraActionLibNull.inf

  DebugAgentLib|MdeModulePkg/Library/DebugAgentLibNull/DebugAgentLibNull.inf
  DebugAgentTimerLib|EmbeddedPkg/Library/DebugAgentTimerLibNull/DebugAgentTimerLibNull.inf

  DxeServicesLib|MdePkg/Library/DxeServicesLib/DxeServicesLib.inf
  SortLib|MdeModulePkg/Library/UefiSortLib/UefiSortLib.inf
  FileExplorerLib|MdeModulePkg/Library/FileExplorerLib/FileExplorerLib.inf

  IntrinsicLib|CryptoPkg/Library/IntrinsicLib/IntrinsicLib.inf
  OpensslLib|CryptoPkg/Library/OpensslLib/OpensslLib.inf
  BaseCryptLib|CryptoPkg/Library/BaseCryptLib/BaseCryptLib.inf

[LibraryClasses.common.SEC]
  HobLib|MdePkg/Library/PeiHobLib/PeiHobLib.inf
  PeiServicesTablePointerLib|ArmPkg/Library/PeiServicesTablePointerLib/PeiServicesTablePointerLib.inf
  MemoryAllocationLib|MdePkg/Library/PeiMemoryAllocationLib/PeiMemoryAllocationLib.inf

  PcdLib|MdePkg/Library/BasePcdLibNull/BasePcdLibNull.inf
  ArmPlatformLib|Silicon/AMD/Styx/Library/AmdStyxLib/AmdStyxLibSec.inf

  DebugAgentLib|ArmPkg/Library/DebugAgentSymbolsBaseLib/DebugAgentSymbolsBaseLib.inf

  ArmGicArchLib|ArmPkg/Library/ArmGicArchSecLib/ArmGicArchSecLib.inf

[LibraryClasses.common.PEIM, LibraryClasses.common.SEC]
  MemoryInitPeiLib|Silicon/AMD/Styx/Library/MemoryInitPei/MemoryInitPeiLib.inf
  BaseMemoryLib|MdePkg/Library/BaseMemoryLib/BaseMemoryLib.inf

[LibraryClasses.common.PEI_CORE]
  BaseMemoryLib|MdePkg/Library/BaseMemoryLib/BaseMemoryLib.inf
  PcdLib|MdePkg/Library/PeiPcdLib/PeiPcdLib.inf
  HobLib|MdePkg/Library/PeiHobLib/PeiHobLib.inf
  MemoryAllocationLib|MdePkg/Library/PeiMemoryAllocationLib/PeiMemoryAllocationLib.inf
  PeiCoreEntryPoint|MdePkg/Library/PeiCoreEntryPoint/PeiCoreEntryPoint.inf
  PerformanceLib|MdeModulePkg/Library/PeiPerformanceLib/PeiPerformanceLib.inf
  OemHookStatusCodeLib|MdeModulePkg/Library/OemHookStatusCodeLibNull/OemHookStatusCodeLibNull.inf
  PeCoffGetEntryPointLib|MdePkg/Library/BasePeCoffGetEntryPointLib/BasePeCoffGetEntryPointLib.inf
  ExtractGuidedSectionLib|MdePkg/Library/PeiExtractGuidedSectionLib/PeiExtractGuidedSectionLib.inf

  PeiServicesTablePointerLib|ArmPkg/Library/PeiServicesTablePointerLib/PeiServicesTablePointerLib.inf

[LibraryClasses.common.PEIM]
  PcdLib|MdePkg/Library/PeiPcdLib/PeiPcdLib.inf
  HobLib|MdePkg/Library/PeiHobLib/PeiHobLib.inf
  MemoryAllocationLib|MdePkg/Library/PeiMemoryAllocationLib/PeiMemoryAllocationLib.inf
  PeimEntryPoint|MdePkg/Library/PeimEntryPoint/PeimEntryPoint.inf
  PerformanceLib|MdeModulePkg/Library/PeiPerformanceLib/PeiPerformanceLib.inf
  OemHookStatusCodeLib|MdeModulePkg/Library/OemHookStatusCodeLibNull/OemHookStatusCodeLibNull.inf
  PeCoffGetEntryPointLib|MdePkg/Library/BasePeCoffGetEntryPointLib/BasePeCoffGetEntryPointLib.inf
  PeiResourcePublicationLib|MdePkg/Library/PeiResourcePublicationLib/PeiResourcePublicationLib.inf
  ExtractGuidedSectionLib|MdePkg/Library/PeiExtractGuidedSectionLib/PeiExtractGuidedSectionLib.inf

  PeiServicesTablePointerLib|ArmPkg/Library/PeiServicesTablePointerLib/PeiServicesTablePointerLib.inf

[LibraryClasses.common.DXE_CORE]
  HobLib|MdePkg/Library/DxeCoreHobLib/DxeCoreHobLib.inf
  MemoryAllocationLib|MdeModulePkg/Library/DxeCoreMemoryAllocationLib/DxeCoreMemoryAllocationLib.inf
  DxeCoreEntryPoint|MdePkg/Library/DxeCoreEntryPoint/DxeCoreEntryPoint.inf
  ExtractGuidedSectionLib|MdePkg/Library/DxeExtractGuidedSectionLib/DxeExtractGuidedSectionLib.inf
  PerformanceLib|MdeModulePkg/Library/DxeCorePerformanceLib/DxeCorePerformanceLib.inf

[LibraryClasses.common.DXE_DRIVER]
  SecurityManagementLib|MdeModulePkg/Library/DxeSecurityManagementLib/DxeSecurityManagementLib.inf
  PerformanceLib|MdeModulePkg/Library/DxePerformanceLib/DxePerformanceLib.inf
  MemoryAllocationLib|MdePkg/Library/UefiMemoryAllocationLib/UefiMemoryAllocationLib.inf
  NonDiscoverableDeviceRegistrationLib|MdeModulePkg/Library/NonDiscoverableDeviceRegistrationLib/NonDiscoverableDeviceRegistrationLib.inf

[LibraryClasses.common.DXE_RUNTIME_DRIVER]
  HobLib|MdePkg/Library/DxeHobLib/DxeHobLib.inf
  MemoryAllocationLib|MdePkg/Library/UefiMemoryAllocationLib/UefiMemoryAllocationLib.inf
  CapsuleLib|MdeModulePkg/Library/DxeCapsuleLibNull/DxeCapsuleLibNull.inf
!if $(TARGET) != RELEASE
  DebugLib|MdePkg/Library/DxeRuntimeDebugLibSerialPort/DxeRuntimeDebugLibSerialPort.inf
!endif

[LibraryClasses.common.UEFI_APPLICATION]
  PerformanceLib|MdeModulePkg/Library/DxePerformanceLib/DxePerformanceLib.inf
  MemoryAllocationLib|MdePkg/Library/UefiMemoryAllocationLib/UefiMemoryAllocationLib.inf
  HiiLib|MdeModulePkg/Library/UefiHiiLib/UefiHiiLib.inf

[LibraryClasses.common.UEFI_DRIVER]
  ExtractGuidedSectionLib|MdePkg/Library/DxeExtractGuidedSectionLib/DxeExtractGuidedSectionLib.inf
  PerformanceLib|MdeModulePkg/Library/DxePerformanceLib/DxePerformanceLib.inf
  MemoryAllocationLib|MdePkg/Library/UefiMemoryAllocationLib/UefiMemoryAllocationLib.inf

[LibraryClasses.ARM]
  #
  # It is not possible to prevent the ARM compiler for generic intrinsic functions.
  # This library provides the instrinsic functions generate by a given compiler.
  # [LibraryClasses.ARM] and NULL mean link this library into all ARM images.
  #
  NULL|ArmPkg/Library/CompilerIntrinsicsLib/CompilerIntrinsicsLib.inf

[LibraryClasses.AARCH64]
  NULL|ArmPkg/Library/CompilerIntrinsicsLib/CompilerIntrinsicsLib.inf
  NULL|MdePkg/Library/BaseStackCheckLib/BaseStackCheckLib.inf

###################################################################################################
# BuildOptions Section - Define the module specific tool chain flags that should be used as
#                        the default flags for a module. These flags are appended to any
#                        standard flags that are defined by the build process.
###################################################################################################

[BuildOptions]
  RVCT:RELEASE_*_*_CC_FLAGS  = -DMDEPKG_NDEBUG
  GCC:RELEASE_*_*_CC_FLAGS  = -DMDEPKG_NDEBUG

[BuildOptions.common.EDKII.DXE_RUNTIME_DRIVER]
  GCC:*_*_AARCH64_DLINK_FLAGS = -z common-page-size=0x10000

[BuildOptions.common.EDKII.DXE_DRIVER,BuildOptions.common.EDKII.UEFI_DRIVER,BuildOptions.common.EDKII.UEFI_APPLICATION]
  GCC:*_*_AARCH64_DLINK_FLAGS = -z common-page-size=0x1000

################################################################################
#
# Pcd Section - list of all EDK II PCD Entries defined by this Platform
#
################################################################################

[PcdsFeatureFlag.common]
  # Use the Vector Table location in CpuDxe. We will not copy the Vector Table at PcdCpuVectorBaseAddress
  gArmTokenSpaceGuid.PcdRelocateVectorTable|FALSE

  gEmbeddedTokenSpaceGuid.PcdPrePiProduceMemoryTypeInformationHob|TRUE

  gEfiMdeModulePkgTokenSpaceGuid.PcdTurnOffUsbLegacySupport|TRUE

  ## If TRUE, Graphics Output Protocol will be installed on virtual handle
  ## created by ConsplitterDxe. It could be set FALSE to save size.
  gEfiMdeModulePkgTokenSpaceGuid.PcdConOutGopSupport|FALSE

[PcdsFixedAtBuild.common]
  gEfiMdePkgTokenSpaceGuid.PcdMaximumUnicodeStringLength|1000000
  gEfiMdePkgTokenSpaceGuid.PcdMaximumAsciiStringLength|1000000
  gEfiMdePkgTokenSpaceGuid.PcdMaximumLinkedListLength|1000000
  gEfiMdePkgTokenSpaceGuid.PcdSpinLockTimeout|10000000
  gEfiMdePkgTokenSpaceGuid.PcdDebugClearMemoryValue|0xAF
  gEfiMdePkgTokenSpaceGuid.PcdPerformanceLibraryPropertyMask|1
  gEfiMdePkgTokenSpaceGuid.PcdPostCodePropertyMask|0
  gEfiMdePkgTokenSpaceGuid.PcdUefiLibMaxPrintBufferSize|320

  # DEBUG_ASSERT_ENABLED       0x01
  # DEBUG_PRINT_ENABLED        0x02
  # DEBUG_CODE_ENABLED         0x04
  # CLEAR_MEMORY_ENABLED       0x08
  # ASSERT_BREAKPOINT_ENABLED  0x10
  # ASSERT_DEADLOOP_ENABLED    0x20
!if $(TARGET) == RELEASE
  gEfiMdePkgTokenSpaceGuid.PcdDebugPropertyMask|0x21
!else
  gEfiMdePkgTokenSpaceGuid.PcdDebugPropertyMask|0x2f
!endif

  #  DEBUG_INIT      0x00000001  // Initialization
  #  DEBUG_WARN      0x00000002  // Warnings
  #  DEBUG_LOAD      0x00000004  // Load events
  #  DEBUG_FS        0x00000008  // EFI File system
  #  DEBUG_POOL      0x00000010  // Alloc & Free's
  #  DEBUG_PAGE      0x00000020  // Alloc & Free's
  #  DEBUG_INFO      0x00000040  // Verbose
  #  DEBUG_DISPATCH  0x00000080  // PEI/DXE Dispatchers
  #  DEBUG_VARIABLE  0x00000100  // Variable
  #  DEBUG_BM        0x00000400  // Boot Manager
  #  DEBUG_BLKIO     0x00001000  // BlkIo Driver
  #  DEBUG_NET       0x00004000  // SNI Driver
  #  DEBUG_UNDI      0x00010000  // UNDI Driver
  #  DEBUG_LOADFILE  0x00020000  // UNDI Driver
  #  DEBUG_EVENT     0x00080000  // Event messages
  #  DEBUG_GCD       0x00100000  // Global Coherency Database changes
  #  DEBUG_CACHE     0x00200000  // Memory range cachability changes
  #  DEBUG_ERROR     0x80000000  // Error
  gEfiMdePkgTokenSpaceGuid.PcdDebugPrintErrorLevel|0x8000000F

  gEfiMdePkgTokenSpaceGuid.PcdReportStatusCodePropertyMask|0x07

  #
  # Optional feature to help prevent EFI memory map fragments
  # Turned on and off via: PcdPrePiProduceMemoryTypeInformationHob
  # Values are in EFI Pages (4K). DXE Core will make sure that
  # at least this much of each type of memory can be allocated
  # from a single memory range. This way you only end up with
  # maximum of two fragements for each type in the memory map
  # (the memory used, and the free memory that was prereserved
  # but not used).
  #
  gEmbeddedTokenSpaceGuid.PcdMemoryTypeEfiACPIReclaimMemory|0
  gEmbeddedTokenSpaceGuid.PcdMemoryTypeEfiACPIMemoryNVS|0
  gEmbeddedTokenSpaceGuid.PcdMemoryTypeEfiReservedMemoryType|0
  gEmbeddedTokenSpaceGuid.PcdMemoryTypeEfiRuntimeServicesData|1000
  gEmbeddedTokenSpaceGuid.PcdMemoryTypeEfiRuntimeServicesCode|1000
  gEmbeddedTokenSpaceGuid.PcdMemoryTypeEfiBootServicesCode|400
  gEmbeddedTokenSpaceGuid.PcdMemoryTypeEfiBootServicesData|12000
  gEmbeddedTokenSpaceGuid.PcdMemoryTypeEfiLoaderCode|20
  gEmbeddedTokenSpaceGuid.PcdMemoryTypeEfiLoaderData|0

  gEfiMdeModulePkgTokenSpaceGuid.PcdResetOnMemoryTypeInformationChange|FALSE
  gEfiMdeModulePkgTokenSpaceGuid.PcdBootManagerMenuFile|{ 0x21, 0xaa, 0x2c, 0x46, 0x14, 0x76, 0x03, 0x45, 0x83, 0x6e, 0x8a, 0xb6, 0xf4, 0x66, 0x23, 0x31 }

!ifdef $(FIRMWARE_VENDOR)
  gEfiMdeModulePkgTokenSpaceGuid.PcdFirmwareVendor|L"$(FIRMWARE_VENDOR)"
!endif

  # Number of configured cores
  gArmPlatformTokenSpaceGuid.PcdCoreCount|$(NUM_CORES)

  # Stacks for MPCores in Normal World
  gArmPlatformTokenSpaceGuid.PcdCPUCoresStackBase|0x8001680000
  gArmPlatformTokenSpaceGuid.PcdCPUCorePrimaryStackSize|0x10000
  gArmPlatformTokenSpaceGuid.PcdCPUCoreSecondaryStackSize|0x800

  # Declare system memory base
  gArmTokenSpaceGuid.PcdSystemMemoryBase|0x8000000000

  # Size of the region used by UEFI in permanent memory (Reserved 64MB)
  gArmPlatformTokenSpaceGuid.PcdSystemMemoryUefiRegionSize|0x04000000

  #
  # ARM PrimeCell
  #

  ## PL011 - Serial Terminal (Atlas UART)
  gEfiMdeModulePkgTokenSpaceGuid.PcdSerialRegisterBase|0x0E1010000
  gEfiMdePkgTokenSpaceGuid.PcdUartDefaultBaudRate|115200
  gEfiMdePkgTokenSpaceGuid.PcdUartDefaultReceiveFifoDepth|0
  # serial port is clocked at 100MHz
  gArmPlatformTokenSpaceGuid.PL011UartClkInHz|100000000
  gEfiMdePkgTokenSpaceGuid.PcdDefaultTerminalType|4

  gAmdStyxTokenSpaceGuid.PcdSerialDbgRegisterBase|0x0E1010000
  gAmdStyxTokenSpaceGuid.PcdUartDbgBaudRate|115200

  #
  # ARM General Interrupt Controller
  #
  gArmTokenSpaceGuid.PcdGicDistributorBase|0xE1110000
  gArmTokenSpaceGuid.PcdGicInterruptInterfaceBase|0xE112F000

  #
  # Cello has 2 SATA ports on the first controller.
  #
  gAmdStyxTokenSpaceGuid.PcdSata0PortCount|2
  gAmdStyxTokenSpaceGuid.PcdSata1PortCount|0
  gAmdStyxTokenSpaceGuid.PcdSataPortMode|0xf

  # PCIe Support
  gEfiMdePkgTokenSpaceGuid.PcdPciExpressBaseAddress|0xF0000000

  gArmTokenSpaceGuid.PcdPciBusMin|0x0
  gArmTokenSpaceGuid.PcdPciBusMax|0xFF

  gArmTokenSpaceGuid.PcdPciIoBase|0x1000
  gArmTokenSpaceGuid.PcdPciIoSize|0xF000
  gArmTokenSpaceGuid.PcdPciIoTranslation|0xEFFF0000
  gEmbeddedTokenSpaceGuid.PcdPrePiCpuIoSize|16

  gArmTokenSpaceGuid.PcdPciMmio32Base|0x40000000
  gArmTokenSpaceGuid.PcdPciMmio32Size|0x80000000
  gArmTokenSpaceGuid.PcdPciMmio32Translation|0x0

  gArmTokenSpaceGuid.PcdPciMmio64Base|0x100000000
  gArmTokenSpaceGuid.PcdPciMmio64Size|0x7F00000000
  gArmTokenSpaceGuid.PcdPciMmio64Translation|0x0

  ## ACPI (no tables < 4GB)
  gEfiMdeModulePkgTokenSpaceGuid.PcdAcpiExposedTableVersions|0x20

  #
  # Enable strict image permissions for all images. (This applies
  # only to images that were built with >= 4 KB section alignment.)
  #
  gEfiMdeModulePkgTokenSpaceGuid.PcdImageProtectionPolicy|0x3

  #
  # Enable NX memory protection for all non-code regions, including OEM and OS
  # reserved ones, with the exception of LoaderData regions, of which OS loaders
  # (i.e., GRUB) may assume that its contents are executable.
  #
  gEfiMdeModulePkgTokenSpaceGuid.PcdDxeNxMemoryProtectionPolicy|0xC000000000007FD1

  # SMBIOS 3.0 only
  gEfiMdeModulePkgTokenSpaceGuid.PcdSmbiosEntryPointProvideMethod|0x2

  gAmdModulePkgTokenSpaceGuid.PcdSataNumChPerSerdes|2
  gAmdModulePkgTokenSpaceGuid.PcdSataSerdesBase|0xE1200000
  gAmdModulePkgTokenSpaceGuid.PcdSataSerdesOffset|0x00010000

  # map the stack as non-executable when entering the DXE phase
  gEfiMdeModulePkgTokenSpaceGuid.PcdSetNxForStack|TRUE

[PcdsPatchableInModule]
# PCIe Configuration: x4x2x2
  gAmdModulePkgTokenSpaceGuid.PcdPcieCoreConfiguration|2
  gAmdModulePkgTokenSpaceGuid.PcdPciePort0Present|1
  gAmdModulePkgTokenSpaceGuid.PcdPciePort1Present|1
  gAmdModulePkgTokenSpaceGuid.PcdPciePort2Present|1
  gAmdModulePkgTokenSpaceGuid.PcdPcieHardcodeEnumeration|TRUE

[PcdsDynamicDefault.common]
  gAmdStyxTokenSpaceGuid.PcdSocCoreCount|$(NUM_CORES)
  gArmTokenSpaceGuid.PcdSystemMemorySize|0x0400000000

  gEfiMdeModulePkgTokenSpaceGuid.PcdFlashNvStorageVariableBase64|0x0
  gEfiMdeModulePkgTokenSpaceGuid.PcdFlashNvStorageFtwWorkingBase64|0x0
  gEfiMdeModulePkgTokenSpaceGuid.PcdFlashNvStorageFtwSpareBase64|0x0

[PcdsDynamicHii]
  gEfiMdePkgTokenSpaceGuid.PcdPlatformBootTimeOut|L"Timeout"|gEfiGlobalVariableGuid|0x0|5

  gAmdStyxTokenSpaceGuid.PcdEnableSmmus|L"StyxEnableSmmus"|gAmdStyxVariableGuid|0x0|FALSE

################################################################################
#
# Components Section - list of all EDK II Modules needed by this Platform
#
################################################################################
[Components.common]

  #
  # PEI Phase modules
  #
  ArmPlatformPkg/PrePeiCore/PrePeiCoreUniCore.inf
  MdeModulePkg/Core/Pei/PeiMain.inf
  MdeModulePkg/Universal/PCD/Pei/Pcd.inf {
    <LibraryClasses>
      PcdLib|MdePkg/Library/BasePcdLibNull/BasePcdLibNull.inf
  }
  ArmPlatformPkg/PlatformPei/PlatformPeim.inf
  Silicon/AMD/Styx/AmdModulePkg/Iscp/IscpPei.inf
  Silicon/AMD/Styx/Drivers/PlatInitPei/PlatInitPei.inf
  ArmPlatformPkg/MemoryInitPei/MemoryInitPeim.inf
  ArmPkg/Drivers/CpuPei/CpuPei.inf
  MdeModulePkg/Universal/Variable/Pei/VariablePei.inf
  MdeModulePkg/Core/DxeIplPeim/DxeIpl.inf {
    <LibraryClasses>
      NULL|MdeModulePkg/Library/LzmaCustomDecompressLib/LzmaCustomDecompressLib.inf
  }

  #
  # DXE
  #
  MdeModulePkg/Core/Dxe/DxeMain.inf {
    <LibraryClasses>
      DevicePathLib|MdePkg/Library/UefiDevicePathLib/UefiDevicePathLib.inf
      NULL|MdeModulePkg/Library/DxeCrc32GuidedSectionExtractLib/DxeCrc32GuidedSectionExtractLib.inf
  }
  MdeModulePkg/Universal/PCD/Dxe/Pcd.inf {
    <LibraryClasses>
      PcdLib|MdePkg/Library/BasePcdLibNull/BasePcdLibNull.inf
  }
  MdeModulePkg/Universal/DevicePathDxe/DevicePathDxe.inf {
    <LibraryClasses>
      DevicePathLib|MdePkg/Library/UefiDevicePathLib/UefiDevicePathLib.inf
      PcdLib|MdePkg/Library/BasePcdLibNull/BasePcdLibNull.inf
  }

  #
  # Architectural Protocols
  #
  ArmPkg/Drivers/CpuDxe/CpuDxe.inf
  MdeModulePkg/Core/RuntimeDxe/RuntimeDxe.inf
  MdeModulePkg/Universal/SecurityStubDxe/SecurityStubDxe.inf
  MdeModulePkg/Universal/CapsuleRuntimeDxe/CapsuleRuntimeDxe.inf
  MdeModulePkg/Universal/FaultTolerantWriteDxe/FaultTolerantWriteDxe.inf
  MdeModulePkg/Universal/MonotonicCounterRuntimeDxe/MonotonicCounterRuntimeDxe.inf
  MdeModulePkg/Universal/ResetSystemRuntimeDxe/ResetSystemRuntimeDxe.inf
  EmbeddedPkg/RealTimeClockRuntimeDxe/RealTimeClockRuntimeDxe.inf
  EmbeddedPkg/MetronomeDxe/MetronomeDxe.inf
  MdeModulePkg/Universal/EbcDxe/EbcDxe.inf

  #
  # Console IO support
  #
  MdeModulePkg/Universal/Console/TerminalDxe/TerminalDxe.inf
  MdeModulePkg/Universal/SerialDxe/SerialDxe.inf

  MdeModulePkg/Universal/HiiDatabaseDxe/HiiDatabaseDxe.inf
  MdeModulePkg/Universal/WatchdogTimerDxe/WatchdogTimer.inf

  ArmPkg/Drivers/ArmGic/ArmGicDxe.inf
  ArmPkg/Drivers/TimerDxe/TimerDxe.inf

  #
  # Environment Variables Protocol
  #
  MdeModulePkg/Universal/Variable/RuntimeDxe/VariableRuntimeDxe.inf {
    <LibraryClasses>
      AuthVariableLib|MdeModulePkg/Library/AuthVariableLibNull/AuthVariableLibNull.inf
      TpmMeasurementLib|MdeModulePkg/Library/TpmMeasurementLibNull/TpmMeasurementLibNull.inf
      VarCheckLib|MdeModulePkg/Library/VarCheckLib/VarCheckLib.inf
      NULL|MdeModulePkg/Library/VarCheckUefiLib/VarCheckUefiLib.inf
  }
  Silicon/AMD/Styx/Drivers/StyxSpiFvDxe/StyxSpiFvDxe.inf

  #
  # Iscp support
  #
  Silicon/AMD/Styx/AmdModulePkg/Iscp/IscpDxe.inf

  #
  # FDT support
  #
  EmbeddedPkg/Drivers/DtPlatformDxe/DtPlatformDxe.inf {
    <LibraryClasses>
      FdtLib|EmbeddedPkg/Library/FdtLib/FdtLib.inf
      DtPlatformDtbLoaderLib|Silicon/AMD/Styx/Library/StyxDtbLoaderLib/StyxDtbLoaderLib.inf
  }
  Platform/AMD/OverdriveBoard/DeviceTree/OverdriveBoard.inf

  #
  # PCI support
  #
  Silicon/AMD/Styx/AmdModulePkg/Gionb/Gionb.inf
  ArmPkg/Drivers/ArmPciCpuIo2Dxe/ArmPciCpuIo2Dxe.inf
  MdeModulePkg/Bus/Pci/PciHostBridgeDxe/PciHostBridgeDxe.inf
  MdeModulePkg/Bus/Pci/PciBusDxe/PciBusDxe.inf

  #
  # AHCI Support
  #
  MdeModulePkg/Bus/Ata/AtaAtapiPassThru/AtaAtapiPassThru.inf
  MdeModulePkg/Bus/Ata/AtaBusDxe/AtaBusDxe.inf
  MdeModulePkg/Bus/Scsi/ScsiBusDxe/ScsiBusDxe.inf
  MdeModulePkg/Bus/Scsi/ScsiDiskDxe/ScsiDiskDxe.inf
  MdeModulePkg/Bus/Pci/SataControllerDxe/SataControllerDxe.inf
  MdeModulePkg/Bus/Pci/NonDiscoverablePciDeviceDxe/NonDiscoverablePciDeviceDxe.inf
  Silicon/AMD/Styx/Drivers/StyxSataPlatformDxe/StyxSataPlatformDxe.inf

  #
  # USB Support
  #
  MdeModulePkg/Bus/Pci/UhciDxe/UhciDxe.inf
  MdeModulePkg/Bus/Pci/EhciDxe/EhciDxe.inf
  MdeModulePkg/Bus/Pci/XhciDxe/XhciDxe.inf
  MdeModulePkg/Bus/Usb/UsbBusDxe/UsbBusDxe.inf
  MdeModulePkg/Bus/Usb/UsbMassStorageDxe/UsbMassStorageDxe.inf

  #
  # Networking stack
  #
!include NetworkPkg/Network.dsc.inc

  #
  # Core Info
  #
  Silicon/AMD/Styx/Drivers/PlatInitDxe/PlatInitDxe.inf

  #
  # ACPI Support
  #
  MdeModulePkg/Universal/Acpi/AcpiTableDxe/AcpiTableDxe.inf {
    <LibraryClasses>
      NULL|EmbeddedPkg/Library/PlatformHasAcpiLib/PlatformHasAcpiLib.inf
  }
  Silicon/AMD/Styx/Drivers/AcpiPlatformDxe/AcpiPlatformDxe.inf

  #
  # SMBIOS Support
  #
  MdeModulePkg/Universal/SmbiosDxe/SmbiosDxe.inf
  Silicon/AMD/Styx/Drivers/PlatformSmbiosDxe/PlatformSmbiosDxe.inf

  #
  # FAT filesystem + GPT/MBR partitioning
  #
  MdeModulePkg/Universal/Disk/DiskIoDxe/DiskIoDxe.inf
  MdeModulePkg/Universal/Disk/PartitionDxe/PartitionDxe.inf
  FatPkg/EnhancedFatDxe/Fat.inf
  MdeModulePkg/Universal/Disk/UnicodeCollation/EnglishDxe/EnglishDxe.inf

  #
  # Bds
  #
  MdeModulePkg/Universal/DisplayEngineDxe/DisplayEngineDxe.inf
  MdeModulePkg/Universal/SetupBrowserDxe/SetupBrowserDxe.inf
  MdeModulePkg/Universal/BdsDxe/BdsDxe.inf
  MdeModulePkg/Application/UiApp/UiApp.inf {
    <LibraryClasses>
      NULL|MdeModulePkg/Library/DeviceManagerUiLib/DeviceManagerUiLib.inf
      NULL|MdeModulePkg/Library/BootManagerUiLib/BootManagerUiLib.inf
      NULL|MdeModulePkg/Library/BootMaintenanceManagerUiLib/BootMaintenanceManagerUiLib.inf
  }

  #
  # Crypto Accelerator support (RNG only)
  #
  Silicon/AMD/Styx/Drivers/StyxRngDxe/StyxRngDxe.inf

  #
  # UEFI application (Shell Embedded Boot Loader)
  #
  ShellPkg/Application/Shell/Shell.inf {
    <LibraryClasses>
      ShellCommandLib|ShellPkg/Library/UefiShellCommandLib/UefiShellCommandLib.inf
      NULL|ShellPkg/Library/UefiShellLevel2CommandsLib/UefiShellLevel2CommandsLib.inf
      NULL|ShellPkg/Library/UefiShellLevel1CommandsLib/UefiShellLevel1CommandsLib.inf
      NULL|ShellPkg/Library/UefiShellLevel3CommandsLib/UefiShellLevel3CommandsLib.inf
      NULL|ShellPkg/Library/UefiShellDriver1CommandsLib/UefiShellDriver1CommandsLib.inf
      NULL|ShellPkg/Library/UefiShellDebug1CommandsLib/UefiShellDebug1CommandsLib.inf
      NULL|ShellPkg/Library/UefiShellInstall1CommandsLib/UefiShellInstall1CommandsLib.inf
      NULL|ShellPkg/Library/UefiShellNetwork1CommandsLib/UefiShellNetwork1CommandsLib.inf
      NULL|ShellPkg/Library/UefiShellAcpiViewCommandLib/UefiShellAcpiViewCommandLib.inf
      HandleParsingLib|ShellPkg/Library/UefiHandleParsingLib/UefiHandleParsingLib.inf
      PrintLib|MdePkg/Library/BasePrintLib/BasePrintLib.inf
      BcfgCommandLib|ShellPkg/Library/UefiShellBcfgCommandLib/UefiShellBcfgCommandLib.inf

      FileHandleLib|MdePkg/Library/UefiFileHandleLib/UefiFileHandleLib.inf
      ShellLib|ShellPkg/Library/UefiShellLib/UefiShellLib.inf

    <PcdsFixedAtBuild>
      gEfiMdePkgTokenSpaceGuid.PcdDebugPropertyMask|0xFF
      gEfiShellPkgTokenSpaceGuid.PcdShellLibAutoInitialize|FALSE
      gEfiMdePkgTokenSpaceGuid.PcdUefiLibMaxPrintBufferSize|8000
  }

!ifdef $(RENESAS_XHCI_FW_DIR)
  OpenPlatformPkg/Drivers/Xhci/RenesasFirmwarePD720202/RenesasFirmwarePD720202.inf
!endif
