## @file
# Component description file for QNCInit driver.
#
# QNCInit driver implement QuarkNcSocId related drivers, includes:
# PciHostBridge, PciExpress, SmmAccess driver and LegacyRegion driver.
#
# This driver mainly do full initialization for the QNC chipet includes:
# 1. Initialize the PCI Express device.
# 2. Initialize the PciHostBridge, and allocate the I/O and memory space from GCD service.
# 3. Initialize the SmmAccess module and install EFI_SMM_ACCESS_PROTOCOL
# 4. Initialize the LegacyRegion module, install EFI_LEGACY_REGION_PROTOCOL and set below 1M
#    memory attribute from MTRR.
#
# Copyright (c) 2013 - 2018, Intel Corporation. All rights reserved.<BR>
#
# SPDX-License-Identifier: BSD-2-Clause-Patent
#
##

[Defines]
  INF_VERSION                    = 0x00010005
  BASE_NAME                      = QNCInitDxe
  FILE_GUID                      = 74D3B506-EE9C-47ed-B749-41261401DA78
  MODULE_TYPE                    = DXE_DRIVER
  VERSION_STRING                 = 1.0
  ENTRY_POINT                    = QNCInit

#
# The following information is for reference only and not required by the build tools.
#
#  VALID_ARCHITECTURES           = IA32 X64 EBC
#

[Sources]
  LegacyRegion.h
  LegacyRegion.c
  DxeQNCSmbus.c
  DxeQNCSmbus.h
  QNCSmbusExec.c
  QNCSmbus.h
  QNCInit.c
  QNCInit.h
  CommonHeader.h
  QNCRootPorts.c

[Packages]
  MdePkg/MdePkg.dec
  UefiCpuPkg/UefiCpuPkg.dec
  QuarkSocPkg/QuarkSocPkg.dec

[LibraryClasses]
  UefiDriverEntryPoint
  BaseLib
  UefiBootServicesTableLib
  DxeServicesTableLib
  BaseMemoryLib
  DebugLib
  PcdLib
  MtrrLib
  IoLib
  SmbusLib
  S3IoLib
  S3BootScriptLib
  IntelQNCLib
  QNCAccessLib

[Protocols]
  gEfiLegacyRegion2ProtocolGuid                 # PROTOCOL ALWAYS_PRODUCED
  gEfiSmbusHcProtocolGuid                       # PROTOCOL ALWAYS_PRODUCED
  gEfiQncS3SupportProtocolGuid                  # PROTOCOL ALWAYS_CONSUMED

[FeaturePcd]
  gEfiQuarkNcSocIdTokenSpaceGuid.PcdSmbaIoBaseAddressFixed

[FixedPcd]
  gEfiQuarkNcSocIdTokenSpaceGuid.PcdIoApicBaseAddress
  gEfiQuarkNcSocIdTokenSpaceGuid.PcdIoApicSize
  gEfiQuarkNcSocIdTokenSpaceGuid.PcdHpetBaseAddress
  gEfiQuarkNcSocIdTokenSpaceGuid.PcdHpetSize

[Pcd]
  gUefiCpuPkgTokenSpaceGuid.PcdCpuApStackSize                           ## CONSUMES
  gUefiCpuPkgTokenSpaceGuid.PcdCpuS3DataAddress|0x0|UINT64|0x60000010   ## PRODUCES
  gEfiMdePkgTokenSpaceGuid.PcdPciExpressBaseAddress                     ## CONSUMES
  gEfiQuarkNcSocIdTokenSpaceGuid.PcdPciExpressSize                      ## CONSUMES
  gEfiQuarkNcSocIdTokenSpaceGuid.PcdSmbaIoBaseAddress
  gEfiQuarkNcSocIdTokenSpaceGuid.PcdDeviceEnables
  gEfiQuarkNcSocIdTokenSpaceGuid.PcdPlatformSmbusAddrNum
  gEfiQuarkNcSocIdTokenSpaceGuid.PcdPlatformSmbusAddrTable

[Depex]
  gEfiPlatformPolicyProtocolGuid AND gEfiQncS3SupportProtocolGuid
