/** @file
  Differentiated System Description Table Fields (DSDT)

  Copyright (c) 2014, ARM Ltd. All rights reserved.<BR>
  Copyright (c) 2018, Hisilicon Limited. All rights reserved.<BR>
  Copyright (c) 2015, Linaro Limited. All rights reserved.<BR>
    SPDX-License-Identifier: BSD-2-Clause-Patent

  Based on the files under ArmPlatformPkg/ArmJunoPkg/AcpiTables/

**/
Scope(_SB)
{
  Device(LOC0) {
    Name(_HID, "HISI02F1")
    Name(_UID, 0)
    Name (_CRS, ResourceTemplate ()  {
      Interrupt(ResourceConsumer, Level, ActiveHigh, Exclusive)
      {
        488,489
      }
    })
  }

  Device(MCT0) {
    Name(_HID, "HISI0301")
    Name(_UID, 0)
    Name (_CRS, ResourceTemplate ()  {
      Interrupt (ResourceConsumer, Edge, ActiveHigh, Exclusive, 0, "\\_SB.MBI4")
      {
        656
      }
    })
  }
}
