### @file
# This module will perform specific PCI-Express devices
# resource configuration.
#
# Copyright (c) 2018, Intel Corporation. All rights reserved.<BR>
#
# SPDX-License-Identifier: BSD-2-Clause-Patent
#
###

[Defines]
  INF_VERSION                    = 0x00010017
  BASE_NAME                      = PciHotPlug
  FILE_GUID                      = 3022E512-B94A-4F12-806D-7EF1177899D8
  VERSION_STRING                 = 1.0
  MODULE_TYPE                    = DXE_DRIVER
  ENTRY_POINT                    = PciHotPlug
#
# The following information is for reference only and not required by the build tools.
#
# VALID_ARCHITECTURES = IA32 X64 EBC
#

[LibraryClasses]
  UefiDriverEntryPoint
  UefiBootServicesTableLib
  UefiRuntimeServicesTableLib
  BaseMemoryLib
  MemoryAllocationLib
  DevicePathLib
  DebugLib
  UefiLib
  HobLib
  PchPcieRpLib
  ConfigBlockLib
  TbtCommonLib

[Packages]
  MdePkg/MdePkg.dec
  MinPlatformPkg/MinPlatformPkg.dec
  KabylakeOpenBoardPkg/OpenBoardPkg.dec
  KabylakeSiliconPkg/SiPkg.dec

[Sources]
  PciHotPlug.c
  PciHotPlug.h

[Protocols]
  gEfiPciHotPlugInitProtocolGuid                ## PRODUCES
  gSaPolicyProtocolGuid                         ## CONSUMES

[Guids]
  gEfiHobListGuid                               ## CONSUMES
  gPcieRpConfigGuid                  ## CONSUMES

[Pcd]
 gBoardModuleTokenSpaceGuid.PcdPchPcieRootPortHpe

[Depex]
  gDxeTbtPolicyProtocolGuid
