/** @file

  Serial Port Console Redirection Table
  © 2000 - 2014 Microsoft Corporation. All rights reserved.
  http://go.microsoft.com/fwlink/?linkid=403368

  Copyright (c) 2014 - 2016, AMD Inc. All rights reserved.

  SPDX-License-Identifier: BSD-2-Clause-Patent

**/

#include <IndustryStandard/SerialPortConsoleRedirectionTable.h>

#include "AcpiPlatform.h"

#pragma pack(push, 1)

#define EFI_ACPI_SERIAL_PORT_CONSOLE_REDIRECTION_TABLE_INTERFACE_TYPE_PL011   3

STATIC EFI_ACPI_SERIAL_PORT_CONSOLE_REDIRECTION_TABLE AcpiSpcr = {
  //
  // Header
  //
  AMD_ACPI_HEADER (EFI_ACPI_5_0_SERIAL_PORT_CONSOLE_REDIRECTION_TABLE_SIGNATURE,
                   EFI_ACPI_SERIAL_PORT_CONSOLE_REDIRECTION_TABLE,
                   2), /* New MS definition for PL011 support */
  //
  // InterfaceType
  //
  EFI_ACPI_SERIAL_PORT_CONSOLE_REDIRECTION_TABLE_INTERFACE_TYPE_PL011,
  //
  // Reserved[3]
  //
  {EFI_ACPI_RESERVED_BYTE, EFI_ACPI_RESERVED_BYTE, EFI_ACPI_RESERVED_BYTE},
  //
  // BaseAddress
  //
  AMD_GASN(FixedPcdGet64(PcdSerialRegisterBase)),
  //
  // InterruptType
  //
  0,
  //
  // Irq
  //
  0,
  //
  // GlobalSystemInterrupt
  //
  0x148,
  //
  // BaudRate
  //
  EFI_ACPI_SERIAL_PORT_CONSOLE_REDIRECTION_TABLE_BAUD_RATE_115200,
  //
  // Parity
  //
  EFI_ACPI_SERIAL_PORT_CONSOLE_REDIRECTION_TABLE_PARITY_NO_PARITY,
  //
  // StopBits
  //
  EFI_ACPI_SERIAL_PORT_CONSOLE_REDIRECTION_TABLE_STOP_BITS_1,
  //
  // FlowControl
  //
  0,
  //
  // TerminalType
  //
  EFI_ACPI_SERIAL_PORT_CONSOLE_REDIRECTION_TABLE_TERMINAL_TYPE_ANSI,
  //
  // Language
  //
  EFI_ACPI_RESERVED_BYTE,
  //
  // PciDeviceId
  //
  0xFFFF,
  //
  // PciVendorId
  //
  0xFFFF,
  //
  // PciBusNumber
  //
  0x00,
  //
  // PciDeviceNumber
  //
  0x00,
  //
  // PciFunctionNumber
  //
  0x00,
  //
  // PciFlags
  //
  0,
  //
  // PciSegment
  //
  0,
  //
  // Reserved2
  //
  EFI_ACPI_RESERVED_DWORD
};

#pragma pack(pop)

VOID* CONST ReferenceAcpiTable = &AcpiSpcr;
