/** @file

  Serial Port Console Redirection Table
  (c) 2000 - 2014 Microsoft Corporation. All rights reserved.
  http://go.microsoft.com/fwlink/?linkid=403368

  Copyright (c) 2014 - 2016, AMD Inc. All rights reserved.
  Copyright (c) 2018, Linaro Ltd. All rights reserved.

  SPDX-License-Identifier: BSD-2-Clause-Patent

**/

#include <IndustryStandard/Acpi61.h>
#include <IndustryStandard/SerialPortConsoleRedirectionTable.h>
#include <Platform/MemoryMap.h>

#include "AcpiTables.h"

#pragma pack(push, 1)

STATIC EFI_ACPI_SERIAL_PORT_CONSOLE_REDIRECTION_TABLE Spcr = {
  //
  // Header
  //
  __ACPI_HEADER (EFI_ACPI_5_0_SERIAL_PORT_CONSOLE_REDIRECTION_TABLE_SIGNATURE,
                 EFI_ACPI_SERIAL_PORT_CONSOLE_REDIRECTION_TABLE,
                 2), /* New MS definition for PL011 support */
  //
  // InterfaceType
  //
  EFI_ACPI_SERIAL_PORT_CONSOLE_REDIRECTION_TABLE_INTERFACE_TYPE_ARM_PL011_UART,
  //
  // Reserved[3]
  //
  { EFI_ACPI_RESERVED_BYTE, EFI_ACPI_RESERVED_BYTE, EFI_ACPI_RESERVED_BYTE },
  //
  // BaseAddress
  //
  {
    EFI_ACPI_5_1_SYSTEM_MEMORY,
    32,
    0,
    EFI_ACPI_5_1_DWORD,
    SYNQUACER_UART0_BASE
  },
  //
  // InterruptType
  //
  EFI_ACPI_SERIAL_PORT_CONSOLE_REDIRECTION_TABLE_INTERRUPT_TYPE_GIC,
  //
  // Irq
  //
  0,
  //
  // GlobalSystemInterrupt
  //
  95,
  //
  // BaudRate
  //
  EFI_ACPI_SERIAL_PORT_CONSOLE_REDIRECTION_TABLE_BAUD_RATE_115200,
  //
  // Parity
  //
  EFI_ACPI_SERIAL_PORT_CONSOLE_REDIRECTION_TABLE_PARITY_NO_PARITY,
  //
  // StopBits
  //
  EFI_ACPI_SERIAL_PORT_CONSOLE_REDIRECTION_TABLE_STOP_BITS_1,
  //
  // FlowControl
  //
  0,
  //
  // TerminalType
  //
  EFI_ACPI_SERIAL_PORT_CONSOLE_REDIRECTION_TABLE_TERMINAL_TYPE_ANSI,
  //
  // Language
  //
  EFI_ACPI_RESERVED_BYTE,
  //
  // PciDeviceId
  //
  0xFFFF,
  //
  // PciVendorId
  //
  0xFFFF,
  //
  // PciBusNumber
  //
  0x00,
  //
  // PciDeviceNumber
  //
  0x00,
  //
  // PciFunctionNumber
  //
  0x00,
  //
  // PciFlags
  //
  0,
  //
  // PciSegment
  //
  0,
  //
  // Reserved2
  //
  EFI_ACPI_RESERVED_DWORD
};

#pragma pack(pop)

//
// Reference the table being generated to prevent the optimizer from removing
// the data structure from the executable
//
VOID* CONST ReferenceAcpiTable = &Spcr;
