/*
 * Copyright (c) 2016 Linaro Limited
 * Copyright (c) 2016 Hisilicon Limited
 *. All rights reserved.
 * SPDX-License-Identifier: BSD-2-Clause-Patent
 *
 * Contributors:
 *     Yi Li - yi.li@linaro.org
*/

#include <IndustryStandard/Acpi.h>
#include "Hi1616Platform.h"

#define EFI_ACPI_SYSTEM_LOCALITIES_ENTRY_COUNT 0x0000000000000004

#pragma pack(1)
typedef struct {
  UINT8   Entry[EFI_ACPI_SYSTEM_LOCALITIES_ENTRY_COUNT];
} EFI_ACPI_6_1_NUMBER_OF_SYSTEM_LOCALITIES_STRUCTURE;

typedef struct {
  EFI_ACPI_6_1_SYSTEM_LOCALITY_DISTANCE_INFORMATION_TABLE_HEADER    Header;
  EFI_ACPI_6_1_NUMBER_OF_SYSTEM_LOCALITIES_STRUCTURE                NumSlit[EFI_ACPI_SYSTEM_LOCALITIES_ENTRY_COUNT];

} EFI_ACPI_6_1_SYSTEM_LOCALITY_INFORMATION_TABLE;
#pragma pack()

//
// System Locality Information Table
// Please modify all values in Slit.h only.
//
EFI_ACPI_6_1_SYSTEM_LOCALITY_INFORMATION_TABLE Slit = {
  {
    {
      EFI_ACPI_6_1_SYSTEM_LOCALITY_INFORMATION_TABLE_SIGNATURE,
      sizeof (EFI_ACPI_6_1_SYSTEM_LOCALITY_INFORMATION_TABLE),
      EFI_ACPI_6_1_SYSTEM_LOCALITY_DISTANCE_INFORMATION_TABLE_REVISION,
      0x00,                                                     // Checksum will be updated at runtime
      {EFI_ACPI_ARM_OEM_ID},
      EFI_ACPI_ARM_OEM_TABLE_ID,
      EFI_ACPI_ARM_OEM_REVISION,
      EFI_ACPI_ARM_CREATOR_ID,
      EFI_ACPI_ARM_CREATOR_REVISION,
    },
    //
    // Beginning of SLIT specific fields
    //
    EFI_ACPI_SYSTEM_LOCALITIES_ENTRY_COUNT,
  },
  {
    {{0x0A, 0x0F, 0x14, 0x14}}, //Locality   0
    {{0x0F, 0x0A, 0x14, 0x14}}, //Locality   1
    {{0x14, 0x14, 0x0A, 0x0F}}, //Locality   2
    {{0x14, 0x14, 0x0F, 0x0A}}, //Locality   3
  },
};

//
// Reference the table being generated to prevent the optimizer from removing the
// data structure from the executable
//
VOID* CONST ReferenceAcpiTable = &Slit;
