From 11aa07ed939193e85516c287a57dee1837242972 Mon Sep 17 00:00:00 2001
From: Thomas Haller <thaller@redhat.com>
Date: Mon, 4 Jan 2016 18:54:26 +0100
Subject: [PATCH 1/7] core: fix failure to configure routes due to wrong
 device-route for IPv4 peer-addresses

As in the case of a OpenVPN connection, we might add an address like:
  10.8.0.58/32 ptp 10.8.0.57

In this case, kernel would automatically add a device-route like:
  10.8.0.57/32 via 0.0.0.0 dev 32 metric 0 mss 0 src rtprot-kernel scope link pref-src 10.8.0.58

nm_ip4_config_commit() checks all IP addresses to figure out
the present device-routes. Then the routes are synced by NMRouteManager.
Due to a bug, we would not consider the peer-address, but the local-address
and configure a route 10.8.0.58/32, instead of 10.8.0.57/32.

That stays mostly unnoticed, because usually the peer and the local-address are
in the same subnet, so that there is no difference (/32 is an example of the
peer-address being in a different subnet).

It also seems that due to a bug fixed by df4e5357521 this issue didn't surface.
Probably because we would not notice the 10.8.0.57/32 right away and thus
nm_route_manager_ip4_route_sync() would not wrongly delete it.

https://bugzilla.gnome.org/show_bug.cgi?id=759892

https://bugs.debian.org/cgi-bin/bugreport.cgi?bug=809195
https://bugs.debian.org/cgi-bin/bugreport.cgi?bug=809494
https://bugs.debian.org/cgi-bin/bugreport.cgi?bug=809526
https://bugs.archlinux.org/task/47535
https://bugzilla.redhat.com/show_bug.cgi?id=1294309
https://mail.gnome.org/archives/networkmanager-list/2015-December/msg00059.html
---
 src/nm-ip4-config.c | 3 ++-
 1 file changed, 2 insertions(+), 1 deletion(-)

diff --git a/src/nm-ip4-config.c b/src/nm-ip4-config.c
index f625d35..61e29af 100644
--- a/src/nm-ip4-config.c
+++ b/src/nm-ip4-config.c
@@ -298,7 +298,8 @@ nm_ip4_config_commit (const NMIP4Config *config, int ifindex, gboolean routes_fu
 
 				route.ifindex = ifindex;
 				route.source = NM_IP_CONFIG_SOURCE_KERNEL;
-				route.network = nm_utils_ip4_address_clear_host_address (addr->address, addr->plen);
+				route.network = nm_utils_ip4_address_clear_host_address (addr->peer_address ? : addr->address,
+				                                                         addr->plen);
 				route.plen = addr->plen;
 				route.pref_src = addr->address;
 				route.metric = default_route_metric;
-- 
2.5.0

