SUMMARY = "USB hub per-port power control"
HOMEPAGE = "https://github.com/mvp/uhubctl"
BUGTRACKER = "https://github.com/mvp/uhubctl/issues"
DEPENDS = "libusb1"

LICENSE = "GPLv2"
LIC_FILES_CHKSUM = "file://COPYING;md5=b234ee4d69f5fce4486a80fdaf4a4263"

SRCREV = "1b52efddbd68b4395df3ac9cd10eeb984af22439"
SRC_URI = "git://github.com/mvp/${BPN}"
S = "${WORKDIR}/git"

# uhubctl gets its program version from "git describe". As we use the source
# archive do reduce download size replace the call with our hardcoded version.
do_configure_append() {
    sed -i "s/^\(GIT_VERSION :=\).*$/\1 ${PV}/g" ${S}/Makefile
}

do_install () {
    oe_runmake install DESTDIR=${D}
}
