# Australia / Sutherland
#
# Australia modulation params:
# - http://www.dba.org.au/index.asp?sectionID=120
#
#
# North (Broadcast Site Escarpment Road BROKERS NOSE)
# - http://www.dba.org.au/index.asp?query=true&sectionID=22&recLocation=Wollongong+%2D+North
#
#Channel 7 stations
[CHANNEL]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 177500000
	BANDWIDTH_HZ = 7000000
	CODE_RATE_HP = 3/4
	CODE_RATE_LP = NONE
	MODULATION = QAM/64
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/16
	HIERARCHY = NONE
	INVERSION = AUTO

#Channel 9 bundle
# T 191500000 7MHz AUTO AUTO AUTO AUTO AUTO AUTO
#One and Channel 10
[CHANNEL]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 219500000
	BANDWIDTH_HZ = 7000000
	CODE_RATE_HP = 3/4
	CODE_RATE_LP = NONE
	MODULATION = QAM/64
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/16
	HIERARCHY = NONE
	INVERSION = AUTO

#Aunty
[CHANNEL]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 226500000
	BANDWIDTH_HZ = 7000000
	CODE_RATE_HP = 3/4
	CODE_RATE_LP = NONE
	MODULATION = QAM/64
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/16
	HIERARCHY = NONE
	INVERSION = AUTO

#SBS
[CHANNEL]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 571500000
	BANDWIDTH_HZ = 7000000
	CODE_RATE_HP = 3/4
	CODE_RATE_LP = NONE
	MODULATION = QAM/64
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/16
	HIERARCHY = NONE
	INVERSION = AUTO

