# Hong Kong (DMB-TH)

# TVB (band 35)
[CHANNEL]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 586000000
	BANDWIDTH_HZ = 8000000
	CODE_RATE_HP = AUTO
	CODE_RATE_LP = NONE
	MODULATION = QAM/64
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/32
	HIERARCHY = NONE
	INVERSION = AUTO

# ATV (band 37)
[CHANNEL]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 602000000
	BANDWIDTH_HZ = 8000000
	CODE_RATE_HP = AUTO
	CODE_RATE_LP = NONE
	MODULATION = QAM/64
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/32
	HIERARCHY = NONE
	INVERSION = AUTO


# Simulcast (band 22)
[CHANNEL]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 482000000
	BANDWIDTH_HZ = 8000000
	CODE_RATE_HP = AUTO
	CODE_RATE_LP = NONE
	MODULATION = QAM/64
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/32
	HIERARCHY = NONE
	INVERSION = AUTO

# Simulcast (band 30)
[CHANNEL]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 546000000
	BANDWIDTH_HZ = 8000000
	CODE_RATE_HP = AUTO
	CODE_RATE_LP = NONE
	MODULATION = QAM/64
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/32
	HIERARCHY = NONE
	INVERSION = AUTO

# Simulcast (band 32)
[CHANNEL]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 562000000
	BANDWIDTH_HZ = 8000000
	CODE_RATE_HP = AUTO
	CODE_RATE_LP = NONE
	MODULATION = QAM/64
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/32
	HIERARCHY = NONE
	INVERSION = AUTO

# Simulcast (band 40)
[CHANNEL]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 628000000
	BANDWIDTH_HZ = 8000000
	CODE_RATE_HP = AUTO
	CODE_RATE_LP = NONE
	MODULATION = QAM/64
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/32
	HIERARCHY = NONE
	INVERSION = AUTO

# Simulcast (band 43)
[CHANNEL]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 650000000
	BANDWIDTH_HZ = 8000000
	CODE_RATE_HP = AUTO
	CODE_RATE_LP = NONE
	MODULATION = QAM/64
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/32
	HIERARCHY = NONE
	INVERSION = AUTO

