# in OE we use TARGET_CC_ARCH="-march=mips32" but by
# default uclibc uses mips1 ISA for o32 ABI which ends
# up with conflicting march options to gcc. Here we
# ask for MIPS32 ISA to match the OE defaults

CONFIG_MIPS_ISA_MIPS32=y

# Below options are exact copy of general
# uClibc.machine file
#
FORCE_OPTIONS_FOR_ARCH=y
ARCH_HAS_MMU=y
ARCH_USE_MMU=y
KERNEL_HEADERS="/usr/include"
HAVE_DOT_CONFIG=y

